
[image: ./media/logo.png]
	oneM2M Technical Specification

	Document Number
	oneM2M-TS-0018-V-4.6.1

	Document Name:
	Test Suite Structure and Test Purposes

	Date:
	2025-09-07

	Abstract:
	The Test Suite Structure and Test Purposes document for conformance testing consists of: - Defining the test suite structure by grouping the test purposes according to different criteria; - Specifying test purposes for conformance test. A test purpose is an informal description of the expected test behaviour.

	Template Version: 23 February 2015 (Do not modify)



This Specification is provided for future development work within oneM2M only. The Partners accept no liability for any use of this Specification.
The present document has not been subject to any approval process by the oneM2M Partners Type 1. Published oneM2M specifications and reports for implementation should be obtained via the oneM2M Partners' Publications Offices.

About oneM2M
The purpose and goal of oneM2M is to develop technical specifications which address the need for a common M2M Service Layer that can be readily embedded within various hardware and software, and relied upon to connect the myriad of devices in the field with M2M application servers worldwide.
More information about oneM2M may be found at: http//www.oneM2M.org
Copyright Notification
© 2016, oneM2M Partners Type 1 (ARIB, ATIS, CCSA, ETSI, TIA, TSDSI, TTA, TTC).
All rights reserved.
The copyright extends to reproduction in all media.
Notice of Disclaimer & Limitation of Liability
The information provided in this document is directed solely to professionals who have the appropriate degree of experience to understand and interpret its contents in accordance with generally accepted engineering or other professional standards and applicable regulations. No recommendation as to products or vendors is made or should be implied.
NO REPRESENTATION OR WARRANTY IS MADE THAT THE INFORMATION IS TECHNICALLY ACCURATE OR SUFFICIENT OR CONFORMS TO ANY STATUTE, GOVERNMENTAL RULE OR REGULATION, AND FURTHER, NO REPRESENTATION OR WARRANTY IS MADE OF MERCHANTABILITY OR FITNESS FOR ANY PARTICULAR PURPOSE OR AGAINST INFRINGEMENT OF INTELLECTUAL PROPERTY RIGHTS. NO oneM2M PARTNER TYPE 1 SHALL BE LIABLE, BEYOND THE AMOUNT OF ANY SUM RECEIVED IN PAYMENT BY THAT PARTNER FOR THIS DOCUMENT, WITH RESPECT TO ANY CLAIM, AND IN NO EVENT SHALL oneM2M BE LIABLE FOR LOST PROFITS OR OTHER INCIDENTAL OR CONSEQUENTIAL DAMAGES. oneM2M EXPRESSLY ADVISES ANY AND ALL USE OF OR RELIANCE UPON THIS INFORMATION PROVIDED IN THIS DOCUMENT IS AT THE RISK OF THE USER.
Contents
1 Scope
2 References
    2.1 Normative references
    2.2 Informative references
3 Definitions and abbreviations
    3.1 Definitions
    3.2 Abbreviations
4 Conventions
5 Prerequisites and Test Configurations
    5.1 Test Configurations
6 Test Suite Structure (TSS)
    6.1 Test groups
    6.1.1 Functional Entity Groups
        6.1.2 Common Services Functions Subgroups
        6.1.3 oneM2M Resource Primitives specific Operations
    6.2 Test Suite Structure (TSS) for oneM2M
7 Test Purposes (TP)
    7.1 Introduction
        7.1.1 TP definition conventions
        7.1.2 TP Identifier naming conventions
        7.1.3 Rules for the behaviour description
        7.1.4 ICS reference
PICS Items
    7.2 Test Purposes for oneM2M Service Primitives
        7.2.1 Group AE (AE)
            7.2.1.1 General Capability (GEN)
                7.2.1.1.1 CREATE Operation
                    TP/oneM2M/AE/GEN/CRE/001
                    TP/oneM2M/AE/GEN/CRE/002
                7.2.1.1.2 UPDATE Operation
                    TP/oneM2M/AE/GEN/UPD/001
                    TP/oneM2M/AE/GEN/UPD/002
                7.2.1.1.3 RETRIEVE Operation
                    TP/oneM2M/AE/GEN/RET/001
                    TP/oneM2M/AE/GEN/RET/002
                7.2.1.1.4 DELETE Operation
                    TP/oneM2M/AE/GEN/DEL/001
                    TP/oneM2M/AE/GEN/DEL/002
            7.2.1.2 Registration (REG)
                7.2.1.2.1 CREATE Operation
                    TP/oneM2M/AE/REG/CRE/001
                    TP/oneM2M/AE/REG/CRE/002
                    Editor's Note: Reference need to be checked
                7.2.1.2.2 DELETE Operation
                    TP/oneM2M/AE/REG/DEL/001
            7.2.1.3 Data Management and Repository (DMR)
                7.2.1.3.1 CREATE Operation
                    TP/oneM2M/AE/DMR/CRE/001
                    TP/oneM2M/AE/DMR/CRE/002
                    TP/oneM2M/AE/DMR/CRE/003
                    TP/oneM2M/AE/DMR/CRE/004
                7.2.1.3.2 UPDATE Operation
                    TP/oneM2M/AE/DMR/UPD/001
                    TP/oneM2M/AE/DMR/UPD/002
                7.2.1.3.3 RETRIEVE Operation
                    TP/oneM2M/AE/DMR/RET/001
                    TP/oneM2M/AE/DMR/RET/002
                    TP/oneM2M/AE/DMR/RET/003
                    TP/oneM2M/AE/DMR/RET/004
                    TP/oneM2M/AE/DMR/RET/005
                7.2.1.3.4 DELETE Operation
                    TP/oneM2M/AE/DMR/DEL/001
                    TP/oneM2M/AE/DMR/DEL/002
                    TP/oneM2M/AE/DMR/DEL/003
                    TP/oneM2M/AE/DMR/DEL/004
            7.2.1.4 Subscription and Notification (SUB)
                7.2.1.4.1 CREATE Operation
                    TP/oneM2M/AE/SUB/CRE/001
                    TP/oneM2M/AE/SUB/CRE/002
                    TP/oneM2M/AE/SUB/CRE/003
                7.2.1.4.2 NOTIFY Operation
                    TP/oneM2M/AE/SUB/NTF/001
                    TP/oneM2M/AE/SUB/NTF/002
            7.2.1.5 Communication Management and Delivery Handling (CMDH)
                7.2.1.5.1 Resource pollingChannel (PCH)
                    TP/oneM2M/AE/PCH/001
                    TP/oneM2M/AE/PCH/002
            7.2.1.6 Ontology based Interworking IPE (OBI)
                7.2.1.6.1 Initialization sequence
                7.2.1.6.2 CREATE Operation
                7.2.1.6.3 RETRIEVE Operation
            7.2.1.7 Home Appliance Information Model and Mapping (HAIM)
                7.2.1.7.1 CREATE Operation
            7.2.1.8 Security (SEC)
                7.2.1.8.1 Authentication
                7.2.1.8.1.1 ESPrim (ESP)
                    7.2.1.8.1.1.1 NOTIFY Operation
                    7.2.1.8.1.1.2 RETRIEVE Operation
                    7.2.1.8.1.2.1 CREATE Operation
                    7.2.1.8.1.3.1 NOTIFY Operation
        7.2.2 Group CSE (CE)
            7.2.2.1 General Capability (GEN)
                7.2.2.1.1 CREATE Operation
                    TP/oneM2M/CSE/GEN/CRE/001
                    TP/oneM2M/CSE/GEN/CRE/002
                    TP/oneM2M/CSE/GEN/CRE/003
                    TP/oneM2M/CSE/GEN/CRE/004
                7.2.2.1.2 UPDATE Operation
                    TP/oneM2M/CSE/GEN/UPD/001
                    TP/oneM2M/CSE/GEN/UPD/002
                    TP/oneM2M/CSE/GEN/UPD/003
                    TP/oneM2M/CSE/GEN/UPD/004
                7.2.2.1.3 RETRIEVE Operation
                    TP/oneM2M/CSE/GEN/RET/001
                    TP/oneM2M/CSE/GEN/RET/002
                    TP/oneM2M/CSE/GEN/RET/003
                    TP/oneM2M/CSE/GEN/RET/004
                7.2.2.1.4 DELETE Operation
                    TP/oneM2M/CSE/GEN/DEL/001
                    TP/oneM2M/CSE/GEN/DEL/002
                    TP/oneM2M/CSE/GEN/DEL/003
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            7.2.2.3 Data Management and Repository Function (DMR)
                7.2.2.3.1 RETRIEVE Operation
                    TP/oneM2M/CSE/DMR/RET/001
                    TP/oneM2M/CSE/DMR/RET/002
                    TP/oneM2M/CSE/DMR/RET/003
                    TP/oneM2M/CSE/DMR/RET/004
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                    TP/oneM2M/CSE/DMR/RET/011
                    TP/oneM2M/CSE/DMR/RET/012
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                    TP/oneM2M/CSE/DMR/RET/023
                    TP/oneM2M/CSE/DMR/RET/024
                    TP/oneM2M/CSE/DMR/RET/025
                    TP/oneM2M/CSE/DMR/RET/028
                    TP/oneM2M/CSE/DMR/RET/029
                7.2.2.3.2 UPDATE Operation
                    TP/oneM2M/CSE/DMR/UPD/001
                    TP/oneM2M/CSE/DMR/UPD/002
                    TP/oneM2M/CSE/DMR/UPD/003
                    TP/oneM2M/CSE/DMR/UPD/004
                    TP/oneM2M/CSE/DMR/UPD/005
                    TP/oneM2M/CSE/DMR/UPD/006
                    TP/oneM2M/CSE/DMR/UPD/007
                    TP/oneM2M/CSE/DMR/UPD/008
                    TP/oneM2M/CSE/DMR/UPD/009
                    TP/oneM2M/CSE/DMR/UPD/010
                    TP/oneM2M/CSE/DMR/UPD/011
                    TP/oneM2M/CSE/DMR/UPD/012
                    TP/oneM2M/CSE/DMR/UPD/013
                    TP/oneM2M/CSE/DMR/UPD/014
                    TP/oneM2M/CSE/DMR/UPD/015
                    TP/oneM2M/CSE/DMR/UPD/016
                    TP/oneM2M/CSE/DMR/UPD/017
                    TP/oneM2M/CSE/DMR/UPD/018
                7.2.2.3.3 CREATE Operation
                    TP/oneM2M/CSE/DMR/CRE/001
                    TP/oneM2M/CSE/DMR/CRE/002
                    TP/oneM2M/CSE/DMR/CRE/003
                    TP/oneM2M/CSE/DMR/CRE/004
                    TP/oneM2M/CSE/DMR/CRE/005
                    TP/oneM2M/CSE/DMR/CRE/006
                    TP/oneM2M/CSE/DMR/CRE/007
                    TP/oneM2M/CSE/DMR/CRE/008
                    TP/oneM2M/CSE/DMR/CRE/009
                    TP/oneM2M/CSE/DMR/CRE/010
                    TP/oneM2M/CSE/DMR/CRE/011
                    TP/oneM2M/CSE/DMR/CRE/012
                    TP/oneM2M/CSE/DMR/CRE/013
                    TP/oneM2M/CSE/DMR/CRE/014
                    TP/oneM2M/CSE/DMR/CRE/015
                    TP/oneM2M/CSE/DMR/CRE/016
                    TP/oneM2M/CSE/DMR/CRE/017
                    TP/oneM2M/CSE/DMR/CRE/018
                    TP/oneM2M/CSE/DMR/CRE/021
                    TP/oneM2M/CSE/DMR/CRE/022
                    TP/oneM2M/CSE/DMR/CRE/023
                7.2.2.3.4 DELETE Operation
                    TP/oneM2M/CSE/DMR/DEL/001
                    TP/oneM2M/CSE/DMR/DEL/002
                    TP/oneM2M/CSE/DMR/DEL/003
                    TP/oneM2M/CSE/DMR/DEL/004
                    TP/oneM2M/CSE/DMR/DEL/005
                    TP/oneM2M/CSE/DMR/DEL/006
                    TP/oneM2M/CSE/DMR/DEL/007
                    TP/oneM2M/CSE/DMR/DEL/008
                    TP/oneM2M/CSE/DMR/DEL/009
                    TP/oneM2M/CSE/DMR/DEL/010
                7.2.2.3.5 BASIC Operation
            7.2.2.4 Subscription and Notification (SUB)
                7.2.2.4.1 CREATE Operation
                    TP/oneM2M/CSE/SUB/CRE/001
                    TP/oneM2M/CSE/SUB/CRE/002
                    TP/oneM2M/CSE/SUB/CRE/003
                    TP/oneM2M/CSE/SUB/CRE/004
                    TP/oneM2M/CSE/SUB/CRE/005
                    TP/oneM2M/CSE/SUB/CRE/006
                    TP/oneM2M/CSE/SUB/CRE/007
                    TP/oneM2M/CSE/SUB/CRE/008
                7.2.2.4.2 DELETE Operation
                    TP/oneM2M/CSE/SUB/DEL/001
                    TP/oneM2M/CSE/SUB/DEL/002
                    TP/oneM2M/CSE/SUB/DEL/003
                7.2.2.4.3 UPDATE Operation
                    TP/oneM2M/CSE/SUB/UPD/001
                    TP/oneM2M/CSE/SUB/UPD/002
                    TP/oneM2M/CSE/SUB/UPD/003
                    TP/oneM2M/CSE/SUB/UPD/004
                    TP/oneM2M/CSE/SUB/UPD/005
                    TP/oneM2M/CSE/SUB/UPD/006
                    TP/oneM2M/CSE/SUB/UPD/007
                    TP/oneM2M/CSE/SUB/UPD/008
                    TP/oneM2M/CSE/SUB/UPD/009
                7.2.2.4.4 NOTIFY Operation
                    TP/oneM2M/CSE/SUB/NTF/001
                    TP/oneM2M/CSE/SUB/NTF/002
                    TP/oneM2M/CSE/SUB/NTF/003
                    TP/oneM2M/CSE/SUB/NTF/004
                    TP/oneM2M/CSE/SUB/NTF/005
                    TP/oneM2M/CSE/SUB/NTF/006
                    TP/oneM2M/CSE/SUB/NTF/007
                    TP/oneM2M/CSE/SUB/NTF/008
                    TP/oneM2M/CSE/SUB/NTF/009
                    TP/oneM2M/CSE/SUB/NTF/010
                    TP/oneM2M/CSE/SUB/NTF/011
                    TP/oneM2M/CSE/SUB/NTF/012
                    TP/oneM2M/CSE/SUB/NTF/013
                    TP/oneM2M/CSE/SUB/NTF/014
                    TP/oneM2M/CSE/SUB/NTF/015
                    TP/oneM2M/CSE/SUB/NTF/016
                    TP/oneM2M/CSE/SUB/NTF/017
                    TP/oneM2M/CSE/SUB/NTF/018
                    TP/oneM2M/CSE/SUB/NTF/019
                    TP/oneM2M/CSE/SUB/NTF/020
                    TP/oneM2M/CSE/SUB/NTF/021
                    TP/oneM2M/CSE/SUB/NTF/022
                    TP/oneM2M/CSE/SUB/NTF/023
                    TP/oneM2M/CSE/SUB/NTF/024
            7.2.2.5 Group Management (GMG)
                7.2.2.5.1 CREATE Operation
                    TP/oneM2M/CSE/GMG/CRE/001
                    TP/oneM2M/CSE/GMG/CRE/002
                    TP/oneM2M/CSE/GMG/CRE/003
                    TP/oneM2M/CSE/GMG/CRE/004
                    TP/oneM2M/CSE/GMG/CRE/005
                    TP/oneM2M/CSE/GMG/CRE/006
                    TP/oneM2M/CSE/GMG/CRE/007
                    TP/oneM2M/CSE/GMG/CRE/008
                7.2.2.5.2 UPDATE Operation
                    TP/oneM2M/CSE/GMG/UPD/001
                    TP/oneM2M/CSE/GMG/UPD/002
                    TP/oneM2M/CSE/GMG/UPD/003
                    TP/oneM2M/CSE/GMG/UPD/004
                    TP/oneM2M/CSE/GMG/UPD/005
                    TP/oneM2M/CSE/GMG/UPD/006
                    TP/oneM2M/CSE/GMG/UPD/007
                    TP/oneM2M/CSE/GMG/UPD/008
                    TP/oneM2M/CSE/GMG/UPD/009
                    TP/oneM2M/CSE/GMG/UPD/010
                7.2.2.5.3 RETRIEVE Operation
                    TP/oneM2M/CSE/GMG/RET/001
                7.2.2.5.4 BASIC OPERATION
                    TP/oneM2M/CSE/GMG/001
                    TP/oneM2M/CSE/GMG/002
                    TP/oneM2M/CSE/GMG/003
                    TP/oneM2M/CSE/GMG/004
                    TP/oneM2M/CSE/GMG/005
                    TP/oneM2M/CSE/GMG/006
                    TP/oneM2M/CSE/GMG/007
            7.2.2.6 Discovery (DIS)
                7.2.2.6.1 RETRIEVE Operation
                    TP/oneM2M/CSE/DIS/001
                    TP/oneM2M/CSE/DIS/002
                    TP/oneM2M/CSE/DIS/003
                    TP/oneM2M/CSE/DIS/004
                    TP/oneM2M/CSE/DIS/005
                    TP/oneM2M/CSE/DIS/006
                    TP/oneM2M/CSE/DIS/007
                    TP/oneM2M/CSE/DIS/008
                    TP/oneM2M/CSE/DIS/009
                    TP/oneM2M/CSE/DIS/031
                    TP/oneM2M/CSE/DIS/032
            7.2.2.7 Location (LOC)
                7.2.2.7.1 CREATE Operation
                    TP/oneM2M/CSE/LOC/CRE/001
                    TP/oneM2M/CSE/LOC/CRE/002
                    TP/oneM2M/CSE/LOC/CRE/003
                    TP/oneM2M/CSE/LOC/CRE/004
                    TP/oneM2M/CSE/LOC/CRE/005
                    TP/oneM2M/CSE/LOC/CRE/006
                    TP/oneM2M/CSE/LOC/CRE/007
                    TP/oneM2M/CSE/LOC/CRE/008
                    TP/oneM2M/CSE/LOC/CRE/009
                7.2.2.7.2 UPDATE Operation
                    TP/oneM2M/CSE/LOC/UPD/001
                7.2.2.7.3 RETRIEVE Operation
                    TP/oneM2M/CSE/LOC/RET/001
                    TP/oneM2M/CSE/LOC/RET/002
                    TP/oneM2M/CSE/LOC/RET/003
                    TP/oneM2M/CSE/LOC/RET/004
                    TP/oneM2M/CSE/LOC/RET/005
                7.2.2.7.4 NOTIFY Operation
                    TP/oneM2M/CSE/LOC/NTF/001
                    TP/oneM2M/CSE/LOC/NTF/002
            7.2.2.8 Device Management (DMG)
                7.2.2.8.1 Resource timeSeries (TS)
                    TP/oneM2M/CSE/TS/001
                    TP/oneM2M/CSE/TS/002
                    TP/oneM2M/CSE/TS/003
                    TP/oneM2M/CSE/TS/004
                    TP/oneM2M/CSE/TS/005
            7.2.2.9 Communication Management and Delivery Handling(CMDH)
                7.2.2.9.1 Resource pollingChannel (PCH)
                    TP/oneM2M/CSE/PCH/001
                    TP/oneM2M/CSE/PCH/002
                    TP/oneM2M/CSE/PCH/003
                    TP/oneM2M/CSE/PCH/004
                    TP/oneM2M/CSE/PCH/005
                    TP/oneM2M/CSE/PCH/006
                7.2.2.9.2 Response Type (RT)
                    7.2.2.9.2.1 nonBlockingRequestSynch (NBS)
                    TP/oneM2M/CSE/RT/NBS/001
                    TP/oneM2M/CSE/RT/NBS/002
                    TP/oneM2M/CSE/RT/NBS/003
                    7.2.2.9.2.2 nonBlockingRequestAsynch (NBA)
                    TP/oneM2M/CSE/RT/NBA/001
                    TP/oneM2M/CSE/RT/NBA/002
                    TP/oneM2M/CSE/RT/NBA/003
                    TP/oneM2M/CSE/RT/NBA/004
                    TP/oneM2M/CSE/RT/NBA/005
            7.2.2.10 Security(SEC)
                7.2.2.10.1 CREATE Operation
                    TP/oneM2M/CSE/SEC/ACP/CRE/001
                    TP/oneM2M/CSE/SEC/ACP/CRE/002
                    TP/oneM2M/CSE/SEC/ACP/CRE/003
                    TP/oneM2M/CSE/SEC/ACP/CRE/004
                    TP/oneM2M/CSE/SEC/ACP/CRE/005
                7.2.2.10.2 UPDATE Operation
                    TP/oneM2M/CSE/SEC/ACP/UPD/001
                    TP/oneM2M/CSE/SEC/ACP/UPD/002
                7.2.2.10.3 BASIC OPERATION
                    TP/oneM2M/CSE/SEC/ACP/001
                    TP/oneM2M/CSE/SEC/ACP/002
                    TP/oneM2M/CSE/SEC/ACP/003
                    TP/oneM2M/CSE/SEC/ACP/004
                    TP/oneM2M/CSE/SEC/ACP/005
                    TP/oneM2M/CSE/SEC/ACP/006
                    TP/oneM2M/CSE/SEC/ACP/007
                    TP/oneM2M/CSE/SEC/ACP/008
                    TP/oneM2M/CSE/SEC/ACP/009
                    TP/oneM2M/CSE/SEC/ACP/010
                    TP/oneM2M/CSE/SEC/ACP/011
                    TP/oneM2M/CSE/SEC/ACP/012
                    TP/oneM2M/CSE/SEC/ACP/013
                    TP/oneM2M/CSE/SEC/ACP/014
                    TP/oneM2M/CSE/SEC/ACP/015
                    TP/oneM2M/CSE/SEC/ACP/016
                    TP/oneM2M/CSE/SEC/ACP/017
                7.2.2.10.4 Authentication
                    7.2.2.10.4.1 ESPrim (ESP)
                        7.2.2.10.4.1.1 NOTIFY Operation
                        7.2.2.10.4.1.2 RETRIEVE Operation
                    7.2.2.10.4.2 Roles (ROL)
                        7.2.2.10.4.2.1 CREATE Operation
                        7.2.2.10.4.2.2 RETRIEVE Operation
                        7.2.2.10.4.2.3 UPDATE Operation
                        7.2.2.10.4.2.4 NOTIFY Operation
                    7.2.2.10.4.3 DAS (DAS)
                        7.2.2.10.4.3.1 NOTIFY Operation
                    7.2.2.10.4.4 ESCertKE (ESC)
                        7.2.2.10.4.4.1 NOTIFY Operation
            7.2.2.11 Resource Announcement (ANNC)
                7.2.2.11.1 BASIC Operation
                    TP/oneM2M/CSE/ANNC/001
                7.2.2.11.2 CREATE Operation
                    TP/oneM2M/CSE/ANNC/CRE/001
                    TP/oneM2M/CSE/ANNC/CRE/002
                    TP/oneM2M/CSE/ANNC/CRE/003
                    TP/oneM2M/CSE/ANNC/CRE/004
                    TP/oneM2M/CSE/ANNC/CRE/005
                    TP/oneM2M/CSE/ANNC/CRE/006
                    TP/oneM2M/CSE/ANNC/CRE/007
                    TP/oneM2M/CSE/ANNC/CRE/008
                    TP/oneM2M/CSE/ANNC/CRE/009
                7.2.2.11.3 RETRIEVE Operation
                    TP/oneM2M/CSE/ANNC/RET/001
                    TP/oneM2M/CSE/ANNC/RET/002
                7.2.2.11.4 UPDATE Operation
                    TP/oneM2M/CSE/ANNC/UPD/001
                    TP/oneM2M/CSE/ANNC/UPD/002
                    TP/oneM2M/CSE/ANNC/UPD/003
                    TP/oneM2M/CSE/ANNC/UPD/004
                    TP/oneM2M/CSE/ANNC/UPD/005
                    TP/oneM2M/CSE/ANNC/UPD/006
                    TP/oneM2M/CSE/ANNC/UPD/007
                    TP/oneM2M/CSE/ANNC/UPD/008
                    TP/oneM2M/CSE/ANNC/UPD/009
                    TP/oneM2M/CSE/ANNC/UPD/010
                    TP/oneM2M/CSE/ANNC/UPD/011
                    TP/oneM2M/CSE/ANNC/UPD/012
                    TP/oneM2M/CSE/ANNC/UPD/013
                    TP/oneM2M/CSE/ANNC/UPD/014
                7.2.2.11.5 DELETE Operation
                    TP/oneM2M/CSE/ANNC/DEL/001
                    TP/oneM2M/CSE/ANNC/DEL/002
            7.2.2.12 3GPP interworking (3GPP)
                7.2.2.12.1 BASIC Operation
                    TP/oneM2M/CSE/3GPP/TRIG/001
                    TP/oneM2M/CSE/3GPP/TRIG/002
                    TP/oneM2M/CSE/3GPP/TRIG/003
                    TP/oneM2M/CSE/3GPP/TRIG/004
                    TP/oneM2M/CSE/3GPP/TRIG/005
                    TP/oneM2M/CSE/3GPP/TRIG/006
                    TP/oneM2M/CSE/3GPP/TRIG/007
                    TP/oneM2M/CSE/3GPP/TRIG/008
                    TP/oneM2M/CSE/3GPP/TRIG/009
                    TP/oneM2M/CSE/3GPP/TRIG/010
                    TP/oneM2M/CSE/3GPP/TRIG/011
                    TP/oneM2M/CSE/3GPP/TRIG/012
                    TP/oneM2M/CSE/3GPP/TRIG/013
                    TP/oneM2M/CSE/3GPP/TRIG/014
                7.2.2.12.2 SCEF-based NIDD
                    TP/oneM2M/CSE/3GPP/NIDD/001
                    TP/oneM2M/CSE/3GPP/NIDD/002
                    TP/oneM2M/CSE/3GPP/NIDD/003
                    TP/oneM2M/CSE/3GPP/NIDD/004
                    TP/oneM2M/CSE/3GPP/NIDD/005
                    TP/oneM2M/CSE/3GPP/NIDD/006
                    TP/oneM2M/CSE/3GPP/NIDD/007
                    TP/oneM2M/CSE/3GPP/NIDD/008
                    TP/oneM2M/CSE/3GPP/NIDD/009
            7.2.2.13 FlexContainer (FLXC)
                7.2.2.13.1 CREATE Operation
                    TP/oneM2M/CSE/FLXC/CRE/001
                    TP/oneM2M/CSE/FLXC/CRE/002
                    TP/oneM2M/CSE/FLXC/CRE/003
                    TP/oneM2M/CSE/FLXC/CRE/004
                7.2.2.13.2 UPDATE Operation
                    TP/oneM2M/CSE/FLXC/UPD/001
                    TP/oneM2M/CSE/FLXC/UPD/002
                    TP/oneM2M/CSE/FLXC/UPD/003
                    TP/oneM2M/CSE/FLXC/UPD/004
                    TP/oneM2M/CSE/FLXC/UPD/005
                    TP/oneM2M/CSE/FLXC/UPD/006
                    TP/oneM2M/CSE/FLXC/UPD/007
                    TP/oneM2M/CSE/FLXC/UPD/008
                7.2.2.13.3 RETRIEVE Operation
                    TP/oneM2M/CSE/FLXC/RET/001
                    TP/oneM2M/CSE/FLXC/RET/002
                7.2.2.13.4 DELETE Operation
                    TP/oneM2M/CSE/FLXC/DEL/001
                    TP/oneM2M/CSE/FLXC/DEL/002
            7.2.2.14 Dynamic Authorization (DAU)
                7.2.1.14.1 NOTIFY Operation
                    TP/oneM2M/CSE/DAU/NOT/001
                    TP/oneM2M/CSE/DAU/NOT/002
                    TP/oneM2M/CSE/DAU/NOT/003
                    TP/oneM2M/CSE/DAU/NOT/004
                    TP/oneM2M/CSE/DAU/NOT/005
                    TP/oneM2M/CSE/DAU/NOT/006
                    TP/oneM2M/CSE/DAU/NOT/007
                    TP/oneM2M/CSE/DAU/NOT/008
            7.2.2.15 Semantic (SEM)
                7.2.2.15.1 CREATE Operation
                    TP/oneM2M/CSE/SEM/CRE/001
                    TP/oneM2M/CSE/SEM/CRE/002
                    TP/oneM2M/CSE/SEM/CRE/003
                    TP/oneM2M/CSE/SEM/CRE/004
                    TP/oneM2M/CSE/SEM/CRE/005
                    TP/oneM2M/CSE/SEM/CRE/006
                    TP/oneM2M/CSE/SEM/CRE/007
                    TP/oneM2M/CSE/SEM/CRE/008
                    TP/oneM2M/CSE/SEM/CRE/009
                    TP/oneM2M/CSE/SEM/CRE/010
                    TP/oneM2M/CSE/SEM/CRE/011
                    TP/oneM2M/CSE/SEM/CRE/012
                    TP/oneM2M/CSE/SEM/CRE/013
                    TP/oneM2M/CSE/SEM/CRE/014
                    TP/oneM2M/CSE/SEM/CRE/015
                    TP/oneM2M/CSE/SEM/CRE/016
                    TP/oneM2M/CSE/SEM/CRE/017
                7.2.2.15.2 UPDATE Operation
                    TP/oneM2M/CSE/SEM/UPD/001
                    TP/oneM2M/CSE/SEM/UPD/002
                    TP/oneM2M/CSE/SEM/UPD/003
                    TP/oneM2M/CSE/SEM/UPD/004
                    TP/oneM2M/CSE/SEM/UPD/005
                    TP/oneM2M/CSE/SEM/UPD/006
                    TP/oneM2M/CSE/SEM/UPD/007
                    TP/oneM2M/CSE/SEM/UPD/008
                    TP/oneM2M/CSE/SEM/UPD/009
                    TP/oneM2M/CSE/SEM/UPD/010
                    TP/oneM2M/CSE/SEM/UPD/011
                    TP/oneM2M/CSE/SEM/UPD/012
                    TP/oneM2M/CSE/SEM/UPD/013
                    TP/oneM2M/CSE/SEM/UPD/014
                    TP/oneM2M/CSE/SEM/UPD/015
                7.2.2.15.3 RETRIEVE Operation
                    TP/oneM2M/CSE/SEM/RET/001
                    TP/oneM2M/CSE/SEM/RET/002
                    TP/oneM2M/CSE/SEM/RET/003
                    TP/oneM2M/CSE/SEM/RET/004
                    TP/oneM2M/CSE/SEM/RET/005
                    TP/oneM2M/CSE/SEM/RET/006
                    TP/oneM2M/CSE/SEM/RET/007
                    TP/oneM2M/CSE/SEM/RET/008
                    TP/oneM2M/CSE/SEM/RET/009
                    TP/oneM2M/CSE/SEM/RET/010
                    TP/oneM2M/CSE/SEM/RET/011
                    TP/oneM2M/CSE/SEM/RET/012
                    TP/oneM2M/CSE/SEM/RET/013
                    TP/oneM2M/CSE/SEM/RET/014
                    TP/oneM2M/CSE/SEM/RET/015
                    TP/oneM2M/CSE/SEM/CRE/016
                    TP/oneM2M/CSE/SEM/CRE/017
                7.2.2.15.4 DELETE Operation
                    TP/oneM2M/CSE/SEM/DEL/001
                    TP/oneM2M/CSE/SEM/DEL/002
                    TP/oneM2M/CSE/SEM/DEL/003
            7.2.2.16 Initial Service Provisioning (ISP)
                7.2.2.16.1 BASIC Operation
            7.2.2.17 Service Charging and Accounting (CSA)
                7.2.2.17.1 Event Based Charging (EBC)
            7.2.2.18 Service Subscription Management(SSM)
                7.2.2.18.1 Service Subscription User Profile(SSUP)
                7.2.2.18.2 Service Subscription Profile(SSP)
                    7.2.2.18.2.1 Basic Operation
                    7.2.2.18.2.2 UPDATE
                7.2.2.18.3 Service Subscribed App Rule(SSAR)
                7.2.2.18.4 Service Subscribed Node(SSN)
                    7.2.2.18.4.1 Basic Operation
                    7.2.2.18.4.2 CREATE Operation
            7.2.2.19 Primitive Profile (PP)
                7.2.2.19.1 Basic Operation
                    TP/oneM2M/CSE/PP/001
                    TP/oneM2M/CSE/PP/002
                    TP/oneM2M/CSE/PP/003
                    TP/oneM2M/CSE/PP/004
                    TP/oneM2M/CSE/PP/005
                    TP/oneM2M/CSE/PP/006
                    TP/oneM2M/CSE/PP/007
                    TP/oneM2M/CSE/PP/008
                    TP/oneM2M/CSE/PP/009
                    TP/oneM2M/CSE/PP/010
                    TP/oneM2M/CSE/PP/011
                    TP/oneM2M/CSE/PP/012
                    TP/oneM2M/CSE/PP/013
                    TP/oneM2M/CSE/PP/014
                    TP/oneM2M/CSE/PP/015
                    TP/oneM2M/CSE/PP/016
                    TP/oneM2M/CSE/PP/017
                    TP/oneM2M/CSE/PP/018
                    TP/oneM2M/CSE/PP/019
                    TP/oneM2M/CSE/PP/020
                    TP/oneM2M/CSE/PP/021
                    TP/oneM2M/CSE/PP/022
                    TP/oneM2M/CSE/PP/023
            7.2.2.20 Transaction Management(TMG)
                7.2.2.20.1 CREATE Operation
                    TP/oneM2M/CSE/TMG/CRE/001
                    TP/oneM2M/CSE/TMG/CRE/002
                    TP/oneM2M/CSE/TMG/CRE/003
                    TP/oneM2M/CSE/TMG/CRE/004
                    TP/oneM2M/CSE/TMG/CRE/005
                7.2.2.20.2 UPDATE Operation
                    TP/oneM2M/CSE/TMG/UPD/001
                    TP/oneM2M/CSE/TMG/UPD/002
                    TP/oneM2M/CSE/TMG/UPD/003
                    TP/oneM2M/CSE/TMG/UPD/004
                    TP/oneM2M/CSE/TMG/UPD/005
                    TP/oneM2M/CSE/TMG/UPD/006
                    TP/oneM2M/CSE/TMG/UPD/007
                7.2.2.20.3 DELETE Operation
                    TP/oneM2M/CSE/TMG/DEL/001
            7.2.2.21 Resource Schedule (SCH)
                7.2.2.21.1 BASIC Operation
            7.2.2.22 Process Management(PMG)
                7.2.2.22.1 CREATE Operation
                7.2.2.22.2 DELETE Operation
                7.2.2.22.3 UPDATE Operation
            7.2.2.23 Software Management(SM)
                7.2.2.23.1 BASIC Operation
                    TP/oneM2M/CSE/SM/003
                    TP/oneM2M/CSE/SM/004
                    TP/oneM2M/CSE/SM/005
                    TP/oneM2M/CSE/SM/006
                    TP/oneM2M/CSE/SM/007
                    TP/oneM2M/CSE/SM/011
                    TP/oneM2M/CSE/SM/012
    A.1 MQTT Protocol Conformance Test Requirement
    B.1 TP template
History


1	Scope
The present document specifies oneM2M test suite structure and test purposes that are designed to evaluate the conformity of oneM2M implementations to the oneM2M specifications. It also specifies
Guidelines for description of test behaviours and definition of test purpose structure,
Notations to define a test purpose for conformance testing, and
Test configurations for conformance testing.
2	References
2.1	Normative references
References are either specific (identified by date of publication and/or edition number or version number) or nonspecific. For specific references, only the cited version applies. For non‑specific references, the latest version of the referenced document (including any amendments) applies.
The following referenced documents are necessary for the application of the present document.
· [1] oneM2M TS‑0001: "Functional Architecture".
· [2] oneM2M TS‑0004: "Service Layer Core Protocol Specification".
· [3] oneM2M TS‑0015: "Testing Framework".
· [4] oneM2M TS‑0017: "Implementation Conformance Statements".
· [5] oneM2M TS‑0026: "3GPP Interworking".
· [6] oneM2M TS‑0034: "Semantics Support".
· [7] oneM2M TS‑0023: "Home Appliances Information Model and Mapping".
· [8] oneM2M TS‑0030: "Ontology based Interworking".
2.2	Informative references
The following referenced documents are not necessary for the application of the present document but they assist the user with regard to a particular subject area.
· [i.1] oneM2M Drafting Rules > NOTE: Available at http://www.onem2m.org/images/files/oneM2M‑Drafting‑Rules.pdf.
· [i.2] oneM2M TS‑0010: "MQTT Protocol Binding".
· [i.3] oneM2M TS‑0031: "oneM2M Features".
3	Definitions and abbreviations
3.1	Definitions
For the purposes of the present document, the terms and definitions given in TS‑0015 [3] Testing Framework and the following ones apply:
valid <OPERATION> Request : a oneM2M Request primitive that only contains all mandatory primitive parameters with correct values which are not required to be explicitly specified in the test purpose. If specific values need to be specified, parameters need to be explicitly indicated in the test purpose. Operation parameter is set to <OPERATION>.
valid Response : a oneM2M Response primitive that only contains all mandatory primitive parameters with correct values which are not required to be explicitly specified in the test purpose. If specific values need to be specified, parameters need to be explicitly indicated in the test purpose. Request Identifier parameter contains the Request Identifier value of the corresponding Request.
valid <ATTRIBUTE_NAME> : correct value for the <ATTRIBUTE_NAME> attribute which is not required to be explicitly specified in the test purpose
Editor's Note: This may contain additional information.
3.2	Abbreviations
For the purposes of the present document, the abbreviations given in TS‑0001[1] and the follwing apply:
ADN	Application Dedicated Node
ADN-AE	AE which resides in the Application Dedicated Node
AE	Application Entity
ASN	Application Service Node
CSE	Common Service Entity
CSF	Common Service Function
IN	Infrastructure Node
IN-CSE	CSE which resides in the Infrastructure Node
IUT	Implementation Under Test
MN	Middle Node
SUT	System Under Test

4	Conventions
The key words "Shall", "Shall not", "May", "Need not", "Should", "Should not" in the present document are to be interpreted as described in the oneM2M Drafting Rules [i.1]
5	Prerequisites and Test Configurations
5.1	Test Configurations
Test configurations are defined to test different entities such as CSE and AE etc.
Figure 5.1‑1 and Figure 5.1‑2 show CSE test configurations where CSE as a IUT can be tested against TTCN‑3 Test System, which is acting as AE or AE and CSE respectively. Test system may include as well other entities which are necessary for each configuration, i.e. a second AE (AE2) for receiving notifications These entities are represented with dashed rectangles.
Figure 5.1‑3 shows AE test configuration (CF03) for ADN‑AE testing scenario where ADN‑AE is IUT and TTCN‑3 Test System is acting as a CSE.
Figure 5.1‑4 depicts test configurations between two CSEs, where one CSE is acting as a Test System, the other is SUT.
Figure 5.1‑5 shows test configurations for 3GPP interworking testing scenario where 3GPP SCEF is working in a Test System.
[image: ./media/image1.png]
Figure 5.1-1: Test configuration 1 (CF01)
[image: ./media/image2.png]
Figure 5.1-2: Test configuration 2 (CF02)
[image: ./media/image3.png]
Figure 5.1-3: Test configuration 3 (CF03)
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Figure 5.1-4: Test configuration 4 (CF04)
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Figure 5.1-5 : Test configuration 5 (CF05)
[image: ./media/image6.png]
Figure 5.1-6: Test configuration 6 (CF06)
[image: ./media/image7.png]
Figure 5.1-7 : Test configuration 7 (CF07)
6	Test Suite Structure (TSS)
6.1	Test groups
The test groups are organized in 2 levels. The first level defines the functional entity of oneM2M. The second level defines the common services functions which are represented in oneM2M functional architecture.
6.1.1	Functional Entity Groups
The functional entity groups identify the types of entity which are specified in oneM2M functional architecture(TS‑0001 [1]).
· AE
· CSE
6.1.2	Common Services Functions Subgroups
The common services functions subgroups identify the general procedures in each common services functions specified in oneM2M functional architecture (TS‑0001 [1]):
· Registration
· Data Management and Repository
· Subscription and Notification
· Group Management
· Discovery
· Location
· Device Management
· Communication Management and Delivery Handling
· Security
6.1.3	oneM2M Resource Primitives specific Operations
A group of resource type specific procedures are defined in oneM2M functional architecture (TS‑0001 [1]) and service layer core protocol (TS‑0004 [2]). Those procedures can be potentially abstracted with requirements for generating test purposes for conformance testing purpose. Those resource type specific procedures are the complementary procedures to the general procedures defined in oneM2M Common Service Functions (CSF) and will use for subgroups of structures for oneM2M tests. A list of those procedures are including:
· Resource announcement
· timeSeries
· location
· 3GPP interworking
· Semantic
· HAIM
· Dynamic Authorization
· FlexContainer
6.2	Test Suite Structure (TSS) for oneM2M
The Test Suite Structure (TSS) for oneM2M will be present as below:
· Group 1: General Capability (GEN):
· Subgroup 1.1: Protocol Bindings
· Subgroup 1.2: Serializations
· Group 2: AE(AE):
· Subgroup 2.1: General Capability (GEN)
· Subgroup 2.2: Registration(REG)
· Subgroup 2.3: Data Management and Repository(DMR)
· Subgroup 2.4: Subscription and Notification(SUB)
· Subgroup 2.5: Communication Management and Delivery Handling(CMDH)
· Subgroup 2.5.1: Request Message Polling(PCH)
· Group 3: CSE(CE):
· Subgroup 3.1: General Capability (GEN)
· Subgroup 3.2: Registration(REG)
· Subgroup 3.3: Data Management and Repository(DMR)
· Subgroup 3.4: Subscription and Notification(SUB)
· Subgroup 3.5: Group Management(GMG)
· Subgroup 3.6: Discovery(DIS)
· Subgroup 3.7: Location(LOC)
· Subgroup 3.8: Device Management(DMG)
· Subgroup 3.8.1: Data Management using TimeSeries(TS)
· Subgroup 3.9: Communication Management and Delivery Handling(CMDH)
· Subgroup 3.9.1: Request Message Polling(PCH)
· Subgroup 3.9.2: Response Type(RT)
· Subgroup 3.10: Security(SEC)
· Subgroup 3.11: Resource Announcement (ANNC)
· Subgroup 3.12: 3GPP Interworking(3GPP)
· Subgroup 3.13: FlexContainer (FLXC)
· Subgroup 3.14: Dynamic Authorization (DAU)
· Subgroup 3.15: Semantic (SEM)
· Subgroup 3.16: Initial Service Provisioning (ISP)
· Subgroup 3.17: Service Charging and Accounting (CSA)
· Subgroup 3.18: Service Subscription Management(SSM)
· Subgroup 3.19: Primitive Profile (PP)
· Subgroup 3.20: Transaction Management (TMG)
· Subgroup 3.21: Resource Schedule (SCH)
· Subgroup 3.22: Process Management (PMG)
· Subgroup 3.23: Software Management (SM)
7	Test Purposes (TP)
7.1	Introduction
7.1.1	TP definition conventions
The TP definition is constructed according to Test Suite Structure & Test Purposes(TSS&TP) in Testing Framework(TS‑0015 [3]).
7.1.2	TP Identifier naming conventions
The identifier of the TP is constructed according to table 7.1.2‑1.
Table 7.1.2-1: TP naming convention for oneM2M
	Name
	Option
	Interpretation

	TP///[/][/]/_

	 = root
	oneM2M
	oneM2M

	 = entity
	AE
	Application Entity

	
	CSE
	Common Services Entity

	 = group
	GEN
	Common Service Function

	
	REG
	

	
	DMR
	

	
	SUB
	

	
	GMG
	

	
	DIS
	

	
	LOC
	

	
	DMG
	

	
	CMDH
	

	
	SEC
	

	
	ANNC
	

	
	FLXC
	

	
	DAU
	

	
	SEM
	

	
	ISP
	

	 = sub-group
	ACP
	AccessControlPolicy

	 = operation
	CRE
	Create

	
	UPD
	Update

	
	RET
	Retrieve

	
	DEL
	Delete

	
	NTF
	Notify

	 = sequential number
	001 to 999
	023

	 = permutation part
	May be number, short name of attribute or resource type depending on the permutated part in the TP. If there are more than one permutated variables, they should be separated by slash '/'.
	Enumerated type attribute and its value is represented as /, e.g. TP/oneM2M/CSE/DMR/RET/020_RCN/0
When resourceType attribute is involved in a TP Id, the resourceType shall be put in first order followed by any other attribute(s), if any: // e.g. TP/oneM2M/CSE/DMR/CRE/015_CNT/ACPI



7.1.3	Rules for the behaviour description
The description of the TP is built according to TS‑0015 [3] Testing Framework.
In addition, the following rules apply:
Primitive parameters shall use their Parameter name as indicated in TS‑0004 [2] table 8.2.2‑1
Resource attributes shall use their Attribute name as indicated in TS‑0004 [2] tables 8.2.3 followed by "attribute".
When_Content_ request parameter contains a resource representation, such representation shall contain all mandatory attributes and could contain some optional attributes. Only those attributes and/or child resources required by the test purpose will be explicitly indicated.
When_Content_ response parameter contains a resource representation, such representation shall contain attributes and/or child resources according to the Result Content parameter of the corresponding request. Only those attributes and/or child resources required by the test purpose will be explicitly indicated.
7.1.4	ICS reference
Table 7.1.4-1: Node
	Item
	Name of field
	Reference
	Status
	Support

	1
	ASN (Application Service Node)
	5.1.2
	o.1
	

	2
	ADN (Application Dedicated Node)
	5.1.2
	o.1
	

	3
	IN (Infrastructure Node)
	5.1.2
	o.1
	

	4
	MN (Middle Node)
	5.1.2
	o.1
	

	o.1: Exactly one item shall be supported



Table 7.1.4-2: Functional entity type
	Prerequisite: A.1

	Item
	Name of field
	Reference
	Status
	Support

	1
	AE
	5.1.1
	c.1
	

	2
	CSE
	5.1.1
	c.2
	

	c.1: If A.1-1 or A.1-2 then m else o
c.2: If A.1-2 x else m



Table: Table 7.1.4-: Mnemonics for PICS reference
PICS Items
	Mnemonic
	PICS item

	PICS_AE
	TS-0017 [4], clause A.5.1.1/1

	PICS_CSE
	TS-0017 [4], clause A.5.1.1/2

	PICS_ASN_CSE
	TS-0017 [4], clause A.5.1.2/1

	PICS_ADN
	TS-0017 [4], clause A.5.1.2/7

	PICS_IN_CSE
	TS-0017 [4], clause A.5.1.2/3

	PICS_MN_CSE
	TS-0017 [4], clause A.5.1.2/2

	PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT
	TS-0017 [4], clause A.5.2.1/2

	PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT
	TS-0017 [4], clause A.5.2.1/1

	PICS_SP_RELATIVE_RESOURCE_ID
	TS-0017 [4], clause A.5.2.1

	PICS_ABSOLUTE_RESOURCE_ID
	TS-0017 [4], clause A.5.2.1

	PICS_ACP_SUPPORT
	TS-0017 [4], clause A.5.3.1/10

	PICS_CB_CST
	TS-0017 [4], clause A.5.7.1/3

	PICS_CB_NL
	TS-0017 [4], clause A.5.7.1/4

	PICS_CSR_RN
	TS-0017 [4], clause A.5.7.2/10

	PICS_CSR_ET
	TS-0017 [4], clause A.5.7.2/11

	PICS_CSR_LBL
	TS-0017 [4], clause A.5.7.2/2

	PICS_CSR_POA
	TS-0017 [4], clause A.5.7.2/6

	PICS_CSR_NL
	TS-0017 [4], clause A.5.7.2/9

	PICS_CSR_CST
	TS-0017 [4], clause A.5.7.2/5

	PICS_CSR_RR
	TS-0017 [4], clause A.5.7.2/12

	PICS_AE_LBL
	TS-0017 [4], clause A.5.7.3/2

	PICS_AE_APN
	TS-0017 [4], clause A.5.7.3/5

	PICS_AE_POA
	TS-0017 [4], clause A.5.7.3/6

	PICS_AE_NL
	TS-0017 [4], clause A.5.7.3/8

	PICS_AE_CSZ
	TS-0017 [4], clause A.5.7.3/9

	PICS_CNT_ACPI
	TS-0017 [4], clause A.5.7.5/1

	PICS_CNT_MNI
	TS-0017 [4], clause A.5.7.5/6

	PICS_CNT_MBS
	TS-0017 [4], clause A.5.7.5/7

	PICS_CNT_MIA
	TS-0017 [4], clause A.5.7.5/8

	PICS_CNT_OR
	TS-0017 [4], clause A.5.7.5/10

	PICS_CNT_LI
	TS-0017 [4], clause A.5.7.5/9

	PICS_CNT_RN
	TS-0017 [4], clause A.5.7.5/11

	PICS_CNT_ET
	TS-0017 [4], clause A.5.7.5/12

	PICS_CNT_LBL
	TS-0017 [4], clause A.5.7.5/2

	PICS_CNT_CR
	TS-0017 [4], clause A.5.7.5/5

	PICS_CIN_CNF
	TS-0017 [4], clause A.5.7.6/5

	PICS_CIN_RN
	TS-0017 [4], clause A.5.7.6/7

	PICS_CIN_ET
	TS-0017 [4], clause A.5.7.6/8

	PICS_CIN_LBL
	TS-0017 [4], clause A.5.7.6/1

	PICS_CIN_CR
	TS-0017 [4], clause A.5.7.6/4

	PICS_ACP_LBL
	TS-0017 [4], clause A.5.7.4/1

	PICS_SUB_ACPI
	TS-0017 [4], clause A.5.7.7/2

	PICS_SUB_LBL
	TS-0017 [4], clause A.5.7.7/1

	PICS_SUB_ENC
	TS-0017 [4], clause A.5.7.7/3

	PICS_SUB_EXC
	TS-0017 [4], clause A.5.7.7/4

	PICS_SUB_GPI
	TS-0017 [4], clause A.5.7.7/5

	PICS_SUB_NFU
	TS-0017 [4], clause A.5.7.7/6

	PICS_SUB_BN
	TS-0017 [4], clause A.5.7.7/7

	PICS_SUB_RL
	TS-0017 [4], clause A.5.7.7/8

	PICS_SUB_PN
	TS-0017 [4], clause A.5.7.7/10

	PICS_SUB_NSP
	TS-0017 [4], clause A.5.7.7/11

	PICS_SUB_LN
	TS-0017 [4], clause A.5.7.7/12

	PICS_SUB_NCT
	TS-0017 [4], clause A.5.7.7/13

	PICS_SUB_NEC
	TS-0017 [4], clause A.5.7.7/14

	PICS_SUB_CR
	TS-0017 [4], clause A.5.7.7/15

	PICS_SUB_SU
	TS-0017 [4], clause A.5.7.7/16

	PICS_GRP_LBL
	TS-0017 [4], clause A.5.7.8/2

	PICS_GRP_ACPI
	TS-0017 [4], clause A.5.7.8/1

	PICS_GRP_MACP
	TS-0017 [4], clause A.5.7.8/6

	PICS_GRP_GN
	TS-0017 [4], clause A.5.7.8/9

	PICS_SCA
	TS-0017 [4], clause A.5.6



7.2	Test Purposes for oneM2M Service Primitives
7.2.1	Group AE (AE)
7.2.1.1	General Capability (GEN)
7.2.1.1.1	CREATE Operation
TP/oneM2M/AE/GEN/CRE/001
	TP Id
	TP/oneM2M/AE/GEN/CRE/001

	Test objective
	Check that the IUT sends the creation of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUT being configured to use NON_HIERARCHICAL_RESOURCE_ADDRESS and
the IUThaving privileges to perform CREATE operation on resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid Container CREATE Request to CSE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+———————————————————————————————-+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/CRE/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/CRE/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/CRE/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID.



TP/oneM2M/AE/GEN/CRE/002
	TP Id
	TP/oneM2M/AE/GEN/CRE/002

	Test objective
	Check that the IUT sends the creation of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUT being configured to use HIERARCHICAL_RESOURCE_ADDRESS and
the IUThaving privileges to perform CREATE operation on resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 3 (container) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | To set to HIERARCHICA_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 3 (container) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/CRE/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/CRE/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/CRE/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID.



7.2.1.1.2	UPDATE Operation
TP/oneM2M/AE/GEN/UPD/001
	TP Id
	TP/oneM2M/AE/GEN/UPD/001

	Test objective
	Check that the IUT sends the update of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registered and
the IUT being switched on and
the IUT being configured to use NON_HIERARCHICAL_RESOURCE_ADDRESS and
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and
the IUThaving privileges to perform UPDATE operation on resource CONTAINER_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid UPDATE Request containing  | |
                     | Toset to CONTAINER_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid labels attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid UPDATE request to CSE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/UPD/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/UPD/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/UPD/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID.



TP/oneM2M/AE/GEN/UPD/002
	TP Id
	TP/oneM2M/AE/GEN/UPD/002

	Test objective
	Check that the IUT sends the update of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registered and
the IUT being switched on and
the IUT being configured to use HIERARCHICAL_RESOURCE_ADDRESS and
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and
the IUThaving privileges to perform UPDATE operation on resource CONTAINER_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid UPDATE Request containing  | |
                     | Toset to CONTAINER_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid labels attribute  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid UPDATE request to CSE containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | Container resource containing  | |
                     | valid labels attribute  | |
                     |} | |
+———————-+——————————————————————————————+————-+
	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/UPD/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/UPD/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/UPD/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID.



7.2.1.1.3	RETRIEVE Operation
TP/oneM2M/AE/GEN/RET/001
	TP Id
	TP/oneM2M/AE/GEN/RET/001

	Test objective
	Check that the IUT sends the retrieval of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registered and
the IUT being switched on and
the IUT being configured to use NON_HIERARCHICAL_RESOURCE_ADDRESS and
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and the IUThaving privileges to perform RETRIEVE operation on container resource
}



·                  +-----------------------------------------------------------------+-----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | Toset to CONTAINER_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------+-----------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid RETRIEVE request to CSE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+—————————————————————–+———————————————————————————————–+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/RET/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/RET/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/RET/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID



TP/oneM2M/AE/GEN/RET/002
	TP Id
	TP/oneM2M/AE/GEN/RET/002

	Test objective
	Check that the IUT sends the retrieval of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registered and
the IUT being switched on and
the IUT being configured to use HIERARCHICAL_RESOURCE_ADDRESS and
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and the IUThaving privileges to perform RETRIEVE operation on container resource
}



·                  +-------------------------------------------------------------------+---------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | Toset to CONTAINER_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-------------------------------------------------------------------+---------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid RETRIEVE request to CSE containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+——————————————————————-+———————————————————————————————+————-+


	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/RET/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/RET/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/RET/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID




7.2.1.1.4	DELETE Operation
TP/oneM2M/AE/GEN/DEL/001
	TP Id
	TP/oneM2M/AE/GEN/DEL/001

	Test objective
	Check that the IUT sends the deletion of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registered and
the IUT being switched on and
the IUT being configured to use NON_HIERARCHICAL_RESOURCE_ADDRESS and
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and
the IUThaving privileges to perform DELETE operation on container resource
}



·                  +----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid DELETE Request containing  | |
                     | Toset to CONTAINER_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid DELETE request to CSE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+———————————————————————————————-+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/DEL/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/DEL/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/DEL/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID



TP/oneM2M/AE/GEN/DEL/002
	TP Id
	TP/oneM2M/AE/GEN/DEL/002

	Test objective
	Check that the IUT sends the deletion of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being registered and
the IUT being switched on and
the IUT being configured to use HIERARCHICAL_RESOURCE_ADDRESS and
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and
the IUThaving privileges to perform DELETE operation on container resource
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid DELETE Request containing  | |
                     | Toset to CONTAINER_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid DELETE request to CSE containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+——————————————————————————————–+————-+

	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/AE/GEN/DEL/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/AE/GEN/DEL/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/AE/GEN/DEL/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



7.2.1.2	Registration (REG)
7.2.1.2.1	CREATE Operation
TP/oneM2M/AE/REG/CRE/001
	TP Id
	TP/oneM2M/AE/REG/CRE/001

	Test objective
	Check that the IUT sends an AE initial registration request with no AE-ID-STEM provided when it is started

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case C, and clause 9.6.19

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT never being registered and
the IUT being switched off and
the IUThaving got a valid APP-ID
}



·                  +---------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | Toset to CSE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 2 (AE) and   | |
                     | Content containing  | |
                     |AE resource representation  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | Resource Type set to 2 (AE) and  | |
                     | To set to CSE_RESOURCE_ADDRESS and  | |
                     | From set to empty and  | |
                     | Content containing  | |
                     |AE resource representation  | |
                     |} | |
+———————-+———————————————————————————————+————-+
TP/oneM2M/AE/REG/CRE/002
	TP Id
	TP/oneM2M/AE/REG/CRE/002

	Test objective
	Check that the IUT sends a registration CREATE Request with the value of the attribute ATTRIBUTE_NAME of the AE resource

	Reference
	TS-0004 [2], clause 7.4.6.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT never being registered and
the IUT being switched off and
the IUThaving got a valid APP-ID
}



·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 2 (AE) and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid CREATE Request containing  | IUT => CSE |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | AE resourcecontaining  | |
                     | valid_ATTRIBUTE_NAME_ attribute  | |
                     |} | |
+———————-+—————————————————————————————————————+————-+
	TP Id
	Reference
	ATTRIBUTE_NAME

	TP/oneM2M/AE/REG/CRE/002_RN
	TS-0004 [2], clause 2
	resourceName

	TP/oneM2M/AE/REG/CRE/002_ET
	TS-0004 [2], clause 2
	expirationTime

	TP/oneM2M/AE/REG/CRE/002_LBL
	TS-0004 [2], clause 2
	labels

	TP/oneM2M/AE/REG/CRE/002_APN
	TS-0004 [2], clause 2
	appName

	TP/oneM2M/AE/REG/CRE/002_API
	TS-0004 [2], clause 2
	App-ID

	TP/oneM2M/AE/REG/CRE/002_POA
	TS-0004 [2], clause 2
	pointOfAccess

	TP/oneM2M/AE/REG/CRE/002_OR
	TS-0004 [2], clause 2
	ontologyRef

	TP/oneM2M/AE/REG/CRE/002_NL
	TS-0004 [2], clause 2
	nodeLink

	TP/oneM2M/AE/REG/CRE/002_RR
	TS-0004 [2], clause 2
	requestReachability

	TP/oneM2M/AE/REG/CRE/002_CSZ
	TS-0004 [2], clause 2
	contentSerialization



Editor's Note: Reference need to be checked
7.2.1.2.2	DELETE Operation
TP/oneM2M/AE/REG/DEL/001
	TP Id
	TP/oneM2M/AE/REG/DEL/001

	Test objective
	Check that the IUT sends AE deregistration request to CSE

	Reference
	TS-0001 [1], clause 10.1.4.2.2

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being in the "initial state"
the IUT having registered to CSE and
the IUThaving privileges to perform DELETE operation on the resource AE to CSE
}



·                  +---------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid DELETE Request containing| |
                     | To set to AE_RESOURCE_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid DELETE Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+—————————————————————————+————-+

7.2.1.3	Data Management and Repository (DMR)
7.2.1.3.1	CREATE Operation
TP/oneM2M/AE/DMR/CRE/001
	TP Id
	TP/oneM2M/AE/DMR/CRE/001

	Test objective
	Check that the IUT sends a Container creation request when it is triggered

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.1, TS-0004 [2], clause 7.2.2.1 and 7.4.7.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUThaving privileges to perform CREATE operation on resource AE_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 3 (container) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |container resource representation  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 3 (container) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |container resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————–+————-+
TP/oneM2M/AE/DMR/CRE/002
	TP Id
	TP/oneM2M/AE/DMR/CRE/002

	Test objective
	Check that the IUT sends a ContentInstance creation request when it is triggered

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.1, TS-0004 [2], clause 7.2.2.1 and 7.4.8.2.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE.

	Initial conditions
	with {
the IUT being registeredand
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and
the IUThaving privileges to perform CREATE operation on resource CONTAINER_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 4 (contentInstance) and  | |
                     | Content containing  | |
                     |contentInstance resource representation  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 4 (contentInstance) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |contentInstance resource representation  | |
                     |} | |
+———————-+——————————————————————————————————————-+————-+
TP/oneM2M/AE/DMR/CRE/003
	TP Id
	TP/oneM2M/AE/DMR/CRE/003

	Test objective
	Check that the IUT sends a ContentInstance creation request with optional attribute ATTRIBUTE_NAME

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.1, TS-0004 [2], clause 7.2.2.1 and 7.4.8.2.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered and
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS through preconfiguration request and
the IUThaving privileges to perform CREATE operation on resource CONTAINER_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 4 (contentInstance) and  | |
                     | Content containing  | |
                     | ContentInstance resource c ontaining  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 4 (contentInstance) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | ContentInstance resource c ontaining  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
+———————-+——————————————————————————————————————-+————-+
	TP Id
	PICS Selection
	ATTRIBUTE_NAME

	TP/oneM2M/AE/DMR/CRE/003_CNF
	PICS_CIN_CNF
	contentInfo

	TP/oneM2M/AE/DMR/CRE/003_RN
	PICS_CIN_RN
	resourceName

	TP/oneM2M/AE/DMR/CRE/003_ET
	PICS_CIN_ET
	expirationTime

	TP/oneM2M/AE/DMR/CRE/003_LBL
	PICS_CIN_LBL
	labels

	TP/oneM2M/AE/DMR/CRE/003_CR
	PICS_CIN_CR
	creator



TP/oneM2M/AE/DMR/CRE/004
	TP Id
	TP/oneM2M/AE/DMR/CRE/004

	Test objective
	Check that the IUT sends a Container creation request with optional attribute ATTRIBUTE_NAME when it is triggered

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.1, TS-0004 [2], clause 7.2.2.1 and 7.4.7.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUThaving privileges to perform CREATE operation on resource AE_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 3 (container) and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 3 (container) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
+———————-+—————————————————————————————————————–+————-+
	TP Id
	PICS Selection
	ATTRIBUTE_NAME

	TP/oneM2M/AE/DMR/CRE/004_ACPI
	PICS_CNT_ACPI
	accessControlPolicyIDs

	TP/oneM2M/AE/DMR/CRE/004_MNI
	PICS_CNT_MNI
	maxNrOfInstances

	TP/oneM2M/AE/DMR/CRE/004_MBS
	PICS_CNT_MBS
	maxByteSize

	TP/oneM2M/AE/DMR/CRE/004_MIA
	PICS_CNT_MIA
	maxInstanceAge

	TP/oneM2M/AE/DMR/CRE/004_OR
	PICS_CNT_OR
	ontologyRef

	TP/oneM2M/AE/DMR/CRE/004_LI
	PICS_CNT_LI
	locationID

	TP/oneM2M/AE/DMR/CRE/004_RN
	PICS_CNT_RN
	resourceName

	TP/oneM2M/AE/DMR/CRE/004_ET
	PICS_CNT_ET
	expirationTime

	TP/oneM2M/AE/DMR/CRE/004_LBL
	PICS_CNT_LBL
	labels

	TP/oneM2M/AE/DMR/CRE/004_CR
	PICS_CNT_CR
	creator



Editor's Note: Combination of optional attributes that are included in the Content of container creation request can be extended to generate more test cases based on this test case.
7.2.1.3.2	UPDATE Operation
TP/oneM2M/AE/DMR/UPD/001
	TP Id
	TP/oneM2M/AE/DMR/UPD/001

	Test objective
	Check that the IUT sends an UPDATE Request with the value of the attribute ATTRIBUTE_NAME of the AE resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered containing
a RW attribute ATTRIBUTE_NAME
}



·                  +--------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     | the IUT is triggered to send a valid UPDATE Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | AE resourcecontaining  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid UPDATE Request containing  | IUT => CSE |
                     | To set to AE _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | AE resourcecontaining  | |
                     | valid_ATTRIBUTE_NAME_ attribute | |
                     |} | |
+———————-+————————————————————————————————–+————-+
	TP Id
	Reference
	ATTRIBUTE_NAME

	TP/oneM2M/AE/DMR/UPD/001_ET
	TS-0004 [2], clause 7.4.6.1
	expirationTime

	TP/oneM2M/AE/DMR/UPD/001_LBL
	TS-0004 [2], clause 7.4.6.1
	labels

	TP/oneM2M/AE/DMR/UPD/001_APN
	TS-0004 [2], clause 7.4.6.1
	appName

	TP/oneM2M/AE/DMR/UPD/001_POA
	TS-0004 [2], clause 7.4.6.1
	pointOfAccess

	TP/oneM2M/AE/DMR/UPD/001_OR
	TS-0004 [2], clause 7.4.6.1
	ontologyRef

	TP/oneM2M/AE/DMR/UPD/001_NL
	TS-0004 [2], clause 7.4.6.1
	nodeLink

	TP/oneM2M/AE/DMR/UPD/001_RR
	TS-0004 [2], clause 7.4.6.1
	requestReachability

	TP/oneM2M/AE/DMR/UPD/001_CSZ
	TS-0004 [2], clause 7.4.6.1
	contentSerialization



TP/oneM2M/AE/DMR/UPD/002
	TP Id
	TP/oneM2M/AE/DMR/UPD/002

	Test objective
	Check that the IUT sends an UPDATE Request with the value of the attribute ATTRIBUTE_NAME of the <container> resource

	Reference
	TS-0004 [2], clause 7.4.7.2.3

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered containing
the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS and
the IUThaving privileges to perform UPDATE operation on resource CONTAINER_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     | the IUT is triggered to send a valid UPDATE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | container resourcecontaining  | |
                     | valid_ATTRIBUTE_NAME_ attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid UPDATE Request containing  | IUT => CSE |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resourcecontaining  | |
                     | valid_ATTRIBUTE_NAME_ attribute  | |
                     |} | |
+———————-+————————————————————————————————————–+————-+
	TP Id
	Reference
	ATTRIBUTE_NAME

	TP/oneM2M/AE/DMR/UPD/002_ET
	TS-0004 [2], clause 7.4.7.2.3
	expirationTime

	TP/oneM2M/AE/DMR/UPD/002_LBL
	TS-0004 [2], clause 7.4.7.2.3
	labels

	TP/oneM2M/AE/DMR/UPD/002_MNI
	TS-0004 [2], clause 7.4.7.2.3
	maxNrOfInstances

	TP/oneM2M/AE/DMR/UPD/002_MBS
	TS-0004 [2], clause 7.4.7.2.3
	maxByteSize

	TP/oneM2M/AE/DMR/UPD/002_MIA
	TS-0004 [2], clause 7.4.7.2.3
	maxInstanceAge



7.2.1.3.3	RETRIEVE Operation
TP/oneM2M/AE/DMR/RET/001
	TP Id
	TP/oneM2M/AE/DMR/RET/001

	Test objective
	Check that the IUT sends a RETRIEVE Request on the TARGET_RESOURCE_ADDRESS to CSE

	Reference
	TS-0001 [1], claus
e 10.1.2, TS-0004 [2], clause 7.2.2.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE.

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the CSE having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the IUT having privileges to perform RETRIEVE operation on resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     |the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------+-------------+

·                      |then {   |  |
                     | the IUT sends a valid RETRIEVE Request containing  |IUT => CSE |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+———————————————————————————————+————-+
	TP Id
	Reference
	RESOURCE_TYPE

	TP/oneM2M/AE/DMR/RET/001_CB
	TS-0001 [1], clause 10.2.3.2
	5 (CSEBase)

	TP/oneM2M/AE/DMR/RET/001_AE
	TS-0001 [1], clause 10.2.1.2
	2 (AE)

	TP/oneM2M/AE/DMR/RET/001_CNT
	TS-0001 [1], clause 10.2.4.2
	3 (Container)



TP/oneM2M/AE/DMR/RET/002
	TP Id
	TP/oneM2M/AE/DMR/RET/002

	Test objective
	Check that the IUT sends a RETRIEVE Request of oldest virtual resource

	Reference
	TS-0001 [1], clause 10.2.23.1, TS-0004 [2], clause 7.4.29.2.3

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the CSE having created a container resource
and the CSE having created a contentInstance resource under container resource
and the IUT having privileges to perform RETRIEVE operation on contentInstance resource
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     |the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/oldest  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid RETRIEVE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/oldest and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
TP/oneM2M/AE/DMR/RET/003
	TP Id
	TP/oneM2M/AE/DMR/RET/003

	Test objective
	Check that the IUT sends a RETRIEVE Request of latest virtual resource

	Reference
	TS-0001 [1], clause 10.2.22.1, TS-0004 [2], clause 7.4.28.2.3

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the CSE having created a container resource
and the CSE having created a contentInstance resource under container resource
and the IUT having privileges to perform RETRIEVE operation on contentInstance resource
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     |the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/latest  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid RETRIEVE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/latest and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
TP/oneM2M/AE/DMR/RET/004
	TP Id
	TP/oneM2M/AE/DMR/RET/004

	Test objective
	Check that the IUT sends a <container> resource RETRIEVE Request to CSE

	Reference
	TS-0004 [2], clause 7.4.7.2.2

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS
and the IUThaving privileges to perform RETRIEVE operation on container resource
}



·                  +----------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     |the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------+-------------+

·                      |then {   |  |
                     | the IUT sends a valid RETRIEVE Request containing  |IUT => CSE |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+—————————————————————————-+————-+
TP/oneM2M/AE/DMR/RET/005
	TP Id
	TP/oneM2M/AE/DMR/RET/005

	Test objective
	Check that the IUT sends a <contentInstance> resource RETRIEVE Request to CSE

	Reference
	TS-0004 [2], clause 7.4.8.2.2

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the CSE having created a container resource
and the CSE having created a contentInstance resource under container resource
and the IUT having privileges to perform RETRIEVE operation on contentInstance resource
}



·                  +-----------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     |the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to CONTENTINSTANCE_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------+-------------+

·                      |then {   |  |
                     | the IUT sends a valid RETRIEVE Request containing  |IUT => CSE |
                     | To set to CONTENTINSTANCE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+———————————————————————————–+————-+
7.2.1.3.4	DELETE Operation
TP/oneM2M/AE/DMR/DEL/001
	TP Id
	TP/oneM2M/AE/DMR/DEL/001

	Test objective
	Check that the IUT sends a DELETE Request of oldest virtual resource

	Reference
	TS-0001 [1], clause 10.2.23.2, TS-0004 [2], clause 7.4.29.2.5

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the CSE having created a container resource
and the CSE having created a contentInstance resource under container resource
and the IUT having privileges to perform DELETE operation on contentInstance resource
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     |the IUT is triggered to send a valid DELETE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/oldest  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid DELETE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/oldest and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
TP/oneM2M/AE/DMR/DEL/002
	TP Id
	TP/oneM2M/AE/DMR/DEL/002

	Test objective
	Check that the IUT sends a DELETE Request of latest virtual resource

	Reference
	TS-0001 [1], clause 10.2.22.2, TS-0004 [2], clause 7.4.28.2.5

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the CSE having created a container resource
and the CSE having created a contentInstance resource under container resource
and the IUT having privileges to perform DELETE operation on contentInstance resource
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid DELETE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/oldest  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid DELETE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/latest and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
TP/oneM2M/AE/DMR/DEL/003
	TP Id
	TP/oneM2M/AE/DMR/DEL/003

	Test objective
	Check that the IUT sends a <container> resource DELETE request to CSE

	Reference
	TS-0004 [2], clause 7.4.7.2.4

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered and
and the IUT being switched on
and the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS
and the IUThaving privileges to perform DELETE operation on container resource
}



·                  +----------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid DELETE Request containing | |
                     | To set to CONTAINER_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid DELETE Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+—————————————————————————-+————-+
TP/oneM2M/AE/DMR/DEL/004
	TP Id
	TP/oneM2M/AE/DMR/DEL/004

	Test objective
	Check that the IUT sends a <contentInstance> resource DELETE request to CSE

	Reference
	TS-0004 [2], clause 7.4.8.2.4

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the CSE having created a container resource
and the CSE having created a contentInstance resource under container resource
and the IUT having privileges to perform DELETE operation on contentInstance resource
}



·                  +---------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid DELETE Request containing  | |
                     | To set to CONTENTINSTANCE_RESOURCE_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid DELETE Request containing  | |
                     | To set to CONTENTINSTANCE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
+———————-+———————————————————————————+————-+
7.2.1.4	Subscription and Notification (SUB)
7.2.1.4.1	CREATE Operation
TP/oneM2M/AE/SUB/CRE/001
	TP Id
	TP/oneM2M/AE/SUB/CRE/001

	Test objective
	Check that the IUT sends a subscription creation request

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.1, TS-0004 [2], clause 7.2.2.1 and 7.4.9.2.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched off and
the IUThaving privileges to perform CREATE operation on resource AE_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | Toset to AE_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     |subscription resource representation  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | Toset to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |subscription resource representation  | |
                     |} | |
+———————-+——————————————————————————————————————-+————-+
TP/oneM2M/AE/SUB/CRE/002
	TP Id
	TP/oneM2M/AE/SUB/CRE/002

	Test objective
	Check that the IUT sends a subscription creation request with optional attribute ATTRIBUTE_NAME when it is triggered

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.11.2, TS-0004 [2], clause 7.2.2.1 and 7.4.9.2.1

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUThaving privileges to perform CREATE operation on resource AE_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | notificationURI attribute and  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | notificationURI attribute and  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
+———————-+——————————————————————————————————————–+————-+
	TP Id
	PICS Selection
	Reference
	ATTRIBUTE_NAME

	TP/oneM2M/AE/SUB/CRE/002_ACPI
	PICS_SUB_ACPI
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.4.9.1
	accessControlPolicyIDs

	TP/oneM2M/AE/SUB/CRE/002_ENC
	PICS_SUB_ENC
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.4.9.1
	eventNotificationCriteria

	TP/oneM2M/AE/SUB/CRE/002_NCT
	PICS_SUB_NCT
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.4.9.1
	notificationContentType

	TP/oneM2M/AE/SUB/CRE/002_NEC
	PICS_SUB_NEC
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.4.9.1
	notificationEventCat

	TP/oneM2M/AE/SUB/CRE/002_SU
	PICS_SUB_SU
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.4.9.1
	subscriberURI



TP/oneM2M/AE/SUB/CRE/003
	TP Id
	TP/oneM2M/AE/SUB/CRE/003

	Test objective
	Check that the IUT sends a <group>/fopt subscription creation request with optional attributes notificationForwardingURI and groupID when it is triggered

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.7.10, TS-0004 [2], clause 7.4.14.2.3

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
and the IUT having a <group> resource as TARGET_RESOURCE_ADDRESS containing members which are subscribable
the IUThaving privileges to perform CREATE operation on <group> members
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | groupID, notificationURI attribute and  | |
                     | notificationForwardingURI attribute set  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | groupID, notificationURI attribute and  | |
                     | notificationForwardingURI attribute set  | |
                     |} | |
+———————-+———————————————————————————————————————————————–+————-+
7.2.1.4.2	NOTIFY Operation
TP/oneM2M/AE/SUB/NTF/001
	TP Id
	TP/oneM2M/AE/SUB/NTF/001

	Test objective
	Check that the IUT sends a Notify Response to the hosting CSE when receiving a Notify request containing a single notification

	Reference
	TS-0001 [1], clause 6.1.12, TS-0004 [2], clause 7.5.1.2

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT having been registered and
the IUT having created subscription resource under the CSE and
the IUT being reachable through a URL ACCESSIBLE_URL
}



·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE |
                     | the IUT receives a NOTIFY Request from hosting CSE containing  | |
                     | Content containing  | |
                     | notification message representation  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid NOTIFY Response to the hosting CSE containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————–+————-+
TP/oneM2M/AE/SUB/NTF/002
	TP Id
	TP/oneM2M/AE/SUB/NTF/002

	Test objective
	Check that the IUT sends a Notify Response to the hosting CSE when receiving a Notify request containing aggregated notifications

	Reference
	TS-0001 [1], clause 6.2.12, TS-0004 [2], clause 7.5.1.2

	Config Id
	CF03

	Parent Release
	Release 1

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT having been registered and
the IUT having created subscription resource at <group>/fopt with notificationForwardingURI set and
the IUT being reachable through a URL ACCESSIBLE_URL
}



·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE |
                     | the IUT receives a NOTIFY Request from hosting CSE containing  | |
                     | Content containing  | |
                     |aggregatedNotification message representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid Response to the hosting CSE containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+——————————————————————————————————————–+————-+
7.2.1.5	Communication Management and Delivery Handling (CMDH)
7.2.1.5.1	Resource pollingChannel (PCH)
TP/oneM2M/AE/PCH/001
	TP Id
	TP/oneM2M/AE/PCH/001

	Test objective
	Check that the IUT which performs polling sends the Notify request to <pollingChannelURI> Hosting CSE after receiving response using polling channel

	Reference
	TS-0001 [1], clause 10.2.13.8 & TS-0004 [2], clause 7.4.22.2.5

	Config Id
	CF03

	Parent Release
	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT be ing in the "initial state"
and the IUT having registered to a CSE1
and the IUT having a <pollingChannel> resource
and the IUT having sent a retrieve Request to the CSE
To set to POLLINGCHANNELURI_RESOURCE_ADDRESS
and the CSE having re ceived the Request from Originator containing
To set to AE_RESOURCE_ADDRESS and
From set to ORIGINATOR_ID
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a polling Response from the CSE containing  | |
                     |Response Status Code set to 2000 (OK)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a NOTIFY Request to the CSE containing  | |
                     | To set to POLLINGCHANNELURI_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
	Note: Based on figure 10.2.13.1-1 in TS-0001[1] step 004 and 005



TP/oneM2M/AE/PCH/002
	TP Id
	TP/oneM2M/AE/PCH/002

	Test objective
	Check that the IUT sends an RETRIEVE Request to <pollingChannelURI> resource
See the Note below

	Reference
	TS-0001 [1], clause 10.2.13.6, TS-0004 [2], clause 7.4.22.2.2

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the AEhaving a child <pollingChannel> resource
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to POLLINGCHANNELURI _RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid RETRIEVE Request c ontaining  | |
                     | To set to POLLINGCHANNELURI _RESOURCE_ADDRESS  | |
                     |From set to AE_ID  | |
                     |} | |
	Note: Based on figure 10.2.5.12-1 in TS-0001[1] step 001.



7.2.1.6	Ontology based Interworking IPE (OBI)
7.2.1.6.1	Initialization sequence
TP/oneM2M/AE/OBI/INI/001
	TP Id
	TP/oneM2M/AE/OBI/INI/001

	Test objective
	Check that the IUT starts the Initialization sequence of an Ontology based Interworking IPE and retrieves the formal description of the ontology

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.16, TS-0004 [2], clause 7.2.2.1 and 7.4.37, TS-0030 [8], clause 6.2.1.2 item 1.

	Config Id
	CF07

	Parent Release
	Release 3

	Initial conditions
	with {
the IUT being registeredand
the IUT being in the "initial state" and
the IUThaving privileges to perform RETRIEVE operation on formal description of the ontology at AE_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a request to get the formal description of the Ontology  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |Ontology server <= IUT|
                     | the IUT sends a valid HTTP GET Request to Ontology server containing  | |
                     | anURI  | |
                     | indicating the address where to get the Ontology  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————-+———————-+
7.2.1.6.2	CREATE Operation
TP/oneM2M/AE/OBI/CRE/001
	TP Id
	TP/oneM2M/AE/OBI/CRE/001

	Test objective
	Check that the IUT sends an AE initial registration request when it is started

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case C, and clause 9.6.19, TS-0030 [8], clause 6.2.1.2

	Config Id
	CF07

	Parent Release
	Release 3

	PICS Selection
	PICS_AE_IPE

	Initial conditions
	with {
the IUT never being registered and
the IUT being in the "initial state" and
the IUThaving got a valid APP-ID
}



·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | Toset to CSE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 2 (AE) and  | |
                     | Content containing  | |
                     |AE resource representation  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request to CSE containing  | |
                     | Resource Type set to 2 (AE) and  | |
                     | To set to CSE_RESOURCE_ADDRESS and  | |
                     | From set to empty and  | |
                     | Content containing  | |
                     |AE‑IPE resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————-+————-+
7.2.1.6.3	RETRIEVE Operation
TP/oneM2M/AE/OBI/RET/001
	TP Id
	TP/oneM2M/AE/OBI/RET/001

	Test objective
	Check that the IUT accepts a retrieval request resource and responds 2000 (OK) status

	Reference
	TS-0001 [1], clause 10.2.3.2 and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.2, TS-0030 [8], clause 6.2.2.2.1.

	Config Id
	CF07

	Parent Release
	Release 3

	PICS Selection
	PICS_AE_IPE

	Initial conditions
	with {
the IUT being registeredand
the IUT being in the "initial state" and
the IUThaving retrieved and parsed the formal description of the ontology and
the IUThaving performed DISCOVERY of non-oneM2M devices
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid RETRIEVE Request from CSE containing  | |
                     | To set to AE_IPE_ID and  | |
                     | From set to CSE_RESOURCE_ADDRESS and  | |
                     | no Content   | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Resource Type set to 28 (flexContainer) and   | |
                     | Content containing  | |
                     | Non‑oneM2M AE resource representation as a specialization of <flexContainer>  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+
TP/oneM2M/AE/OBI/RET/002
	TP Id
	TP/oneM2M/AE/OBI/RET/002

	Test objective
	Check that the IUT accepts a retrieval request resource with the optional ATTRIBUTE

	Reference
	TS-0001 [1], clause 10.2.3.2and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.2, TS-0030 [8], clause 6.2.2.2.1.

	Config Id
	CF07

	Parent Release
	Release 3

	PICS Selection
	PICS_AE_IPE

	Initial conditions
	with {
the IUT being registeredand
the IUT being in the "initial state" and
the IUThaving retrieved and parsed the formal description of the ontology and
the IUThaving performed DISCOVERY of non-oneM2M devices
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Resource Type set to 28 (flexContainer) and   | |
                     | Content containing  | |
                     | Non‑oneM2M resource as a specialization of <flexContainer> containing  | |
                     | valid ATTRIBUTE attribute  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+
TP/oneM2M/AE/OBI/RET/003
	TP Id
	TP/oneM2M/AE/OBI/RET/003

	Test objective
	Check that the IUT has performed DISCOVERY of non-oneM2M devices during initialization sequence

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.16, TS-0004 [2], clause 7.2.2.1 and 7.4.37, TS-0030 [8], clause 6.2.1.2 item 5.

	Config Id
	CF07

	Parent Release
	Release 3

	PICS Selection
	PICS_AE_IPE, PICS_AE_IPE_DISCOVERY

	Initial conditions
	with {
the IUT being registeredand
the IUT being in the "initial state" and
the IUThaving retrieved and parsed the formal description of the ontology and
the IUThaving performed DISCOVERY of non-oneM2M devices and
the IUT having discovered a non-oneM2M device with
a valid address value
indicating NON_ONEM2M_AE_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid RETRIEVE Request from CSE containing  | |
                     | To set to NON_ONEM2M_AE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | non‑oneM2M devices resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————-+————-+
TP/oneM2M/AE/OBI/RET/004
	TP Id
	TP/oneM2M/AE/OBI/RET/004

	Test objective
	Check that the IUT continues to discover the devices in the non-oneM2M area

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.16, TS-0004 [2], clause 7.2.2.1 and 7.3.3.14, TS-0030 [8], clause 6.2.2.1.

	Config Id
	CF07

	Parent Release
	Release 3

	PICS Selection
	PICS_AE_IPE, PICS_AE_IPE_DISCOVERY

	Initial conditions
	with {
the IUT being registeredand
the IUT being in the "initial state" and
the IUThaving retrieved and parsed the formal description of the ontology and
the IUThaving performed DISCOVERY of non-oneM2M devices and
the IUT having discovered a new non-oneM2M device with
a valid address value
indicating NON_ONEM2M_NEW_AE_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid RETRIEVE Request from CSE containing  | |
                     | To set to NON_ONEM2M_NEW_AE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | non‑oneM2M devices resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————–+————-+
TP/oneM2M/AE/OBI/RET/005
	TP Id
	TP/oneM2M/AE/OBI/RET/005

	Test objective
	Check that the IUT continues to discover the devices in the non-oneM2M area

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.16, TS-0004 [2], clause 7.2.2.1 and 7.3.3.14, TS-0030 [8], clause 6.2.2.1.

	Config Id
	CF07

	Parent Release
	Release 3

	PICS Selection
	PICS_AE_IPE, PICS_AE_IPE_DISCOVERY

	Initial conditions
	with {
the IUT being registeredand
the IUT being in the "initial state" and
the IUThaving retrieved and parsed the formal description of the ontology and
the IUThaving performed DISCOVERY of non-oneM2M devices and
An existing non-oneM2M (NON_ONEM2M_NEW_AE_RESOURCE_ADDRESS) device was switched off
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid RETRIEVE Request from CSE containing  | |
                     | To set to NON_ONEM2M_NEW_AE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————–+————-+
TP/oneM2M/AE/OBI/RET/006
	TP Id
	TP/oneM2M/AE/OBI/RET/006

	Test objective
	Check that the IUT accepts "on demand" discovery

	Reference
	TS-0001 [1], clause 10.1.1.1 and 10.2.4.16, TS-0004 [2], clause 7.2.2.1 and 7.3.3.14, TS-0030 [8], clause 6.2.2.1.

	Config Id
	CF07

	Parent Release
	Release 3

	PICS Selection
	PICS_AE_IPE, PICS_AE_IPE_DISCOVERY

	Initial conditions
	with {
the IUT being registeredand
the IUT being in the "initial state" and
the IUThaving retrieved and parsed the formal description of the ontology and
the IUThaving performed DISCOVERY of non-oneM2M devices
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to IPE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 28 (flexContainer) and   | |
                     | From set to CSE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsageset to 1 (IPE On‑demand Discovery)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————–+————-+
7.2.1.7	Home Appliance Information Model and Mapping (HAIM)
7.2.1.7.1	CREATE Operation
TP/oneM2M/AE/HAIM/CRE/001
	TP Id
	TP/oneM2M/AE/HAIM/CRE/001

	Test objective
	Check that the IUT creates a [_ _HAIM_DEVICE] resource as a specialization of the <flexContainer> resource on the hosting CSE using the appropriate 'DeviceClass ID'

	Reference
	TS-0001 [1], clause 9.6.1.2.2.3, and TS-0023 [7], clauses 5.4, 6.2.2 and 6.4.2

	Config Id
	CF03

	Parent Release
	Release 3

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUThaving privileges to perform CREATE operation on resource
TARGET_RESOURCE_ADDRESS and
the IUT exposing a controlling interface for a HAIM_DEVICE
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     | Content set to [HAIM_DEVICE] resource  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | Content containing  | |
                     | [HAIM_DEVICE] resource as a specialization of <flexContainer> containing  | |
                     | containerDefinition attributeset to  | |
                     | "org.onem2m.home.device._HAIM_DEVICE"_  | |
                     |} | |
+———————-+————————————————————————————————————————————————————-+————-+
	TP Id
	HAIM_DEVICE

	TP/oneM2M/AE/HAIM/CRE/001_AIR
	deviceAirConditioner

	TP/oneM2M/AE/HAIM/CRE/001_CLO
	deviceClothesWasher

	TP/oneM2M/AE/HAIM/CRE/001_ELE
	deviceElectricVehicleCharger

	TP/oneM2M/AE/HAIM/CRE/001_LIG
	deviceLight

	TP/oneM2M/AE/HAIM/CRE/001_MIC
	deviceMicrogeneration

	TP/oneM2M/AE/HAIM/CRE/001_OVE
	deviceOven

	TP/oneM2M/AE/HAIM/CRE/001_REF
	deviceRefrigerator

	TP/oneM2M/AE/HAIM/CRE/001_ROB
	deviceRobotCleaner

	TP/oneM2M/AE/HAIM/CRE/001_SMA
	deviceSmartElectricMeter

	TP/oneM2M/AE/HAIM/CRE/001_STO
	deviceStorageBattery

	TP/oneM2M/AE/HAIM/CRE/001_TEL
	deviceTelevision

	TP/oneM2M/AE/HAIM/CRE/001_THE
	deviceThermostat

	TP/oneM2M/AE/HAIM/CRE/001_WAT
	deviceWaterHeater



TP/oneM2M/AE/HAIM/CRE/002
	TP Id
	TP/oneM2M/AE/HAIM/CRE/002

	Test objective
	Check that the IUT creates a [_ _HAIM_MODULE] resource as a specialization of the <flexContainer> resource and as a child of [HAIM_DEVICE] resouce on the hosting CSE using the appropriate ModuleClass ID

	Reference
	TS-0001 [1], clause 9.6.1.2.2.3, and TS-0023 [7], clauses 5.3, 5.4, 6.2.2 and 6.4.3

	Config Id
	CF03

	Parent Release
	Release 3

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUThaving privileges to perform CREATE operation on resource
TARGET_RESOURCE_ADDRESS and
the IUT exposing a controlling interface for a HAIM_DEVIC E
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     | Content set to [HAIM_DEVICE] resource  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | Content containing  | |
                     | [HAIM_DEVICE] resource containing  | |
                     | [HAIM_MODULE] resource as a specialization of  | |
                     | <flexContainer> as an instance of the HAIM_MODULE  | |
                     | ModuleClass containing  | |
                     | containerDefinition attributeset to  | |
                     | "org.onem2m.home. moduleclass._HAIM_MODULE"_  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————+————-+
	TP Id
	HAIM_MODULE
	HAIM_DEVICE

	TP/oneM2M/AE/HAIM/CRE/002_SEL
	binarySwitch
	deviceElectricVehicleCharger

	TP/oneM2M/AE/HAIM/CRE/002_SLI
	binarySwitch
	deviceLight

	TP/oneM2M/AE/HAIM/CRE/002_SWA
	binarySwitch
	deviceWaterHeater

	TP/oneM2M/AE/HAIM/CRE/002_FEL
	faultDetection
	deviceElectricVehicleCharger

	TP/oneM2M/AE/HAIM/CRE/002_REL
	runState
	deviceElectricVehicleCharger

	TP/oneM2M/AE/HAIM/CRE/002_BEL
	battery
	deviceElectricVehicleCharger

	TP/oneM2M/AE/HAIM/CRE/002_BST
	battery
	deviceStorageBattery

	TP/oneM2M/AE/HAIM/CRE/002_VEL
	electricVehicleConnector
	deviceElectricVehicleCharger

	TP/oneM2M/AE/HAIM/CRE/002_GMI
	energyGeneration
	deviceMicrogeneration

	TP/oneM2M/AE/HAIM/CRE/002_CSM
	energyConsumption
	deviceSmartElectricMeter

	TP/oneM2M/AE/HAIM/CRE/002_TTH
	temperature
	deviceThermostat



TP/oneM2M/AE/HAIM/CRE/003
	TP Id
	TP/oneM2M/AE/HAIM/CRE/003

	Test objective
	Check that the IUT creates the appropriate Properties, according to the HAIM_DEVICE model, as [customAttribute] attributes of a [deviceInfo] resource which is a child-resource of the <node> resource linked by the nodelink attribute of the HAIM_DEVICE model

	Reference
	TS-0001 [1], clause 9.6.1.2.2.3, and TS-0023 [7], clauses 5.4, 5.6 and 6.2.5

	Config Id
	CF03

	Parent Release
	Release 3

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUThaving privileges to perform CREATE operation on resource
TARGET_RESOURCE_ADDRESS and
the IUT exposing a controlling interface for a HAIM_DEVICE
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     | Content set to [HAIM_DEVICE] resource  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | Content containing  | |
                     | [HAIM_DEVICE] resource containing  | |
                     | nodelink attribute containing  | |
                     | link to a <node> resource on the same hosting CSE containing  | |
                     | [deviceInfo] resource  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	HAIM_DEVICE

	TP/oneM2M/AE/HAIM/CRE/003_AIR
	deviceAirConditioner

	TP/oneM2M/AE/HAIM/CRE/003_CLO
	deviceClothesWasher

	TP/oneM2M/AE/HAIM/CRE/003_ELE
	deviceElectricVehicleCharger

	TP/oneM2M/AE/HAIM/CRE/003_LIG
	deviceLight

	TP/oneM2M/AE/HAIM/CRE/003_MIC
	deviceMicrogeneration

	TP/oneM2M/AE/HAIM/CRE/003_OVE
	deviceOven

	TP/oneM2M/AE/HAIM/CRE/003_REF
	deviceRefrigerator

	TP/oneM2M/AE/HAIM/CRE/003_ROB
	deviceRobotCleaner

	TP/oneM2M/AE/HAIM/CRE/003_SMA
	deviceSmartElectricMeter

	TP/oneM2M/AE/HAIM/CRE/003_STO
	deviceStorageBattery

	TP/oneM2M/AE/HAIM/CRE/003_TEL
	deviceTelevision

	TP/oneM2M/AE/HAIM/CRE/003_THE
	deviceThermostat

	TP/oneM2M/AE/HAIM/CRE/003_WAT
	deviceWaterHeater



TP/oneM2M/AE/HAIM/CRE/004
	TP Id
	TP/oneM2M/AE/HAIM/CRE/004

	Test objective
	Check that the IUT creates the appropriate Properties, according to the HAIM_MODULE model, as [customAttribute] attributes of the [HAIM_MODULE] resource on the hosting CSE, with [customAttribute] name set to the prefix 'prop' plus the Property name

	Reference
	TS-0001 [1], clause 9.6.1.2.2.3, and TS-0023 [7], clauses 5.3 and 6.2.5

	Config Id
	CF03

	Parent Release
	Release 3

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUThaving privileges to perform CREATE operation on resource
TARGET_RESOURCE_ADDRESS and
the IUT exposing a controlling interface for a HAIM_DEVICE
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     | Content set to [HAIM_DEVICE] resource  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |CSE <= IUT |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | [HAIM_DEVICE ] resource containing  | |
                     | [HAIM_MODULE ] resource as a specialization of  | |
                     | <flexContainer> containing  | |
                     | appropriate [customAttribute] attributes with name set to  | |
                     | "prop_"_ prefix plus the Property name  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	HAIM_DEVICE
	HAIM_MODULE

	TP/oneM2M/AE/HAIM/CRE/004_VBT
	deviceElectricVehicleCharger
	battery

	TP/oneM2M/AE/HAIM/CRE/004_SBT
	deviceStorageBattery
	battery

	TP/oneM2M/AE/HAIM/CRE/004_VCN
	deviceElectricVehicleCharger
	electricVehicleConnector



TP/oneM2M/AE/HAIM/CRE/005
	TP Id
	TP/oneM2M/AE/HAIM/CRE/005

	Test objective
	Check that the IUT creates the appropriate DataPoints, according to the HAIM_MODULE model, as [customAttribute] attributes of the [HAIM_MODULE] resource on the hosting CSE, with [customAttribute] name set to the Datapoint name

	Reference
	TS-0001 [1], clause 9.6.1.2.2.3, and TS-0023 [7], clauses 5.3 and 6.2.6

	Config Id
	CF03

	Parent Release
	Release 3

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUThaving privileges to perform CREATE operation on resource
TARGET_RESOURCE_ADDRESS and
the IUT exposing a controlling interface for a HAIM_DEVICE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     | Content set to [HAIM_DEVICE] resource  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |CSE <= IUT |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | [HAIM_DEVICE ] resource containing  | |
                     | [HAIM_MODULE ] resource as a specialization of  | |
                     | <flexContainer> containing  | |
                     | appropriate [customAttribute] attributes with name set to  | |
                     | the DataPoint name  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	HAIM_DEVICE
	HAIM_MODULE

	TP/oneM2M/AE/HAIM/CRE/005_ACT
	deviceAirConditioner
	temperature

	TP/oneM2M/AE/HAIM/CRE/005_ACU
	deviceAirConditioner
	turbo

	TP/oneM2M/AE/HAIM/CRE/005_ACW
	deviceAirConditioner
	airflow

	TP/oneM2M/AE/HAIM/CRE/005_CWS
	deviceClothesWasher
	spinLevel

	TP/oneM2M/AE/HAIM/CRE/005_CWW
	deviceClothesWasher
	waterFlow

	TP/oneM2M/AE/HAIM/CRE/005_VCB
	deviceElectricVehicleCharger
	battery

	TP/oneM2M/AE/HAIM/CRE/005_VCE
	deviceElectricVehicleCharger
	electricVehicleConnector

	TP/oneM2M/AE/HAIM/CRE/005_LBR
	deviceLight
	brightness

	TP/oneM2M/AE/HAIM/CRE/005_LCL
	deviceLight
	colour

	TP/oneM2M/AE/HAIM/CRE/005_LCS
	deviceLight
	colourSaturation

	TP/oneM2M/AE/HAIM/CRE/005_LFD
	deviceLight
	faultDetection

	TP/oneM2M/AE/HAIM/CRE/005_RDS
	deviceRefrigerator
	doorStatus

	TP/oneM2M/AE/HAIM/CRE/005_RPS
	deviceRefrigerator
	powerSave

	TP/oneM2M/AE/HAIM/CRE/005_EEC
	deviceSmartElectricMeter
	energyConsumption

	TP/oneM2M/AE/HAIM/CRE/005_TVA
	deviceTelevision
	mediaInput

	TP/oneM2M/AE/HAIM/CRE/005_TVV
	deviceTelevision
	audioVolume

	TP/oneM2M/AE/HAIM/CRE/005_TVB
	deviceTelevision
	binarySwitch

	TP/oneM2M/AE/HAIM/CRE/005_TVC
	deviceTelevision
	televisionChannel

	TP/oneM2M/AE/HAIM/CRE/005_WHB
	deviceWaterHeater
	boiler

	TP/oneM2M/AE/HAIM/CRE/005_WHC
	deviceWaterHeater
	clock

	TP/oneM2M/AE/HAIM/CRE/005_WHH
	deviceWaterHeater
	hotWaterSupply

	TP/oneM2M/AE/HAIM/CRE/005_WHR
	deviceWaterHeater
	runState



TP/oneM2M/AE/HAIM/CRE/006
	TP Id
	TP/oneM2M/AE/HAIM/CRE/006

	Test objective
	Check that the IUT creates the child Action module resources according to the SDT_MODULE model

	Reference
	TS-0001 [1], clause 9.6.1.2.2.3, and TS-0023 [7], clauses 5.3, 5.4, 5.5, 6.2, 6.4

	Config Id
	CFG03

	Parent Release
	Release 4

	PICS Selection
	PICS_???

	Initial conditions
	with {
the IUT being registeredand
the IUT being switched on and
the IUThaving privileges to perform CREATE operation on resource
TARGET_RESOURCE_ADDRESS and
the IUT having created a resource at SDT_DEVICE_ADDRESS of type SDT_DEVICE
containing child SDT_MODULE resource at SDT_MODULE_RESOURCE_ADDRESS
}



·                   +----------------------------------------------------------------------------------------------------------------+-------------+

·                       |when {   |NA |
                      | } | |
·                   +----------------------------------------------------------------------------------------------------------------+-------------+

·                       |then {  |IUT => CSE |
                      | the IUT sends a valid CREATE Request containing  | |
                      | To set to SDT_MODULE _RESOURCE_ADDRESS and  | |
                      | Content containing  | |
                      | ACTION_NAME resource as a specialization of  | |
                      | <flexContainer> containing  | |
                      | CUSTOM_ATTRIBUTES attributes and  | |
                      | containerDefinition attributeset to  | |
                      | "org.onem2m._DOMAIN_ .action._ACTION_NAME_ " and  | |
                      | resourceName attributeset to ACTION_NAME  | |
                      |} | |
+———————–+—————————————————————————————————————-+————-+
	TP Id
	DOMAIN
	HAIM**_DEVICE**
	CUSTOM_ ATTRIBUTES (of action)
	HAIMMODULE(parent resource)
	ACTION_NAME

	TP/oneM2M/AE/HAIM/CRE/006_STPR
	Common
	device3DPrinter
	none
	3Dprinter
	start3Dprint

	TP/oneM2M/AE/HAIM/CRE/006_SPPR
	Common
	device3DPrinter
	none
	3Dprinter
	stop3Dprint

	TP/oneM2M/AE/HAIM/CRE/006_UPV
	Common
	deviceAudioReceiver,device3DDisplay,deviceSetTopBox,deviceTelevision,deviceHandheldPTTTerminal,deviceTrainborneTerminal,deviceCardRecharingMachine,deviceSmartGate,deviceSmartScreenDoor
	none
	audioVolume
	upVolume

	TP/oneM2M/AE/HAIM/CRE/006_DWV
	Common
	deviceAudioReceiver,device3DDisplay,deviceSetTopBox,deviceTelevision,deviceHandheldPTTTerminal,deviceTrainborneTerminal,deviceCardRecharingMachine,deviceSmartGate,deviceSmartScreenDoor
	none
	audioVolume
	downVolume

	TP/oneM2M/AE/HAIM/CRE/006_TBS
	Common
	device3DPrinter, deviceAudioReceiver,deviceLight,deviceMultiFunctionPrinter,devicePrinter,deviceScanner,deviceSmartPlug,deviceSwitch,device3DDisplay,device3DScanner,subDeviceCuff,subDevicePowerOutlet
	none
	binarySwitch
	toggle

	TP/oneM2M/AE/HAIM/CRE/006_TBS
	City
	deviceOutdoorLamp,deviceSmartElectricMeter,deviceSmartGasMeter,deviceSmartWaterMeter
	none
	binarySwitch
	toggle

	TP/oneM2M/AE/HAIM/CRE/006_TBS
	Health
	deviceBloodPressureMonitor
	none
	binarySwitch
	toggle

	TP/oneM2M/AE/HAIM/CRE/006_TBS
	Home
	deviceAirConditioner,deviceAirPurifier,deviceClothesDryer,deviceClothesWasher,deviceClothesWasherDryer,deviceCoffeeMachine,deviceCookerHood,deviceDehumidifier,deviceDishWasher,deviceFan,deviceHomeCCTV,deviceHumidifier,deviceKettle,deviceMicrogeneration,deviceOven,deviceRefrigerator,deviceRiceCooker,deviceRobotCleaner,deviceSetTopBox,deviceSteamCloset,deviceStorageBattery,deviceTelevision,deviceWaterHeater,deviceBottleWarmer,deviceGarbageDisposal,deviceWaterPurifier
	none
	binarySwitch
	toggle

	TP/oneM2M/AE/HAIM/CRE/006_TBS
	Vehicular
	deviceElectricVehicleCharger
	none
	binarySwitch
	toggle

	TP/oneM2M/AE/HAIM/CRE/006_TBS
	Railway
	deviceHandheldPTTTerminal,deviceCardRecharingMachine,deviceSmartGate,deviceSmartScreenDoor
	none
	binarySwitch
	toggle

	TP/oneM2M/AE/HAIM/CRE/006_DNV
	Common
	subDevicePowerOutlet
	none
	numberValue
	decrementNumberValue

	TP/oneM2M/AE/HAIM/CRE/006_INV
	Common
	subDevicePowerOutlet
	none
	numberValue
	incrementNumberValue

	TP/oneM2M/AE/HAIM/CRE/006_RNV
	Common
	subDevicePowerOutlet
	none
	numberValue
	resetNumberValue

	TP/oneM2M/AE/HAIM/CRE/006_OOL
	Common
	deviceDoor,waterValve
	none
	openLevel
	open

	TP/oneM2M/AE/HAIM/CRE/006_OOL
	Home
	deviceWindowShade
	none
	openLevel
	open

	TP/oneM2M/AE/HAIM/CRE/006_COL
	Common
	deviceDoor,waterValve
	none
	openLevel
	close

	TP/oneM2M/AE/HAIM/CRE/006_COL
	Home
	deviceWindowShade
	none
	openLevel
	close

	TP/oneM2M/AE/HAIM/CRE/006_CPC
	Railway
	deviceHandheldPTTTerminal,deviceTrainborneTerminal
	none
	phoneCall
	call

	TP/oneM2M/AE/HAIM/CRE/006_APC
	Railway
	deviceHandheldPTTTerminal,deviceTrainborneTerminal
	none
	phoneCall
	answer

	TP/oneM2M/AE/HAIM/CRE/006_HPC
	Railway
	deviceHandheldPTTTerminal,deviceTrainborneTerminal
	none
	phoneCall
	hangup

	TP/oneM2M/AE/HAIM/CRE/006_NTPC
	Common
	deviceCamera
	none
	playerControl
	nextTrack

	TP/oneM2M/AE/HAIM/CRE/006_NTPC
	Home
	deviceHomeCCTV,deviceTelevision
	none
	playerControl
	nextTrack

	TP/oneM2M/AE/HAIM/CRE/006_PTPC
	Common
	deviceCamera
	none
	playerControl
	previousTrack

	TP/oneM2M/AE/HAIM/CRE/006_PTPC
	Home
	deviceHomeCCTV,deviceTelevision
	none
	playerControl
	previousTrack

	TP/oneM2M/AE/HAIM/CRE/006_MSS
	Common
	deviceGenericSensor
	none
	smokeSensor
	mute

	TP/oneM2M/AE/HAIM/CRE/006_MSS
	Home
	deviceHomeCCTV
	none
	smokeSensor
	mute

	TP/oneM2M/AE/HAIM/CRE/006_UCTC
	Home
	deviceSetTopBox,deviceTelevision
	none
	televisionChannel
	upChannel

	TP/oneM2M/AE/HAIM/CRE/006_DCTC
	Home
	deviceSetTopBoxdeviceTelevision
	none
	televisionChannel
	downChannel

	TP/oneM2M/AE/HAIM/CRE/006_RTM
	Common
	deviceServiceButton
	none
	textMessage
	resetTextMessage

	TP/oneM2M/AE/HAIM/CRE/006_ACT
	Common
	deviceLight,deviceThermostat
	none
	timer
	activateClockTimer

	TP/oneM2M/AE/HAIM/CRE/006_ACT
	City
	deviceOutdoorLamp
	none
	timer
	activateClockTimer

	TP/oneM2M/AE/HAIM/CRE/006_ACT
	Home
	deviceAirConditioner,deviceAirPurifier,deviceClothesWasher,deviceClothesWasherDryer,deviceDehumidifier,deviceOven,deviceRiceCooker,deviceRobotCleaner,deviceWindowShade,deviceWaterPurifier
	none
	timer
	activateClockTimer

	TP/oneM2M/AE/HAIM/CRE/006_DCT
	Common
	deviceLight,deviceThermostat
	none
	timer
	deactivateClockTimer

	TP/oneM2M/AE/HAIM/CRE/006_DCT
	City
	deviceOutdoorLamp
	none
	timer
	deactivateClockTimer

	TP/oneM2M/AE/HAIM/CRE/006_DCT
	Home
	deviceAirConditioner,deviceAirPurifier,deviceClothesWasher,deviceClothesWasherD ryer,deviceDehumidifier,deviceOven,deviceRiceCooker,deviceRobotCleaner,deviceWindowShade,deviceWaterPurifier
	none
	timer
	deactivateClockTimer

	TP/oneM2M/AE/HAIM/CRE/006_RRG
	City
	deviceWeatherStation
	none
	rainGauge
	reset

	TP/oneM2M/AE/HAIM/CRE/006_RDMA
	management
	flexNode
	rebootType
	dmAgent
	reboot

	TP/oneM2M/AE/HAIM/CRE/006_DPDMA
	management
	flexNode
	resut, name, version, url
	dmAgent
	deployPackage

	TP/oneM2M/AE/HAIM/CRE/006_RDMIO
	management
	flexNode
	resut, address
	dmDataModelIO
	readIO

	TP/oneM2M/AE/HAIM/CRE/006_WDMIO
	management
	flexNode
	resut, address, payload
	dmDataModelIO
	writeIO

	TP/oneM2M/AE/HAIM/CRE/006_UDMF
	management
	flexNode
	Result, url, version
	dmFirmware
	updateFirmware

	TP/oneM2M/AE/HAIM/CRE/006_TDMF
	management
	flexNode
	resut
	dmFirmware
	toggle

	TP/oneM2M/AE/HAIM/CRE/006_ADMS
	management
	flexNode
	none
	dmSoftware
	activate

	TP/oneM2M/AE/HAIM/CRE/006_DDMS
	management
	flexNode
	none
	dmSoftware
	deactivate

	TP/oneM2M/AE/HAIM/CRE/006_RDMEL
	management
	flexNode
	Start, end
	dmEventLog
	retrieveLog

	TP/oneM2M/AE/HAIM/CRE/006_IDMP
	management
	flexNode
	none
	dmPackage
	install

	TP/oneM2M/AE/HAIM/CRE/006_UDMP
	management
	flexNode
	none
	dmPackage
	uninstall

	TP/oneM2M/AE/HAIM/CRE/006_UPDMP
	management
	flexNode
	Version, url
	dmPackage
	update

	TP/oneM2M/AE/HAIM/CRE/006_EDMC
	management
	flexNode
	resut
	dmCapability
	enable

	TP/oneM2M/AE/HAIM/CRE/006_DDMC
	management
	flexNode
	resut
	dmCapability
	disable

	TP/oneM2M/AE/HAIM/CRE/006_FDMS
	management
	flexNode
	none
	dmStorage
	format

	TP/oneM2M/AE/HAIM/CRE/006_UDMS
	management
	flexNode
	none
	dmStorage
	unmount



TP/oneM2M/AE/HAIM/CRE/007
	TP Id
	TP/oneM2M/AE/HAIM/CRE/007

	Test objective
	Check that the IUT responds correctly when its ACTION_NAME resource is triggered.

	Reference
	TS-0001 [1], clause 9.6.1.2.2.3, and TS-0023 [7], clauses 5.3, 5.8 and 6.2.6

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered to CSE and
the IUT exposing a controlling interface for an ACTION_NAME and
the IUT having created on the CSE a SDT_MODULE at SDT_MODULE_ADDRESS
SDT_MODULE containing DATA_POINT set to a valid value and
the IUT having created on the CSE an ACTION_NAME at ACTION_NAME_ADDRESS
the IUT having created on the CSE a <subscription> at ACTION_NAME_ADDRESS
}



·                   +-----------------------------------------------------------------------------------------------------------+-------------+

·                       |when {   |CSE |
                      | The IUT receives a valid NOTIFY Request containing  | |
                      | operation set to UPDATE  | |
                      | subscriptionReference set to resource identifier of ACTION_NAME  | |
                      | containing valid ACTION_NAME representation containing  | |
                      | CUSTOM_ATTRIBUTE set to valid value  | |
                      |} | |
·                   +-----------------------------------------------------------------------------------------------------------+-------------+

·                       |then {  |IUT => CSE |
                      | the IUT sends a valid UPDATE Request containing  | |
                      | To set to SDT_MODULE_ADDRESS and  | |
                      | Content containing SDT_MODULE resource containing  | |
                      | a valid_DATA_POINT_ attribute  | |
                      | the IUT sends a valid NOTIFY Response containing  | |
                      | response status code 2000  | |
                      |} | |
+———————–+———————————————————————————————————–+————-+
	TP Id
	CUSTOM_ ATTRIBUTES (of HAIM module or ACTION module)
	**HAIM _MODULE(parent resource)**
	ACTION_NAME

	TP/oneM2M/AE/HAIM/UPD/007_STPR
	none
	3Dprinter
	start3Dprint

	TP/oneM2M/AE/HAIM/UPD/007_SPPR
	none
	3Dprinter
	stop3Dprint

	TP/oneM2M/AE/HAIM/UPD/006_UPV
	volumePercentage
	audioVolume
	upVolume

	TP/oneM2M/AE/HAIM/UPD/006_DWV
	volumePercentage
	audioVolume
	downVolume

	TP/oneM2M/AE/HAIM/UPD/006_TBS
	state
	binarySwitch
	toggle

	TP/oneM2M/AE/HAIM/UPD/006_DNV
	numberValue
	numberValue
	decrementNumberValue

	TP/oneM2M/AE/HAIM/UPD/006_INV
	numberValue
	numberValue
	incrementNumberValue

	TP/oneM2M/AE/HAIM/UPD/006_RNV
	numberValue
	numberValue
	resetNumberValue

	TP/oneM2M/AE/HAIM/UPD/006_OOL
	openLevel
	openLevel
	open

	TP/oneM2M/AE/HAIM/UPD/006_COL
	openLevel
	openLevel
	close

	TP/oneM2M/AE/HAIM/UPD/006_CPC
	callState
	phoneCall
	call

	TP/oneM2M/AE/HAIM/UPD/006_APC
	callState
	phoneCall
	answer

	TP/oneM2M/AE/HAIM/UPD/006_HPC
	callState
	phoneCall
	hangup

	TP/oneM2M/AE/HAIM/UPD/006_NTPC
	none
	playerControl
	nextTrack

	TP/oneM2M/AE/HAIM/UPD/006_PTPC
	none
	playerControl
	previousTrack

	TP/oneM2M/AE/HAIM/UPD/006_MSS
	dismantled
	smokeSensor
	mute

	TP/oneM2M/AE/HAIM/UPD/006_UCTC
	channelNumber
	televisionChannel
	upChannel

	TP/oneM2M/AE/HAIM/UPD/006_DCTC
	channelNumber
	televisionChannel
	downChannel

	TP/oneM2M/AE/HAIM/UPD/006_RTM
	textMessage
	textMessage
	resetTextMessage

	TP/oneM2M/AE/HAIM/UPD/006_ACT
	none
	timer
	activateClockTimer

	TP/oneM2M/AE/HAIM/UPD/006_DCT
	none
	timer
	deactivateClockTimer

	TP/oneM2M/AE/HAIM/UPD/006_RRG
	height
	rainGauge
	reset

	TP/oneM2M/AE/HAIM/UPD/006_RDMA
	state
	dmAgent
	reboot

	TP/oneM2M/AE/HAIM/UPD/006_DPDMA
	state
	dmAgent
	deployPackage

	TP/oneM2M/AE/HAIM/UPD/006_RDMIO
	resut
	dmDataModelIO
	readIO

	TP/oneM2M/AE/HAIM/UPD/006_WDMIO
	resut
	dmDataModelIO
	writeIO

	TP/oneM2M/AE/HAIM/UPD/006_UDMF
	resut
	dmFirmware
	updateFirmware

	TP/oneM2M/AE/HAIM/UPD/006_TDMF
	resut, primaryState, secondaryState
	dmFirmware
	toggle

	TP/oneM2M/AE/HAIM/UPD/006_ADMS
	state
	dmSoftware
	activate

	TP/oneM2M/AE/HAIM/UPD/006_DDMS
	state
	dmSoftware
	deactivate

	TP/oneM2M/AE/HAIM/UPD/006_RDMEL
	data
	dmEventLog
	retrieveLog

	TP/oneM2M/AE/HAIM/UPD/006_IDMP
	state
	dmPackage
	install

	TP/oneM2M/AE/HAIM/UPD/006_UDMP
	state
	dmPackage
	uninstall

	TP/oneM2M/AE/HAIM/UPD/006_UPDMP
	state
	dmPackage
	update

	TP/oneM2M/AE/HAIM/UPD/006_EDMC
	resut, currentState
	dmCapability
	enable

	TP/oneM2M/AE/HAIM/UPD/006_DDMC
	resut, currentState
	dmCapability
	disable

	TP/oneM2M/AE/HAIM/UPD/006_FDMS
	status
	dmStorage
	format

	TP/oneM2M/AE/HAIM/UPD/006_UDMS
	mounts
	dmStorage
	unmount



7.2.1.8	Security (SEC)
7.2.1.8.1	Authentication
7.2.1.8.1.1	ESPrim (ESP)
7.2.1.8.1.1.1	NOTIFY Operation
TP/oneM2M/AE/SEC/ESP/NTF/001
	TP Id
	TP/oneM2M/AE/SEC/ESP/NTF/001

	Test objective
	Check that the IUT sends a request for receiverESPrimRandObject, if the e2eSecInfo attribute of the Receiver's <remoteCSE> resource in CSE2 does not include a sharedReceiverESPrimRandObject

	Reference
	TS-0003 8.4.2 - step B.2D, TS-0004 7.5.1.2.11

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT having established a pairwiseESPrimKey with the Receiver (CSE1)
and the IUT having sent a RETRIEVE Request on the e2eSecInfo attribute in resource
TARGET_REMOTE_CSE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE2 |
                     | the IUT receives a valid Response from CSE2 containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     |<remoteCSE>resource containing   | |
                     | e2eSecInfo attribute containing  | |
                     | no sharedReceiverESPrimRandObject parameter  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE1 <= IUT |
                     | the IUT sends a valid NOTIFY Request to Receiver CSE(CSE1) containing  | |
                     | To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 3  | |
                     | (receiverESPrimRandObject Request)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————–+————-+
TP/oneM2M/AE/SEC/ESP/NTF/002
	TP Id
	TP/oneM2M/AE/SEC/ESP/NTF/002

	Test objective
	Check that the IUT sends a request for receiverESPrimRandObject to the Receiver if the_sharedReceiverESPrimRandObject_ parameter in the Receiver's <remoteCSE> resource located in CSE2 has expired

	Reference
	TS-0003 8.4.2 - step B.2D, TS-0004 7.5.1.2.11

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT having established a pairwiseESPrimKey with the Receiver CSE(CSE1)
and the IUT having sent a RETRIEVE Request on the e2eSecInfo on resource
TARGET_REMOTE_CSE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE2 |
                     | the IUT receives a valid Response from CSE2 containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     |<remoteCSE> resource containing   | |
                     | e2eSecInfo attribute containing  | |
                     | sharedReceiverESPrimRandObject parameter containing  | |
                     | ESPrimRandExpiry field set to an expired date  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE1 <= IUT |
                     | the IUT sends a valid NOTIFY Request to Receiver CSE containing  | |
                     | To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 3 (receiverESPrimRandObject  | |
                     | Request)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/AE/SEC/ESP/NTF/003
	TP Id
	TP/oneM2M/AE/SEC/ESP/NTF/003

	Test objective
	Check that the IUT sends a valid ESPrim object to the Receiver CSE

	Reference
	TS-0003 8.4.2 - step C.4, TS-0004 7.5.1.2.13, TS-0001 11.4.2

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUThaving received receiverESPrimRandObject
and the IUT having established a sessionESPrimKey with the Receiver CSE
}



·                  +-----------------------------------------------------------------------------------------------+-----------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid NOTIFY Request containing  | |
                     | To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 5 (ESPrim Object) and   | |
                     | esprimObject element  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------+-----------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid NOTIFY Request to the Receiver CSE containing To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 5 (ESPrim Object) and   | |
                     | esprimObject element set to a JSON Web Encryption (JWE)  | |
                     | Compact Serialization on inner request primitive  | |
                     |} | |
+———————-+———————————————————————————————–+—————————————————–+————-+
7.2.1.8.1.1.2	RETRIEVE Operation
TP/oneM2M/AE/SEC/ESP/RET/001
	TP Id
	TP/oneM2M/AE/SEC/ESP/RET/001

	Test objective
	Check that the IUT sends a valid request for e2eSecInfo attribute of the Receiver's <remoteCSE> resource in the CSE Registered with Receiver CSE

	Reference
	TS-0003 8.4.2 - step B.2A, TS-0004 7.5.1.2.11

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUThaving established a pairwiseESPrimKey with the Receiver CSE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE1 <= IUT |
                     | the IUT sends a valid RETRIEVE Request to CSE1 containing  | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | remoteCSE resourcecontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
+———————-+————————————————————————————————————————————–+————-+
TP/oneM2M/AE/SEC/ESP/RET/002
	TP Id
	TP/oneM2M/AE/SEC/ESP/RET/002

	Test objective
	Check that the IUT sends a notification containing an inner "receiverESPrimRandObject request" to the Receiver if the sharedReceiverESPrimRandObject parameter is not present in the <remoteCSE> resource in the CSE Registered with Receiver CSE

	Reference
	TS-0003 8.4.2 - step B.2D, TS-0004 7.5.1.2.11

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having established a pairwiseESPrimKey with the Originator
and the <remoteCSE> resource at TARGET_REMOTE_CSE_ADDRESS contain ing
e2eSecInfo attribute with no sharedReceiverESPrimRandObject parameter

}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing   | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFICATION Request containing  | |
                     | To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 3 (receiverESPrimRandObject  | |
                     | Request)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ESP/RET/003
	TP Id
	TP/oneM2M/AE/SEC/ESP/RET/003

	Test objective
	Check that the IUT sends a notification containing an inner "receiverESPrimRandObject request" to the Receiver if the sharedReceiverESPrimRandObject in the <remoteCSE> resource is expired

	Reference
	TS-0003 8.4.2 - step B.2D, TS-0004 7.5.1.2.11

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having established a pairwiseESPrimKey with the Originator
and the <remoteCSE> resource at TARGET_REMOTE_CSE_ADDRESS contain ing
e2eSecInfo attribute with an expired sharedReceiverESPrimRandObject parameter
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing   | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFICATION Request containing  | |
                     | To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 3 (receiverESPrimRandObject  | |
                     | Request)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————+————-+
7.2.1.8.1.2 Roles (ROL)
7.2.1.8.1.2.1	CREATE Operation
7.2.1.8.1.3 ESCertKE (ESC)
7.2.1.8.1.3.1	NOTIFY Operation
TP/oneM2M/AE/SEC/ESC/NTF/001
	TP Id
	TP/oneM2M/AE/SEC/ESC/NTF/001

	Test objective
	Check that the IUT sends a notify request with ESCertKE message 1 when triggered

	Reference
	TS-0003 8.7.2.2 - step C.1.a, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Terminating End-Point's Certificate Info & Identity
}



·                  +-------------------------------------------------+-------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid NOTIFY Request containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 1 (TLS Message: Client Hello) | |
                     |} | |
·                  +-------------------------------------------------+-------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Request to CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 1 (TLS Message: Client Hello) | |
                     |} | |
+———————-+————————————————-+——————————————————————-+————-+
TP/oneM2M/AE/SEC/ESC/NTF/002
	TP Id
	TP/oneM2M/AE/SEC/ESC/NTF/002

	Test objective
	Check that the IUT sends a notify response with ESCertKE message 2 when it receives a notify request with ESCertKE message 1

	Reference
	TS-0003 8.7.2.2 - step C.1.b, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Initiating End-Point's Certificate Info & Identity
}



·                  +-----+---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE1 |
                     | the IUT receives a valid NOTIFY Request from CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE1_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 1 (TLS Message: Client Hello) | |
                     |} | |
·                  +-----+---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Response to CSE containing  | |
                     | To set to INITIATING_ENDPOINT_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 2 (TLS  | |
                     | Messages: Server Hello, Certificate*,  | |
                     | ServerKeyExchange*, CertificateRequest*,  | |
                     | ServerHelloDone)  | |
                     |} | |
+———————-+—–+—————————————————————————————————————+————-+
TP/oneM2M/AE/SEC/ESC/NTF/003
	TP Id
	TP/oneM2M/AE/SEC/ESC/NTF/003

	Test objective
	Check that the IUT sends a notify request with ESCertKE message 3 when it receives a notify response with ESCertKE message 2

	Reference
	TS-0003 8.7.2.2 - step C.1.c, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF03

	PICS Selection
	PICS_AE,

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Terminating End-Point's Certificate Info & Identity
and the IUT having sent a notify request to the Terminating End-Point with ESCertKE Message 1
}



·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE1 |
                     | the IUT receives a valid NOTIFY Response from CSE1 containing  | |
                     | To set to INITIATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE1_ID and  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 2 (TLS  | |
                     | Messages: Server Hello, Certificate*,  | |
                     | ServerKeyExchange*, CertificateRequest*,  | |
                     | ServerHelloDone)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Request to CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 3 (TLS  | |
                     | Messages: Certificate*, ClientKeyExchange,  | |
                     | CertificateVerify*, [ChangeCipherSpec], Finished)  | |
                     |} | |
+———————-+—————————————————————————————————————+————-+
TP/oneM2M/AE/SEC/ESC/NTF/004
	TP Id
	TP/oneM2M/AE/SEC/ESC/NTF/004

	Test objective
	Check that the IUT sends a notify response with ESCertKE message 4 when it receives a notify request with ESCertKE message 3

	Reference
	TS-0003 8.7.2.2 - step C.1.d, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF03

	PICS Selection
	PICS_AE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Initiating End-Point's Certificate Info & Identity
and the IUT having sent a notify request to the Initiating End-Point with ESCertKE
Message 2
}



·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE1 |
                     | the IUT receives a valid NOTIFY Request from CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE1_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 3 (TLS  | |
                     | Messages: Certificate*, ClientKeyExchange,  | |
                     | CertificateVerify*, [ChangeCipherSpec], Finished)  | |
                     |  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Response to CSE1 containing  | |
                     | To set to INITIATING_ENDPOINT_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 4 (TLS  | |
                     | Messages: ChangeCipherSpec], Finished)  | |
                     |} | |
+———————-+—————————————————————————————————————+————-+
7.2.2	Group CSE (CE)
7.2.2.1	General Capability (GEN)
7.2.2.1.1	CREATE Operation
TP/oneM2M/CSE/GEN/CRE/001
	TP Id
	TP/oneM2M/CSE/GEN/CRE/001

	Test objective
	Check that the IUT accepts the creation of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------+------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE request from AE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to 3 (container) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
·                  +------+------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+——+————————————————————————————————+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/CRE/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/CRE/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/CRE/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID




TP/oneM2M/CSE/GEN/CRE/002
	TP Id
	TP/oneM2M/CSE/GEN/CRE/002

	Test objective
	Check that the IUT accepts the creation of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------+----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE request from AE containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to 3 (container) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
·                  +--------+----------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+——–+———————————————————————————————-+————-+
	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/CRE/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/CRE/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/CRE/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/CRE/003
	TP Id
	TP/oneM2M/CSE/GEN/CRE/003

	Test objective
	Check that the IUT accepts the creation of a <container> resource using shortcut structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE request from AE containing  | |
                     | To set to SHORTCUT_H IERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to 3 (container) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+——————————————————————————————————-+————-+
	TP Id
	SHORTCUT_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/CRE/003_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/CRE/003_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/CRE/003_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/CRE/004
	TP Id
	TP/oneM2M/CSE/GEN/CRE/004

	Test objective
	Check that the IUT accepts the creation of a <container> resource using structured resource identifier with hybrid addressing

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the IUT having created a <group> resource GROUP_RESOURCE_ADDRESS containing
membersIDs attribute set to TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE request from AE containing  | |
                     | To set to HYBRID __HIERARCHICAL_ _ RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to 3 (container) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+———————————————————————————————————————+————-+
	TP Id
	HYBRID_HIERARCHICAL_RESOURCE_ADDRESS
	

	TP/oneM2M/CSE/GEN/CRE/004_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID (see note)
	

	TP/oneM2M/CSE/GEN/CRE/004_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)
	

	TP/oneM2M/CSE/GEN/CRE/004_ABS
	ABSOLUTE_RESOURCE_ID, (see note)
	

	NOTE: These addresses are constructed with the UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID of group plus "/fopt"
	CSE_RELATIVE_RESOURCE_ID of group plus "/fopt" |




7.2.2.1.2	UPDATE Operation
TP/oneM2M/CSE/GEN/UPD/001
	TP Id
	TP/oneM2M/CSE/GEN/UPD/001

	Test objective
	Check that the IUT accepts the update of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------+----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE request from AE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid labels attribute  | |
                     |} | |
·                  +----------+----------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+———-+———————————————————————————————-+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/UPD/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/UPD/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/UPD/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID




TP/oneM2M/CSE/GEN/UPD/002
	TP Id
	TP/oneM2M/CSE/GEN/UPD/002

	Test objective
	Check that the IUT accepts the update of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------+--------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE request from AE containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid l abels attribute  | |
                     |} | |
·                  +----------+--------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+———-+——————————————————————————————–+————-+
	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/UPD/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/UPD/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/UPD/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/UPD/003
	TP Id
	TP/oneM2M/CSE/GEN/UPD/003

	Test objective
	Check that the IUT accepts the update of a <container> resource using shortcut structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-+-----------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE request from AE containing  | |
                     | To set to SHORTCUT_H IERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid l abels attribute  | |
                     |} | |
·                  +-+-----------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+-+—————————————————————————————————–+————-+
	TP Id
	SHORTCUT_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/UPD/003_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/UPD/003_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/UPD/003_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/UPD/004
	TP Id
	TP/oneM2M/CSE/GEN/UPD/004

	Test objective
	Check that the IUT accepts the update of a <container> resource using structured resource identifier with hybrid addressing

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the IUT having created a <group> resource GROUP_RESOURCE_ADDRESS containing
membersIDs attribute set to TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE request from AE containing  | |
                     | To set to HYBRID __HIERARCHICAL_RESOURCE_ADDRESS_ and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid l abels attribute  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+——————————————————————————————————————-+————-+
	TP Id
	HYBRID_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/UPD/004_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID (see note)

	TP/oneM2M/CSE/GEN/UPD/004_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/UPD/004_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID of group plus "/fopt"




7.2.2.1.3	RETRIEVE Operation
TP/oneM2M/CSE/GEN/RET/001
	TP Id
	TP/oneM2M/CSE/GEN/RET/001

	Test objective
	Check that the IUT accepts the retrieval of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------+-------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE request from AE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +-------+-------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
+———————-+——-+————————————————————————————————-+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/RET/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/RET/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/RET/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID




TP/oneM2M/CSE/GEN/RET/002
	TP Id
	TP/oneM2M/CSE/GEN/RET/002

	Test objective
	Check that the IUT accepts the retrieval of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------+-----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE request from AE containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +---------+-----------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
+———————-+———+———————————————————————————————–+————-+
	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/RET/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/RET/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/RET/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/RET/003
	TP Id
	TP/oneM2M/CSE/GEN/RET/003

	Test objective
	Check that the IUT accepts the retrieval of a <container> resource using shortcut structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE request from AE containing  | |
                     | To set to SHORTCUT_H IERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
+———————-+——————————————————————————————————–+————-+
	TP Id
	SHORTCUT_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/RET/003_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/RET/003_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/RET/003_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/RET/004
	TP Id
	TP/oneM2M/CSE/GEN/RET/004

	Test objective
	Check that the IUT accepts the retrieval of a <container> resource using structured resource identifier with hybrid addressing

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the IUT having created a <group> resource GROUP_RESOURCE_ADDRESS containing
membersIDs attribute set to TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE request from AE containing  | |
                     | To set to HYBRID __HIERARCHICAL_RESOURCE_ADDRESS_ and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | container resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————-+————-+
	TP Id
	HYBRID_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/RET/004_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID (see note)

	TP/oneM2M/CSE/GEN/RET/004_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/RET/004_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID of group plus "/fopt"



7.2.2.1.4	DELETE Operation
TP/oneM2M/CSE/GEN/DEL/001
	TP Id
	TP/oneM2M/CSE/GEN/DEL/001

	Test objective
	Check that the IUT accepts the deletion of a <container> resource using unstructured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE, PICS_UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------+------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE request from AE containing  | |
                     | To set to NON_HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +------+------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+——+————————————————————————————————+————-+
	TP Id
	NON_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/DEL/001_CSR
	UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/DEL/001_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/DEL/001_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Unstructured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/DEL/002
	TP Id
	TP/oneM2M/CSE/GEN/DEL/002

	Test objective
	Check that the IUT accepts the deletion of a <container> resource using structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------+----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE request from AE containing  | |
                     | To set to HIERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +--------+----------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+——–+———————————————————————————————-+————-+
	TP Id
	HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/DEL/002_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/DEL/002_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/DEL/002_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/DEL/003
	TP Id
	TP/oneM2M/CSE/GEN/DEL/003

	Test objective
	Check that the IUT accepts the deletion of a <container> resource using shortcut structured resource identifier

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE request from AE containing  | |
                     | To set to SHORTCUT_H IERARCHICAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+——————————————————————————————————-+————-+
	TP Id
	SHORTCUT_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/DEL/003_CSR/
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/DEL/003_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/DEL/003_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the Structured-CSE-Relative-Resource-ID



TP/oneM2M/CSE/GEN/DEL/004
	TP Id
	TP/oneM2M/CSE/GEN/DEL/004

	Test objective
	Check that the IUT accepts the deletion of a <container> resource using structured resource identifier with hybrid addressing

	Reference
	TS-0001 [1], clause 9.3.1-1

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE, PICS_STRUCTURED_CSE_RELATIVE_RESOURCE_ID_FORMAT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <container> resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE request from AE containing  | |
                     | To set to HYBRID __HIERARCHICAL_RESOURCE_ADDRESS_ and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+———————————————————————————————————————+————-+
	TP Id
	HYBRID_HIERARCHICAL_RESOURCE_ADDRESS

	TP/oneM2M/CSE/GEN/DEL/004_CSR
	STRUCTURED_CSE_RELATIVE_RESOURCE_ID

	TP/oneM2M/CSE/GEN/DEL/004_SPR
	SP_RELATIVE_RESOURCE_ID, (see note)

	TP/oneM2M/CSE/GEN/DEL/004_ABS
	ABSOLUTE_RESOURCE_ID, (see note)

	NOTE: These addresses are constructed with the UNSTRUCTURED_CSE_RELATIVE_RESOURCE_ID of group plus "/fopt"



7.2.2.2	Registration (REG)
7.2.2.2.1	RETRIEVE Operation
TP/oneM2M/CSE/REG/RET/001
	TP Id
	TP/oneM2M/CSE/REG/RET/001

	Test objective
	Check that the IUT accepts a retrieval request of <CSEBase> resource and responds with all attributes that have multiplicity equals to 1

	Reference
	TS-0001 [1], clause 10.2.3.2 and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform RETRIEVE operation on the CSEBase resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content   | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | CSEBase resource representation  | |
                     |} | |
+———————-+——————————————————————————————————————————-+————-+
TP/oneM2M/CSE/REG/RET/002
	TP Id
	TP/oneM2M/CSE/REG/RET/002

	Test objective
	Check that the IUT accepts a retrieval request of <CSEBase> resource with the optional ATTRIBUTE

	Reference
	TS-0001 [1], clause 10.2.3.2 and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform RETRIEVE operation on the CSEBase resource
and the IUT having a CSEBase resource containing
the valid ATTRIBUTE attribute
}



·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | CSEBase resource containing  | |
                     | valid ATTRIBUTE attribute  | |
                     |} | |
+———————-+———————————————————————————————————–+————-+
	TP Id
	PICS Selection
	Reference
	ATTRIBUTE

	TP/oneM2M/CSE/REG/RET/002_CST
	PICS_CB_CST
	TS-0001 9.6.3
	cseType

	TP/oneM2M/CSE/REG/RET/002_NL
	PICS_CB_NL
	TS-0001 9.6.3
	nodeLink



TP/oneM2M/CSE/REG/RET/003
	TP Id
	TP/oneM2M/CSE/REG/RET/003

	Test objective
	Check that the IUT accepts a retrieval request of <AE> resource with attributes multiplicity equals to 1

	Reference
	TS-0001 [1], clause 10.2.1.2, and clause 9.6.5, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform RETRIEVE operation on the AE resource
}



·                  +------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID   | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
+———————-+————————————————————————————————————+————-+
TP/oneM2M/CSE/REG/RET/004
	TP Id
	TP/oneM2M/CSE/REG/RET/004

	Test objective
	Check that the IUT accepts a retrieval request of <AE> resource with optional ATTRIBUTE

	Reference
	TS-0001 [1], clause 10.2.1.2 and clause 9.6.5, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
valid ATTRIBUTE attribute
and the AE having privileges to perform RETRIEVE operation on the AE resource
}



·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | AE resource containing ATTRIBUTE attribute  | |
                     |} | |
+———————-+———————————————————————————————————–+————-+
	TP Id
	PICS Selection
	Reference
	ATTRIBUTE

	TP/oneM2M/CSE/REG/RET/004_LBL
	PICS_AE_LBL
	TS-0001 [1], clause 9.6.5
	labels

	TP/oneM2M/CSE/REG/RET/004_APN
	PICS_AE_APN
	TS-0001 [1], clause 9.6.5
	appName

	TP/oneM2M/CSE/REG/RET/004_POA
	PICS_AE_POA
	TS-0001 [1], clause 9.6.5
	pointOfAccess

	TP/oneM2M/CSE/REG/RET/004_NL
	PICS_AE_NL
	TS-0001 [1], clause 9.6.5
	nodeLink

	TP/oneM2M/CSE/REG/RET/004_CSZ
	PICS_AE_CSZ
	TS-0001 [1], clause 9.6.5
	contentSerialization




TP/oneM2M/CSE/REG/RET/005
	TP Id
	TP/oneM2M/CSE/REG/RET/005

	Test objective
	Check that the IUT accepts a retrieval request of <CSEBase> resource including the cseType attribute

	Reference
	TS-0001 [1], clause 10.2.3.2 and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform RETRIEVE operation on the CSEBase resource
}



·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | CSEBase resource containing  | |
                     | cseType attribute set to 1 (IN_CSE)  | |
                     |} | |
+———————-+———————————————————————————————————–+————-+
TP/oneM2M/CSE/REG/RET/006
	TP Id
	TP/oneM2M/CSE/REG/RET/006

	Test objective
	Check that the IUT accepts a retrieval request of <remoteCSE> resource

	Reference
	TS-0001 [1], clause 10.1.1.2.1 and, clause 9.6.4 TS-0004 [2], clause 7.4.4.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the ORIGINATOR
and the ORIGINATOR having privileges to perform RETRIEVE operation on the remoteCSE resource
}



·                  +---------------------------------------------------------------------------------------------------------+-----------------+

·                      |when {   |IUT <= ORIGINATOR|
                     | the IUT receives a valid RETRIEVE Request from ORIGINATOR containing  | |
                     | To set to REMOTECSE_RESOURCE_ADDRESS and  | |
                     | From set to ORIGINATOR_ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------+-----------------+

·                      |then {   |IUT => ORIGINATOR|
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | remoteCSE resource representation  | |
                     |} | |
+———————-+———————————————————————————————————+—————–+
TP/oneM2M/CSE/REG/RET/007
	TP Id
	TP/oneM2M/CSE/REG/RET/007

	Test objective
	Check that the IUT accepts a retrieval request of <remoteCSE> resource with optional ATTRIBUTE

	Reference
	TS-0001 [1], clause 10.1.1.2.1 and clause 9.6.4, TS-0004 [2], clause 7.4.4.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the ORIGINATOR
and the ORIGINATOR having privileges to perform RETRIEVE operation on the remoteCSE resource
}



·                  +---------------------------------------------------------------------------------------------------------+-----------------+

·                      |when {   |IUT <= ORIGINATOR|
                     | the IUT receives a valid RETRIEVE Request from ORIGINATOR containing  | |
                     | To set to REMOTECSE_RESOURCE_ADDRESS and  | |
                     | From set to ORIGINATOR_ID   | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------+-----------------+

·                      |then {   |IUT => ORIGINATOR|
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | remoteCSE resource containing  | |
                     | ATTRIBUTE attribute  | |
                     |} | |
+———————-+———————————————————————————————————+—————–+
	TP Id
	PICS Selection
	Reference
	ATTRIBUTE

	TP/oneM2M/CSE/REG/RET/007_LBL
	PICS_CSR_LBL
	TS-0001 [1], clause 9.6.4
	labels

	TP/oneM2M/CSE/REG/RET/007_CST
	PICS_CSR_CST
	TS-0001 [1], clause 9.6.4
	cseType

	TP/oneM2M/CSE/REG/RET/007_POA
	PICS_CSR_POA
	TS-0001 [1], clause 9.6.4
	pointOfAccess

	TP/oneM2M/CSE/REG/RET/007_NL
	PICS_CSR_NL
	TS-0001 [1], clause 9.6.4
	nodeLink




TP/oneM2M/CSE/REG/RET/008
	TP Id
	TP/oneM2M/CSE/REG/RET/008

	Test objective
	Check that the IUT accepts a retrieval request of <CSEBase> resource and responds with supportedResourceTypes attribute containing a list of the supported resources and pointOfAccess containing the list of physical addresses to be used by Registree to connect to this CSE (e.g. IP address, FQDN)

	Reference
	TS-0001 [1], clause 10.2.3.2 and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform RETRIEVE operation on the CSEBase resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | CSEBase resource containing  | |
                     | supportedResourceType set to PX_SRT  | |
                     | pointOfAccess set to PX_POA  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/REG/RET/009
	TP Id
	TP/oneM2M/CSE/REG/RET/009

	Test objective
	Check that IUT sends a <remoteCSE> retrieve request on
TARGET_REMOTE_CSE_ADDRESS

	Reference
	TS-0001 [1], clause 10.2.2.2, TS-0004 [2], clause 7.4.5.2.3

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having created a resource TARGET_REMOTE_CSE_ADDRESS and
the IUT having privileges to perform RETRIEVE operation on the resource TARGET_REMOTE_CSE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT is triggered to send a valid RETRIEVE Request containing
To set to TARGET_REMOTE_CSE_ADDRESS
}
	NA
	

	then {
the IUT sends a valid RETRIEVE Request containing
To set to TARGET_REMOTE_CSE_ADDRESSand
From set to CSE_ID and
no Content
}
	IUT => CSE
	



TP/oneM2M/CSE/REG/RET/010
	TP Id
	TP/oneM2M/CSE/REG/RET/010

	Test objective
	Check that IUT accepts a <remoteCSE> retrieve request

	Reference
	TS-0001 [1], clause 10.2.2.2, TS-0004 [2], clause 7.4.5.2.3

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having created a resource TARGET_REMOTE_CSE_ADDRESS
and the IUT having privileges to perform RETRIEVE operation on the resource TARGET_REMOTE_CSE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT receives a valid RETRIEVE Request containing
To set to TARGET_REMOTE_CSE_ADDRESSand
From set to CSE_ID and
no Content
}
	IUT <= CSE
	

	then {
the IUT sends a valid Response containing
Response Status Code set to 2000 (OK) and
Contentcontaining
remoteCSE resource representation
}
	IUT => CSE
	



7.2.2.2.2	CREATE Operation
TP/oneM2M/CSE/REG/CRE/001
	TP Id
	TP/oneM2M/CSE/REG/CRE/001

	Test objective
	Check that the IUT accepts a create request of <AE> resource with attributes multiplicity equals to 1 and provided preprovisioned SP_ _ AE_ID

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case b, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS SELECTION

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having preconfigured AE_ID_stem
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to SP_RELATIVE_AE_ID and  | |
                     | Resource Typeset to 2(AE) and  | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	SP_ RELATIVE _ AE_ID
	PICS S ELECTION

	TP/oneM2M/CSE/REG/CRE/001_CAE
	Release 1
	Starting with "C"
	PICS_CSE

	TP/oneM2M/CSE/REG/CRE/001_SAE
	Release 2
	Starting with "S"
	PICS_IN_CSE



TP/oneM2M/CSE/REG/CRE/002
	TP Id
	TP/oneM2M/CSE/REG/CRE/002

	Test objective
	Check that the IUT accepts a create request of <AE> resource with attributes multiplicity equals to 1 and provided preprovisioned AE_ID of AE-ID-STEM format

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case d, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS SELECTION

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having preconfigured AE_ID_stem
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID_STEM and  | |
                     | Resource Typeset to 2 (AE) and   | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	AE_ID _ STEM
	PICS Selection

	TP/oneM2M/CSE/REG/CRE/002_CAE
	Release 1
	Starting with "C"
	PICS_CSE

	TP/oneM2M/CSE/REG/CRE/002_SAE
	Release 2
	Starting with "S"
	PICS_IN_CSE



Editor's Note: Test purpose TP/oneM2M/CSE/REG/CRE/002 is duplicated with TP/oneM2M/CSE/REG/CRE/026 in terms of testing AE re‑registration in TS‑0001 10.1.1.2.2. case d. Therefore, test purpose TP/oneM2M/CSE/REG/CRE/026 is going to be removed.
TP/oneM2M/CSE/REG/CRE/003
	TP Id
	TP/oneM2M/CSE/REG/CRE/003

	Test objective
	Check that the IUT accepts a create request of <AE> resource with attributes multiplicity equals to 1 and provided preprovisioned S-AE-ID-STEM

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case b, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered to the IN-CSE
}



·                  +------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | From set to S‑AE‑ID‑STEM and  | |
                     | Resource Typeset to 2(AE) and   | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => IN‑CSE|
                     | the IUT sends a valid CREATE Request to IN‑CSE containing  | |
                     | From set to SP‑RELATIVE‑AE‑ID and  | |
                     | Content containing  | |
                     | AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID and  | |
                     | labels attribute set to "Credential‑IDs:None"  | |
                     |} | |
	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM }
S-AE-ID-STEM = Valid AE-ID-Stem starting with "S"



Editor's Note: need to clarify if there is duplication.


TP/oneM2M/CSE/REG/CRE/004
	TP Id
	TP/oneM2M/CSE/REG/CRE/004

	Test objective
	Check that the IUT rejects an AE registration (allowed App-ID, not allowed C-AE-ID-STEM provided by AE)

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - step 3 and clause 9.6.19

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT not allowing to register an AE containing
allowed App-ID attribute indicating APP-ID and
no t allowed AE-ID attribute indicating C-AE-ID-STEM
}



·                  +------------------------------------------+------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing Resource Type set to 2 (AE) and | |
                     | From set to C‑AE‑ID‑STEM and  | |
                     | Content containing  | |
                     |AE resource containing  | |
                     | App‑ID attribute set to APP‑ID  | |
                     |} | |
·                  +------------------------------------------+------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the AE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4126(APP_RULE_VALIDATION_FAILED)  | |
                     |} | |
+———————-+——————————————+——————————————————————————————+————-+


TP/oneM2M/CSE/REG/CRE/005
	TP Id
	TP/oneM2M/CSE/REG/CRE/005

	Test objective
	Check that the IUT accepts an AE registration (allowed App-ID, S-AE-ID-STEM not provided by AE)

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case a, and clause 9.6.19

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"and
the IUT having registered to the IN-CSE and
and the IUT allowing to register an AE containing
App-ID attributeset to APP-ID
}



·                  +--------------------------------------------------+----------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing Resource Type set to 2 (AE) and | |
                     | From set to "S" and  | |
                     | Content containing  | |
                     |AE resource containing  | |
                     | App‑ID attribute set to APP‑ID  | |
                     |} | |
·                  +--------------------------------------------------+----------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => IN‑CSE|
                     | the IUT sends a valid CREATE Request to the IN‑CSEcontaining  | |
                     | Resource Type set to 10002 (AEAnnc) and  | |
                     | From set to SP‑RELATIVE‑CSE‑ID followed by '/S' and  | |
                     | Content containing  | |
                     |AEAnnc resource containing  | |
                     | App‑ID attribute set to APP‑ID and  | |
                     | valid link attribute and  | |
                     | labels attribute indicating 'Credential‑ID:None'  | |
                     |} | |
+———————-+————————————————–+———————————————————————————-+————-+ Editor's Note: Double check the value of attribute nodeLink!!
TP/oneM2M/CSE/REG/CRE/006
	TP Id
	TP/oneM2M/CSE/REG/CRE/006

	Test objective
	Check that the IUT accepts a create request of <AE> resource with attributes multiplicity equals to 1 and provided character 'S' in AE_ID_Stem

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case a, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered to the IN-CSE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | From set to character 'S' and  | |
                     | Resource Typeset to 2(AE) and  | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => IN‑CSE|
                     | the IUT sends a valid CREATE Request to IN_CSE containing  | |
                     | From set to SP‑RELATIVE‑CSE‑ID followed by '/S' and  | |
                     | Content containing  | |
                     | AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID  | |
                     |} | |
	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{AE_ID_Stem}
AE_ID_Stem = "S"



TP/oneM2M/CSE/REG/CRE/007
	TP Id
	TP/oneM2M/CSE/REG/CRE/007

	Test objective
	Check that the IUT accepts an response of AEANNC create request during AE registration with provided character 'S' in AE_ID_Stem

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case a, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered to the IN-CSE and
the IUT having received a valid AE create request containing
From set to "S"and
the IUT having sent a valid AEANNC create to IN_CSE
}



·                  +------------------------------------------------------------------------------------------------------------------+----------------+

·                      |when{  |IUT <- IN‑CSE|
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------+----------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | ResourceID attribute set to S‑AE‑ID‑STEM and  | |
                     | AE‑ID attribute set to S‑AE‑ID‑STEM  | |
                     |} | |
	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM}
S-AE-ID-STEM = Valid AE-ID-Stem assigned by IN-CSE




TP/oneM2M/CSE/REG/CRE/008
	TP Id
	TP/oneM2M/CSE/REG/CRE/008

	Test objective
	Check that the IUT accepts an AE re-registration (allowed M2M-SP-assigned AE-ID, S-AE-ID-STEM provided by AE), transfer request to the IN-CSE

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case b, step 5 and clause 9.6.19

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
the IUT having registered to the IN-CSE and
the AE having already been registered containing
AE-ID set to S-AE-ID-STEM and
the AE having deregistered
}



·                  +----+--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing Resource Type set to 2 (AE) and | |
                     | From set to S‑AE‑ID‑STEM and  | |
                     | Content containing  | |
                     |AE resource representation  | |
                     |} | |
·                  +----+--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => IN‑CSE|
                     | the IUT sends a valid UPDATE Request to the IN‑CSE containing  | |
                     | From set to SP‑RELATIVE‑AE‑ID and  | |
                     | Content containing  | |
                     |AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID and  | |
                     | labels attribute indicating 'Credential‑ID:None'  | |
                     |} | |
	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM }
S-AE-ID-STEM = Value starting with "S" assigned by IN-CSE


· 

TP/oneM2M/CSE/REG/CRE/009
	TP Id
	TP/oneM2M/CSE/REG/CRE/009

	Test objective
	Check that the IUT accepts an AE re-registration (allowed M2M-SP-assigned AE-ID, S-AE-ID-STEM provided by AE), communication between MN-CSE and IN-CSE

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case b, step 5-8

	Config Id
	CF03

	Parent Release
	Release 2

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the MN-CSE and
the AE having already been registered containing
AE-ID set to S-AE-ID-STEM and
the AE having deregistered
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT<= MN‑CSE |
                     | the IUT receives a valid UPDATE Request from the MN‑CSE containing  | |
                     | To set to AEANNC_RESOURCE_ADDRESS and  | |
                     | From set to SP‑RELATIVE‑AE‑ID and  | |
                     | Content containing  | |
                     |AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID and  | |
                     | labels attribute indicating 'Credential‑ID:None'  | |
                     |} | |
	then {

	IUT => MN-CSE the IUT updates the AEANNC_RESOURCE_ADDRESS resource and
the IUT sends a valid Response to MN-CSE containing
Response Status Code set to 2004 (UPDATED) and
Content containing
AEAnnc resource containing
link attribute set to SP-RELATIVE-AE-ID and
labels attribute indicating 'Credential-ID:None'
}
	

	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM }
S-AE-ID-STEM = Value starting with "S" assigned by IN-CSE



TP/oneM2M/CSE/REG/CRE/010
	TP Id
	TP/oneM2M/CSE/REG/CRE/010

	Test objective
	Check that the IUT accepts an AE re-registration (allowed M2M-SP-assigned AE-ID, S-AE-ID-STEM provided by AE), transfer response to the AE

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case b, step 8

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the MN-CSE and
the AE having already been registered containing
AE-ID set to S-AE-ID-STEM and
the AE having deregistered and
the AE having sent a registration containing
From set to S-AE-ID-STEM and
the IUT having sent a valid AEAnnc UPDATE Request to IN-CSE
}



·                  +-----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= IN‑CSE|
                     | the IUT receives a valid UPDATE Response from IN‑CSE containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     |AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID and  | |
                     | labels attribute indicating 'Credential‑ID:None'   | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response to the AE containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | AE‑ID attribute set to S‑AE‑ID‑STEM  | |
                     |} | |
	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM }
S-AE-ID-STEM = Value starting with "S" assigned by IN-CSE




TP/oneM2M/CSE/REG/CRE/011
	TP Id
	TP/oneM2M/CSE/REG/CRE/011

	Test objective
	Check that the IUT accepts a create request of <AE> resource with attributes multiplicity equals to 1 and asking AE_ID_Stem by indicating AE_ID_Stem starting with character 'C'

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case c, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having preconfigured AE_ID_stem
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to 'C' and  | |
                     | Resource Typeset to 2(AE) and   | |
                     | Content containing  | |
                     | AE resource representation   | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | ResourceID attribute indicating a value  | |
                     | starting with 'C'  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————–+————-+


TP/oneM2M/CSE/REG/CRE/012
	TP Id
	TP/oneM2M/CSE/REG/CRE/012

	Test objective
	Check that the IUT accepts an AE registration with the optional attribute OPTIONAL_ATTRIBUTE provided

	Reference
	TS-0001 [1], clause 10.1.1.2.2 and clause 9.6.5-2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a CSEBase resource
}



·                  +-------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 2 (AE) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |AE resource containing  | |
                     | valid OPTIONAL_ATTRIBUTE attribute   | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     |AE resource containing  | |
                     | valid OPTIONAL_ATTRIBUTE attribute  | |
                     |} | |
+———————-+——————————————————————————————-+————-+
	TP Id
	PICS Selection
	Reference
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/REG/CRE/012_AE/LBL
	PICS_AE_LBL
	TS-0001 [1], clause 9.6.5-2
	labels

	TP/oneM2M/CSE/REG/CRE/012_AE/APN
	PICS_AE_APN
	TS-0001 [1], clause 9.6.5-2
	AppName

	TP/oneM2M/CSE/REG/CRE/012_AE/POA
	PICS_AE_POA
	TS-0001 [1], clause 9.6.5-2
	pointOfAccess

	TP/oneM2M/CSE/REG/CRE/012_AE/NL
	PICS_AE_NL
	TS-0001 [1], clause 9.6.5-2
	nodeLink

	TP/oneM2M/CSE/REG/CRE/012_AE/OR
	PICS_AE_OR
	TS-0001 [1], clause 9.6.5-2
	ontologyRef



TP/oneM2M/CSE/REG/CRE/013
	TP Id
	TP/oneM2M/CSE/REG/CRE/013

	Test objective
	Check that the IUT accepts a create request of <remoteCSE> resource with OPTIONAL_ATTRIBUTE

	Reference
	TS-0001 [1], clause 10.1.1.2.1 and clause 9.6.4 TS-0004 [2], clause 7.4.4.2.1

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid CREATE Request from CSE containing
To set to CSEBASE_RESOURCE_ADDRESS and
From set to CSE_ID and
Resource Type set to 16(remoteCSE) and
Content containing
remoteCSE resource representation containing
OPTIONAL_ATTRIBUTE attribute }
	IUT <= CSE

	then {

	IUT => CSE the IUT sends a valid Response containing
Response Status Code set to 2001 (CREATED) and
Content containing
remoteCSE resource representation }
	



	TP Id
	PICS Selection
	Reference
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/REG/CRE/013_LBL
	PICS_CSR_LBL
	TS-0001 [1], clause 9.6.4
	labels

	TP/oneM2M/CSE/REG/CRE/013_CST
	PICS_CSR_CST
	TS-0001 [1], clause 9.6.4
	cseType

	TP/oneM2M/CSE/REG/CRE/013_POA
	PICS_CSR_POA
	TS-0001 [1], clause 9.6.4
	pointOfAccess

	TP/oneM2M/CSE/REG/CRE/013_NL
	PICS_CSR_NL
	TS-0001 [1], clause 9.6.4
	nodeLink




TP/oneM2M/CSE/REG/CRE/014
	TP Id
	TP/oneM2M/CSE/REG/CRE/014

	Test objective
	Check that the IUT retargets the request to the remoteCSE according to pointOfAccess in the <remoteCSE> resource

	Reference
	TS-0001 [1], clause 9.6.4 and clause 9.3.2.2.3, TS-0004 [2], clause 6.2.3

	Config Id
	CF02

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUThaving created the remoteCSE resource containing
POINT_OF_ACCESS attribute
}



·                  +----------------------------------------------------------------------------------------------------+-----------------+

·                      |when {   |IUT <= Originator|
                     | the IUT receives a valid REQUEST from Originator containing  | |
                     | To set to RESOURCE_ADDRESS and  | |
                     | From set to Originator_ID   | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------+-----------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends the REQUEST to POINT_OF_ACCESS  | |
                     |} | |
+———————-+—————————————————————————————————-+—————–+
TP/oneM2M/CSE/REG/CRE/015
	TP Id
	TP/oneM2M/CSE/REG/CRE/015

	Test objective
	Check that the IUT retargets the request to the CSE according to pointOfAccess in the <remoteCSE> resource and forward the response back to the originator

	Reference
	TS-0001 [1], clause 9.6.4 and clause 9.3.2.2.3, TS-0004 [2], clause 6.2.3

	Config Id
	CF02

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE , PICS_SP_RELATIVE_RESOURCE_ID, PICS_ABSOLUTE_RESOURCE_ID

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having received a valid REQUEST from Originator and
The IUT having sent the REQUEST to the remoteCSE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid RESPONSE from the remoteCSE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |then {   |IUT => Originator|
                     | the IUT sends the RESPONSE to the Originator  | |
                     |} | |
+———————-+——————————————————————————————————————————————–+—————–+


TP/oneM2M/CSE/REG/CRE/016
	TP Id
	TP/oneM2M/CSE/REG/CRE/016

	Test objective
	Check that the IUT rejects an AE registration (not allowed App-ID)

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - step 3 and clause 9.6.19

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT not allowing to register an AE containing
not allowed App-ID attribute indicating APP-ID
}



·                  +------------------------------------------------------------------+------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing Resource Type set to 2 (AE) and | |
                     | Content containing  | |
                     |AE resource containing  | |
                     | App‑ID attribute set to APP‑ID  | |
                     |} | |
·                  +------------------------------------------------------------------+------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the AE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4126(APP_RULE_VALIDATION_FAILED)  | |
                     |} | |
+———————-+——————————————————————+——————————————————————+————-+

TP/oneM2M/CSE/REG/CRE/017
	TP Id
	TP/oneM2M/CSE/REG/CRE/017

	Test objective
	Check that the IUT rejects a create request of <AE> resource that doesn't include the MANDATORY_ATTRIBUTE

	Reference
	TS-0001 [1], clause 10.1.1.2.2, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having preconfigured AE_ID_stem
}



·                  +--------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Typeset to 2(AE) and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | no _MANDATORY ATTRIBUTE attribute   | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD Request)  | |
                     |} | |
+———————-+————————————————————————————————–+————-+
	TP Id
	Reference
	ATTRIBUTE

	TP/oneM2M/CSE/REG/CRE/017_API
	TS-0001 [1], clause 9.6.5
	App-ID

	TP/oneM2M/CSE/REG/CRE/017_RR
	TS-0001 [1], clause 9.6.5
	requestReachability



TP/oneM2M/CSE/REG/CRE/018
	TP Id
	TP/oneM2M/CSE/REG/CRE/018

	Test objective
	Check that the IUT accepts a create request of <remoteCSE> resource with attributes multiplicity equals to 1

	Reference
	TS-0001 [1], clause 10.1.1.2.1 and clause 9.6.4, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
}



·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid CREATE Request from CSE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Resource Typeset to 16(remoteCSE) and  | |
                     | Content containing  | |
                     | remoteCSE resource representation  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | remoteCSE resource representation  | |
                     |} | |
+———————-+————————————————————————————————————-+————-+
TP/oneM2M/CSE/REG/CRE/019
	TP Id
	TP/oneM2M/CSE/REG/CRE/019

	Test objective
	Check that the IUT accepts a create request of <remoteCSE> resource with attributes multiplicity equals to 1 without the preconfigured CSE-ID

	Reference
	TS-0001 [1], clause 10.1.1.2.1 and clause 9.6.4 TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid CREATE Request from CSE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | no From and  | |
                     | Resource Typeset to 16(remoteCSE) and  | |
                     | Content containing  | |
                     | remoteCSE resource representation  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | remoteCSE resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————————–+————-+

TP/oneM2M/CSE/REG/CRE/020
	TP Id
	TP/oneM2M/CSE/REG/CRE/020

	Test objective
	Check that the IUT accepts a create request of <AE> resource with attributes multiplicity equals to 1 and asking AE_ID_Stem by indicating AE_ID_Stem starting with character 'S'

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case a, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | From set to 'S' and  | |
                     | Resource Typeset to 2(AE) and   | |
                     | Content containing  | |
                     | AE resource representation   | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | ResourceID attribute set to S‑AE‑ID‑STEM  | |
                     |} | |
	NOTE: S-AE-ID-STEM = Value starting with "S" assigned by IN-CSE



TP/oneM2M/CSE/REG/CRE/021
	TP Id
	TP/oneM2M/CSE/REG/CRE/021

	Test objective
	Check that the IUT rejects the create request of <CSEBase> resource

	Reference
	TS-0001 [1], clause 10.2.3.1 and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
}



·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 5 (CSEBase) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | CSEBase resource representation  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+———————————————————————————————————–+————-+
TP/oneM2M/CSE/REG/CRE/022
	TP Id
	TP/oneM2M/CSE/REG/CRE/022

	Test objective
	Check that the IUT accepts an AE registration (allowed App-ID, C-AE-ID-STEM not provided by AE)

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case C and clause 9.6.19

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE containing
App-ID attribute indicating APP-ID and
AE-ID attribute indicating C-AE-ID-STEM
}



·                  +----------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 2 (AE) and  | |
                     | From set to 'C' and  | |
                     | Content containing  | |
                     |AE resource containing  | |
                     | App‑ID attribute set to APP‑ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT creates the AE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+———————————————————————————-+————-+
TP/oneM2M/CSE/REG/CRE/023
	TP Id
	TP/oneM2M/CSE/REG/CRE/023

	Test objective
	Check that the IUT rejects registration of already registered AE (C-AE-ID-STEM provided by AE)

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - step 4 and clause 9.6.19

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"and
the IUT having registered the AE with
AE-ID attribute set to C-AE-ID-STEM
}



·                  +----------------------------------------------------------+---------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing Resource Type set to 2 (AE) and | |
                     |To set to TARGE_CSE_RESOURCE_ADDRESS and  | |
                     | From set to C‑AE‑ID‑STEM and  | |
                     | Content containing  | |
                     | AE resource representation  | |
                     |} | |
·                  +----------------------------------------------------------+---------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the AE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4105 (CONFLICT)  | |
                     |} | |
+———————-+———————————————————-+———————————————————————————+————-+
TP/oneM2M/CSE/REG/CRE/024
	TP Id
	TP/oneM2M/CSE/REG/CRE/024

	Test objective
	Check that IUT sends a CSE registration request with attributes multiplicity equals to 1

	Reference
	TS-0001 [1], clause 10.1.1.2.1, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_MN_CSE or PICS_ASN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having privileges to perform CREATE operation on the resource CSEBASE_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT is triggered to send a valid CREATE Request containing
To set to CSEBASE_RESOURCE_ADDRESS and
Resource Type set to 16 (remoteCSE) and
Content containing
remoteCSE resource representation
}
	NA
	

	then {
the IUT sends a valid CREATE Request containing
To set to CSEBASE_RESOURCE_ADDRESS and
From set to CSE_ID and
Resource Type set to 16 (remoteCSE) and
Content containing
remoteCSE resource representation
}
	IUT => CSE
	



TP/oneM2M/CSE/REG/CRE/025
	TP Id
	TP/oneM2M/CSE/REG/CRE/025

	Test objective
	Check that IUT accepts a CSE registration request with attributes multiplicity equals to 1

	Reference
	TS-0001 [1], clause 10.1.1.2.1, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having privileges to perform CREATE operation on the resource CSEBASE_RESOURCE_ADDRESS
}



·                  +-+--------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Resource Type set to 16 (remoteCSE) and  | |
                     | Content containing  | |
                     | remoteCSE resource representation  | |
                     |} | |
·                  +-+--------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED) and  | |
                     |Content containing  | |
                     | remoteCSE resource representation  | |
                     |  | |
                     |and the IUT creates the <remoteCSE> resource  | |
                     |} | |
+———————-+-+——————————————————————————————–+————-+
TP/oneM2M/CSE/REG/CRE/026
	TP Id
	TP/oneM2M/CSE/REG/CRE/026

	Test objective
	Check that IUT sends a CSE registration request with OPTIONAL_ATTRIBUTE attribute

	Reference
	TS-0001 [1], clause 10.1.1.2.1, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_MN_CSE or PICS_ASN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having privileges to perform CREATE operation on the resource CSEBASE_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT is triggered to send a valid CREATE Request containing
To set to CSEBASE_RESOURCE_ADDRESS an d
Content containing
remoteCSE resource containing
cseType attribute set to 2 (MN_CSE) and
valid attribute OPTIONAL_ATTRIBUTE

}
	NA
	

	then {
the IUT sends a valid CREATE Request containing
To set to CSEBASE_RESOURCE_ADDRESS and
From set to CSE_ID and
Resource Type set to 16 (remoteCSE) and
Content containing
remoteCSE resource containing
cseType attribute set to 2 (MN_CSE) and
valid attribute OPTIONAL_ATTRIBUTE
}
	IUT => CSE
	



	TP Id
	PICS Selection
	Reference
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/REG/CRE/026_RN
	PICS_CSR_RN
	TS-0001 [1], clause 9.6.4-2
	resourceName

	TP/oneM2M/CSE/REG/CRE/026_ET
	PICS_CSR_ET
	TS-0001 [1], clause 9.6.4-2
	expirationTime

	TP/oneM2M/CSE/REG/CRE/026_LBL
	PICS_CSR_LBL
	TS-0001 [1], clause 9.6.4-2
	labels

	TP/oneM2M/CSE/REG/CRE/026_POA
	PICS_CSR_POA
	TS-0001 [1], clause 9.6.4-2
	pointOfAccess

	TP/oneM2M/CSE/REG/CRE/026_NL
	PICS_CSR_NL
	TS-0001 [1], clause 9.6.4-2
	nodeLink

	TP/oneM2M/CSE/REG/CRE/026_CST
	PICS_CSR_CST
	TS-0001 [1], clause 9.6.4-2
	cseType



TP/oneM2M/CSE/REG/CRE/027
	TP Id
	TP/oneM2M/CSE/REG/CRE/027

	Test objective
	Check that IUT accepts a CSE registration request with cseType attribute set to 'MN_CSE'

	Reference
	TS-0001 [1], clause 10.1.1.2.1, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having privileges to perform CREATE operation on the resource CSEBASE_RESOURCE_ADDRESS
}



·                  +-+--------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Resource Type set to 16 (remoteCSE) and  | |
                     | Content containing  | |
                     | remoteCSE resource containing  | |
                     | cseType attribute set to 2 (MN_CSE)  | |
                     |} | |
·                  +-+--------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED) and  | |
                     |Content containing  | |
                     | remoteCSE resource containing  | |
                     | cseType attribute set to 2 (MN_CSE)  | |
                     |  | |
                     | and the IUT creates a <remoteCSE> resource  | |
                     |} | |
+———————-+-+——————————————————————————————–+————-+
TP/oneM2M/CSE/REG/CRE/028
	TP Id
	TP/oneM2M/CSE/REG/CRE/028

	Test objective
	Check that IUT accepts a CSE registration request with OPTIONAL_ATTRIBUTE attribute

	Reference
	TS-0001 [1], clause 10.1.1.2.1, TS-0004 [2], clause 7.4.5.2.2

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the CSE having privileges to perform CREATE operation on the resource CSEBASE_RESOURCE_ADDRESS
}



·                  +-+--------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Resource Type set to 16 (remoteCSE) and  | |
                     | Content containing  | |
                     | remoteCSE resource containing  | |
                     | cseType attribute set to 2 (MN_CSE) and  | |
                     | valid attribute OPTIONAL_ATTRIBUTE  | |
                     |} | |
·                  +-+--------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED) and  | |
                     |Content containing  | |
                     | remoteCSE resource containing  | |
                     | cseType attribute set to 2 (MN_CSE) and  | |
                     | valid attribute OPTIONAL_ATTRIBUTE  | |
                     |  | |
                     |and the IUT creates a <remoteCSE> resource  | |
                     |} | |
+———————-+-+——————————————————————————————–+————-+
	TP Id
	PICS Selection
	Reference
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/REG/CRE/028_LBL
	PICS_CSR_LBL
	TS-0001 [1], clause 9.6.4-2
	labels

	TP/oneM2M/CSE/REG/CRE/028_POA
	PICS_CSR_POA
	TS-0001 [1], clause 9.6.4-2
	pointOfAccess

	TP/oneM2M/CSE/REG/CRE/028_NL
	PICS_CSR_NL
	TS-0001 [1], clause 9.6.4-2
	nodeLink



TP/oneM2M/CSE/REG/CRE/029
	TP Id
	TP/oneM2M/CSE/REG/CRE/029

	Test objective
	Check that the IUT accepts an AE registration (preprovisioned S-AE-ID-STEM provided by AE), communication between MN-CSE and IN-CSE

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case a, step 5-8

	Config Id
	CF04

	Parent Release
	Release 2

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
}



·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT<= MN‑CSE |
                     | the IUT receives a valid CREATE Request from the CSE containing  | |
                     | Resource Type set to 10002 (AEAnnc) and  | |
                     | From set to SP‑RELATIVE‑AE‑ID and  | |
                     | Content containing  | |
                     |AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID and  | |
                     | labels attribute indicating 'Credential‑ID:None'  | |
                     |} | |
	then {

	IUT => MN-CSE the IUT creates the AEANNC_RESOURCE_ADDRESS resource
and the IUT sends a valid Response to CSE containing
Response Status Code set to 2001 (CREATED) and
Content containing
AEAnnc resource containing
link attribute set to SP-RELATIVE-AE-ID and
labels indicating 'Credential-ID:None' }
	

	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM}
S-AE-ID-STEM = Valid AE-ID-Stem starting with "S"



TP/oneM2M/CSE/REG/CRE/030
	TP Id
	TP/oneM2M/CSE/REG/CRE/030

	Test objective
	Check that the IUT accepts an AE re-registration (allowed M2M-SP-assigned AE-ID, S-AE-ID-STEM provided by AE), transfer response to the AE

	Reference
	TS-0001 [1], clause 10.1.1.2.2 - case b, step 8

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the MN-CSE and
the AE having sent a registration containing
From set to S-AE-ID-STEM and
the IUT having sent a valid AEAnnc CREATE Request to IN-CSE
}



·                  +-----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= IN‑CSE|
                     | the IUT receives a valid Response from IN‑CSE containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     |AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID and  | |
                     | labels attribute indicating 'Credential‑ID:None'   | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response to the AE containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | AE‑ID attribute set to S‑AE‑ID‑STEM  | |
                     |} | |
	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM }
S-AE-ID-STEM = Value starting with "S" assigned by IN-CSE



TP/oneM2M/CSE/REG/CRE/031
	TP Id
	TP/oneM2M/CSE/REG/CRE/031

	Test objective
	Check that the IUT accepts an AE registration (S-AE-ID-STEM not provided by AE), communication between MN-CSE and IN-CSE

	Reference
	TS-0001 [1], clause 10.1.1.2.2 case a, TS-0004 [2], clause 7.4.5.2.1

	Config Id
	CF04

	Parent Release
	Release 2

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
}



·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= MN‑CSE|
                     | the IUT receives a valid CREATE Request from MN‑CSE containing  | |
                     | Resource Type set to 10002 (AEAnnc) and  | |
                     | From set to SP‑RELATIVE‑AE‑ID and  | |
                     | Content containing  | |
                     | AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID and  | |
                     | labels indicating 'Credential‑ID:None'  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => MN‑CSE|
                     | the IUT creates the AEANNC_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response to CSE containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     |AEAnnc resource containing  | |
                     | link attribute set to SP‑RELATIVE‑AE‑ID* and  | |
                     | labels indicating 'Credential‑ID:None'  | |
                     |} | |
	NOTE: SP-RELATIVE-AE-ID = {SP-RELATIVE-CSE-ID}/{AE-ID-STEM}
SP-RELATIVE-AE-ID* = {SP-RELATIVE-CSE-ID}/{S-AE-ID-STEM}
AE-ID-STEM = "S"
S-AE-ID-STEM = Valid AE-ID-Stem starting with "S"



TP/oneM2M/CSE/REG/CRE/032
	TP Id
	TP/oneM2M/CSE/REG/CRE/032

	Test objective
	Check that the IUT rejects an AE registration for CSEs for which the associated <serviceSubscribeNode> resource is not linked with the <serviceSubscribedAppRule> via the ruleLinks attribute of the <serviceSubscribedNode> resource

	Reference
	TS-0001 [1], clause 10.2.2.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having the serviceSubscribedNode resource For the CSE
containing
ruleLinks attribute not set
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing Resource Type set to 2 (AE)  | |
                     | } | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the AE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4126(APP_RULE_VALIDATION_FAILED)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————–+————-+
7.2.2.2.3	DELETE Operation
TP/oneM2M/CSE/REG/DEL/001
	TP Id
	TP/oneM2M/CSE/REG/DEL/001

	Test objective
	Check that the IUT rejects the delete request of <CSEBase> resource.

	Reference
	TS-0001 [1], clause 10.2.3.4 and [1], clause 9.6.3, TS-0004 [2], clause 7.4.3.2.4

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+—————————————————————————————————————————————+————-+


TP/oneM2M/CSE/REG/DEL/002
	TP Id
	TP/oneM2M/CSE/REG/DEL/002

	Test objective
	Check that IUT accepts a <remoteCSE> delete request on TARGET_REMOTE_CSE_ADDRESS, and deletes the <remoteCSE> resource

	Reference
	TS-0001 [1], clause 10.2.2.4 and clause 9.6.4, TS-0004 [2], clause 7.4.4.2.1

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the CSE
and the CSE originator having privileges to perform DELETE operation on the remoteCSE resource
}



·                  +------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid DELETE Request from CSE containing  | |
                     | To set to REMOTECSE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |and the IUT deletes the remoteCSE resource  | |
                     |} | |
+———————-+——————————————————————————————————————+————-+
TP/oneM2M/CSE/REG/DEL/003
	TP Id
	TP/oneM2M/CSE/REG/DEL/003

	Test objective
	Check that the IUT accepts an AE de-registration.

	Reference
	TS-0001 [1], clause 10.1.4.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform DELETE operation on the resource AE
}



·                  +------------------------------------+---------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +------------------------------------+---------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT deletes the AE_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+————————————+—————————————+————-+
TP/oneM2M/CSE/REG/DEL/004
	TP Id
	TP/oneM2M/CSE/REG/DEL/004

	Test objective
	Check that IUT sends a <remoteCSE> delete request on
TARGET_REMOTE_CSE_ADDRESS

	Reference
	TS-0001 [1], clause 10.2.2.4, TS-0004 [2], clause 7.4.5.2.5

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having created a resource TARGET_REMOTE_CSE_ADDRESS and
the IUT having privileges to perform DELETE operation on the resource TARGET_REMOTE_CSE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT is triggered to send a valid DELETE Request containing
To set to TARGET_REMOTE_CSE_ADDRESSS
}
	NA
	

	then {
the IUT sends a valid DELETE Request containing
To set to TARGET_REMOTE_CSE_ADDRESSand
From set to CSE_ID and
no Content
}
	IUT => CSE
	



TP/oneM2M/CSE/REG/DEL/005
	TP Id
	TP/oneM2M/CSE/REG/DEL/005

	Test objective
	Check that the IUT accepts an AE de-registration when AE-ID is starting with "S"

	Reference
	TS-0001 [1], clause 10.1.4.2.2

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
From set to "S"
and the AE having privileges to perform DELETE operation on the resource AE
}



·                  +--------+-------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +--------+-------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT deletes the AE_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+——–+——————————————————————-+————-+
TP/oneM2M/CSE/REG/DEL/006
	TP Id
	TP/oneM2M/CSE/REG/DEL/006

	Test objective
	Check that the IUT accepts an AE de-registration when AE-ID is starting with "S"

	Reference
	TS-0001 [1], clause 10.1.1.2.2

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
From set to "S"
and the AE having privileges to perform DELETE operation on the resource AE
}



·                  +--------+-------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +--------+-------------------------------------------------------------------+-------------+

·                      |then {   |IUT => IN‑CSE|
                     | the IUT sends a valid UPDATE Request containing  | |
                     | Contentcontaining  | |
                     | AEANNC_RESOURCE_ADDRESS resource containing  | |
                     | link attribute set to "INACTIVE"  | |
                     |} | |
+———————-+——–+——————————————————————-+————-+
TP/oneM2M/CSE/REG/DEL/007
	TP Id
	TP/oneM2M/CSE/REG/DEL/007

	Test objective
	Check that the IUT accepts the response from IN-CSE for the AE de-registration when AE-ID is starting with "S"

	Reference
	TS-0001 [1], clause 10.1.1.2.2

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
From set to "S"
and the AE having privileges to perform DELETE operation on the resource AE
and the AE having sent a valid DELETE Request at AE_RESOURCE_ADDRESS resource
and the IUT having sent a valid UPDATE Request to IN-CSE containing
Content containing
AEANNC_RESOURCE_ADDRESS resource containing
link attribute set to empty
}



·                  +-------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= IN‑CSE|
                     | the IUT receives a valid Response from IN‑CSE containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT deletes the AE_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+————————————————————————————————-+————-+
7.2.2.2.4	UPDATE Operation
TP/oneM2M/CSE/REG/UPD/001
	TP Id
	TP/oneM2M/CSE/REG/UPD/001

	Test objective
	Check that the IUT rejects the update request of <CSEBase> resource.

	Reference
	TS-0001 [1], clause 10.2.3.3 and clause 9.6.3, TS-0004 [2], clause 7.4.3.2.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
}



·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to CSEBASE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | CSEBase resource representation  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+———————————————————————————————————–+————-+ TP/oneM2M/CSE/REG/UPD/002
	TP Id
	TP/oneM2M/CSE/REG/UPD/002

	Test objective
	Check that IUT accepts a <remoteCSE> update request with OPTIONAL_ATTRIBUTE attribute

	Reference
	TS-0001 [1], clause 10.2.2.3, TS-0004 [2], clause 7.4.5.2.4

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having created a resource TARGET_REMOTE_CSE_ADDRESS containing
a RW OPTIONAL_ATTRIBUTE attribute set to VALUE_1 and
the CSE having privileges to perform UPDATE operation on the resource TARGET_REMOTE_CSE_ADDRESS
}



·                  +-----+------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE |
                     | the IUT receives a valid UPDATE Request containing  | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | remoteCSE resource containing  | |
                     | OPTIONAL_ATTRIBUTE attribute set to VALUE_2  | |
                     |} | |
·                  +-----+------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2004 (UPDATED) and  | |
                     |Content containing  | |
                     | remoteCSE resource containing  | |
                     | OPTIONAL_ATTRIBUTE attribute set to VALUE_2  | |
                     |} | |
+———————-+—–+——————————————————————————————+————-+
	TP Id
	Reference
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/REG/UPD/002_LBL
	TS-0001 [1], clause 9.6.4-2
	labels

	TP/oneM2M/CSE/REG/UPD/002_POA
	TS-0001 [1], clause 9.6.4-2
	pointOfAccess

	TP/oneM2M/CSE/REG/UPD/002_NL
	TS-0001 [1], clause 9.6.4-2
	nodeLink



TP/oneM2M/CSE/REG/UPD/003
	TP Id
	TP/oneM2M/CSE/REG/UPD/003

	Test objective
	Check that IUT sends a <remoteCSE> update request with OPTIONAL_ATTRIBUTE attribute

	Reference
	TS-0001 [1], clause 10.2.2.3, TS-0004 [2], clause 7.4.5.2.4

	Config Id
	CF04

	Parent Release
	Release 1

	PICS Selection
	PICS_MN_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having created a resource TARGET_REMOTE_CSE_ADDRESS containing
a RW OPTIONAL_ATTRIBUTE attribute set to VALU_1 and
the IUT having privileges to perform UPDATE operation on the resource TARGET_REMOTE_CSE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT is triggered to send a valid UPDATE Request containing
To set to TARGET_REMOTE_CSE_ADDRESS an d
Content containing
remoteCSE resource containing
attribute OPTIONAL_ATTRIBUTE set to VALUE_2

}
	NA
	

	then {
the IUT sends a valid UPDATE Request containing
To set to TARGET_REMOTE_CSE_ADDRESSand
From set to CSE_ID and
Content containing
remoteCSE resource containing
attribute OPTIONAL_ATTRIBUTE set to VALUE_2
}
	IUT => CSE
	



	TP Id
	PICS Selection
	Reference
	OPTIONAL_ ATTRIBUTE

	TP/oneM2M/CSE/REG/UPD/003_ET
	PICS_CSR_ET
	TS-0001 [1], clause 9.6.4-2
	expirationTime

	TP/oneM2M/CSE/REG/UPD/003_LBL
	PICS_CSR_LBL
	TS-0001 [1], clause 9.6.4-2
	labels

	TP/oneM2M/CSE/REG/UPD/003_POA
	PICS_CSR_POA
	TS-0001 [1], clause 9.6.4-2
	pointOfAccess

	TP/oneM2M/CSE/REG/UPD/003_NL
	PICS_CSR_NL
	TS-0001 [1], clause 9.6.4-2
	nodeLink

	TP/oneM2M/CSE/REG/UPD/003_RR
	PICS_CSR_RR
	TS-0001 [1], clause 9.6.4-2
	requestReachability




7.2.2.3	Data Management and Repository Function (DMR)
7.2.2.3.1	RETRIEVE Operation
TP/oneM2M/CSE/DMR/RET/001
	TP Id
	TP/oneM2M/CSE/DMR/RET/001

	Test objective
	Check that the IUT returns successfully the TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the AE resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------+-----------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +-------------------------------------------------+-----------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
+———————-+————————————————-+—————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/001_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/001_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/001_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/001_CIN
	Release 1
	TS-0001 [1], clause 10.2.4.2
	4 (contentInstance)

	TP/oneM2M/CSE/DMR/RET/001_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/001_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/001_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/001_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/001_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/001_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/002
	TP Id
	TP/oneM2M/CSE/DMR/RET/002

	Test objective
	Check that the IUT responds with an error when the AE tries to retrieve the resource TARGET_RESOURCE_ADDRESS which does not exist

	Reference
	TS-0001 [1], clause 10.1.2 - item 1)

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having not yet created a resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+———————————————————————————————————————-+————-+
TP/oneM2M/CSE/DMR/RET/003
	TP Id
	TP/oneM2M/CSE/DMR/RET/003

	Test objective
	Check that the IUT responds with an error when the AE tries to retrieve a resource TARGET_RESOURCE_ADDRESS under AE without having privileges for the RETRIEVE operation

	Reference
	TS-0001 [1], clause 10.1.2 - item 2)

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the AE resource
and the AE having no privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/003_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/003_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/003_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/003_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/003_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/003_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/003_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/003_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/004
	TP Id
	TP/oneM2M/CSE/DMR/RET/004

	Test objective
	Check that the IUT returns successfully the ATTRIBUTE of TARGET_RESOURCE_ADDRESS resource ("To" option)

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the AE resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                           +----------------------+--------------------------------------------------------------------------------------------+-------------+

·                               |when {   |IUT <= AE |
                              | the IUT receives a valid RETRIEVE Request from AE containing  | |
                              | To set to TARGET_ATTRIBUTE_ADDRESS and  | |
                              | From set to AE_ID and  | |
                              |no Content  | |
                              |} | |
·                           +----------------------+--------------------------------------------------------------------------------------------+-------------+

·                               |then {   |IUT => AE |
                              | the IUT sends a valid Response containing  | |
                              | Response Status Code set to 2000 (OK) and  | |
                              | Content containing  | |
                              | RESOURCE_TYPE resource containing  | |
                              | valid ATTRIBUTE attribute and  | |
                              | no other attribute  | |
                              |} | |
	Notes: TARGET_ATTRIBUTE_ADDRESS is represented as TARGET_RESOURCE_ADDRESS#ATTRIBUTE where '#' is present between TARGET_RESOURCE_ADDRESS and ATTRIBUTE.
ATTRIBUTE indicates common attribute for all RESOURCE_TYPE resources listed in the table below.



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/004_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/004_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/004_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/004_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/004_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/004_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/004_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/004_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/004_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/005
	TP Id
	TP/oneM2M/CSE/DMR/RET/005

	Test objective
	Check that the IUT returns successfully the ATTRIBUTE of TARGET_RESOURCE_ADDRESS resource ("Content" option)

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the AE resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------+--------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | ATTRIBUTE name  | |
                     |} | |
·                  +----------------+--------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid ATTRIBUTE attribute and  | |
                     | no other attribute  | |
                     |} | |
	Notes: ATTRIBUTE indicates common attribute for all RESOURCE_TYPE resources listed in the table below



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/005_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/005_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/005_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/005_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/005_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/005_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/005_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/005_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/005_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/006
	TP Id
	TP/oneM2M/CSE/DMR/RET/006

	Test objective
	Check that the IUT returns successfully multiple attributes of TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the AE resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------+-------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontainin   | |
                     | ATTRIBUTE_1 name and  | |
                     | ATTRIBUTE_2 name  | |
                     |} | |
·                  +-----------------------------+-------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid ATTRIBUTE_1 attribute and  | |
                     | valid ATTRIBUTE_2 attribute and  | |
                     | no other attribute  | |
                     |} | |
	Notes: ATTRIBUTE_1 indicates common attribute for all RESOURCE_TYPE resources listed in the table below
ATTRIBUTE_2 indicates common attribute for all RESOURCE_TYPE resources listed in the table below



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_ TYPE

	TP/oneM2M/CSE/DMR/RET/006_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/006_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/006_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/006_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/006_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/006_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/006_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/006_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/006_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/007
	TP Id
	TP/oneM2M/CSE/DMR/RET/007

	Test objective
	Check that the IUT responds with an error when the AE tries to retrieve a non-existing attribute of the TARGET_RESOURCE_ADDRESS resource ("single" attribute case)

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the AE resourcecontaining
no attribute ATTRIBUTE
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | ATTRIBUTE name  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE

	TP/oneM2M/CSE/DMR/RET/007_CNT/LBL
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)
	labels

	TP/oneM2M/CSE/DMR/RET/007_ACP/LBL
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)
	labels

	TP/oneM2M/CSE/DMR/RET/007_SUB/LBL
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)
	labels

	TP/oneM2M/CSE/DMR/RET/007_GRP/LBL
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)
	labels

	TP/oneM2M/CSE/DMR/RET/007_SCH/LBL
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels

	TP/oneM2M/CSE/DMR/RET/007_PCH/LBL
	Release 2
	TS-0001 [1], clause 10.2.13.3
	15 (pollingChallenge)
	labels

	TP/oneM2M/CSE/DMR/RET/007_TS/LBL
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)
	labels

	TP/oneM2M/CSE/DMR/RET/007_TRAM/LBL
	Release 4
	TS-0001 [1], clause10.2.18.3
	50(transactionMgmt)
	labels

	TP/oneM2M/CSE/DMR/RET/007_TRAC/LBL
	Release 4
	TS-0001 [1], clause10.2.18.7
	51(transaction)
	labels



Editor Note: A common ATTRIBUTE has been chosen for all types of resource. A note could replace ATTRIBUTE column.
TP/oneM2M/CSE/DMR/RET/008
	TP Id
	TP/oneM2M/CSE/DMR/RET/008

	Test objective
	Check that the IUT responds with an error when the AE tries to retrieve a non-existing attributes of the TARGET_RESOURCE_ADDRESS resource ("multiple" attributes case)

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the AE resource containing
no ATTRIBUTE_1 attribute and
no ATTRIBUTE_2 attribute
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | ATTRIBUTE_1 name a nd   | |
                     | ATTRIBUTE_2 name  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_1
	ATTRIBUTE_2

	TP/oneM2M/CSE/DMR/RET/008_CNT/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/008_SUB/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/008_ACP/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/008_GRP/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/008_SCH/LBL/AT
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/008_TS/LBL/AT
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/008_TRAM/LBL/TEXT
	Release 4
	TS-0001 [1], clause10.2.18.3
	50(transactionMgmt)
	labels
	transactionExecuteTime

	TP/oneM2M/CSE/DMR/RET/008_TRAC/LBL/TEXT
	Release 4
	TS-0001 [1], clause10.2.18.7
	51(transaction)
	labels
	transactionExecuteTime



Editor Note: The references to the TS‑0001 for the operations (CREATE, RETRIEVE) procedures of the resource type <schedule> have not been found. To check whether these procedures are missing or they have been added in newer versions (TS‑0001 v1.12.0 as basis)


TP/oneM2M/CSE/DMR/RET/009
	TP Id
	TP/oneM2M/CSE/DMR/RET/009

	Test objective
	Check that the IUT rejects the RETRIEVE Request of a latest resource target to a container resource that has no direct child contentInstance resources

	Reference
	TS-0001 [1], clause 10.2.22.1, TS-0004 [2], clause 7.4.28.2.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource containing
no direct child contentInstance resources
}

	Expected behaviour
	Test events
	Direction



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/DMR/RET/010
	TP Id
	TP/oneM2M/CSE/DMR/RET/010

	Test objective
	Check that the IUT accepts the RETRIEVE Request of the oldest contentInstance target to a <container> resource

	Reference
	TS-0001 [1], clause 10.2.23.1, TS-0004 [2], clause 7.4.29.2.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a container resource containing
CONTENT_INSTANCE_1 contentInstance resource and
CONTENT_INSTANCE_2 contentInstance resource
and the AE having privileges to perform RETRIEVE operation on the container resource
and creationTime attribute of CONTENT_INSTANCE_1 < creationTime attribute of CONTENT_INSTANCE_2
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid RETRIEVE Request from AE containing
To set to CONTAINER_RESOURCE_ADDRESS/ol and
From set to AE_ID and
no Content
}
	IUT <= AE

	
	then {
the IUT sends a valid Response containing
Response Status Code set to 2000 (OK) and
Content containing
contentInstance resource containing
resourceName attributeset to CONTENT_INSTANCE_1
}
	IUT => AE



TP/oneM2M/CSE/DMR/RET/011
	TP Id
	TP/oneM2M/CSE/DMR/RET/011

	Test objective
	Check that the IUT rejects the RETRIEVE Request of an oldest resource target to a container resource that has no direct child contentInstance resources.

	Reference
	TS-0001 [1], clause 10.2.23.1, TS-0004 [2], clause 7.4.29.2.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource containing
no direct child contentInstance resources
}

	Expected behaviour
	Test events
	Direction



·                  +-------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+——————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/DMR/RET/012
	TP Id
	TP/oneM2M/CSE/DMR/RET/012

	Test objective
	Check that the IUT accepts the RETRIEVE Request of the latest contentInstance target to a <container> resource

	Reference
	TS-0001 [1], clause 10.2.22.1, TS-0004 [2], clause 7.4.28.2.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
and the IUT having created a container resource containing
CONTENT_INSTANCE_1 contentInstance resource and
CONTENT_INSTANCE_2 contentInstance resource
and the AE having privileges to perform RETRIEVE operation on the container resource
and creationTime attribute of CONTENT_INSTANCE_1 < creationTime attribute of CONTENT_INSTANCE_2
}



·                  +--+----------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/la and  | |
                     | From set to AE_ID and   | |
                     |no Content  | |
                     |} | |
·                  +--+----------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a Response containing  | |
                     |Response Status Code set to 2000 (OK) and  | |
                     |Content containing  | |
                     | contentInstance resource containing  | |
                     | resourceName attributeset to CONTENT_INSTANCE_2  | |
                     |} | |
+———————-+–+—————————————————————————————————-+————-+
TP/oneM2M/CSE/DMR/RET/013
	TP Id
	TP/oneM2M/CSE/DMR/RET/013

	Test objective
	Check that the IUT returns successfully the TARGET_RESOURCE_ADDRESS resource under CSEBase

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------+-------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +----------------------------------------+-------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
+———————-+—————————————-+——————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/013_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/013_AE
	Release 1
	TS-0001 [1], clause 10.2.1.2
	2 (AE)

	TP/oneM2M/CSE/DMR/RET/013_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/013_CSR
	Release 1
	TS-0001 [1], clause 10.2.2.2
	16 (remoteCSE)

	TP/oneM2M/CSE/DMR/RET/013_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/013_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/013_DLV
	Release 4
	TS-0001 [1], clause 10.2.5.3
	6 (delivery)

	TP/oneM2M/CSE/DMR/RET/013_LCP
	Release 3
	TS-0001 [1], clause 10.2.10.1.2
	10 (locationPolicy)

	TP/oneM2M/CSE/DMR/RET/013_MGC
	Release 4
	TS-0001 [1], clause 10.2.8.3
	12 (mgmtCmd)

	TP/oneM2M/CSE/DMR/RET/013_NOD
	Release 4
	TS-0001 [1], clause 10.2.14.2
	14 (node)

	TP/oneM2M/CSE/DMR/RET/013_REQ
	Release 2
	TS-0001 [1], clause 10.2.20.2
	17 (request)

	TP/oneM2M/CSE/DMR/RET/013_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/013_STCL
	Release 4
	TS-0001 [1], clause 10.2.15.11
	21 (statsCollect)

	TP/oneM2M/CSE/DMR/RET/013_STCG
	Release 4
	TS-0001 [1], clause 10.2.15.3
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/RET/013_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/013_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/013_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/014
	TP Id
	TP/oneM2M/CSE/DMR/RET/014

	Test objective
	Check that the IUT responds with an error when the AE tries to retrieve a resource TARGET_RESOURCE_ADDRESS under CSEBase without having privileges for the RETRIEVE operation

	Reference
	TS-0001 [1], clause 10.1.2 - item 2)

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resource
and the AE having no privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/014_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/014_AE
	Release 1
	TS-0001 [1], clause 10.2.1.2
	2 (AE)

	TP/oneM2M/CSE/DMR/RET/014_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/014_CSR
	Release 1
	TS-0001 [1], clause 10.2.2.2
	16 (remoteCSE)

	TP/oneM2M/CSE/DMR/RET/014_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/014_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/014_DLV
	Release 4
	TS-0001 [1], clause 10.2.5.3
	6 (delivery)

	TP/oneM2M/CSE/DMR/RET/014_LCP
	Release 3
	TS-0001 [1], clause 10.2.10.1.2
	10 (locationPolicy)

	TP/oneM2M/CSE/DMR/RET/014_MGC
	Release 4
	TS-0001 [1], clause 10.2.8.3
	12 (mgmtCmd)

	TP/oneM2M/CSE/DMR/RET/014_NOD
	Release 4
	TS-0001 [1], clause 10.2.14.2
	14 (node)

	TP/oneM2M/CSE/DMR/RET/014_REQ
	Release 2
	TS-0001 [1], clause 10.2.20.2
	17 (request)

	TP/oneM2M/CSE/DMR/RET/014_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/014_STCL
	Release 4
	TS-0001 [1], clause 10.2.15.11
	21 (statsCollect)

	TP/oneM2M/CSE/DMR/RET/014_STCG
	Release 4
	TS-0001 [1], clause 10.2.15.3
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/RET/014_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/014_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/014_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/015
	TP Id
	TP/oneM2M/CSE/DMR/RET/015

	Test objective
	Check that the IUT returns successfully the ATTRIBUTE of TARGET_RESOURCE_ADDRESS resource ("To" option) under CSEBase

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------+----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_ATTRIBUTE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +-------------+----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid ATTRIBUTE attribute and  | |
                     | no other attribute  | |
                     |} | |
	Notes: TARGET_ATTRIBUTE_ADDRESS is represented as TARGET_RESOURCE_ADDRESS # ATTRIBUTE
ATTRIBUTE indicates common attribute for all_RESOURCE_TYPE_ resources listed in the table below



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/015_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/015_AE
	Release 1
	TS-0001 [1], clause 10.2.1.2
	2 (AE)

	TP/oneM2M/CSE/DMR/RET/015_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/015_CSR
	Release 1
	TS-0001 [1], clause 10.2.2.2
	16 (remoteCSE)

	TP/oneM2M/CSE/DMR/RET/015_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/015_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/015_DLV
	Release 4
	TS-0001 [1], clause 10.2.5.3
	6 (delivery)

	TP/oneM2M/CSE/DMR/RET/015_LCP
	Release 3
	TS-0001 [1], clause 10.2.10.1.2
	10 (locationPolicy)

	TP/oneM2M/CSE/DMR/RET/015_MGC
	Release 4
	TS-0001 [1], clause 10.2.8.3
	12 (mgmtCmd)

	TP/oneM2M/CSE/DMR/RET/015_NOD
	Release 4
	TS-0001 [1], clause 10.2.14.2
	14 (node)

	TP/oneM2M/CSE/DMR/RET/015_REQ
	Release 2
	TS-0001 [1], clause 10.2.20.2
	17 (request)

	TP/oneM2M/CSE/DMR/RET/015_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/015_STCL
	Release 4
	TS-0001 [1], clause 10.2.15.11
	21 (statsCollect)

	TP/oneM2M/CSE/DMR/RET/015_STCG
	Release 4
	TS-0001 [1], clause 10.2.15.3
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/RET/015_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/015_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/015_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



Editor's Note: Update the reference of schedule resource to TS‑0001 9.6.9
TP/oneM2M/CSE/DMR/RET/016
	TP Id
	TP/oneM2M/CSE/DMR/RET/016

	Test objective
	Check that the IUT returns successfully the ATTRIBUTE of TARGET_RESOURCE_ADDRESS resource ("Content" option) under CSEBase

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS}



·                  +--------+---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining   | |
                     | ATTRIBUTE name  | |
                     |} | |
·                  +--------+---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid ATTRIBUTE attribute and  | |
                     | no other attribute  | |
                     |} | |
	Notes: ATTRIBUTE indicates common attribute for all RESOURCE_TYPE resources listed in the table below



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/016_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/016_AE
	Release 1
	TS-0001 [1], clause 10.2.1.2
	2 (AE)

	TP/oneM2M/CSE/DMR/RET/016_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/016_CSR
	Release 1
	TS-0001 [1], clause 10.2.2.2
	16 (remoteCSE)

	TP/oneM2M/CSE/DMR/RET/016_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/016_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/016_DLV
	Release 4
	TS-0001 [1], clause 10.2.5.3
	6 (delivery)

	TP/oneM2M/CSE/DMR/RET/016_LCP
	Release 3
	TS-0001 [1], clause 10.2.10.1.2
	10 (locationPolicy)

	TP/oneM2M/CSE/DMR/RET/016_MGC
	Release 4
	TS-0001 [1], clause 10.2.8.3
	12 (mgmtCmd)

	TP/oneM2M/CSE/DMR/RET/016_NOD
	Release 4
	TS-0001 [1], clause 10.2.14.2
	14 (node)

	TP/oneM2M/CSE/DMR/RET/016_REQ
	Release 2
	TS-0001 [1], clause 10.2.20.2
	17 (request)

	TP/oneM2M/CSE/DMR/RET/016_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/016_STCL
	Release 4
	TS-0001 [1], clause 10.2.15.11
	21 (statsCollect)

	TP/oneM2M/CSE/DMR/RET/016_STCG
	Release 4
	TS-0001 [1], clause 10.2.15.3
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/RET/016_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/016_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/016_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/017
	TP Id
	TP/oneM2M/CSE/DMR/RET/017

	Test objective
	Check that the IUT returns successfully multiple attributes of TARGET_RESOURCE_ADDRESS resource under CSEBase

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------+---------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | ATTRIBUTE_1 name  | |
                     | and ATTRIBUTE_2 name  | |
                     |} | |
·                  +--------------------+---------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid ATTRIBUTE_1 attribute and  | |
                     | valid ATTRIBUTE_2 attribute and  | |
                     | no other attribute  | |
                     |} | |
	Notes: ATTRIBUTE_1 indicates common attribute for all RESOURCE_TYPE resources listed in the table below
ATTRIBUTE_2 indicates common attribute for all RESOURCE_TYPE resources listed in the table below



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/017_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/017_AE
	Release 1
	TS-0001 [1], clause 10.2.1.2
	2 (AE)

	TP/oneM2M/CSE/DMR/RET/017_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/017_CSR
	Release 1
	TS-0001 [1], clause 10.2.2.2
	16 (remoteCSE)

	TP/oneM2M/CSE/DMR/RET/017_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/017_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/017_DLV
	Release 4
	TS-0001 [1], clause 10.2.5.3
	6 (delivery)

	TP/oneM2M/CSE/DMR/RET/017_LCP
	Release 3
	TS-0001 [1], clause 10.2.10.1.2
	10 (locationPolicy)

	TP/oneM2M/CSE/DMR/RET/017_MGC
	Release 4
	TS-0001 [1], clause 10.2.8.3
	12 (mgmtCmd)

	TP/oneM2M/CSE/DMR/RET/017_NOD
	Release 4
	TS-0001 [1], clause 10.2.14.2
	14 (node)

	TP/oneM2M/CSE/DMR/RET/017_REQ
	Release 2
	TS-0001 [1], clause 10.2.20.2
	17 (request)

	TP/oneM2M/CSE/DMR/RET/017_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/017_STCL
	Release 4
	TS-0001 [1], clause 10.2.15.11
	21 (statsCollect)

	TP/oneM2M/CSE/DMR/RET/017_STCG
	Release 4
	TS-0001 [1], clause 10.2.15.3
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/RET/017_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/017_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)

	TP/oneM2M/CSE/DMR/RET/017_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)



TP/oneM2M/CSE/DMR/RET/018
	TP Id
	TP/oneM2M/CSE/DMR/RET/018

	Test objective
	Check that the IUT responds with an error when the AE tries to retrieve a non-existing attribute of the TARGET_RESOURCE_ADDRESS resource ("single" attribute case) under CSEBase

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resourcecontaining
no attribute ATTRIBUTE
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | ATTRIBUTE name  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE

	TP/oneM2M/CSE/DMR/RET/018_ACP/LBL
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)
	labels

	TP/oneM2M/CSE/DMR/RET/018_AE/LBL
	Release 1
	TS-0001 [1], clause 10.2.1.2
	2 (AE)
	labels

	TP/oneM2M/CSE/DMR/RET/018_CNT/LBL
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)
	labels

	TP/oneM2M/CSE/DMR/RET/018_CSR/LBL
	Release 1
	TS-0001 [1], clause 10.2.2.2
	16 (remoteCSE)
	labels

	TP/oneM2M/CSE/DMR/RET/018_SUB/LBL
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)
	labels

	TP/oneM2M/CSE/DMR/RET/018_GRP/LBL
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)
	labels

	TP/oneM2M/CSE/DMR/RET/018_DLV/LBL
	Release 4
	TS-0001 [1], clause 10.2.5.3
	6 (delivery)
	labels

	TP/oneM2M/CSE/DMR/RET/018_LCP/LBL
	Release 3
	TS-0001 [1], clause 10.2.10.1.2
	10 (locationPolicy)
	labels

	TP/oneM2M/CSE/DMR/RET/018_MGC/LBL
	Release 4
	TS-0001 [1], clause 10.2.8.3
	12 (mgmtCmd)
	labels

	TP/oneM2M/CSE/DMR/RET/018_NOD/LBL
	Release 4
	TS-0001 [1], clause 10.2.14.2
	14 (node)
	labels

	TP/oneM2M/CSE/DMR/RET/018_REQ/LBL
	Release 2
	TS-0001 [1], clause 10.2.20.2
	17 (request)
	labels

	TP/oneM2M/CSE/DMR/RET/018_SCH/LBL
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels

	TP/oneM2M/CSE/DMR/RET/018_STCL/LBL
	Release 4
	TS-0001 [1], clause 10.2.15.11
	21 (statsCollect)
	labels

	TP/oneM2M/CSE/DMR/RET/018_STCG/LBL
	Release 4
	TS-0001 [1], clause 10.2.15.3
	22 (statsConfig)
	labels

	TP/oneM2M/CSE/DMR/RET/018_TS
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)
	labels

	TP/oneM2M/CSE/DMR/RET/018_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgmt)
	labels

	TP/oneM2M/CSE/DMR/RET/018_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)
	labels



TP/oneM2M/CSE/DMR/RET/019
	TP Id
	TP/oneM2M/CSE/DMR/RET/019

	Test objective
	Check that the IUT responds with an error when the AE tries to retrieve a non-existing attribute of the TARGET_RESOURCE_ADDRESS resource ("multiple" attributes case) under CSEBase

	Reference
	TS-0001 [1], clause 10.1.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the <CSEBase> resourcecontaining
no ATTRIBUTE_1 attribute and
no ATTRIBUTE_2 attribute
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | ATTRIBUTE_1 name  | |
                     | and ATTRIBUTE_2 name  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————+————-+
	TP Id
	PARENT_R ELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_1
	ATTRIBUTE_2

	TP/oneM2M/CSE/DMR/RET/019_ACP/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.21.2
	1 (accessControlPolicy)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_AE/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.1.2
	2 (AE)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_CNT/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.4.2
	3 (container)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_CSR/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.2.2
	16 (remoteCSE)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_SUB/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.11.3
	23 (subscription)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_GRP/LBL/AT
	Release 1
	TS-0001 [1], clause 10.2.7.3
	9 (group)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_DLV/LBL/AT
	Release 4
	TS-0001 [1], clause 10.2.5.3
	6 (delivery)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_LCP/LBL/AT
	Release 3
	TS-0001 [1], clause 10.2.10.1.2
	10 (locationPolicy)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_MGC/LBL/AT
	Release 4
	TS-0001 [1], clause 10.2.8.3
	12 (mgmtCmd)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_NOD/LBL/AT
	Release 4
	TS-0001 [1], clause 10.2.14.2
	14 (node)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_REQ/LBL/AT
	Release 3
	TS-0001 [1], clause 10.2.20.2
	17 (request)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_SCH/LBL/AT
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_STCL/LBL/AT
	Release 4
	TS-0001 [1], clause 10.2.15.11
	21 (statsCollect)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_STCG/LBL/AT
	Release 4
	TS-0001 [1], clause 10.2.15.3
	22 (statsConfig)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_TS/LBL/AT
	Release 3
	TS-0001 [1], clause 10.2.30.2
	29 (timeSeries)
	labels
	announceTo

	TP/oneM2M/CSE/DMR/RET/019_TRAM/LBL/TEXT
	Release 4
	TS-0001 [1], clause 10.2.18.3
	50(transactionMgm)
	labels
	transactionExecuteTime

	TP/oneM2M/CSE/DMR/RET/019_TRAC/LBL/TEXT
	Release 4
	TS-0001 [1], clause 10.2.18.7
	51(transaction)
	labels
	transactionExecuteTime



TP/oneM2M/CSE/DMR/RET/020
	TP Id
	TP/oneM2M/CSE/DMR/RET/020

	Test objective
	Check that the IUT rejects a RETRIEVE Request target to TARGET_ RESOURCE_ADDRESS resource when the Result Content set to RESULT_CONTENT

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 7.3.2.1

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Contentand  | |
                     | Result Content set to RESULT_CONTENT  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+——————————————————————————————————————————+————-+
	TP Id
	Reference
	RESULT_CONTENT

	TP/oneM2M/CSE/DMR/RET/020_RCN/0
	TS-0004 [2], clause 6.3.4.2.7
	0 (Nothing)

	TP/oneM2M/CSE/DMR/RET/020_RCN/2
	
	2 (hierarchical address)

	TP/oneM2M/CSE/DMR/RET/020_RCN/3
	
	3 (attributes and hierarchichal address)

	TP/oneM2M/CSE/DMR/RET/020_RCN/9
	
	9 (modified attributes)



TP/oneM2M/CSE/DMR/RET/021
	TP Id
	
	TP/oneM2M/CSE/DMR/RET/021
	
	

	Test objective
	
	Check that the IUT returns successfully only attributes of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 1 (attributes)
	
	

	Reference
	
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7
	
	

	Config Id
	
	CF01
	
	

	Parent Release
	
	PARENT_RELEASE
	
	

	PICS Selection
	
	PICS_CSE
	
	

	Initial conditions
	with {  the IUT being in the "initial state" and the IUT having registered the AE and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing a child resource and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS}
	
	
	

	Expected behaviour
	Test events
	
	
	Direction

	
	
	when {  the IUT receives a valid RETRIEVE Request from AE containing To set to TARGET_RESOURCE_ADDRESS and From set to AE_ID andno Contentand Result Content set to 1 (attributes)}
	
	IUT <= AE

	
	
	
	then {  the IUT sends a valid Response containing Response Status Code set to 2000 (OK) and Content containing RESOURCE_TYPE resource containing attributes and no hierarchichal address and no child resources and no child resource references}
	



	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/021_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/RET/021_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/RET/021_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/021_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/021_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/021_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/021_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/021_TRAM
	Release 4
	50 (TransactionMgmt)

	TP/oneM2M/CSE/DMR/RET/021_TRAC
	Release 4
	51 (Transaction)



TP/oneM2M/CSE/DMR/RET/022
	TP Id
	TP/oneM2M/CSE/DMR/RET/022

	Test objective
	Check that the IUT returns successfully only attributes and child resources of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 4 (attributes and child resources)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Contentand  | |
                     | Result Content set to 4 (attributes and child resources)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | attributes and  | |
                     | no hierarchichal address and  | |
                     | child resources and  | |
                     | no child resource references  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/022_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/RET/022_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/022_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/022_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/022_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/022_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/022_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/022_TRAM
	Release 4
	50 (TransactionMgmt)

	TP/oneM2M/CSE/DMR/RET/022_TRAC
	Release 4
	51 (Transaction)



TP/oneM2M/CSE/DMR/RET/023
	TP Id
	TP/oneM2M/CSE/DMR/RET/023

	Test objective
	Check that the IUT returns successfully only attributes and child resource references of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 5 (attributes and child resource references)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content and  | |
                     | Result Content set to 5 (attributes and child resource references)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | attributes and  | |
                     | no hierarchichal address and  | |
                     | no child resources and  | |
                     | child resource references  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/023_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/RET/023_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/023_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/023_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/023_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/023_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/023_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/023_TRAM
	Release 4
	50 (TransactionMgmt)

	TP/oneM2M/CSE/DMR/RET/023_TRAC
	Release 4
	51 (Transaction)



TP/oneM2M/CSE/DMR/RET/024
	TP Id
	TP/oneM2M/CSE/DMR/RET/024

	Test objective
	Check that the IUT returns successfully only child resource references of TARGET_RESOURCE_ADDRESS resource when Result Content is set to 6 (child resource references)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Contentand  | |
                     | Result Content set to 6 (child resource references)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | resourceRefList element containing  | |
                     | child resource reference  | |
                     |} | |
+———————-+———————————————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/024_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/RET/024_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/024_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/024_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/024_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/024_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/024_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/024_TRAM
	Release 4
	50 (TransactionMgmt)

	TP/oneM2M/CSE/DMR/RET/024_TRAC
	Release 4
	51 (Transaction)



TP/oneM2M/CSE/DMR/RET/025
	TP Id
	TP/oneM2M/CSE/DMR/RET/025

	Test objective
	Check that the IUT returns successfully only child resources of TARGET_RESOURCE_ADDRESS resource when Result Content is set to 8 (child resources)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Contentand  | |
                     | Result Content set to 8 (child resources)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | CHILD_RESOURCE_TYPE resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/025_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/RET/025_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/025_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/025_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/025_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/025_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/025_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/RET/025_TRAM
	Release 4
	50 (TransactionMgmt)

	TP/oneM2M/CSE/DMR/RET/025_TRAC
	Release 4
	51 (Transaction)



TP/oneM2M/CSE/DMR/RET/026
	TP Id
	TP/oneM2M/CSE/DMR/RET/026

	Test objective
	Check that the IUT sends a RETRIEVE request to ORIGINAL_RESOURCE_ADDRESS resource when receiving a RETRIEVE request with Result Content set to 7 (original resource)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered the CSE
and the IUT having a resource ANNC_ORIGINAL_RESOURCE_ADDRESS containing
link set to ORIGINAL_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource ANNC_ORIGINAL_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to ANNC_ORIGINAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Contentand  | |
                     | Result Content set to 7 (original resource)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid RETRIEVE Request to CSE containing  | |
                     | To set to ORIGINAL_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID or IUT CSE ID?? and  | |
                     |no Content  | |
                     |} | |
+———————-+———————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/026_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/RET/026_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/026_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/026_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/026_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/026_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/026_PCH
	Release 3
	15 (pollingChannel)




TP/oneM2M/CSE/DMR/RET/027
	TP Id
	TP/oneM2M/CSE/DMR/RET/027

	Test objective
	Check that the IUT returns successfully the representation of the original resource of the ANNC_ORIGINAL_RESOURCE_ADDRESS resource when receiving a RETRIEVE request with Result Content is set to 7 (original resource)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered the CSE
and the IUT having a resource ANNC_ORIGINAL_RESOURCE_ADDRESS containing
link set to ORIGINAL_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource ANNC_ORIGINAL_RESOURCE_ADDRESS
and the IUT having received a valid RETRIEVE Request containing
To set to ANNC_ORIGINAL_RESOURCE_ADDRESS and
Result Content set to 7 (original resource)
and the IUT having sent a valid RETRIEVE Request containing
To set to ORIGINAL_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid Response from CSE containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | a valid resource representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a valid Response to AE containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | a valid resource representation  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/RET/027_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/RET/027_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/RET/027_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/RET/027_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/RET/027_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/RET/027_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/RET/027_PCH
	Release 3
	15 (pollingChannel)



TP/oneM2M/CSE/DMR/RET/028
	TP Id
	TP/oneM2M/CSE/DMR/RET/028

	Test objective
	Check that the IUT successfully returns the privileges of the ORIGINATOR on the TARGET_RESOURCE_ADDRESS when the RETRIEVE request contains Result Content set to permissions

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7, clause 7.5.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having resource at TARGET_RESOURCE_ADDRESS
and AE having the privileges to perform the RETRIEVE operation on
TARGET_RESOURCE_ADDRESS
and AE having privileges to perform the RETRIEVE operation on
the <accessControlPolicy> resources mentioned in accessControlPolicyIDs attribute of TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to 12 (permissions)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | permissions containing  | |
                     | representation of access control privileges  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/DMR/RET/029
	TP Id
	TP/oneM2M/CSE/DMR/RET/029

	Test objective
	Check that the IUT rejects a RETRIEVE request from the AE containing Result Content set to permissions when AE has no RETRIEVE privileges on the <accessControlPolicy> resources associated with the TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having resource at TARGET_RESOURCE_ADDRESS
and AE having the privileges to perform the RETRIEVE operation on
TARGET_RESOURCE_ADDRESS
and AE not having the privileges to perform the RETRIEVE operation on
<accessControlPolicy> resources mentioned in accessControlPolicyIDs attribute of TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content and  | |
                     | Result Content set to 12 (permissions)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4130 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————–+————-+


7.2.2.3.2	UPDATE Operation
TP/oneM2M/CSE/DMR/UPD/001
	TP Id
	TP/oneM2M/CSE/DMR/UPD/001

	Test objective
	Check that the IUT updates successfully the value of the attribute ATTRIBUTE_NAME of the TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a RW ATTRIBUTE_NAME attribute set to VALUE_1
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT updates the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
+———————-+—————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYP E
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/DMR/UPD/001_CNT/LBL
	Release 1
	TS-0001 [1], clause 10.2.4.3
	3 (container)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_ACP/LBL
	Release 1
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_SUB/LBL
	Release 1
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_GRP/LBL
	Release 1
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_SCH/LBL
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_PCH/LBL
	Release 2
	TS-0001 [1], clause 10.2.13.4
	15 (pollingChannel)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_TS/LBL
	Release 3
	TS-0001 [1], clause 10.2.13.4
	29 (timeSeries)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_TRAM/LBL
	Release 4
	TS-0001 [1], clause 10.2.18.4
	50 (transactionMgmt)
	labels

	TP/oneM2M/CSE/DMR/UPD/001_TRAC/LBL
	Release 4
	TS-0001 [1], clause 10.2.18.8
	51 (transaction)
	labels



TP/oneM2M/CSE/DMR/UPD/002
	TP Id
	TP/oneM2M/CSE/DMR/UPD/002

	Test objective
	Check that the IUT adds successfully the attribute ATTRIBUTE_NAME to the TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
no optional RW ATTRIBUTE_NAME attribute
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID and
Content containing
RESOURCE_TYPE resourcecontaining
ATTRIBUTE_NAME attribute set to VALUE_1
}
	IUT <= AE
	

	then {
the IUT updates the TARGET_RESOURCE_ADDRESS resource
and the IUT sends a valid Response containing
Response Status Code set to 2004 (UPDATED) and
Content containing
RESOURCE_TYPE resourcecontaining
ATTRIBUTE_NAME attribute set to VALUE_1
}
	IUT => AE
	



	TP Id
	PARENT_RELEASE
	PICS Selection
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/DMR/UPD/002_CNT/LBL
	Release 1
	PICS_CNT_LBL
	TS-0001 [1], clause 10.2.4.3
	3 (container)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_ACP/LBL
	Release 1
	PICS_ACP_LBL
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_SUB/LBL
	Release 1
	PICS_SUB_LBL
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_GRP/LBL
	Release 1
	PICS_GRP_LBL
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_SCH/LBL
	Release 3
	
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_PCH/LBL
	Release 2
	
	TS-0001 [1], clause 10.2.13.4
	15 (pollingChannel)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_TS/LBL
	Release 3
	
	TS-0001 [1], clause 10.2.30.3
	29 (timeSeries)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_TRAM/LBL
	Release 4
	
	TS-0001 [1], clause 10.2.18.4
	50 (transactionMgmt)
	labels

	TP/oneM2M/CSE/DMR/UPD/002_TRAC/LBL
	Release 4
	
	TS-0001 [1], clause 10.2.18.8
	51 (transaction)
	labels



TP/oneM2M/CSE/DMR/UPD/003
	TP Id
	TP/oneM2M/CSE/DMR/UPD/003

	Test objective
	Check that the IUT deletes successfully the attribute ATTRIBUTE_NAME from the TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
an optional RW ATTRIBUTE_NAME attribute
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID and
Content containing
RESOURCE_TYPE resourcecontaining
ATTRIBUTE_NAME attribute set to NULL
}
	IUT <= AE
	

	then {
the IUT updates the TARGET_RESOURCE_ADDRESS resource
and the IUT sends a valid Response containing
Response Status Code set to 2004 (UPDATED) and
Content containing
RESOURCE_TYPE resourcecontaining
ATTRIBUTE_NAME attribute set to NULL
}
	IUT => AE
	



	TP Id
	PARENT_RELEASE
	PICS Selection
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/DMR/UPD/003_CNT/LBL
	Release 1
	PICS_CNT_LBL
	TS-0001 [1], clause 10.2.4.3
	3 (container)
	labels

	TP/oneM2M/CSE/DMR/UPD/003_ACP/LBL
	Release 1
	PICS_ACP_LBL
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	labels

	TP/oneM2M/CSE/DMR/UPD/003_SUB/LBL
	Release 1
	PICS_SUB_LBL
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	labels

	TP/oneM2M/CSE/DMR/UPD/003_GRP/LBL
	Release 1
	PICS_GRP_LBL
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	labels

	TP/oneM2M/CSE/DMR/UPD/003_SCH/LBL
	Release 3
	
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels

	TP/oneM2M/CSE/DMR/UPD/003_PCH/LBL
	Release 2
	
	TS-0001 [1], clause 10.2.13.4
	15 (pollingChannel)
	labels

	TP/oneM2M/CSE/DMR/UPD/003_TS/LBL
	Release 3
	
	TS-0001 [1], clause 10.2.30.3
	29 (timeSeries)
	labels

	TP/oneM2M/CSE/DMR/UPD/003_TRAM/LBL
	Release 4
	
	TS-0001 [1], clause 10.2.18.4
	50 (transactionMgmt)
	lables

	TP/oneM2M/CSE/DMR/UPD/003_TRAC/LBL
	Release 4
	
	TS-0001 [1], clause 10.2.18.8
	51 (transaction)
	lables



TP/oneM2M/CSE/DMR/UPD/004
	TP Id
	TP/oneM2M/CSE/DMR/UPD/004

	Test objective
	Check that the IUT updates the value of the attribute ATTRIBUTE_NAME_1 , and creates the ATTRIBUTE_NAME_2 and deletes the ATTRIBUTE_NAME_3 of the TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a RW ATTRIBUTE_NAME_1 attribute set to VALUE_1 and
no optional RW ATTRIBUTE_NAME_2 attribute and
an optional RW ATTRIBUTE_NAME_3 attribute
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID and
Content containing
RESOURCE_TYPE resourcecontaining
ATTRIBUTE_NAME_1 attibute set to VALUE_2 and
ATTRIBUTE_NAME_2 attribute set to VALUE_3 and
ATTRIBUTE_NAME_3 attribute set to NULL
}
	IUT <= AE
	

	then {
the IUT updates the TARGET_RESOURCE_ADDRESS resource
and the IUT sends a valid Response containing
Response Status Code set to 2004 (UPDATED) and
Content containing
RESOURCE_TYPE resourcecontaining
ATTRIBUTE_NAME_1 attribute set to VALUE_2 and
ATTRIBUTE_NAME_2 attribute set to VALUE_ 3 and
ATTRIBUTE_NAME_3 attribute set to NULL
}
	IUT => AE
	

	Editor's Note: Clarification is required in term of the test objective!!



	TP Id
	PARENT_RELEASE
	PICS Selection
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_NAME_1
	ATTRIBUTE_NAME_2
	ATTRIBUTE_NAME_3

	TP/oneM2M/CSE/DMR/UPD/004_CNT/ET/MNI/LBL
	Release 1
	PICS_CNT_MNI and PICS_CNT_LBL
	TS-0001 [1], clause 10.2.4.3
	3 (container)
	expirationTime
	maxNrOfInstances
	labels

	TP/oneM2M/CSE/DMR/UPD/004_ACP/PVS/PV/LBL
	Release 1
	PICS_ACP_LBL
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	selfPrivileges
	privileges
	labels

	TP/oneM2M/CSE/DMR/UPD/004_ACP/PV/AT/LBL
	Release 3
	PICS_ACP_AT and PICS_ACP_LBL
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	privileges
	announceTo
	labels

	TP/oneM2M/CSE/DMR/UPD/004_SUB/ET/LBL/EXC
	Release 1
	PICS_SUB_LBL and PICS_SUB_EXC
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	expirationTime
	labels
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/004_GRP/ET/GN/LBL
	Release 1
	PICS_GRP_GN and PICS_GRP_LBL
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	expirationTime
	groupName
	labels

	TP/oneM2M/CSE/DMR/UPD/004_SCH/SE/AT/LBL
	Release 3
	
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	scheduleElement
	announceTo
	labels

	TP/oneM2M/CSE/DMR/UPD/004_TS/ET/MNI/LBL
	Release 3
	
	TS-0001 [1], clause 10.2.13.4
	15 (pollingChannel)
	expirationTime
	maxNrOfInstances
	labels



TP/oneM2M/CSE/DMR/UPD/005
	TP Id
	TP/oneM2M/CSE/DMR/UPD/005

	Test objective
	Check that the IUT responds with an error when the AE tries to update an attribute of a TARGET_RESOURCE_ADDRESS resource when the resource does not exist

	Reference
	TS-0001 [1], clause 10.1.3 - item 15)

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT not having created a resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID and
Content containing
valid representation resourcecontaining
valid attribute
}
	IUT <= AE

	
	then {
the IUT sends a valid Response containing
Response Status Code set to 4004 (NOT_FOUND)
}
	IUT => AE



TP/oneM2M/CSE/DMR/UPD/006
	TP Id
	TP/oneM2M/CSE/DMR/UPD/006

	Test objective
	Check that the IUT responds with an error when the AE tries to update the attribute ATTRIBUTE_NAME of a TARGET_RESOURCE_ADDRESS resource without having privileges for the UPDATE operation

	Reference
	TS-0001 [1], clause 10.1.3 - 16)

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a RW ATTRIBUTE_NAME attribute set to VALUE_1
and the AE having no privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resourcecontaining  | |
                     | ATTRIBUTE_NAME set to VALUE_2  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not update the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/DMR/UPD/006_CNT/LBL
	Release 1
	TS-0001 [1], clause 10.2.4.3
	3 (container)
	labels

	TP/oneM2M/CSE/DMR/UPD/006_ACP/LBL
	Release 1
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	labels

	TP/oneM2M/CSE/DMR/UPD/006_SUB/LBL
	Release 1
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	labels

	TP/oneM2M/CSE/DMR/UPD/006_GRP/LBL
	Release 1
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	labels

	TP/oneM2M/CSE/DMR/UPD/006_SCH/LBL
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	labels

	TP/oneM2M/CSE/DMR/UPD/005_TS/LBL
	Release 3
	TS-0001 [1], clause 10.2.30.3
	29 (timeSeries)
	labels

	TP/oneM2M/CSE/DMR/UPD/006_TRAM/LBL
	Release 4
	TS-0001 [1], clause 10.2.18.4
	50 (transactionMgmt)
	labels

	TP/oneM2M/CSE/DMR/UPD/006_TRAC/LBL
	Release 4
	TS-0001 [1], clause 10.2.18.8
	51 (transaction)
	labels



TP/oneM2M/CSE/DMR/UPD/007
	TP Id
	TP/oneM2M/CSE/DMR/UPD/007

	Test objective
	Check that the IUT responds with an error when the AE tries to update a non-RW attribute ATTRIBUTE_NAME of a TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a non-RW ATTRIBUTE_NAME attribute
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resourcecontaining  | |
                     | valid ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not update the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/DMR/UPD/007_CNT/CT
	Release 1
	TS-0001 [1], clause 10.2.4.3
	3 (container)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_ACP/CT
	Release 1
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_SUB/CT
	Release 1
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_GRP/CT
	Release 1
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_SCH/CT
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_PCH/CT
	Release 2
	TS-0001 [1], clause 10.2.13.4
	15 (pollingChannel)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_TS/CT
	Release 3
	TS-0001 [1], clause 10.2.30.3
	29 (timeSeries)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_TRAM/CT
	Release 4
	TS-0001 [1], clause 10.2.18.4
	50 (transactionMgmt)
	creationTime

	TP/oneM2M/CSE/DMR/UPD/007_TRAC/CT
	Release 4
	TS-0001 [1], clause 10.2.18.8
	51 (transaction)
	creationTime



TP/oneM2M/CSE/DMR/UPD/008
	TP Id
	TP/oneM2M/CSE/DMR/UPD/008

	Test objective
	Check that the IUT responds with an error when the AE tries to delete a mandatory RW attribute ATTRIBUTE_NAME of a TARGET_RESOURCE_ADDRESS resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a mandatory RW ATTRIBUTE_NAME attribute
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID and
Content containing
RESOURCE_TYPE resourcecontaining
ATTRIBUTE_NAME attribute set to NULL
}
	IUT <= AE

	
	then {
the IUT does not update the TARGET_RESOURCE_ADDRESS resource
and the IUT sends a valid Response containing
Response Status Code set to 4000 (BAD_REQUEST)
}
	IUT => AE



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/DMR/UPD/008_ACP/PVS
	Release 1
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	selfPrivileges

	TP/oneM2M/CSE/DMR/UPD/008_SUB/NU
	Release 1
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	notificationURI

	TP/oneM2M/CSE/DMR/UPD/008_GRP/MNI
	Release 1
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/UPD/008_SCH/SCE
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	expirationTime



Editor's Note: Release 2 test cases which are having expirationTime as attribute_name need to be verified.
TP/oneM2M/CSE/DMR/UPD/009
	TP Id
	TP/oneM2M/CSE/DMR/UPD/009

	Test objective
	Check that the IUT responds with an error when the AE tries to update a RW attribute ATTRIBUTE_NAME of the TARGET_RESOURCE_ADDRESS resource with an UNACCEPTABLE_VALUE

	Reference
	TS-0001 [1], clause 10.1.3 - item 3)

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a valid RW ATTRIBUTE_NAME attribute
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resourcecontaining  | |
                     | not supported ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not update the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/DMR/UPD/009_CNT/EXC
	Release 1
	TS-0001 [1], clause 10.2.4.3
	3 (container)
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/009_ACP/EXC
	Release 1
	TS-0001 [1], clause 10.2.21.3
	1 (accessControlPolicy)
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/009_SUB/MNI
	Release 1
	TS-0001 [1], clause 10.2.11.4
	23 (subscription)
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/UPD/009_GRP/EXC
	Release 1
	TS-0001 [1], clause 10.2.7.4
	9 (group)
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/009_SCH/EXC
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/009_PCH/EXC
	Release 2
	TS-0001 [1], clause 10.2.13.4
	15 (pollingChannel)
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/009_TS/EXC
	Release 3
	TS-0001 [1], clause 10.2.30.3
	29 (timeSeries)
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/009_TRAM/EXT
	Release 4
	TS-0001 [1],, clause 10.2.18.4
	50 (transactionMgmt)
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/009_TRAC/EXT
	Release 4
	TS-0001 [1],, clause 10.2.18.8
	51 (transaction)
	expirationTime



TP/oneM2M/CSE/DMR/UPD/010
	TP Id
	TP/oneM2M/CSE/DMR/UPD/010

	Test objective
	Check that the stateTag attribute of a RESOURCE_TYPE resource is increased when an update operation has been performed on its child resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a RESOURCE_TYPE resource containing
CHILD_RESOURCE_TYPE resource containing
ATTRIBUTE_NAME attribute set to VALUE_1
and the AE having privileges to perform UPDATE operation on the TARGET_CHILD_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_CHILD_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | CHILD_RESOURCE_TYPE resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT increments the stateTag attribute of RESOURCE_TYPE resource   | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+———————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/UPD/010_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.3
	3 (container)

	TP/oneM2M/CSE/DMR/UPD/010_TS
	Release 3
	TS-0001 [1], clause 10.2.30.3
	29 (timeSeries)



TP/oneM2M/CSE/DMR/UPD/011
	TP Id
	TP/oneM2M/CSE/DMR/UPD/011

	Test objective
	Check that the IUT rejects the UPDATE Request of an existing RESOURCE_TYPE resource with error "OPERATION_NOT_ALLOWED"

	Reference
	TS-0001 [1], clause 10.2.19.4, TS-0004 [2], clause 7.3.2.1 and clause 7.4.8.2.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a _PARENT RESOURCE_TYPE resource containing
a RESOURCE_TYPE resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Expected behaviour

	
	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID and
Content containing
RESOURCE_TYPE representation
}
	

	
	then {
the IUT does not update the RESOURCE_TYPE resource
and the IUT sends a valid Response containing
Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)
}
	



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	PARENT_RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/UPD/011_CNT/CIN
	Release 1
	TS-0001 [1], clause 10.2.4.3
	4 (contentInstance)
	3 (container)

	TP/oneM2M/CSE/DMR/UPD/011_TS/TSI
	Release 3
	TS-0001 [1], clause 10.2.31.3
	30 (timeSeriesInstance)
	29 (timeSeries)




TP/oneM2M/CSE/DMR/UPD/012
	TP Id
	TP/oneM2M/CSE/DMR/UPD/012

	Test objective
	Check that the IUT rejects the UPDATE Request of a latest resource as a direct child of a <container> resource with error "OPERATION_NOT_ALLOWED"

	Reference
	TS-0001 [1], clause 10.2.22, TS-0004 [2], clause 7.4.28.2.4 and clause 7.3.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource containing
a contentInstance resource containing
valid creationTime attribute set to the most recent resource creation time
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives an UPDATE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/la and  | |
                     | From set to AE_ID and  | |
                     |no Content   | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT does not update the CONTAINER_RESOURCE_ADDRESS/la resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/DMR/UPD/013
	TP Id
	TP/oneM2M/CSE/DMR/UPD/013

	Test objective
	Check that the IUT rejects the UPDATE Request of an oldest resource as a direct child of a <container> resource with error "OPERATION_NOT_ALLOWED"

	Reference
	TS-0001 [1], clause 10.2.23, TS-0004 [2], clause 7.4.29.2.4 and clause 7.3.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource containing
contentInstance resource(s)
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/ol and  | |
                     | From set to AE_ID and  | |
                     |no Content   | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT does not update the CONTAINER_RESOURCE_ADDRESS/ol resource  | |
                     | and the IUT sends a Response containing  | |
                     |Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+


TP/oneM2M/CSE/DMR/UPD/014
	
TP Id
	TP/oneM2M/CSE/DMR/UPD/014

	Test objective
	Check that the IUT updates successfully the value of the optional attribute OPTIONAL_ATTRIBUTE of the RESOURCE _ resource

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created the RESOURCE_TYPE resource
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE-ID and
Content containing
RESOURCE _ resource containing
OPTIONAL_ATTRIBUTE attribute set to VALUE
}
	IUT <= AE

	
	then {
the IUT sends a valid Response containing
Response Status Code set to 2004 (UPDATED) and
Content containing
RESOURCE_TYPE resourcecontaining
O_PTIONAL_ATTRIBUTE_ attribute set to VALUE
}
	IUT => AE



	TP Id
	PARENT_RELEASE
	PICS Selection
	Reference
	RESOURCE_TYPE
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/DMR/UPD/014_CNT/ACPI
	Release 1
	PICS_CNT_ACPI
	TS-0001 [1], clause 9.6.1.3.2-1
	container
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/014_CNT/ET
	Release 1
	PICS_CNT_ET
	TS-0001 [1], clause 9.6.1.3.1-1
	container
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/014_CNT/LBL
	Release 1
	PICS_CNT_LBL
	TS-0001 [1], clause 9.6.1.3.2-1
	container
	labels

	TP/oneM2M/CSE/DMR/UPD/014_CNT/MNI
	Release 1
	PICS_CNT_MNI
	TS-0001 [1], clause 9.6.6-2
	container
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/UPD/014_CNT/MBS
	Release 1
	PICS_CNT_MBS
	TS-0001 [1], clause 9.6.6-2
	container
	maxByteSize

	TP/oneM2M/CSE/DMR/UPD/014_CNT/MIA
	Release 1
	PICS_CNT_MIA
	TS-0001 [1], clause 9.6.6-2
	container
	maxInstanceAge

	TP/oneM2M/CSE/DMR/UPD/014_CNT/OR
	Release 1
	PICS_CNT_OR
	TS-0001 [1], clause 9.6.6-2
	container
	ontologyRef

	TP/oneM2M/CSE/DMR/UPD/014_ACP/ET
	Release 1
	N/A
	TS-0001 [1], clause 9.6.1.3.1-1
	accessControlPolicy
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/014_ACP/LBL
	Release 1
	PICS_ACP_LBL
	TS-0001 [1], clause 9.6.1.3.2-1
	accessControlPolicy
	labels

	TP/oneM2M/CSE/DMR/UPD/014_SUB/ACPI
	Release 1
	PICS_SUB_ACPI
	TS-0001 [1], clause 9.6.1.3.2-1
	subscription
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/014_SUB/ET
	Release 1
	N/A
	TS-0001 [1], clause 9.6.1.3.1-1
	subscription
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/014_SUB/LBL
	Release 1
	PICS_SUB_LBL
	TS-0001 [1], clause 9.6.1.3.2-1
	subscription
	labels

	TP/oneM2M/CSE/DMR/UPD/014_SUB/ENC
	Release 1
	PICS_SUB_ENC
	TS-0001 [1], clause 9.6.8-2
	subscription
	eventNotificationCriteria

	TP/oneM2M/CSE/DMR/UPD/014_SUB/EXC
	Release 1
	PICS_SUB_EXC
	TS-0001 [1], clause 9.6.8-2
	subscription
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/014_SUB/GPI
	Release 1
	PICS_SUB_GPI
	TS-0001 [1], clause 9.6.8-2
	subscription
	groupID

	TP/oneM2M/CSE/DMR/UPD/014_SUB/NFU
	Release 1
	PICS_SUB_NFU
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationForwardingURI

	TP/oneM2M/CSE/DMR/UPD/014_SUB/BN
	Release 1
	PICS_SUB_BN
	TS-0001 [1], clause 9.6.8-2
	subscription
	batchNotify

	TP/oneM2M/CSE/DMR/UPD/014_SUB/RL
	Release 1
	PICS_SUB_RL
	TS-0001 [1], clause 9.6.8-2
	subscription
	rateLimit

	TP/oneM2M/CSE/DMR/UPD/014_SUB/PN
	Release 1
	PICS_SUB_PN
	TS-0001 [1], clause 9.6.8-2
	subscription
	pendingNotification

	TP/oneM2M/CSE/DMR/UPD/014_SUB/NSP
	Release 1
	PICS_SUB_NSP
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationStoragePriority

	TP/oneM2M/CSE/DMR/UPD/014_SUB/LN
	Release 1
	PICS_SUB_LN
	TS-0001 [1], clause 9.6.8-2
	subscription
	latestNotify

	TP/oneM2M/CSE/DMR/UPD/014_SUB/NCT
	Release 1
	PICS_SUB_NCT
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationContentType

	TP/oneM2M/CSE/DMR/UPD/014_SUB/NEC
	Release 1
	PICS_SUB_NEC
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationEventCat

	TP/oneM2M/CSE/DMR/UPD/014_STCG/LBL
	Release 4
	
	TS-0001 [1], clause 9.6.23-2
	statsConfig
	labels

	TP/oneM2M/CSE/DMR/UPD/014_STCG/ACPI
	Release 4
	
	TS-0001 [1], clause 9.6.23-2
	statsConfig
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/014_TS/ACPI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/014_TS/LBL
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	labels

	TP/oneM2M/CSE/DMR/UPD/014_TS/MNI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	maximumNrOfInstances

	TP/oneM2M/CSE/DMR/UPD/014_TS/MBS
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	maxByteSize

	TP/oneM2M/CSE/DMR/UPD/014_TS/MIA
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	maxInstanceAge

	TP/oneM2M/CSE/DMR/UPD/014_TS/PEI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	periodicInterval

	TP/oneM2M/CSE/DMR/UPD/014_TS/MDD
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	missingDataDetect

	TP/oneM2M/CSE/DMR/UPD/014_TS/MDN
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	missingDataMaxNr

	TP/oneM2M/CSE/DMR/UPD/014_TS/MDT
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	missingDataDetectTimer

	TP/oneM2M/CSE/DMR/UPD/014_TS/OR
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	ontologyRef




TP/oneM2M/CSE/DMR/UPD/015
	TP Id
	TP/oneM2M/CSE/DMR/UPD/015

	Test objective
	Check that the IUT updates successfully the value of the optional attribute OPTIONAL_ATTRIBUTE of the RESOURCE _ resource under CSEBase

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resource containing
no OPTIONAL_ATTRIBUTE attribute
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--+------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE _ resource containing  | |
                     | OPTIONAL_ATTRIBUTE attribute set to VALUE  | |
                     |} | |
·                  +--+------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT updates the RESOURCE_TYPE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resourcecontaining  | |
                     | O_PTIONAL_ATTRIBUTE_ attribute set to VALUE  | |
                     |} | |
+———————-+–+————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	PICS Selection
	Reference
	RESOURCE_TYPE
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/DMR/UPD/015_CSR/LBL
	Release 1
	PICS_CSR_LBL
	TS-0001 [1], clause 9.6.4-2
	remoteCSE
	labels

	TP/oneM2M/CSE/DMR/UPD/015_CSR/POA
	Release 1
	PICS_CSR_POA
	TS-0001 [1], clause 9.6.4-2
	remoteCSE
	pointOfAccess

	TP/oneM2M/CSE/DMR/UPD/015_CSR/NL
	Release 1
	PICS_CSR_NL
	TS-0001 [1], clause 9.6.4-2
	remoteCSE
	nodeLink

	TP/oneM2M/CSE/DMR/UPD/015_AE/LBL
	Release 1
	PICS_AE_LBL
	TS-0001 [1], clause 9.6.5-2
	AE
	labels

	TP/oneM2M/CSE/DMR/UPD/015_AE/ACPI
	Release 1
	PICS_AE_ACPI
	TS-0001 [1], clause 9.6.5-2
	AE
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/015_AE/APN
	Release 1
	PICS_AE_APN
	TS-0001 [1], clause 9.6.5-2
	AE
	AppName

	TP/oneM2M/CSE/DMR/UPD/015_AE/POA
	Release 1
	PICS_AE_POA
	TS-0001 [1], clause 9.6.5-2
	AE
	pointOfAccess

	TP/oneM2M/CSE/DMR/UPD/015_AE/OR
	Release 1
	PICS_AE_OR
	TS-0001 [1], clause 9.6.5-2
	AE
	ontologyRef

	TP/oneM2M/CSE/DMR/UPD/015_CNT/LBL
	Release 1
	PICS_CNT_LBL
	TS-0001 [1], clause 9.6.6-2
	container
	labels

	TP/oneM2M/CSE/DMR/UPD/015_CNT/ACPI
	Release 1
	PICS_CNT_ACPI
	TS-0001 [1], clause 9.6.6-2
	container
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/015_CNT/MNI
	Release 1
	PICS_CNT_MNI
	TS-0001 [1], clause 9.6.6-2
	container
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/UPD/015_CNT/MBS
	Release 1
	PICS_CNT_MBS
	TS-0001 [1], clause 9.6.6-2
	container
	maxByteSize

	TP/oneM2M/CSE/DMR/UPD/015_CNT/MIA
	Release 1
	PICS_CNT_MIA
	TS-0001 [1], clause 9.6.6-2
	container
	maxInstanceAge

	TP/oneM2M/CSE/DMR/UPD/015_CNT/OR
	Release 1
	PICS_CNT_OR
	TS-0001 [1], clause 9.6.6-2
	container
	ontologyRef

	TP/oneM2M/CSE/DMR/UPD/015_CNT/LI
	Release 1
	PICS_CNT_LI
	TS-0001 [1], clause 9.6.6-2
	container
	locationID

	TP/oneM2M/CSE/DMR/UPD/015_ACP/LBL
	Release 1
	PICS_ACP_LBL
	TS-0001 [1], clause 9.6.2-2
	accessControlPolicy
	labels

	TP/oneM2M/CSE/DMR/UPD/015_SUB/ACPI
	Release 1
	PICS_SUB_ACPI
	TS-0001 [1], clause 9.6.8-2
	subscription
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/015_SUB/LBL
	Release 1
	PICS_SUB_LBL
	TS-0001 [1], clause 9.6.8-2
	subscription
	labels

	TP/oneM2M/CSE/DMR/UPD/015_SUB/ENC
	Release 1
	PICS_SUB_ENC
	TS-0001 [1], clause 9.6.8-2
	subscription
	eventNotificationCriteria

	TP/oneM2M/CSE/DMR/UPD/015_SUB/EXC
	Release 1
	PICS_SUB_EXC
	TS-0001 [1], clause 9.6.8-2
	subscription
	expirationCounter

	TP/oneM2M/CSE/DMR/UPD/015_SUB/GPI
	Release 1
	PICS_SUB_GPI
	TS-0001 [1], clause 9.6.8-2
	subscription
	groupID

	TP/oneM2M/CSE/DMR/UPD/015_SUB/NFU
	Release 1
	PICS_SUB_NFU
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationForwardingURI

	TP/oneM2M/CSE/DMR/UPD/015_SUB/BN
	Release 1
	PICS_SUB_BN
	TS-0001 [1], clause 9.6.8-2
	subscription
	batchNotify

	TP/oneM2M/CSE/DMR/UPD/015_SUB/RL
	Release 1
	PICS_SUB_RL
	TS-0001 [1], clause 9.6.8-2
	subscription
	rateLimit

	TP/oneM2M/CSE/DMR/UPD/015_SUB/PN
	Release 1
	PICS_SUB_PN
	TS-0001 [1], clause 9.6.8-2
	subscription
	pendingNotification

	TP/oneM2M/CSE/DMR/UPD/015_SUB/NSP
	Release 1
	PICS_SUB_NSP
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationStoragePriority

	TP/oneM2M/CSE/DMR/UPD/015_SUB/LN
	Release 1
	PICS_SUB_LN
	TS-0001 [1], clause 9.6.8-2
	subscription
	latestNotify

	TP/oneM2M/CSE/DMR/UPD/015_SUB/NEC
	Release 1
	PICS_SUB_NEC
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationEventCat

	TP/oneM2M/CSE/DMR/UPD/015_GRP/LBL
	Release 1
	PICS_GRP_LBL
	TS-0001 [1], clause 9.6.13-2
	group
	labels

	TP/oneM2M/CSE/DMR/UPD/015_GRP/ACPI
	Release 1
	PICS_GRP_ACPI
	TS-0001 [1], clause 9.6.13-2
	group
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/015_GRP/MACP
	Release 1
	PICS_GRP_MACP
	TS-0001 [1], clause 9.6.13-2
	group
	membersAccessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/015_GRP/GN
	Release 1
	PICS_GRP_GN
	TS-0001 [1], clause 9.6.13-2
	group
	groupName

	TP/oneM2M/CSE/DMR/UPD/015_NOD/LBL
	Release 4
	
	TS-0001 [1], clause 9.6.18-2
	node
	labels

	TP/oneM2M/CSE/DMR/UPD/015_NOD/ACPI
	Release 4
	
	TS-0001 [1], clause 9.6.18-2
	node
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/015_NOD/HCL
	Release 4
	
	TS-0001 [1], clause 9.6.18-2
	node
	hostedCSELink

	TP/oneM2M/CSE/DMR/UPD/015_TS/ACPI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/UPD/015_TS/LBL
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	labels

	TP/oneM2M/CSE/DMR/UPD/015_TS/MNI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	maximumNrOfInstances

	TP/oneM2M/CSE/DMR/UPD/015_TS/MBS
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	maxByteSize

	TP/oneM2M/CSE/DMR/UPD/015_TS/MIA
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	maxInstanceAge

	TP/oneM2M/CSE/DMR/UPD/015_TS/PEI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	periodicInterval

	TP/oneM2M/CSE/DMR/UPD/015_TS/MDD
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	missingDataDetect

	TP/oneM2M/CSE/DMR/UPD/015_TS/MDN
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	missingDataMaxNr

	TP/oneM2M/CSE/DMR/UPD/015_TS/MDT
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	missingDataDetectTimer

	TP/oneM2M/CSE/DMR/UPD/015_TS/OR
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	ontologyRef



TP/oneM2M/CSE/DMR/UPD/016
	TP Id
	TP/oneM2M/CSE/DMR/UPD/016

	Test objective
	Check that the IUT updates successfully the value of the attribute MANDATORY_ATTRIBUTE of the RESOURCE _ resource under CSEBase

	Reference
	TS-0001 [1], clause 10.1.3

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE under the CSEBase resource
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE-ID and
Content containing
RESOURCE _ resource containing
MANDATORY_ATTRIBUTE attribute set to VALUE
}
	IUT <= AE

	
	then {
the IUT updates the RESOURCE_TYPE resource
and the IUT sends a valid Response containing
Response Status Code set to 2004 (UPDATED) and
Content containing
RESOURCE_TYPE resourcecontaining
MANDATORY __ATTRIBUTE_ attribute set to VALUE
}
	IUT => AE



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	MANDATORY_ATTRIBUTE

	TP/oneM2M/CSE/DMR/UPD/016_CSR/ET
	Release 1
	TS-0001 [1], clause 9.6.4-2
	remoteCSE
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/016_CSR/RR
	Release 1
	TS-0001 [1], clause 9.6.4-2
	remoteCSE
	requestReachability

	TP/oneM2M/CSE/DMR/UPD/016_AE/ET
	Release 1
	TS-0001 [1], clause 9.6.5-2
	AE
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/016_AE/RR
	Release 1
	TS-0001 [1], clause 9.6.5-2
	AE
	requestReachability

	TP/oneM2M/CSE/DMR/UPD/016_CNT/ET
	Release 1
	TS-0001 [1], clause 9.6.6-2
	container
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/016_ACP/ET
	Release 1
	TS-0001 [1], clause 9.6.2-2
	accessControlPolicy
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/016_ACP/PV
	Release 1
	TS-0001 [1], clause 9.6.2-2
	accessControlPolicy
	privileges

	TP/oneM2M/CSE/DMR/UPD/016_ACP/PVS
	Release 1
	TS-0001 [1], clause 9.6.2-2
	accessControlPolicy
	selfPrivileges

	TP/oneM2M/CSE/DMR/UPD/016_SUB/ET
	Release 1
	TS-0001 [1], clause 9.6.8-2
	subscription
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/016_SUB/NU
	Release 1
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationURI

	TP/oneM2M/CSE/DMR/UPD/016_SUB/NCT
	Release 1
	TS-0001 [1], clause 9.6.8-2
	subscription
	notificationContentType

	TP/oneM2M/CSE/DMR/UPD/016_GRP/ET
	Release 1
	TS-0001 [1], clause 9.6.13-2
	group
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/016_GRP/MNM
	Release 1
	TS-0001 [1], clause 9.6.13-2
	group
	maxNrOfMembers

	TP/oneM2M/CSE/DMR/UPD/016_GRP/MID
	Release 1
	TS-0001 [1], clause 9.6.13-2
	group
	memberIDs

	TP/oneM2M/CSE/DMR/UPD/016_NOD/ET
	Release 4
	TS-0001 [1], clause 9.6.18-2
	node
	expirationTime

	TP/oneM2M/CSE/DMR/UPD/016_NOD/NI
	Release 4
	TS-0001 [1], clause 9.6.18-2
	node
	nodeID

	TP/oneM2M/CSE/DMR/UPD/016_TS/ET
	Release 3
	TS-0001 [1], clause 9.6.36-2
	timeSeries
	expirationTime



TP/oneM2M/CSE/DMR/UPD/017
	
TP Id
	TP/oneM2M/CSE/DMR/UPD/017

	Test objective
	Check that the IUT updates successfully the value of the announceTo optional attribute of the RESOURCE _ resource

	Reference
	TS-0001 [1], clause 10.2.18.4and clause 9.6.1.3.2-1, TS-0004 [2], clause 7.3.3.10

	Config Id
	CF02

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created the PARENT_RESOURCE resource containing
RESOURCE_TYPE resource containing
announceTo attribute set to NULL
and the IUT having announced the PARENT_RESOURCE resource
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid CREATE Request containing  | |
                     | To set ANNC_TARGET_CSE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resourcecontaining  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+—————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/UPD/017_ACP
	accesControlPolicy

	TP/oneM2M/CSE/DMR/UPD/017_CNT
	container

	TP/oneM2M/CSE/DMR/UPD/017_GRP
	group

	TP/oneM2M/CSE/DMR/UPD/017_LCP
	locationPolicy

	TP/oneM2M/CSE/DMR/UPD/017_MGO
	mgmtObj

	TP/oneM2M/CSE/DMR/UPD/017_NOD
	node

	TP/oneM2M/CSE/DMR/UPD/017_SCH
	schedule

	TP/oneM2M/CSE/DMR/UPD/017_TS
	timeSeries

	TP/oneM2M/CSE/DMR/UPD/017_TSI
	timeSeriesInstance



TP/oneM2M/CSE/DMR/UPD/018
	
TP Id
	TP/oneM2M/CSE/DMR/UPD/018

	Test objective
	Check that the IUT updates successfully the value of the announcedAttribute optional attribute of the RESOURCE _ resource

	Reference
	TS-0001 [1], clause 10.2.18.8 and clause 9.6.1.3.2-1, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a RESOURCE_TYPE resource containing
OA_ATTRIBUTE attribute set to VALUE and
announceTo attribute set to ANNC_TARGET_CSE_ADDRESS and
announcedAttribute attribute set to NULL
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announcedAttribute attribute set to OA_ATTRIBUTE  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | The IUT sends a valid UPDATE Request containing  | |
                     | To set to ANNC_TARGET_CSE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resourcecontaining  | |
                     | OA_ATTRIBUTE attribute set to VALUE  | |
                     |} | |
+———————-+——————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE
	OA_ATTRIBUTE

	TP/oneM2M/CSE/DMR/UPD/018_CNT/MBS
	container
	maxByteSize

	TP/oneM2M/CSE/DMR/UPD/018_GRP/MT
	Group
	memberType

	TP/oneM2M/CSE/DMR/UPD/018_LCP/LOI
	locationPolicy
	locationContainerID

	TP/oneM2M/CSE/DMR/UPD/018_MGO/DC
	mgmtObj
	description

	TP/oneM2M/CSE/DMR/UPD/018_NOD/HCL
	Node
	hostedCSELink

	TP/oneM2M/CSE/DMR/UPD/018_SCH/SE
	schedule
	scheduleElement

	TP/oneM2M/CSE/DMR/UPD/018_TS/MBS
	timeSeries
	maxByteSize



TP/oneM2M/CSE/DMR/UPD/019
	TP Id
	TP/oneM2M/CSE/DMR/UPD/019

	Test objective
	Check that the IUT rejects a UPDATE Request target to TARGET_ RESOURCE_ADDRESS resource when the Result Content set to RESULT_CONTENT

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to RESULT_CONTENT  | |
                     | Contentand  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid attribute  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+——————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	RESULT_CONTENT

	TP/oneM2M/CSE/DMR/UPD/019_RCN/2
	Release 2
	2 (hierarchical address)

	TP/oneM2M/CSE/DMR/UPD/019_RCN/3
	Release 2
	3 (attributes and hierarchichal address)

	TP/oneM2M/CSE/DMR/UPD/019_RCN/4
	Release 3
	4 (attributes and child resources)

	TP/oneM2M/CSE/DMR/UPD/019_RCN/5
	Release 3
	5 (attributes and child resource references)

	TP/oneM2M/CSE/DMR/UPD/019_RCN/6
	Release 3
	6 (child resource references)

	TP/oneM2M/CSE/DMR/UPD/019_RCN/7
	Release 3
	7 (original resource)

	TP/oneM2M/CSE/DMR/UPD/019_RCN/8
	Release 3
	8 (child resources)



TP/oneM2M/CSE/DMR/UPD/020
	TP Id
	TP/oneM2M/CSE/DMR/UPD/020

	Test objective
	Check that the IUT returns nothing of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 0 (nothing)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--+---------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to 0 (nothing)  | |
                     | Contentand  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid attribute  | |
                     |} | |
·                  +--+---------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | no Content  | |
                     |} | |
+———————-+–+———————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/UPD/020_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/UPD/020_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/UPD/020_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/UPD/020_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/UPD/020_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/UPD/020_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/UPD/020_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/UPD/020_TRAM
	Release 4
	50 (TransactionMgmt)

	TP/oneM2M/CSE/DMR/UPD/020_TRAC
	Release 4
	51 (Transaction)



TP/oneM2M/CSE/DMR/UPD/021
	TP Id
	
	TP/oneM2M/CSE/DMR/UPD/021
	
	

	Test objective
	
	Check that the IUT returns successfully only attributes of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 1 (attributes)
	
	

	Reference
	
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7
	
	

	Config Id
	
	CF01
	
	

	Parent Release
	
	PARENT_RELEASE
	
	

	PICS Selection
	
	PICS_CSE
	
	

	Initial conditions
	with { / the IUT being in the "initial state"/ and the IUT having registered the AE/ and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing / a child resource / and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS/}
	
	
	

	Expected behaviour
	Test events
	
	
	Direction

	
	
	when { / the IUT receives a valid UPDATE Request from AE containing/ To set to TARGET_RESOURCE_ADDRESS and/ From set to AE_ID and/ Result Content set to 1 (attributes)/ Contentand/ RESOURCE_TYPE resource containing/ valid attribute/}
	
	IUT <= AE

	
	
	
	then { / the IUT sends a valid Response containing/ Response Status Code set to 2004 (UPDATED) and/ Content containing/ RESOURCE_TYPE resource containing/ attributes and/ no hierarchichal address and/ no child resources and/ no child resource references/}
	



	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/UPD/021_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/UPD/021_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/UPD/021_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/UPD/021_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/UPD/021_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/UPD/021_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/UPD/021_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/UPD/021_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/UPD/021_TRAC
	Release 4
	51 (transaction)



TP/oneM2M/CSE/DMR/UPD/022
	TP Id
	
	TP/oneM2M/CSE/DMR/UPD/022
	
	

	Test objective
	
	Check that the IUT returns successfully only modified attributes of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 9 (modified attributes)
	
	

	Reference
	
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7
	
	

	Config Id
	
	CF01
	
	

	Parent Release
	
	PARENT_RELEASE
	
	

	PICS Selection
	
	PICS_CSE
	
	

	Initial conditions
	with { / the IUT being in the "initial state"/ and the IUT having registered the AE/ and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing/ a child resource/ and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS/}
	
	
	

	Expected behaviour
	Test events
	
	
	Direction

	
	
	when { / the IUT receives a valid UPDATE Request from AE containing/ To set to TARGET_RESOURCE_ADDRESS and/ From set to AE_ID and/ Result Content set to 9 (modified attributes)/ Contentand/ RESOURCE_TYPE resource containing/ valid ATTRIBUTE attribute set to VALUE/}
	
	IUT <= AE

	
	
	
	then { / the IUT sends a valid Response containing/ Response Status Code set to 2004 (UPDATED) and/ Content containing/ RESOURCE_TYPE resource containing/ modified attributes and/ no ATTRIBUTE attribute and/ no hierarchichal address and/ no child resources and/ no child resource references/}
	



	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/UPD/022_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/UPD/022_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/UPD/022_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/UPD/022_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/UPD/022_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/UPD/022_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/UPD/022_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/UPD/022_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/UPD/022_TRAC
	Release 4
	51 (transaction)




7.2.2.3.3	CREATE Operation
TP/oneM2M/CSE/DMR/CRE/001
	TP Id
	TP/oneM2M/CSE/DMR/CRE/001

	Test objective
	Check that the IUT accepts the creation of a RESOURCE_TYPE resource on the TARGET_RESOURCE_ADDRESS of type PARENT_RESOURCE_TYPE with resource name not provided

	Reference
	TS-0001 [1], clause 10.1.1.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT receives a valid CREATE Request from AE containing
Resource Type set to RESOURCE_TYPE and
To set to TARGET_RESOURCE_ADDRESS and
From set to AE-ID and
Content containing
RESOURCE_TYPE resource containing
no resourceName attribute
}
	IUT <= AE
	

	then {
the IUT creates the RESOURCE_TYPE resource
and the IUT sends a valid Response containing
Response Status Code set to 2001 (CREATED) and
Content containing
RESOURCE_TYPE resource containing
Valid resourceName attribute
}
	IUT => AE
	



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	PARENT_RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/001_CNT/CB
	Release 1
	TS-0001 [1], clause 10.2.4.1
	3 (container)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_CNT/AE
	Release 1
	TS-0001 [1], clause 10.2.4.1
	3 (container)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_CNT/CNT
	Release 1
	TS-0001 [1], clause 10.2.4.1
	3 (container)
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/001_ACP/CB
	Release 1
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_ACP/AE
	Release 1
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/CB
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/AE
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/CNT
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/ACP
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/CSR
	Release 1
	TS-0001 [1], clause 9.6.4-1
	23 (subscription)
	16 (remoteCSE)

	TP/oneM2M/CSE/DMR/CRE/001_CIN/CNT
	Release 1
	TS-0001 [1], clause 10.2.4.1
	4 (contentInstance)
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/001_GRP/CB
	Release 1
	TS-0001 [1], clause 10.2.7.2
	9 (group)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_GRP/AE
	Release 1
	TS-0001 [1], clause 10.2.7.2
	9 (group)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/GRP
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/001_SCH/CB
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_SCH/SUB
	Release 2
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/001_PCH/AE
	Release 2
	TS-0001 [1], clause 10.2.13.2
	15 (pollingChannel)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/SCH
	Release 3
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/001_NOD/CB
	Release 4
	TS-0001 [1], clause 9.6.3-1
	14 (node)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_MGC/CB
	Release 4
	TS-0001 [1], clause 9.6.3-1
	12 (mgmtCmd)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_LCP/CB
	Release 3
	TS-0001 [1], clause 9.6.3-1
	10 (locationPolicy)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_STCG/CB
	Release 4
	TS-0001 [1], clause 9.6.3-1
	22 (statsConfig)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_STCL/CB
	Release 4
	TS-0001 [1], clause 9.6.3-1
	21 (statsCollect)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_ASAR/CB
	Release 3
	TS-0001 [1], clause 9.6.3-1
	19(serviceSubscribedAppRule)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/AEA
	Release 3
	TS-0001 [1], clause 9.6.5-1
	23 (subscription)
	10002 (AEannc)

	TP/oneM2M/CSE/DMR/CRE/001_CNT/AEA
	Release 3
	TS-0001 [1], clause 9.6.5-1
	3 (container)
	10002 (AEannc)

	TP/oneM2M/CSE/DMR/CRE/001_GRP/AEA
	Release 3
	TS-0001 [1], clause 9.6.5-1
	9 (group)
	10002 (AEannc)

	TP/oneM2M/CSE/DMR/CRE/001_ACP/AEA
	Release 3
	TS-0001 [1], clause 9.6.5-1
	1 (accessControlPolicy)
	10002 (AEannc)

	TP/oneM2M/CSE/DMR/CRE/001_EVCF/STCG
	Release 4
	TS-0001 [1], clause 9.6.23-1
	7 (eventConfig)
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/CRE/001_SUB/STCG
	Release 4
	TS-0001 [1], clause 9.6.23-1
	23 (subscription)
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/CRE/001_TS/CB
	Release 3
	TS-0001 [1], clause 9.6.36-1
	29 (timeSeries)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_TS/AE
	Release 3
	TS-0001 [1], clause 9.6.36-1
	29 (timeSeries)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_TS/CSR
	Release 3
	TS-0001 [1], clause 9.6.36-1
	29 (timeSeries)
	16 (remoteCSE)

	TP/oneM2M/CSE/DMR/CRE/001_TS/AEA
	Release 3
	TS-0001 [1],clause 9.6.36-1
	29 (timeSeries)
	10002 (AEAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TSI/TS
	Release 3
	TS-0001 [1], clause 9.6.37-1
	30 (timeSeriesInstance)
	30 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/001_TRAM/CB
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	50 (transactionMgmt)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_TRAM/AE
	Release 4
	TS-0001 [], Table 9.6.1.1-1
	50 (transactionMgmt)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_TRAM/CSR
	Release 4
	TS-0001 [], Table 9.6.1.1-1
	50 (transactionMgmt)
	16 (RemoteCSE)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/ACP
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	1 (AccessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/AE
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	2 (AE)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/CNT
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	3 (Container)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/CIN
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	4 (ContentInstance)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/CB
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	5 (CSEBase)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/GRP
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	9 (Group)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/LCP
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10 (LocationPolicy)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/MSSP
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	11 (M2MServiceSubscriptionProfile)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/MGC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	12 (MgmtCmd)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/MGO
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	13 (MgmtObj)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/MGO
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	13 (MgmtObj)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/NOD
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	14 (Node)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/CSR
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	16 (RemoteCSE)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/SCH
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	18 (Schedule)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/ASAR
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	19 (ServiceSubscribedAppRule)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/SVSN
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	20 (ServiceSubscribedNode)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/STCL
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	21 (StatsCollect)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/STCG
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	22 (StatsConfig)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/SUB
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	23 (Subscription)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/SMD
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	24 (SemanticDescriptor)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/NTPR
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	25 (NotificationTargetMgmtPolicyRef)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/NTP
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	26 (NotificationTargetPolicy)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/PDR
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	27 (PolicyDeletionRules)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/TS
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	29 (TimeSeries)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/TSI
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	30 (TimeSeriesInstance)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/ROL
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	31 (Role)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/TK
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	32 (Token)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/TS
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	29 (TimeSeries)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/ACPANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10001 (AccessContraolPolicyAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/AEANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10002 (AEAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/CNTANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10003 (ContainerAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/CINANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10001 (ContentInstanceAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/GRPANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10009 (GroupAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/LCPANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10010 (LocationPolicyAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/MGOANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10013 (MgmtObjAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/NODANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10014 (NodeAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/CSRANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10016 (RemoteCSEAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/SCHANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10018 (ScheduleAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/SMDANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10024 (AccessContraolPolicyAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/TSANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10029 (TimeSeriesAnnc)

	TP/oneM2M/CSE/DMR/CRE/001_TRAC/TSIANNC
	Release 4
	TS-0001 [1], Table 9.6.1.1-1
	51 (transaction)
	10030 (TimeSeriesInstanceAnnc)



TP/oneM2M/CSE/DMR/CRE/002
	TP Id
	TP/oneM2M/CSE/DMR/CRE/002

	Test objective
	Check that the IUT accepts the creation of a RESOURCE_TYPE resource with a non-existing resource name provided by AE

	Reference
	TS-0001 [1], clause 10.1.1.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
and the TARGET_RESOURCE_ADDRESScontaining
no child resource containing
resourceName attribute set to NAME
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT receives a valid CREATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
Resource Type set to RESOURCE_TYPE and
From set to AE-ID and
Content containing
RESOURCE_TYPE resource containing
resourceName attribute set to NAME
}
	IUT <= AE
	

	then {
the IUT creates the RESOURCE_TYPE resource
and the IUT sends a valid Response containing
Response Status Code set to 2001 (CREATED)
}
	IUT => AE
	



	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/002_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.1
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/002_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/002_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/002_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/002_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/002_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/002_TS
	Release 3
	TS-0001 [1], clause 10.2.30.1
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/002_FLXC
	Release 2
	TS-0001 [1], clause 10.2.29.1
	28 (flexContainer)

	TP/oneM2M/CSE/DMR/CRE/002_TRAM
	Release 4
	TS-0001 [1], clause 10.1.2, Step-2
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/CRE/002_TRAC
	Release 4
	TS-0001 [1], clause 10.1.2, Step-2
	51 (transaction)




TP/oneM2M/CSE/DMR/CRE/003
	TP Id
	TP/oneM2M/CSE/DMR/CRE/003

	Test objective
	Check that the IUT rejects the creation of a RESOURCE_TYPE resource with an existing resource name provided by AE

	Reference
	TS-0001 [1], clause 10.1.1.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
and the TARGET_RESOURCE_ADDRESS containing
a child resource having
resourceName attribute set to NAME
}




·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to RESOURCE_TYPE and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | resourceName attribute set to NAME  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4105 (CONFLICT)  | |
                     |} | |
+———————-+——————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/003_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.1
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/003_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/003_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/003_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/003_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/003_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/003_TS
	Release 3
	TS-0001 [1], clause 10.2.30.1
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/003_TRAM
	Release 4
	TS-0001 [1], clause 10.1.2, Step-2
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/CRE/003_TRAC
	Release 4
	TS-0001 [1], clause 10.2.30.1
	51 (transaction)




TP/oneM2M/CSE/DMR/CRE/004
	TP Id
	TP/oneM2M/CSE/DMR/CRE/004

	Test objective
	Check that the IUT rejects the creation of a RESOURCE_TYPE resource when AE has no privileges

	Reference
	TS-0001 [1], clause 10.1.1.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having no privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------+-----------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to RESOURCE_TYPE and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource  | |
                     |} | |
·                  +----------------------+-----------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the RESOURCE_TYPE resource   | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————-+———————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/004_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.1
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/004_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/004_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/004_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/004_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/004_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/004_TS
	Release 3
	TS-0001 [1], clause 10.2.30.1
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/004_TRAM
	Release 4
	TS-0001 [1], clause 10.1.2, Step-2
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/CRE/004_TRAC
	Release 4
	TS-0001 [1], clause 10.2.30.1
	51 (transaction)




TP/oneM2M/CSE/DMR/CRE/005
	TP Id
	TP/oneM2M/CSE/DMR/CRE/005

	Test objective
	Check that the IUT rejects the CREATE Request of container resource when the RW ATTRIBUTE is provided with an invalid value

	Reference
	TS-0001 [1], clause 10.2.4.1, TS-0004 [2], clause 7.4.7.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource AE_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid CREATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID and
Resource Type set to 3 (container) and
Content containing
an invalid RW ATTRIBUTE attribute
}
	IUT <= AE

	
	then {
the IUT does not create the container resource
and the IUT sends a valid Response containing
Response Status Code set to 4000 (BAD_REQUEST)
}
	IUT => AE



	TP Id
	Reference
	ATTRIBUTE

	TP/oneM2M/CSE/DMR/CRE/005_MNI
	TS-0001 [1], clause 9.6.6, TS-0004 [2], clause 7.4.7.1
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/CRE/005_MBS
	TS-0001 [1], clause 9.6.6, TS-0004 [2], clause 7.4.7.1
	maxByteSize

	TP/oneM2M/CSE/DMR/CRE/005_MIA
	TS-0001 [1], clause 9.6.6, TS-0004 [2], clause 7.4.7.1
	maxInstanceAge



TP/oneM2M/CSE/DMR/CRE/006
	TP Id
	TP/oneM2M/CSE/DMR/CRE/006

	Test objective
	Check that the IUT returns a default value to RW ATTRIBUTE in the response of a RESOURCE_TYPE resource CREATE Request where no a RW ATTRIBUTE is provided by AE

	Reference
	TS-0001 [1], clause 10.2.4.1, TS-0004 [2], clause 7.4.7.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource AE_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid CREATE Request from AE containing
To set to AE_RESOURCE_ADDRESS and
From set to AE_ID and
Resource Type set to RESOURCE_TYPE and
Content containing
RESOURCE_TYPE resource representation
}
	IUT <= AE

	
	then {
the IUT creates the RESOURCE_TYPE resource
and the IUT sends a valid Response containing
Response Status Code set to 2001 (CREATED) and
Content containing
RESOURCE_TYPE resource containing
valid ATTRIBUTE attribute
}
	IUT => AE



	TP Id
	PARENT _ RELEASE
	Reference
	RESOURCE_TYPE
	ATTRIBUTE

	TP/oneM2M/CSE/DMR/CRE/006_CNT/MNI
	Release 1
	TS-0001 [1], clause 9.6.6, TS-0004 [2], clause 7.4.7.1
	container
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/CRE/006_CNT/MBS
	Release 1
	TS-0001 [1], clause 9.6.6, TS-0004 [2], clause 7.4.7.1
	container
	maxByteSize

	TP/oneM2M/CSE/DMR/CRE/006_CNT/MIA
	Release 1
	TS-0001 [1], clause 9.6.6, TS-0004 [2], clause 7.4.7.1
	container
	maxInstanceAge

	TP/oneM2M/CSE/DMR/CRE/006_TS/MNI
	Release 3
	TS-0001 [1], clause 9.6.36, TS-0004 [2], clause 7.4.38.1
	timeSeries
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/CRE/006_TS/MBS
	Release 3
	TS-0001 [1], clause 9.6.36, TS-0004 [2], clause 7.4.38.1
	timeSeries
	maxByteSize

	TP/oneM2M/CSE/DMR/CRE/006_TS/MIA
	Release 3
	TS-0001 [1], clause 9.6.36, TS-0004 [2], clause 7.4.38.1
	timeSeries
	maxInstanceAge



TP/oneM2M/CSE/DMR/CRE/007
	TP Id
	TP/oneM2M/CSE/DMR/CRE/007

	Test objective
	Checks that the IUT accepts a newly created RESOURCE_TYPE when the currentNrOfInstances exceeds the field value set in maxNrOfInstances in the _PARENT RESOURCE_TYPE resource by removing enough of the oldest RESOURCE_TYPE resources to allow the creation of the new RESOURCE_TYPE resource

	Reference
	TS-0001 [1], clause 10.2.19.2, TS-0004 [2], clause 7.4.8.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a PARENT_RESOURCE_TYPE resource containing
currentNrOfInstances attribute set to MAX_NUMBER_OF_INSTANCES
and maxNrOfInstances attribute set to MAX_NUMBER_OF_INSTANCES
and the AE having privileges to perform CREATE operation on the resource PARENT __RESOURCE_ADDRESS_
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to RESOURCE_TYPE and  | |
                     |Content containing  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT creates the RESOURCE_TYPE resource  | |
                     | and the IUT removes the oldest RESOURCE_TYPE resources   | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RE LEASE
	PARENT_RESOURCE_TYPE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/007_CNT/CIN
	Release 1
	container
	contentInstance

	TP/oneM2M/CSE/DMR/CRE/007_TS/TSI
	Release 3
	timeSeries
	timeSeriesInstance



TP/oneM2M/CSE/DMR/CRE/008
	TP Id
	TP/oneM2M/CSE/DMR/CRE/008

	Test objective
	Checks that the IUT accepts a newly created RESOURCE_TYPE resource when the currentByteSize exceeds the field value set in maxByteSize in the _PARENT RESOURCE_TYPE resource by removing enough of the oldest RESOURCE_TYPE resources to allow the creation of the new RESOURCE_TYPE resource

	Reference
	TS-0001 [1], clause 10.2.19.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a _PARENT RESOURCE_TYPE resource containing
maxByteSize attribute set to MAX_BYTE_SIZE_OF_DATA and
currentByteSize attribute set to MAX_BYTE_SIZE_OF_DATA
and the AE having privileges to perform CREATE operation on the resource PARENT_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |Resource Type set to RESOURCE_TYPE and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource with size less than  | |
                     | MAX_BYTE_SIZE_OF DATA  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {  |IUT => AE |
                     |the IUT creates the RESOURCE_TYPE resource  | |
                     |and the IUT removes the oldest contentInstance resources  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————————————–+———————-+
	TP Id
	PARENT_RE LEASE
	PARENT_RESOURCE_TYPE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/008_CNT/CIN
	Release 1
	container
	contentInstance

	TP/oneM2M/CSE/DMR/CRE/008_TS/TSI
	Release 3
	timeSeries
	timeSeriesInstance



TP/oneM2M/CSE/DMR/CRE/009
	TP Id
	TP/oneM2M/CSE/DMR/CRE/009

	Test objective
	Check that the IUT increaments and then copies the field value of attribute stateTag in parent container resource when contentInstance resource is created as the direct child of the parent container

	Reference
	TS-0001 [1], clause 9.6.1.3.2, TS-0004 [2], clause 7.4.7.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource CONTAINER_RESOURCE_ADDRESScontaining
stateTag attribute
and the AE having privileges to perform CREATE operation on the resource CONTAINER_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |Resource Type set to 4 (contentInstance) and  | |
                     |Content containing  | |
                     | contentInstance resource representation   | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT increments stateTag attribute of CONTAINER_RESOURCE_ADDRESS resource  | |
                     |and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/DMR/CRE/010
	TP Id
	TP/oneM2M/CSE/DMR/CRE/010

	Test objective
	Check that the IUT rejects the CREATE Request of a container resource named "la" as a direct child of a container resource

	Reference
	TS-0001 [1], clause 10.2.22, TS-0004 [2], clause 7.4.28.2.2 and clause 7.3.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS
and the IUT having privileges to perform CREATE operation on the resource CONTAINER_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |Content containing  | |
                     | Container resource containing  | |
                     | resourceName attribute set to "la"  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT does not create the container resource   | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+————————————————————————————————————-+————-+
TP/oneM2M/CSE/DMR/CRE/011
	TP Id
	TP/oneM2M/CSE/DMR/CRE/011

	Test objective
	Check that the IUT rejects the CREATE Request of a container resource named "ol" as a direct child of a container resource

	Reference
	TS-0001 [1], clause 10.2.23, TS-0004 [2], clause 7.4.29.2.2 and clause 7.3.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a container resource CONTAINER_RESOURCE_ADDRESS
and the IUT having privileges to perform CREATE operation on the resource CONTAINER_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |Content containing  | |
                     |container resource containing  | |
                     | resourceName attribute set to "ol"  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT does not create the container resource   | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+————————————————————————————————————-+————-+
TP/oneM2M/CSE/DMR/CRE/012
	
TP Id
	TP/oneM2M/CSE/DMR/CRE/012

	Test objective
	Check that the IUT accepts the creation of a RESOURCE_TYPE resource with the optional attribute OPTIONAL_ATTRIBUTE provided

	Reference
	TS-0001 [1], clause 10.1.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource AE_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid CREATE Request from AE containing
To set to AE_RESOURCE_ADDRESS and
From set to AE-ID and
Content containing
RESOURCE_TYPE resource containing
valid OPTIONAL_ATTRIBUTE attribute
}
	IUT <= AE

	
	then {
the IUT creates the RESOURCE_TYPE resource
and the IUT sends a valid Response containing
Response Status Code set to 2001 (CREATED)
}
	IUT => AE



	TP Id
	PARENT_RELEASE
	PICS Selection
	Reference
	RESOURCE_TYPE
	OPTIONAL_ATTRIBUTE

	TP/oneM2M/CSE/DMR/CRE/012_CNT/ACPI
	Release 1
	PICS_CNT_ACPI
	TS-0001 [1], clause 9.6.1.3.2-1
	3 (container)
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/CRE/012_CNT/ET
	Release 1
	PICS_CNT_ET
	TS-0001 [1], clause 9.6.1.3.1-1
	3 (container)
	expirationTime

	TP/oneM2M/CSE/DMR/CRE/012_CNT/LBL
	Release 1
	PICS_CNT_LBL
	TS-0001 [1], clause 9.6.1.3.2-1
	3 (container)
	labels

	TP/oneM2M/CSE/DMR/CRE/012_CNT/MNI
	Release 1
	PICS_CNT_MNI
	TS-0001 [1], clause 9.6.6-2
	3 (container)
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/CRE/012_CNT/MBS
	Release 1
	PICS_CNT_MBS
	TS-0001 [1], clause 9.6.6-2
	3 (container)
	maxByteSize

	TP/oneM2M/CSE/DMR/CRE/012_CNT/MIA
	Release 1
	PICS_CNT_MIA
	TS-0001 [1], clause 9.6.6-2
	3 (container)
	maxInstanceAge

	TP/oneM2M/CSE/DMR/CRE/012_CNT/OR
	Release 1
	PICS_CNT_OR
	TS-0001 [1], clause 9.6.6-2
	3 (container)
	ontologyRef

	TP/oneM2M/CSE/DMR/CRE/012_CNT/CR
	Release 1
	PICS_CNT_CR
	TS-0001 [1], clause 9.6.6-2
	3 (container)
	creator

	TP/oneM2M/CSE/DMR/CRE/012_CIN/ET
	Release 1
	PICS_CIN_ET
	TS-0001 [1], clause 9.6.1.3.1-1
	4 (contentInstance)
	expirationTime

	TP/oneM2M/CSE/DMR/CRE/012_CIN/LBL
	Release 1
	PICS_CIN_LBL
	TS-0001 [1], clause 9.6.1.3.2-1
	4 (contentInstance)
	labels

	TP/oneM2M/CSE/DMR/CRE/012_CIN/CR
	Release 1
	PICS_CIN_CR
	TS-0001 [1], clause 9.6.7-2
	4 (contentInstance)
	creator

	TP/oneM2M/CSE/DMR/CRE/012_CIN/CNF
	Release 1
	PICS_CIN_CNF
	TS-0001 [1], clause 9.6.7-2
	4 (contentInstance)
	contentInfo

	TP/oneM2M/CSE/DMR/CRE/012_CIN/OR
	Release 1
	PICS_CIN_OR
	TS-0001 [1], clause 9.6.7-2
	4 (contentInstance)
	ontologyRef

	TP/oneM2M/CSE/DMR/CRE/012_ACP/ET
	Release 1
	N/A
	TS-0001 [1], clause 9.6.1.3.1-1
	1 (accesControlPolicy)
	expirationTime

	TP/oneM2M/CSE/DMR/CRE/012_ACP/LBL
	Release 1
	PICS_ACP_LBL
	TS-0001 [1], clause 9.6.1.3.2-1
	1 (accesControlPolicy)
	labels

	TP/oneM2M/CSE/DMR/CRE/012_SUB/ACPI
	Release 1
	PICS_SUB_ACPI
	TS-0001 [1], clause 9.6.1.3.2-1
	23 (subscription)
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/CRE/012_SUB/ET
	Release 1
	N/A
	TS-0001 [1], clause 9.6.1.3.1-1
	23 (subscription)
	expirationTime

	TP/oneM2M/CSE/DMR/CRE/012_SUB/LBL
	Release 1
	PICS_SUB_LBL
	TS-0001 [1], clause 9.6.1.3.2-1
	23 (subscription)
	labels

	TP/oneM2M/CSE/DMR/CRE/012_SUB/ENC
	Release 1
	PICS_SUB_ENC
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	eventNotificationCriteria

	TP/oneM2M/CSE/DMR/CRE/012_SUB/EXC
	Release 1
	PICS_SUB_EXC
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	expirationCounter

	TP/oneM2M/CSE/DMR/CRE/012_SUB/GPI
	Release 1
	PICS_SUB_GPI
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	groupID

	TP/oneM2M/CSE/DMR/CRE/012_SUB/NFU
	Release 1
	PICS_SUB_NFU
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	notificationForwardingURI

	TP/oneM2M/CSE/DMR/CRE/012_SUB/BN
	Release 1
	PICS_SUB_BN
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	batchNotify

	TP/oneM2M/CSE/DMR/CRE/012_SUB/RL
	Release 1
	PICS_SUB_RL
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	rateLimit

	TP/oneM2M/CSE/DMR/CRE/012_SUB/PSN
	Release 1
	PICS_SUB_PSN
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	preSubscriptionNotify

	TP/oneM2M/CSE/DMR/CRE/012_SUB/PN
	Release 1
	PICS_SUB_PN
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	pendingNotification

	TP/oneM2M/CSE/DMR/CRE/012_SUB/NSP
	Release 1
	PICS_SUB_NSP
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	notificationStoragePriority

	TP/oneM2M/CSE/DMR/CRE/012_SUB/LN
	Release 1
	PICS_SUB_LN
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	latestNotify

	TP/oneM2M/CSE/DMR/CRE/012_SUB/NCT
	Release 1
	PICS_SUB_NCT
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	notificationContentType

	TP/oneM2M/CSE/DMR/CRE/012_SUB/NEC
	Release 1
	PICS_SUB_NEC
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	notificationEventCat

	TP/oneM2M/CSE/DMR/CRE/012_SUB/CR
	Release 1
	PICS_SUB_CR
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	creator

	TP/oneM2M/CSE/DMR/CRE/012_SUB/SU
	Release 1
	PICS_SUB_SU
	TS-0001 [1], clause 9.6.8-2
	23 (subscription)
	subscriberURI

	TP/oneM2M/CSE/DMR/CRE/012_STCG/CR
	Release 4
	
	TS-0001 [1], clause 9.6.23-2
	22 (statsConfig)
	creator

	TP/oneM2M/CSE/DMR/CRE/012_TS/ACPI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	accessControlPolicyIDs

	TP/oneM2M/CSE/DMR/CRE/012_TS/ET
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	expirationTime

	TP/oneM2M/CSE/DMR/CRE/012_TS/LBL
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	labels

	TP/oneM2M/CSE/DMR/CRE/012_TS/CR
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	creator

	TP/oneM2M/CSE/DMR/CRE/012_TS/MNI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	maxNrOfInstances

	TP/oneM2M/CSE/DMR/CRE/012_TS/MBS
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	maxByteSize

	TP/oneM2M/CSE/DMR/CRE/012_TS/MIA
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	maxInstanceAge

	TP/oneM2M/CSE/DMR/CRE/012_TS/PEI
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	periodicInterval

	TP/oneM2M/CSE/DMR/CRE/012_TS/MDD
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	missingDataDetect

	TP/oneM2M/CSE/DMR/CRE/012_TS/MDN
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	missingDataMaxNr

	TP/oneM2M/CSE/DMR/CRE/012_TS/MDT
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	missingDataDetectTimer

	TP/oneM2M/CSE/DMR/CRE/012_TS/OR
	Release 3
	
	TS-0001 [1], clause 9.6.36-2
	29 (timeSeries)
	ontologyRef

	TP/oneM2M/CSE/DMR/CRE/012_TSI/ET
	Release 3
	
	TS-0001 [1], clause 9.6.37-2
	30 (timeSeriesInstance)
	expirationTime

	TP/oneM2M/CSE/DMR/CRE/012_TSI/LBL
	Release 3
	
	TS-0001 [1], clause 9.6.37-2
	30 (timeSeriesInstance)
	labels

	TP/oneM2M/CSE/DMR/CRE/012_TSI/SNR
	Release 3
	
	TS-0001 [1], clause 9.6.37-2
	30 (timeSeriesInstance)
	sequenceNr

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TLTM
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionLockTime

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TEXT
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionExecuteTime

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TCT
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionCommitTime

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TEPT
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionExpirationTime

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TMD
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionMode

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TLTP
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionLockType

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TMR
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionMaxRetries

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TMH
	Release 4
	
	TS-0004 [2], Table 7.4.60.1-363
	50 (transactionMgmt)
	transactionManagementHandling

	TP/oneM2M/CSE/DMR/CRE/012_TRAC/TLTM
	Release 4
	
	TS-0004 [2], Table 7.4.61.1-367
	51 (transaction)
	transactionLockTime

	TP/oneM2M/CSE/DMR/CRE/012_TRAC/TEXT
	Release 4
	
	TS-0004 [2], Table 7.4.61.1-367
	51 (transaction)
	transactionExecuteTime

	TP/oneM2M/CSE/DMR/CRE/012_TRAC/TCT
	Release 4
	
	TS-0004 [2], Table 7.4.61.1-367
	51 (transaction)
	transactionCommitTime

	TP/oneM2M/CSE/DMR/CRE/012_TRAM/TLTP
	Release 4
	
	TS-0004 [2], Table 7.4.61.1-367
	51 (transaction)
	transactionLockType



TP/oneM2M/CSE/DMR/CRE/013
	TP Id
	TP/oneM2M/CSE/DMR/CRE/013

	Test objective
	Check that the IUT rejects the CREATE Request of a RESOURCE_TYPE resource with error "NOT_ACCEPTABLE" when contentSize exceeds maxByteSize of the PARENT_RESOURCE_TYPE

	Reference
	TS-0001 [1], clause 10.2.19, TS-0004 [2], clause 7.4.7.2.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a PARENT_RESOURCE_TYPE resource having
maxByteSize attribute set to MAX_BYTE_SIZE
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid CREATE Request from AE containing
To set to PARENT_RESOURCE_ADDRESS and
From set to AE_ID and
Content containing
RESOURCE_TYPE resource containing
valid content with size larger than MAX_BYTE_SIZE
}
	IUT <= AE

	
	then {
the IUT sends a valid Response containing
Response Status Code set to 5207 (NOT_ACCEPTABLE)
}
	IUT => AE



	TP Id
	PARENT_RE LEASE
	PARENT_RESOURCE_TYPE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/013_CNT/CIN
	Release 1
	container
	contentInstance

	TP/oneM2M/CSE/DMR/CRE/013_TS/TSI
	Release 3
	timeSeries
	timeSeriesInstance



TP/oneM2M/CSE/DMR/CRE/014
	TP Id
	TP/oneM2M/CSE/DMR/CRE/014

	Test objective
	Check that the IUT updates the currentByteSize attribute in a PARENT_RESOURCE_TYPE when a new RESOURCE_TYPE is created

	Reference
	TS-0001 [1], clause 10.2.19.2, TS-0004 [2], clause 7.4.8.2

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a PARENT_RESOURCE_TYPE resource at PARENT_RESOURCE_ADDRESS containing
maxByteSize attribute set to MAX_BYTE_SIZE_OF_DATA and
currentByteSize attribute set to 0
and the AE having privileges to perform CREATE operation on the resource PARENT_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to RESOURCE_TYPE and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | valid content attribute with size equal to DATA_SIZE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT increments currentByteSize attribute of PARENT_RESOURCE_ADDRESS resource by DATA_SIZE  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+—————————————————————————————————————-+————-+
	TP Id
	PARENT_RE LEASE
	PARENT_RESOURCE_TYPE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/014_CNT/CIN
	Relase 1
	container
	contentInstance

	TP/oneM2M/CSE/DMR/CRE/014_TS/TSI
	Release 3
	timeSeries
	timeSeriesInstance



TP/oneM2M/CSE/DMR/CRE/015
	TP Id
	TP/oneM2M/CSE/DMR/CRE/015

	Test objective
	Check that the IUT returns successfully after a CREATE request an empty content of created resource when the ResultContent set to 0 (Nothing)

	Reference
	TS-0001 [1], clause 8.1.2, clause 8.1.3 and clause 10.1.1.1, TS-0004 [2], clause 6.3.4.2.7

	Parent Release
	PARENT_RELEASE

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to RESOURCE_TYPE and  | |
                     |Result Content set to 0 (nothing) and  | |
                     |Contentcontaining  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED) and  | |
                     |no Content  | |
                     |} | |
+———————-+——————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/015_CNT
	Release 2
	TS-0001 [1], clause 10.2.4.1
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/015_GRP
	Release 2
	TS-0001 [1], clause 10.2.7.2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/015_ACP
	Release 2
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/015_SUB
	Release 2
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/015_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/015_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/015_TS
	Release 3
	TS-0001 [1], clause 10.2.30.1
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/015_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.2
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/CRE/015_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.6
	51 (transaction)



TP/oneM2M/CSE/DMR/CRE/016
	TP Id
	TP/oneM2M/CSE/DMR/CRE/016

	Test objective
	Check that the IUT returns successfully after a CREATE request only hierarchichal address of the created resource when the Result Content is set to 2 (hierarchical address)

	Reference
	TS-0001 [1], clause 8.1.2, clause 8.1.3 and clause 10.1.1.1, TS-0004 [2], clause 6.3.4.2.7

	Parent Release
	PARENT_RELEASE

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |Resource Type set to RESOURCE_TYPE and  | |
                     | Result Content set to 2 (hierarchical address) and  | |
                     | Contentcontaining  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | Hierarchical address of the RESOURCE_TYPE resource  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/016_CNT
	Release 2
	TS-0001 [1], clause 10.2.4.1
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/016_GRP
	Release 2
	TS-0001 [1], clause 10.2.7.2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/016_ACP
	Release 2
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/016_SUB
	Release 2
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/016_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/016_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/016_TS
	Release 3
	TS-0001 [1], clause 10.2.30.1
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/016_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.2
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/CRE/016_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.6
	51 (transaction)



TP/oneM2M/CSE/DMR/CRE/017
	TP Id
	TP/oneM2M/CSE/DMR/CRE/017

	Test objective
	Check that the IUT returns successfully after a CREATE request only attributes and hierarchichal address of the created resource when Result Content is set 3 (attributes and hierarchichal address)

	Reference
	TS-0001 [1], clause 8.1.2, clause 8.1.3 and clause 10.1.1.1, TS-0004 [2], clause 6.3.4.2.7

	Parent Release
	PARENT_RELEASE

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to RESOURCE_TYPE and  | |
                     | Result Content set to 3 (attributes and hierarchichal address_)_ and  | |
                     | Contentcontaining  | |
                     | RESOURCE_TYPE resource representation  | |
                     |  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | resource element containing  | |
                     | Hierarchical address of the RESOURCE_TYPE resourceand  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/017_CNT
	Release 2
	TS-0001 [1], clause 10.2.4.1
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/017_GRP
	Release 2
	TS-0001 [1], clause 10.2.7.2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/017_ACP
	Release 2
	TS-0001 [1], clause 10.2.21.1
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/017_SUB
	Release 2
	TS-0001 [1], clause 10.2.11.2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/017_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/017_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/017_TS
	Release 3
	TS-0001 [1], clause 10.2.30.1
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/017_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.2
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/CRE/017_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.6
	51 (transaction)



TP/oneM2M/CSE/DMR/CRE/018
	TP Id
	TP/oneM2M/CSE/DMR/CRE/018

	Test objective
	Check that the IUT rejects a CREATE request when the ResultContent is set to RESULT_CONTENT

	Reference
	TS-0001 [1], clause 8.1.2 & TS-0004 [2], clause 7.3.2.1

	Parent Release
	Release 2

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource AE_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction

	when {
the IUT receives a valid CREATE Request from AE containing
To set to AE_RESOURCE_ADDRESS and
From set to AE_ID and
Result Content set to RESULT_CONTENT
}
	IUT <= AE
	

	then {
the IUT sends a valid Response containing
Response Status Code set to 4000 (BAD_REQUEST)
}
	IUT => AE
	



	TP Id
	Reference
	RESULT_CONTENT

	TP/oneM2M/CSE/DMR/CRE/018_RCN/4
	TS-0004 [2], clause 6.3.4.2.7
	4 (attributes and child resources)

	TP/oneM2M/CSE/DMR/CRE/018_RCN/5
	
	5 (attributes and child resources references)

	TP/oneM2M/CSE/DMR/CRE/018_RCN/6
	
	6 (child resrouces references)

	TP/oneM2M/CSE/DMR/CRE/018_RCN/7
	
	7 (original resource)

	TP/oneM2M/CSE/DMR/CRE/018_RCN/8
	
	8 (child resources)



TP/oneM2M/CSE/DMR/CRE/019
	TP Id
	
	TP/oneM2M/CSE/DMR/CRE/019
	
	

	Test objective
	
	Check that the IUT returns successfully only attributes of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 1 (attributes)
	
	

	Reference
	
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7
	
	

	Config Id
	
	CF01
	
	

	Parent Release
	
	PARENT_RELEASE
	
	

	PICS Selection
	
	PICS_CSE
	
	

	Initial conditions
	with { / the IUT being in the "initial state"/ and the IUT having registered the AE/ and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE/ and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS/}
	
	
	

	Expected behaviour
	Test events
	
	
	Direction

	
	
	when { / the IUT receives a valid CREATE Request from AE containing/ To set to TARGET_RESOURCE_ADDRESS and/ From set to AE_ID and/ Result Content set to 1 (attributes)/ Contentcontaining/ RESOURCE_TYPE resource representation/}
	
	IUT <= AE

	
	
	
	then { / the IUT sends a valid Response containing/ Response Status Code set to 2001 (CREATED) and/ Content containing/ RESOURCE_TYPE resource containing/ attributes and/ no hierarchichal address and/ no child resources and/ no child resource references/}
	



	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/019_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/019_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/019_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/019_PCH
	Release 2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/019_SUB
	Release 2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/019_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/019_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/CRE/019_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/CRE/019_TRAC
	Release 4
	51 (transaction)



TP/oneM2M/CSE/DMR/CRE/020
	TP Id
	
	TP/oneM2M/CSE/DMR/CRE/020
	
	

	Test objective
	
	Check that the IUT returns successfully only modified attributes of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 9 (modified attributes)
	
	

	Reference
	
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7
	
	

	Config Id
	
	CF01
	
	

	Parent Release
	
	PARENT_RELEASE
	
	

	PICS Selection
	
	PICS_CSE
	
	

	Initial conditions
	with { / the IUT being in the "initial state"/ and the IUT having registered the AE/ and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE/ and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS/}
	
	
	

	Expected behaviour
	Test events
	
	
	Direction

	
	
	when { / the IUT receives a valid CREATE Request from AE containing/ To set to TARGET_RESOURCE_ADDRESS and/ From set to AE_ID and/ Result Content set to 1 (attributes)/ Contentcontaining/ RESOURCE_TYPE resource representation/}
	
	IUT <= AE

	
	
	
	then { / the IUT sends a valid Response containing/ Response Status Code set to 2001 (CREATED) and/ Content containing/ RESOURCE_TYPE resource containing/ modified attributes/}
	



	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/020_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/CRE/020_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/CRE/020_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/CRE/020_PCH
	Release 2
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/CRE/020_SUB
	Release 2
	23 (subscription)

	TP/oneM2M/CSE/DMR/CRE/020_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/CRE/020_TS
	Release 3
	29 (timeSeries)



TP/oneM2M/CSE/DMR/CRE/021
	TP Id
	TP/oneM2M/CSE/DMR/CRE/021

	Test objective
	Check that the IUT accepts the creation of a RESOURCE_TYPE resource on the TARGET_RESOURCE_ADDRESS of type announced PARENT_RESOURCE_TYPE

	Reference
	TS-0001 [1], clause 9.6.5

	Parent Release
	Release 3

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the CSE
and the IUT having created the PARENT_RESOURCE_TYPE
and the Originator having privileges to perform CREATE operation on the resource PARENT_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid CREATE Request from CSE containing  | |
                     | Resource Type set to RESOURCE_TYPE and  | |
                     |To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to CSE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | no resourceName attribute  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     |the IUT creates the RESOURCE_TYPE resource   | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | Valid resourceName attribute  | |
                     |} | |
+———————-+————————————————————————————————————————————-+————-+
	TP Id
	Reference
	RESOURCE_TYPE
	PARENT_RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/CRE/021_CNTA/AEA
	TS-0001 [1], clause 9.6.5-1
	(containerAnnc)
	(AEannc)

	TP/oneM2M/CSE/DMR/CRE/021_GRPA/AEA
	TS-0001 [1], clause 9.6.5-1
	(groupAnnc)
	(AEannc)

	TP/oneM2M/CSE/DMR/CRE/021_ACPA/AEA
	TS-0001 [1], clause 9.6.5-1
	(accessControlPolicyAnnc)
	(AEannc)

	TP/oneM2M/CSE/DMR/CRE/021_TSA/AEA
	TS-0001 [1], clause 9.6.5-1
	(timeSeriesAnnc)
	(AEannc)



TP/oneM2M/CSE/DMR/CRE/022
	/TP Id
	
	TP/oneM2M/CSE/DMR/CRE/022
	

	Test objective
	
	Check that the IUT accepts the creation of a RESOURCE_TYPE resource with the optional attribute announceTo provided
	

	Reference
	
	TS-0001 [1], clause 10.2.18.4 and clause 9.6.1.3.2-1, TS-0004 [2], clause 7.3.3.10
	

	Parent Release
	
	Release 3
	

	Config Id
	
	CF02
	

	PICS Selection
	
	PICS_CSE
	

	Initial conditions
	with { / the IUT being in the "initial state"/ and the IUT having registered the AE/ and the IUT having created and announced the PARENT_RESOURCE to the announcement target CSE/ and the AE having privileges to perform CREATE operation on the resource PARENT_RESOURCE_ADDRESS/}
	
	

	Expected behaviour
	Test events
	
	Direction

	
	when { / the IUT receives a valid CREATE Request from AE containing/ To set to PARENT_RESOURCE_ADDRESS and/ From set to AE-ID and/ Content containing/ RESOURCE_TYPE resource containing/ announceTo attribute set to ANNC_TARGET_CSE_ADDRESS/}
	
	IUT <= AE

	
	then {/ The IUT sends a valid CREATE Request containing/ To set to ANNC_TARGET_CSE_ADDRESS and/ Content containing/ RESOURCE_TYPE announced variant resourcecontaining/ MA (mandatory) attributes/}
	
	/IUT => CSE///



	TP Id
	RESOURCE_TYPE
	PICS

	TP/oneM2M/CSE/DMR/CRE/022_ACP
	1 (accesControlPolicy)
	PICS_IN_PROFILE

	TP/oneM2M/CSE/DMR/CRE/022_CNT
	3 (container)
	PICS_IN_PROFILE

	TP/oneM2M/CSE/DMR/CRE/022_CIN
	4 (contentInstance)
	PICS_IN_PROFILE

	TP/oneM2M/CSE/DMR/CRE/022_GRP
	9 (group)
	

	TP/oneM2M/CSE/DMR/CRE/022_LCP
	10 (locationPolicy)
	

	TP/oneM2M/CSE/DMR/CRE/022_MGO
	13 (mgmtObj)
	

	TP/oneM2M/CSE/DMR/CRE/022_NOD
	14 (node)
	

	TP/oneM2M/CSE/DMR/CRE/022_SCH
	18 (schedule)
	

	TP/oneM2M/CSE/DMR/CRE/022_TS
	29 (timeSeries)
	

	TP/oneM2M/CSE/DMR/CRE/022_TSI
	30 (timeSeriesInstance)
	



TP/oneM2M/CSE/DMR/CRE/023
	TP Id
	TP/oneM2M/CSE/DMR/CRE/023

	Test objective
	Check that the IUT accepts the creation of a RESOURCE_TYPE resource with the optional attribute announcedAttribute provided

	Reference
	TS-0001 [1], clause 10.2.18.4 and clause 9.6.1.3.2-1, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created and announced the PARENT_RESOURCE to the announcement target CSE
and the AE having privileges to perform CREATE operation on the resource PARENT_RESOURCE_ADDRESS
}

	Expected behaviour
	Test events
	Direction



·                  +------------------------------------------------------------------------------------+-----------------------------------------+

·                      |then {  |IUT => CSE |
                     |The IUT sends a valid CREATE Request containing  | |
                     |To set to ANNC_TARGET_CSE_ADDRESS and  | |
                     |Content containing  | |
                     |RESOURCE_TYPE announced variant resourcecontaining  | |
                     |MA (mandatory) attributes and  | |
                     |OA_ATTRIBUTE attribute set to VALUE  | |
                     |} | |
+———————-+————————————————————————————+—————————————–+
	TP Id
	RESOURCE_TYPE
	PICS

	TP/oneM2M/CSE/DMR/CRE/023_CNT
	3 (container)
	PICS_IN_PROFILE

	TP/oneM2M/CSE/DMR/CRE/023_CIN
	4 (contentInstance)
	PICS_IN_PROFILE

	TP/oneM2M/CSE/DMR/CRE/023_GRP
	9 (group)
	

	TP/oneM2M/CSE/DMR/CRE/023_LCP
	10 (locationPolicy)
	

	TP/oneM2M/CSE/DMR/CRE/023_MGO
	13 (mgmtObj)
	

	TP/oneM2M/CSE/DMR/CRE/023_NOD
	14 (node)
	

	TP/oneM2M/CSE/DMR/CRE/023_SCH
	18 (schedule)
	

	TP/oneM2M/CSE/DMR/CRE/023_TS
	29 (timeSeries)
	

	TP/oneM2M/CSE/DMR/CRE/023_TSI
	30 (timeSeriesInstance)
	




7.2.2.3.4	DELETE Operation
TP/oneM2M/CSE/DMR/DEL/001
	TP Id
	TP/oneM2M/CSE/DMR/DEL/001

	Test objective
	Check that the IUT accepts the deletion of a RESOURCE_TYPE resource

	Reference
	TS-0001 [1], clause 10.1.4

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------+---------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +-----------------------------------------------+---------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT deletes the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+———————————————–+———————————————————+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/001_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.4
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/001_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.4
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/001_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.5
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/001_CIN
	Release 1
	TS-0001 [1], clause 10.2.4.1
	4 (contentInstance)

	TP/oneM2M/CSE/DMR/DEL/001_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.5
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/001_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/001_PCH
	Release 2
	TS-0001 [1], clause 10.2.13.5
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/DEL/001_STCG
	Release 4
	TS-0001 [1], clause 10.2.15.5
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/DEL/001_TS
	Release 3
	TS-0001 [1], clause 10.2.30.4
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/001_TSI
	Release 3
	TS-0001 [1], clause 10.2.31.4
	30 (timeSeriesInstance)

	TP/oneM2M/CSE/DMR/DEL/001_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.5
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/001_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.9
	51 (transaction)




TP/oneM2M/CSE/DMR/DEL/002
	TP Id
	TP/oneM2M/CSE/DMR/DEL/002

	Test objective
	Check that the IUT responds with an error when the AE tries to delete the resource TARGET_RESOURCE_ADDRESS without having privileges for the DELETE operation

	Reference
	TS-0001 [1], clause 10.1.4

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having no privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not delete the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————–+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/002_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.4
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/002_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.4
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/002_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.5
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/002_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.5
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/002_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/002_TS
	Release 3
	TS-0001 [1], clause 10.2.30.4
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/002_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.5
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/002_TRAC
	Release 4
	TS-0001 [1], clause 10.2.18.9
	51 (transaction)



TP/oneM2M/CSE/DMR/DEL/003
	TP Id
	TP/oneM2M/CSE/DMR/DEL/003

	Test objective
	Check that the IUT responds with an error when the AE tries to delete the resource TARGET_RESOURCE_ADDRESS which does not exist

	Reference
	TS-0001 [1], clause 10.1.4

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having not yet created a resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not delete the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+——————————————————————————————————————–+————-+
TP/oneM2M/CSE/DMR/DEL/004
	TP Id
	TP/oneM2M/CSE/DMR/DEL/004

	Test objective
	Check that the IUT responds with an error when AE tries to delete a child resource of a RESOURCE_TYPE resource when this resource has been already deleted

	Reference
	TS-0001 [1], clause 10.1.4

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
and the AE having deleted the TARGET_RESOURCE_ADDRESS resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_CHILD_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     | } | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+————————————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/004_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.4
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/004_ACP
	Release 1
	TS-0001 [1], clause 10.2.21.4
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/004_SUB
	Release 1
	TS-0001 [1], clause 10.2.11.5
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/004_GRP
	Release 1
	TS-0001 [1], clause 10.2.7.5
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/004_SCH
	Release 3
	TS-0001 [1], clause 10.2.40.2
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/004_STCG
	Release 4
	TS-0001 [1], clause 10.2.15.5
	22 (statsConfig)

	TP/oneM2M/CSE/DMR/DEL/004_TS
	Release 3
	TS-0001 [1], clause 10.2.30.4
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/004_TRAM
	Release 4
	TS-0001 [1], clause 10.2.18.5
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/004_TRAC
	Release 4
	TS-0001 [1], clause 10.2.30.4
	51 (transaction)



TP/oneM2M/CSE/DMR/DEL/005
	TP Id
	TP/oneM2M/CSE/DMR/DEL/005

	Test objective
	Check that the stateTag attribute of a RESOURCE_TYPE resource is increased when a child resource is deleted

	Reference
	TS-0001 [1], clause 10.1.4

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a RESOURCE_TYPE resource containing
a child resource
and the AE having privileges to perform DELETE operation on the TARGET_CHILD_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_CHILD_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and   | |
                     |no Content  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT increments the stateTag attribute of the RESOURCE_TYPE resource   | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/005_CNT
	Release 1
	TS-0001 [1], clause 10.2.4.4
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/005_TS
	Release 3
	TS-0001 [1], clause 10.2.30.4
	29 (timeSeries)



TP/oneM2M/CSE/DMR/DEL/006
	TP Id
	TP/oneM2M/CSE/DMR/DEL/006

	Test objective
	Check that the IUT decreases the field value of attribute currentNrOfInstances and currentByteSize of parent RESOURCE_TYPE when a latest RESOURCE_TYPE resource is deleted successfully

	Reference
	TS-0001 [1], clause 10.2.19.5, TS-0004 [2], clause 7.4.8.2.4

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a _PARENT RESOURCE_TYPE resource containing
currentNrOfInstances attribute set to NR_OF_INSTANCES and
currentByteSize attribute set to BYTE_SIZE_OF_DATA and
a RESOURCE_TYPE resource TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT decreases the currentNrOfInstances attribute of _PARENT RESOURCE_TYPE resource  | |
                     | and the IUT decreases the currentByteSize attribute of _PARENT RESOURCE_TYPE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————–+————-+ Editor's Note: Need to clarify if needed to split into two separate test purposes.
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE
	PARENT_ RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/006_CNT/CIN
	Release 1
	TS-0001 [1], clause 10.2.4.4
	4 (contentInstance)
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/006_TS/TSI
	Release 3
	TS-0001 [1], clause 10.2.30.4
	30 (timeSeriesInstance)
	29 (timeSeries)



TP/oneM2M/CSE/DMR/DEL/007
	TP Id
	TP/oneM2M/CSE/DMR/DEL/007

	Test objective
	Check that the IUT accepts the DELETE Request of the latest contentInstance resource target to a container resource

	Reference
	TS-0001 [1], clause 10.2.22.2, TS-0004 [2], clause 7.4.28.2.5

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a container resource containing
CONTENT_INSTANCE_1 contentInstance resource and
CONTENT_INSTANCE_2 contentInstance resource
and the AE having privileges to perform DELETE operation on the container resource
and creationTime attribute of CONTENT_INSTANCE_1 < creationTime attribute of CONTENT_INSTANCE_2
}



·                  +------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/la and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT deletes the CONTENT_INSTANCE_2_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+——————————————————————————————————+————-+
TP/oneM2M/CSE/DMR/DEL/008
	TP Id
	TP/oneM2M/CSE/DMR/DEL/008

	Test objective
	Check that the IUT rejects the DELETE request of a latest resource in a container resource that has no direct child contentInstance resources

	Reference
	TS-0001 [1], clause 10.2.22.2, TS-0004 [2], clause 7.4.28.2.5

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource containing
no contentInstance resources
}



·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/la and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+———————————————————————————————————————————+————-+


TP/oneM2M/CSE/DMR/DEL/009
	TP Id
	TP/oneM2M/CSE/DMR/DEL/009

	Test objective
	Check that the IUT accepts the DELETE Request of the oldest contentInstance resource target to a container resource

	Reference
	TS-0001 [1], clause 10.2.23.2, TS-0004 [2], clause 7.4.29.2.5

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a container resource containing
CONTENT_INSTANCE_1 contentInstance resource and
CONTENT_INSTANCE_2 contentInstance resource
and the AE having privileges to perform DELETE operation on the container resource
and creationTime attribute of CONTENT_INSTANCE_1 < creationTime attribute of CONTENT_INSTANCE_2
}



·                  +------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT deletes the CONTENT_INSTANCE_1_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+——————————————————————————————————+————-+
TP/oneM2M/CSE/DMR/DEL/010
	TP Id
	TP/oneM2M/CSE/DMR/DEL/010

	Test objective
	Check that the IUT rejects the DELETE request of an oldest resource in a container resource that has no direct child contentInstance resources

	Reference
	TS-0001 [1], clause 10.2.23.2, TS-0004 [2], clause 7.4.29.2.5

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource containing
no contentInstance resources
}



·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS/ol and  | |
                     | From set to AE_ID and  | |
                     |no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+———————————————————————————————————————————-+————-+ TP/oneM2M/CSE/DMR/DEL/011
	TP Id
	TP/oneM2M/CSE/DMR/DEL/011

	Test objective
	Check that the IUT rejects a DELETE Request target to TARGET_ RESOURCE_ADDRESS resource when the Result Content set to RESULT_CONTENT

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to RESULT_CONTENT  | |
                     | no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+——————————————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	RESULT_CONTENT

	TP/oneM2M/CSE/DMR/DEL/011_RCN/2
	Release 2
	2 (hierarchical address)

	TP/oneM2M/CSE/DMR/DEL/011_RCN/3
	Release 2
	3 (attributes and hierarchichal address)

	TP/oneM2M/CSE/DMR/DEL/011_RCN/7
	Release 3
	7 (original resource)

	TP/oneM2M/CSE/DMR/DEL/011_RCN/9
	Release 2
	9 (modified attributes)



TP/oneM2M/CSE/DMR/DEL/012
	TP Id
	TP/oneM2M/CSE/DMR/DEL/012

	Test objective
	Check that the IUT returns nothing of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 0 (nothing)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--+---------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to 0 (nothing)  | |
                     | no Content  | |
                     |} | |
·                  +--+---------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED) and  | |
                     | no Content  | |
                     |} | |
+———————-+–+———————————————————————————————————+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/012_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/012_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/012_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/012_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/012_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/DEL/012_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/012_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/012_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/012_TRAC
	Release 4
	51 (transaction)



TP/oneM2M/CSE/DMR/DEL/013
	TP Id
	
	TP/oneM2M/CSE/DMR/DEL/013
	
	

	Test objective
	
	Check that the IUT returns successfully only attributes of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 1 (attributes)
	
	

	Reference
	
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.3.2.7
	
	

	Config Id
	
	CF01
	
	

	Parent Release
	
	PARENT_RELEASE
	
	

	PICS Selection
	
	PICS_CSE
	
	

	Initial conditions
	with { / the IUT being in the "initial state"/ and the IUT having registered the AE/ and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing/ a child resource/ and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS/}
	
	
	

	Expected behaviour
	Test events
	
	
	Direction

	
	
	when { / the IUT receives a valid DELETE Request from AE containing/ To set to TARGET_RESOURCE_ADDRESS and/ From set to AE_ID and/ Result Content set to 1 (attributes)/ no Content/}
	
	IUT <= AE

	
	
	
	then { / the IUT sends a valid Response containing/ Response Status Code set to 2002 (DELETED) and/ Content containing/ RESOURCE_TYPE resource containing/ attributes and/ no hierarchichal address and/ no child resources and/ no child resource references/}
	



	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/013_CNT
	Release 2
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/013_GRP
	Release 2
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/013_ACP
	Release 2
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/013_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/013_PCH
	Release 3
	15 (pollingChannel)

	TP/oneM2M/CSE/DMR/DEL/013_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/013_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/013_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/013_TRAC
	Release 4
	51 (transaction)



TP/oneM2M/CSE/DMR/DEL/014
	TP Id
	TP/oneM2M/CSE/DMR/DEL/014

	Test objective
	Check that the IUT returns successfully only attributes and child resources of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 4 (attributes and child resources)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to 4 (attributes and child resources)  | |
                     | no Content  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | attributes and  | |
                     | child resources  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/014_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/014_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/014_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/014_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/014_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/014_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/014_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/014_TRAC
	Release 4
	51 (transaction)



TP/oneM2M/CSE/DMR/DEL/015
	TP Id
	TP/oneM2M/CSE/DMR/DEL/015

	Test objective
	Check that the IUT returns successfully only attributes and child resources references of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 5(attributes and child resources references)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to 5 (attributes and child resources references)  | |
                     | no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | attributes and  | |
                     | child resource references  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/015_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/015_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/015_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/015_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/015_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/015_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/015_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/015_TRAC
	Release 4
	51 (transaction)



TP/oneM2M/CSE/DMR/DEL/016
	TP Id
	TP/oneM2M/CSE/DMR/DEL/016

	Test objective
	Check that the IUT returns successfully only child resources references of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 6(child resources references)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to 6 (child resources references)  | |
                     | no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED) and  | |
                     | Content containing  | |
                     | resourceRefList elementcontaining  | |
                     | child resource references  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/016_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/016_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/016_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/016_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/016_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/016_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/016_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/016_TRAC
	Release 4
	51 (transaction)



TP/oneM2M/CSE/DMR/DEL/017
	TP Id
	TP/oneM2M/CSE/DMR/DEL/017

	Test objective
	Check that the IUT returns successfully only child resources of TARGET_RESOURCE_ADDRESS resource when the Result Content is set to 8(child resources)

	Reference
	TS-0001 [1], clause 8.1.2, TS-0004 [2], clause 6.3.4.2.7

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type RESOURCE_TYPE containing
a child resource
and the AE having privileges to perform DELETE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Result Content set to 8 (child resources)  | |
                     | no Content  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED) and  | |
                     | Content containing  | |
                     |CHILD_RESOURCE_TYPE resource representation  | |
                     |  | |
                     |} | |
+———————-+——————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	RESOURCE_TYPE

	TP/oneM2M/CSE/DMR/DEL/017_CNT
	Release 3
	3 (container)

	TP/oneM2M/CSE/DMR/DEL/017_GRP
	Release 3
	9 (group)

	TP/oneM2M/CSE/DMR/DEL/017_ACP
	Release 3
	1 (accessControlPolicy)

	TP/oneM2M/CSE/DMR/DEL/017_SCH
	Release 3
	18 (schedule)

	TP/oneM2M/CSE/DMR/DEL/017_SUB
	Release 3
	23 (subscription)

	TP/oneM2M/CSE/DMR/DEL/017_TS
	Release 3
	29 (timeSeries)

	TP/oneM2M/CSE/DMR/DEL/017_TRAM
	Release 4
	50 (transactionMgmt)

	TP/oneM2M/CSE/DMR/DEL/017_TRAC
	Release 4
	51 (transaction)



7.2.2.3.5	BASIC Operation
TP/oneM2M/CSE/DMR/001
	TP Id
	TP/oneM2M/CSE/DMR/001

	Test objective
	Check that the IUT retargets the request to the hosting CSE when the To parameter contains the hosting CSE-ID which is known by the IUT (a descendant CSE or its Registrar CSE)

	Reference
	TS-0001 [1], clause 8.2.1.1

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered to a Hosting CSE
and the IUT having registered the AE
and the Hosting CSE containing
a resource representation on TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform OPERATION on the Hosting CSE
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from the AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | the IUT sends a OPERATION Request to the Hosting CSE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DMR/001_CRE
	CREATE

	TP/oneM2M/CSE/DMR/001_RET
	RETRIEVE

	TP/oneM2M/CSE/DMR/001_UPD
	UPDATE

	TP/oneM2M/CSE/DMR/001_DEL
	DELETE



TP/oneM2M/CSE/DMR/002
	TP Id
	TP/oneM2M/CSE/DMR/002

	Test objective
	Check that the IUT retargets the response from the hosting CSE after retargeting an OPERATION Request

	Reference
	TS-0001 [1], clause 8.2.1.1

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered to the Hosting CSE
and the IUT having registered the AE
and the Hosting CSE containing
a resource representation on TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform OPERATION on the Hosting CSE
and the IUT having received a valid OPERATION Request from the AE containing
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID
and the IUT sends the OPERATION Request to the Hosting CSE
}



·                  +----------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE |
                     | the IUT receives a valid OPERATION Response from the Hosting CSE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response to the AE  | |
                     |} | |
+———————-+—————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DMR/002_CRE
	CREATE

	TP/oneM2M/CSE/DMR/002_RET
	RETRIEVE

	TP/oneM2M/CSE/DMR/002_UPD
	UPDATE

	TP/oneM2M/CSE/DMR/002_DEL
	DELETE



7.2.2.4	Subscription and Notification (SUB)
7.2.2.4.1	CREATE Operation
TP/oneM2M/CSE/SUB/CRE/001
	TP Id
	TP/oneM2M/CSE/SUB/CRE/001

	Test objective
	Check that the IUT rejects the creation of the <subscription> resource when the target
subscribed-to RESOURCE_TYPE resource is not subscribable

	Reference
	TS-0001 [1], clause 10.2.11.2 & TS-0004 [2], clause 7.4.8.2.1

	Config Id
	CF01

	Parent Release
	PARENT_RELEASE

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE to perform CREATE operation
and the IUT having a resource PARENT_RESOURCE_ADDRESS not being
subscribable RESOURCE_TYPE resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     |subscription resource representation  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the subscription resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5203 (TARGET_NOT_SUBSCRIBABLE) and  | |
                     | no Content  | |
                     |} | |
+———————-+—————————————————————————————————————————————-+————-+
	TP Id
	PARENT_RELEASE
	Reference
	RESOURCE_TYPE

	TP/oneM2M/CSE/SUB/CRE/001_CIN
	Release 1
	TS-0001 [1], clause 9.6.7
	4 (contentInstance)

	TP/oneM2M/CSE/SUB/CRE/001_SUB
	Release 1
	TS-0001 [1], clause 9.6.8
	23 (subscription)

	TP/oneM2M/CSE/SUB/CRE/001_TSI
	Release 3
	TS-0001 [1], clause 9.6.37
	30 (timeSeriesInstance)



TP/oneM2M/CSE/SUB/CRE/002
	TP Id
	TP/oneM2M/CSE/SUB/CRE/002

	Test objective
	Check that the IUT rejects the creation of the <subscription> resource when the originator does
not have privileges for retrieving the subscribed-to resource

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.4.8.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a resource PARENT_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute pointing to
accessControlPolicy resource containing
privileges attribute containing
accessControlRule attribute containing
accessControlOriginators attribute indicating AE-IDand
accessControlOperations attribute not indicating RETRIEVE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     |subscription resource representation  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the subscription resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)and  | |
                     | no Content  | |
                     |} | |
+———————-+—————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/CRE/003
	TP Id
	TP/oneM2M/CSE/SUB/CRE/003

	Test objective
	Check that the IUT rejects the creation of the <subscription> resource when the notificationURI
is not the originator and the IUT cannot send the Notify request to the notificationURI

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.4.8.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE to perform CREATE operation
and the IUT not being able to send the NOTIFY Request to the NOTI_URI_ADDRESS containing verificationRequest set to TRUE
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | From set to AE‑ID and  | |
                     | Content containg  | |
                     | subscription resourcecontaining  | |
                     | notificationURI attribute set to NOTI_URI_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the subscription resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5204  | |
                     |(SUBSCRIPTION_VERIFICATION_INITIATION_FAILED)and  | |
                     | no Content  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/CRE/004
	TP Id
	TP/oneM2M/CSE/SUB/CRE/004

	Test objective
	Check that the IUT stores Originator ID in the notification creator attribute when a <SUBSCRIPTION>
creation request which needs verification is received and the notificationURI is not the Originator

	Reference
	TS-0001 [1], clause 10.2.12.1, TS-0004 [2], clause 7.4.9.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type>
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid CREATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESS and  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 23 (subscription) and  | |
                     | Content containing  | |
                     | subscription resourcecontaining  | |
                     | notificationURI attribute set to AE2_RESOURCE_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE2 |
                     | the IUT sends a valid NOTIFY Request containing  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | verificationRequest attribute set to TRUE and  | |
                     | creator attribute set to AE1_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/CRE/005
	TP Id
	TP/oneM2M/CSE/SUB/CRE/005

	Test objective
	Check that the IUT sends a Notify request to the subscriber resource when
notificationEventType attribute is set to "Create_of_Direct_Child_Resource" and a create
operation has been performed on the subscribed-to resource

	Reference
	TS-0001 [1], clause 9.6.8-3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 3 (Create_of_Direct_Child_Resource)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid CREATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | CHILD_RESOURCE_TYPE resource containing  | |
                     | resourceName attribute set to NAME   | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2001 (CREATED)  |IUT -> AE2  |
                     | and the IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | Notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | CHILD_RESOURCE_TYPE resourcecontaining  | |
                     | All attributes  | |
                     |} | |
+———————-+——————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/CRE/006
	TP Id
	TP/oneM2M/CSE/SUB/CRE/006

	Test objective
	Check that the IUT accepts the creation of a subscription resource with the
eventNotificationCriteria attribute which includes a CONDITION_TAG condition provided

	Reference
	TS-0001 [1], clause 9.6.8

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform CREATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | valid_CONDITION_TAG_ condition  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     |the IUT creates the subscription resource   | |
                     |and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————–+————-+
	TP Id
	Reference
	CONDITION_TAG

	TP/oneM2M/CSE/SUB/CRE/006_CRB
	TS-0001 [1], clause 9.6.8
	createdBefore

	TP/oneM2M/CSE/SUB/CRE/006_CRA
	TS-0001 [1], clause 9.6.8
	createdAfter

	TP/oneM2M/CSE/SUB/CRE/006_MS
	TS-0001 [1], clause 9.6.8
	modifiedSince

	TP/oneM2M/CSE/SUB/CRE/006_US
	TS-0001 [1], clause 9.6.8
	unmodifiedSince

	TP/oneM2M/CSE/SUB/CRE/006_STS
	TS-0001 [1], clause 9.6.8
	stateTagSmaller

	TP/oneM2M/CSE/SUB/CRE/006_STB
	TS-0001 [1], clause 9.6.8
	stateTagBigger

	TP/oneM2M/CSE/SUB/CRE/006_EXB
	TS-0001 [1], clause 9.6.8
	expireBefore

	TP/oneM2M/CSE/SUB/CRE/006_EXA
	TS-0001 [1], clause 9.6.8
	expireAfter

	TP/oneM2M/CSE/SUB/CRE/006_SZA
	TS-0001 [1], clause 9.6.8
	sizeAbove

	TP/oneM2M/CSE/SUB/CRE/006_SZB
	TS-0001 [1], clause 9.6.8
	sizeBelow

	TP/oneM2M/CSE/SUB/CRE/006_ET
	TS-0001 [1], clause 9.6.8
	eventType

	TP/oneM2M/CSE/SUB/CRE/006_OM
	TS-0001 [1], clause 9.6.8
	operationMonitor

	TP/oneM2M/CSE/SUB/CRE/006_ATR
	TS-0001 [1], clause 9.6.8
	attribute

	TP/oneM2M/CSE/SUB/CRE/006_ATR
	TS-0001 [1], clause 9.6.8
	attribute

	TP/oneM2M/CSE/SUB/CRE/006_CRT
	TS-0001 [1], clause 9.6.8
	childResourceType



TP/oneM2M/CSE/SUB/CRE/007
	TP Id
	TP/oneM2M/CSE/SUB/CRE/007

	Test objective
	Check that the IUT accepts the creation of a subscription resource with the eventNotificationCriteria attribute which includes a missingData condition provided

	Reference
	TS-0001 [1], clause 9.6.8, 9.6.36

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a TARGET_RESOURCE_ADDRESS of type <timeSeries >
and the Originator having privileges to perform CREATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | valid missingData condition  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT creates the subscription resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/CRE/008
	TP Id
	TP/oneM2M/CSE/SUB/CRE/008

	Test objective
	Check that the IUT accepts the creation of a subscription resource with the optional attributes
notificationForwardingURI and groupID provided

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.7.10, TS-0004 [2], clause 7.4.14.2.3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource as TARGET_RESOURCE_ADDRESS containing
members which are subscribable and
the Originatorhaving privileges to perform CREATE operation on <group> members
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | groupID_,_ notificationURI attribute, and  | |
                     | notificationForwardingURI attribute set   | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT creates the subscription resource on the <group> members containing  | |
                     | groupID, notificationURI attribute and  | |
                     | notificationForwardingURI attribute set identical to notificationURI  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+—————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/CRE/009
	TP Id
	TP/oneM2M/CSE/SUB/CRE/009

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to 6
(Trigger_Received_For_AE_Resource) in combination of NOTIFICATION_EVENT_TYPE

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to 6  | |
                     | (Trigger_Received_For_AE_Resource) and  | |
                     | NOTIFICATION_EVENT_TYPE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+————————————————————————————————————————————————————–+————-+
	TP Id
	NOTIFICATION_EVENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/009_NET/1
	1 (Update_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/009_NET/2
	2 (Delete_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/009_NET/3
	3 (Create_of_Direct_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/009_NET/4
	4 (Delete_of_Direct_Child_Resource )

	TP/oneM2M/CSE/SUB/CRE/009_NET/5
	5 (Retrieve_of_Container_Resource_With_No_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/009_NET/7
	7 (Blocking_Update)



TP/oneM2M/CSE/SUB/CRE/010
	TP Id
	TP/oneM2M/CSE/SUB/CRE/010

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to 7
(Blocking Update) in combination of NOTIFICATION_EVENT_TYPE

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to 7 (Blocking Update)  | |
                     | and NOTIFICATION_EVENT_TYPE  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+
	TP Id
	NOTIFICATION_EVENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/010_NET/1
	1 (Update_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/010_NET/2
	2 (Delete_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/010_NET/3
	3 (Create_of_Direct_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/010_NET/4
	4 (Delete_of_Direct_Child_Resource )

	TP/oneM2M/CSE/SUB/CRE/010_NET/5
	5 (Retrieve_of_Container_Resource_With_No_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/010_NET/6
	6 (Trigger_Received_For_AE_Resource)




TP/oneM2M/CSE/SUB/CRE/011
	TP Id
	TP/oneM2M/CSE/SUB/CRE/011

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to 6
(Trigger_Received_For_AE_Resource) and notificationContentType is set to
NOTIFICATION_CONTENT_TYPE

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to 6  | |
                     | (Trigger_Received_For_AE_Resource) and  | |
                     | notificationContentType attribute set to  | |
                     | NOTIFICATION_CONTENT_TYPE   | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+————-+
	TP Id
	NOTIFICATION_CONTENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/011_NCT/1
	1 (All Attributes)

	TP/oneM2M/CSE/SUB/CRE/011_NCT/2
	2 (Modified Attributes)

	TP/oneM2M/CSE/SUB/CRE/011_NCT/3
	3 (ResourceID)



TP/oneM2M/CSE/SUB/CRE/012
	TP Id
	TP/oneM2M/CSE/SUB/CRE/012

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to 7
(Blocking Update) and notificationContentType attribute set to NOTIFICATION_CONTENT_TYPE

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to 7 (Blocking Update)  | |
                     | and  | |
                     | notificationContentType attribute set to  | |
                     | NOTIFICATION_CONTENT_TYPE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————-+————-+
	TP Id
	NOTIFICATION_CONTENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/012_NCT/1
	1 (All attributes)

	TP/oneM2M/CSE/SUB/CRE/012_NCT/3
	3 (ResourceID)

	TP/oneM2M/CSE/SUB/CRE/012_NCT/4
	4 (Trigger Payload)



TP/oneM2M/CSE/SUB/CRE/013
	TP Id
	TP/oneM2M/CSE/SUB/CRE/013

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to
NOTIFICATION_EVENT_TYPE and notificationContentType set to 4 (Trigger Payload)

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to  | |
                     | NOTIFICATION_EVENT_TYPE and  | |
                     | notificationContentType attribute set to 4 (Trigger Payload)  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+———————————————————————————————————————————————————-+————-+
	TP Id
	NOTIFICATION_EVENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/013_NET/1
	1 (Update_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/013_NET/2
	2 (Delete_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/013_NET/3
	3 (Create_of_Direct_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/013_NET/4
	4 (Delete_of_Direct_Child_Resource )

	TP/oneM2M/CSE/SUB/CRE/013_NET/5
	5 (Retrieve_of_Container_Resource_With_No_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/013_NET/7
	7 (Blocking_Update)



TP/oneM2M/CSE/SUB/CRE/014
	TP Id
	TP/oneM2M/CSE/SUB/CRE/014

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to
NOTIFICATION_EVENT_TYPE and notificationContentType set to 2(modified attributes)

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving** privileges to perform CREATE operation on TARGET_RESOURCE_ADDRESS resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to  | |
                     | NOTIFICATION_EVENT_TYPE and  | |
                     | notificationContentType attribute set to 2 (Modified Attributes)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+————————————————————————————————————————————————————-+————-+
	TP Id
	NOTIFICATION_EVENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/014_NET/2
	2 (Delete_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/014_NET/3
	3 (Create_of_Direct_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/014_NET/4
	4 (Delete_of_Direct_Child_Resource )

	TP/oneM2M/CSE/SUB/CRE/014_NET/5
	5 (Retrieve_of_Container_Resource_With_No_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/014_NET/6
	6 (Trigger_Received_For_AE_Resource)



TP/oneM2M/CSE/SUB/CRE/015
	TP Id
	TP/oneM2M/CSE/SUB/CRE/015

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to
NOTIFICATION_EVENT_TYPE and notificationContentType set to 3 (ResourceID)

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving** privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to  | |
                     | NOTIFICATION_EVENT_TYPE and  | |
                     | notificationContentType attribute set to 3 (ResourceID)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+—————————————————————————————————————————————————–+————-+
	TP Id
	NOTIFICATION_EVENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/015_NET/6
	6 (Trigger_Received_For_AE_Resource)

	TP/oneM2M/CSE/SUB/CRE/015_NET/7
	7 (Blocking_Update )

	TP/oneM2M/CSE/SUB/CRE/015_NET/8
	8 (Report_on_missing_data_points)



TP/oneM2M/CSE/SUB/CRE/016
	TP Id
	TP/oneM2M/CSE/SUB/CRE/016

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to
NOTIFICATION_EVENT_TYPE and notificationContentType set to 5 (TimeSeries notification)

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is subscribable and
the Originatorhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to  | |
                     | NOTIFICATION_EVENT_TYPE and  | |
                     | notificationContentType attribute set to 5 (TimeSeries notification)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————+————-+
	TP Id
	NOTIFICATION_EVENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/016_NET/1
	1 (Update_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/016_NET/2
	2 (Delete_of_Resource)

	TP/oneM2M/CSE/SUB/CRE/016_NET/3
	3 (Create_of_Direct_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/016_NET/4
	4 (Delete_of_Direct_Child_Resource )

	TP/oneM2M/CSE/SUB/CRE/016_NET/5
	5 (Retrieve_of_Container_Resource_With_No_Child_Resource)

	TP/oneM2M/CSE/SUB/CRE/016_NET/6
	6 (Trigger_Received_For_AE_Resource)

	TP/oneM2M/CSE/SUB/CRE/016_NET/7
	7 (Blocking_Update )



TP/oneM2M/CSE/SUB/CRE/017
	TP Id
	TP/oneM2M/CSE/SUB/CRE/017

	Test objective
	Check that the IUT rejects a CREATE request when the notificationEventType is set to
NOTIFICATION_EVENT_TYPE and notificationContentType set to 1 (All Attributes)

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.10.2, TS-0004 [2], clause 7.4.8.2.1, 6.3.4.2.18-19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource as TARGET_RESOURCE_ADDRESS which is
subscribable and
the Originatorhaving** privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to subscription and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to  | |
                     | NOTIFICATION_EVENT_TYPE and  | |
                     | notificationContentType attribute set to 1 (All Attributes)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST) and  | |
                     | no Content  | |
                     |} | |
+———————-+———————————————————————————————————————————————————+————-+
	TP Id
	NOTIFICATION_EVENT_TYPE

	TP/oneM2M/CSE/SUB/CRE/017_NET/6
	6 (Trigger_Received_For_AE_Resource)

	TP/oneM2M/CSE/SUB/CRE/017_NET/7
	7 (Blocking_Update )

	TP/oneM2M/CSE/SUB/CRE/017_NET/8
	8 (Report_on_missing_data_points)



7.2.2.4.2	DELETE Operation
TP/oneM2M/CSE/SUB/DEL/001
	TP Id
	TP/oneM2M/CSE/SUB/DEL/001

	Test objective
	Check that the IUT sends a Notify request to the AE2_RESOURCE_ADDRESS of the subscriberURI
attribute when the SUBSCRIPTION_RESOURCE_ADDRESS <subscription> resource is deleted

	Reference
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.5.1.2.4

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
subscription resource containing
subscriberURI attribute set to AE2_RESOURCE_ADDRESS
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid DELETE Request from AE1 containing  | |
                     | To set to SUBSCRIPTION_RESOURCE_ADDRESS and  | |
                     | From set to AE1_RESOURCE_ADDRESS  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2002 (DELETED)  |IUT -> AE2 |
                     | and the IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | subscriptionDeletion attribute set to TRUE and  | |
                     | subscriptionReference attribute set to  | |
                     |AE2_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/DEL/002
	TP Id
	TP/oneM2M/CSE/SUB/DEL/002

	Test objective
	Check that the IUT sends a Notify request to the subscriber resource when
eventNotificationCriteria/notificationEventType attribute is set to "Delete_of_Resource" and an delete
operation has been performed the subscribed-to resource

	Reference
	TS-0001 [1], clause 9.6.8-3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 2 (Delete_of_Resource)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid DELETE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2002 (DELETED)  |IUT -> AE2 |
                     | and the IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | a valid representation attribute  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/DEL/003
	TP Id
	TP/oneM2M/CSE/SUB/DEL/003

	Test objective
	Check that the IUT sends a Notify request to the subscriber resource when
eventNotificationCriteria/notificationEventType attribute is set to "Delete_of_Direct_Child_Resource"
and an delete operation has been performed on a child resource of the subscribed-to resource

	Reference
	TS-0001 [1], clause 9.6.8-3

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
a CHILD_RESOURCE_ADDRESS child resource and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 4 (Delete_of_Direct_Child_Resource)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid DELETE Request from AE1 containing  | |
                     | To set to CHILD_RESOURCE_ADDRESS and  | |
                     | From set to AE1_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2002 (DELETED)  |IUT -> AE2 |
                     | and the IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | CHILD_RESOURCE_TYPE resource  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————————–+————-+
7.2.2.4.3	UPDATE Operation
TP/oneM2M/CSE/SUB/UPD/001
	TP Id
	TP/oneM2M/CSE/SUB/UPD/001

	Test objective
	Check that the IUT sends Notify request to the subscriber resource when an update operation
has been performed on the subscribed-to resource

	Reference
	TS-0001 [1], clause 10.2.11.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to
resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME set to VALUE_2  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2004 (UPDATED)  |IUT -> AE2  |
                     | and the IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | All attributes  | |
                     |} | |
+———————-+——————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SUB/UPD/002
	TP Id
	TP/oneM2M/CSE/SUB/UPD/002

	Test objective
	Check that the IUT sends a Notify request to the subscriber resource when the
notificationContentType attribute is set to "modified attributes" and an update operation has been
performed on the subscribed-to resource

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESSand
notificationContentType attribute set to 2 (modified attributes)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2004 (UPDATED)  |IUT -> AE2 |
                     | and the IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/UPD/003
	TP Id
	TP/oneM2M/CSE/SUB/UPD/003

	Test objective
	Check that the IUT sends a Notify request to the subscriber resource when the
notificationContentType attribute is set to "ResourceID" and an update operation has been performed
on the subscribed-to resource

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
notificationContentType attribute set to 3 (ResourceID)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | < subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2004 (UPDATED)  |IUT -> AE2 |
                     | and the IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | subscribed‑to ResourceID  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/UPD/004
	TP Id
	TP/oneM2M/CSE/SUB/UPD/004

	Test objective
	Check that the IUT decreases the expirationCounter attribute of a subscription resource when the
Hosting CSE of the subscribed-to resource successfully sends the notification request to subscriber
resource(s)

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
expirationCounter attribute set to MAX_NUMBER_NOTIFICATION
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESS a nd  | |
                     | From set to AE1_RESOURCE_ADDRESSand  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT decrease s the expirationCounter attribute of the subscription resource  |  |
                     | and the IUT sends a valid Response containing  |IUT -> AE2 |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | and the IUT sends a NOTIFY Request  | |
                     |  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/UPD/005
	TP Id
	TP/oneM2M/CSE/SUB/UPD/005

	Test objective
	Check that the IUT deletes the subscription resource when the the expirationCounter meets zero

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
expirationCounter attribute set to 1
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +---------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESSand  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT decrease s the expirationCounter attribute of the subscription resource |  |
                     | and the IUT deletes the subscription resource  |IUT -> AE2 |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | and the IUT sends a NOTIFY Request  | |
                     |} | |
+———————-+———————————————————————————————+————-+
TP/oneM2M/CSE/SUB/UPD/006
	TP Id
	TP/oneM2M/CSE/SUB/UPD/006

	Test objective
	Check that the IUT doesn't send a Notify request to the subscriber resource when the "attribute"
condition tag of eventNotificationCriteria attribute is set to LIST_OF_ATTRIBUTE and doesn't contain
the ATTRIBUTE_NAME attribute updated

	Reference
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
attribute condition tag set to LIST_OF_ATTRIBUTE containing
no ATTRIBUTE_NAME attribute
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESSand  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | and the IUT does not send a NOTIFY Request  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/UPD/007
	TP Id
	TP/oneM2M/CSE/SUB/UPD/007

	Test objective
	Check that the IUT sends batched notifications to the subscriber resource when the number value of
the batchNotify attribute is set to NUMBER and when this number have been reached

	Reference
	TS-0001 [1], clause 10.2.12.1

	Config Id
	CF01

	Parent release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource having
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
batchNotify attribute containing
number attribute set to NUMBERand
duration attribute set to TIME_LIMIT
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
and the IUT having received (NUMBER- 1) valid UPDATE Requests from
AE1_RESOURCE_ADDRESS to subscribed-to resource
and the timer has not reached the TIME_LIMIT duration value
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+---------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | a valid ATTRIBUTE_NAME attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+---------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2004 (UPDATED)  |IUT -> AE2 |
                     | and the IUT sends NUMBER times a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | a valid notificationEvent attribute  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————+—————+
TP/oneM2M/CSE/SUB/UPD/008
	TP Id
	TP/oneM2M/CSE/SUB/UPD/008

	Test objective
	Check that the IUT sends the latest notification to the subscriber resource when latestNotify is set to
TRUE, the number value of the batchNotify attribute is set to NUMBER and when this number has
been reached

	Reference
	TS-0001 [1], clause 10.2.12.1

	Config Id
	CF01

	Parent release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource having
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
latestNotify attribute set to TRUE and
batchNotify attribute containing
number attribute set to NUMBERand
duration attribute set to TIME_LIMIT
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
and the IUT having received (NUMBER- 1) valid UPDATE Requests from
AE1_RESOURCE_ADDRESS to subscribed-to resource
and the timer has not reached the TIME_LIMIT duration value
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESSand  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | a valid ATTRIBUTE_NAME attribute  | |
                     | } | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2004 (UPDATED)  |IUT -> AE2  |
                     | and the IUT sends a NOTIFY Request contaning  |  |
                     | Content containing  | |
                     | the latest notification message containing  | |
                     | a valid notificationEvent attribute  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/UPD/009
	TP Id
	TP/oneM2M/CSE/SUB/UPD/009

	Test objective
	Check that the IUT sends a Notify request to the subscriber resource when the "attribute" condition
tag of eventNotificationCriteria attribute is set to ATTRIBUTE_NAME and an update operation has
been performed on the subscribed-to resource

	Reference
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
attribute condition tag set to ATTRIBUTE_NAME
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_2  | |
                     | } | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2004 (UPDATED)  |IUT -> AE2  |
                     | and the IUT sends a NOTIFY Request contaning  |  |
                     | Content containing  |  |
                     | notification message containing  |  |
                     | notificationEvent attribute containing  |  |
                     | representation attribute containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | All attributes  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————+————-+
7.2.2.4.4	NOTIFY Operation
TP/oneM2M/CSE/SUB/NTF/001
	TP Id
	TP/oneM2M/CSE/SUB/NTF/001

	Test objective
	Check that the IUT rejects the creation of the < subscription_>_ resource when the notificationURI
is not the originator and the IUT have received the Notify response containing Response Status
Code indicating SUBSCRIPTION_CREATOR_HAS_NO_PRIVILEGE

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.4.8.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE to perform CREATE operation
and notificationURI not being the originator
and the IUT having sent the NOTIFY Request to the NOTI_URI_ADDRESS containing
verificationRequest set to TRUE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Codeset to 4101  | |
                     |(SUBSCRIPTION_CREATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the subscription resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4101  | |
                     |(SUBSCRIPTION_CREATOR_HAS_NO_PRIVILEGE)and  | |
                     | no Content  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/002
	TP Id
	TP/oneM2M/CSE/SUB/NTF/002

	Test objective
	Check that the IUT rejects the creation of the < subscription_>_ resource when the notificationURI
is not the originator and the IUT have received the Notify response containing Response Status
Code indicating SUBSCRIPTION_HOST_HAS_NO_PRIVILEGE

	Reference
	TS-0001 [1], clause 10.2.11.2, TS-0004 [2], clause 7.4.8.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE to perform CREATE operation
and notificationURI not being the originator
and the IUT having sent the NOTIFY Request to the NOTI_URI_ADDRESS containing
verificationRequest set to TRUE
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 5205  | |
                     |(SUBSCRIPTION_HOST_HAS_NO_PRIVILEGE)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the subscription resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5205  | |
                     |(SUBSCRIPTION_HOST_HAS_NO_PRIVILEGE)and  | |
                     | no Content  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/003
	TP Id
	TP/oneM2M/CSE/SUB/NTF/003

	Test objective
	Check that the IUT sends batched notifications to the subscriber resource when the duration value of
the batchNotify attribute is set to TIME_LIMIT and when this timer expires

	Reference
	TS-0001 10.2.12.1

	Config Id
	CF01

	Parent release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME attribute set to VALUE_1 and
subscription child resource having
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
batchNotify attribute containing

duration attrinbute set to TIME_LIMIT
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
and the IUT having received a valid UPDATE Request from AE1_RESOURCE_ADDRESS to
subscribed-to resource
and timer has not reached TIME_LIMIT
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the timer expires after the TIME_LIMIT duration value  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE2 |
                     | The IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | a valid notificationEvent attribute  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SUB/NTF/004
	TP Id
	TP/oneM2M/CSE/SUB/NTF/004

	Test objective
	Check that the IUT sends the latest notification to the subscriber resource when latestNotify is set to
TRUE, the duration value of the batchNotify attribute is set to TIME_LIMIT and when this timer
expires

	Reference
	TS-0001 [1], clause 10.2.12.1

	Config Id
	CF01

	Parent release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1and
subscription child resource having
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
latestNotify attribute set to TRUE and
batchNotify attribute containing

duration attribute set to TIME_LIMIT
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
and the IUT having received a valid UPDATE Request from AE1_RESOURCE_ADDRESS to
subscribed-to resource
and timer has not reached TIME_LIMIT
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the timer expires after the TIME_LIMIT duration value  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE2 |
                     | The IUT sends a NOTIFY Request contaning  | |
                     | Content containing  | |
                     | the latest notification message containing  | |
                     | a valid notificationEvent attribute   | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/005
	TP Id
	TP/oneM2M/CSE/SUB/NTF/005

	Test objective
	Check that the IUT sends the latest cached notification after IUT escapes from connectionless
state when the pendingNotification is set to 1 (sendLatest)

	Reference
	TS-0001 [1], clause 9.6.8

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
pendingNotification attribute set to 1 (sendLatest)
and the AE2 having privileges to perform RETRIEVE operation on the subscribed-to resource
and the IUT being in the "connectionless state" with AE2
and the IUT having frequently received from AE1 a valid UPDATE Requests to subscribed-to
resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT escapes from the "connectionless state"  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE2 |
                     | The IUT sends a valid NOTIFY Request contaning  | |
                     | Content containing  | |
                     | the latest notification message  | |
                     |} | |
+———————-+——————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/006
	TP Id
	TP/oneM2M/CSE/SUB/NTF/006

	Test objective
	Check that the IUT sends the notifications of cached notification messages after IUT escapes
from connectionless state when the pendingNotification is set to 2 (sendAllPending)

	Reference
	TS-0001 [1], clause 9.6.8

	Config Id
	CF01

	Parent release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
subscription child resource having
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
pendingNotification attribute set to 2 (sendAllPending)
and the AE2 having privileges to perform RETRIEVE operation on the subscribed-to resource
and the IUT being in the "connectionless state" with AE2
and the IUT having received from AE1 a NUMBER of valid UPDATE Requests to subscribed-
to resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT escapes from the "connectionless state"  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE2 |
                     | The IUT sends NUMBER times a valid NOTIFY Request contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | a valid notificationEvent attribute  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/007
	TP Id
	TP/oneM2M/CSE/SUB/NTF/007

	Test objective
	Check that the IUT retargets the notification to the AE according to pointOfAccess in the <AE> resource

	Reference
	TS-0001 [1], clause 9.6.5 and clause 9.3.2.3.1 TS-0004 [2], clause 7.3.3.9

	Config Id
	CF02

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUThaving created the AE resource containing
POINT_OF_ACCESS attribute and
REQUEST_REACHABILITYset to true
}



·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- CSE |
                     | the IUT receives a valid NOTIFY from CSE containing  | |
                     | To set to AE_RESOURCE_ADDRESS  | |
                     | From set to CSE_ID   | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends the valid NOTIFY to POINT_OF_ACCESS  | |
                     |} | |
+———————-+———————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/008
	TP Id
	TP/oneM2M/CSE/SUB/NTF/008

	Test objective
	Check that the IUT retargets the notification to the AE according to pointOfAccess in the <AE>
resource and forward the response back to the CSE

	Reference
	TS-0001 [1], clause 9.6.5 and clause 9.3.2.3.1, TS-0004 [2], clause 7.3.3.9

	Config Id
	CF02

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having received a valid NOTIFY from CSE and
The IUT having sent the NOTIFY to the AE
}



·                                                         +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                                                             |when {   |IUT <- AE |
                                                            | the IUT receives a valid NOTIFY RESPONSE from the AE  | |
                                                            |} | |
·                                                         +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                                                             |then {   |IUT -> CSE |
                                                            | the IUT sends the valid NOTIFY RESPONSE to the CSE  | |
                                                            |} | |
+————————————————————-+————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/009
	TP Id
	TP/oneM2M/CSE/SUB/NTF/009

	Test objective
	Check that the IUT sends an aggregatedNotification to the AE according to URI provided in
notificationForwardingURI attribute when an event occurs on <group> resource with its members
having group related subscriptions

	Reference
	TS-0001 [1], clause 9.6.8 and clause 10.2.7.11, TS-0004 [2], clause 7.5.1.2.6

	Config Id
	CF02

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
and the IUT having a <group> resource with members allowing
the AE to perform required operation and <subscription> created on these members with
notificationForwardingURI attribute set identical to notificationURI
}



·                                                            +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                                                                |when {   |NA |
                                                               | the IUT receives a single notifications containing notificationForwardingURI, it  | |
                                                               |forms an aggregatedNotification   | |
                                                               |} | |
·                                                            +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                                                                |then {   |IUT -> AE |
                                                               | the IUT sends the Notify request containing  | |
                                                               | aggregatedNotification message representation to the AE  | |
                                                               |} | |
+—————————————————————-+——————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/010
	TP Id
	TP/oneM2M/CSE/SUB/NTF/010

	Test objective
	Check that the IUT doesn't send a Notify request to the subscriber resource when
"childResourceType" condition tag of eventNotificationCriteria attribute is set to
LIST_OF_RESOURCE_TYPE and this list doesn't contain the CHILD_RESOURCE_TYPE created in
the request

	Reference
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.4.8, 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having created a subscription resource on
SUBSCRIBED_TO_RESOURCE_ADDRESS resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType element set to 3 (Create_of_Direct_Child_Resource) and
childResourceType element set to LIST_OF_RESOURCE_TYPE
and AE1 having create privileges SUBSCRIBED_TO_RESOURCE_ADDRESS resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid CREATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_IDand  | |
                     | Content containing  | |
                     | CHILD_RESOURCE_TYPE resource representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     | and the IUT does not send a NOTIFY Request to  | |
                     |AE2_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/011
	TP Id
	TP/oneM2M/CSE/SUB/NTF/011

	Test objective
	Check that the IUT sends a Notify request to the subscriber resource when "childResourceType"
condition tag of eventNotificationCriteria attribute is set to LIST_OF_RESOURCE_TYPE and this list
contains the CHILD_RESOURCE_TYPE created in the request

	Reference
	TS-0001 [1], clause 9.6.8, TS-0004 [2], clause 7.4.8, 7.5.1.2.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having created a subscription resource on
SUBSCRIBED_TO_RESOURCE_ADDRESS resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType element set to 3 (Create_of_Direct_Child_Resource) and
childResourceType element set to LIST_OF_RESOURCE_TYPE
and AE1 having create privileges SUBSCRIBED_TO_RESOURCE_ADDRESS resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid CREATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_ID and  | |
                     | Content containing  | |
                     | CHILD_RESOURCE_TYPE resource representation  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response containing  |IUT -> AE2 |
                     | Response Status Code set to 2001 (CREATED)  | |
                     | and the IUT sends a NOTIFY Request to AE2_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/012
	TP Id
	TP/oneM2M/CSE/SUB/NTF/012

	Test objective
	Check that the IUT successfully sends a cross-resource notification to the notificationURI when
notifications from resources in regularResourcesAsTarget are received within required TIME_LIMIT
window

	Reference
	TS-0001 [1], clause 9.6.58, TS-0004 [2], clause 7.5.1.2.18

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1 containing
a container resource on CONTAINER_RESOURCE_ADDRESS_1
a container resource on CONTAINER_RESOURCE_ADDRESS_2
and the IUThaving created a <crossResourceSubsription> resource on
CROSS_RESOURCE_SUBS_ADDRESS containing
regularResourcesAsTarget attribute containing
CONTAINER_RESOURCE_ADDRESS_1 and
CONTAINER_RESOURCE_ADDRESS_2 and
timeWindowType attribute set to TIME_WINDOW_TYPE and
timeWindowSize attribute set to DURATION and
notificationURI attribute set to AE2_RESOURCE_ADDRESS
and the IUT having registered the AE2
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |  |
                     | the IUT receives a valid UPDATE Request (Req1) from AE1contaning  |IUT <- AE1  |
                     | To set to CONTAINER_RESOURCE_ADDRESS_1 and  |  |
                     | From set to AE_ID and  |  |
                     | Content containing  |  |
                     | container resource containing  |  |
                     | valid labels attribute  |  |
                     | and the IUT receives a valid UPDATE Request (Req2) from AE1contaning  |IUT <- AE1 |
                     | To set to CONTAINER_RESOURCE_ADDRESS_2 and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid labels attribute  | |
                     | and timer has not reached TIME_LIMIT  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response to AE1 for Req1  |IUT -> AE1  |
                     | and the IUT sends a valid Response to AE1 for Req2  |IUT -> AE1  |
                     | and the IUT sends a NOTIFY Request to AE2 generated from  |IUT -> AE2 |
                     | crossResourceSubsription on CROSS_RESOURCE_SUBS_ADDRESS  | |
                     | containing  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | subscriptionReference attribute set to  | |
                     | CROSS_RESOURCE_SUBS_ADDRESS  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————-+————-+
	TP Id
	TIME_WINDOW_TYPE

	TP/oneM2M/CSE/SUB/NTF/012_TWT/1
	1 (PERIODICWINDOW)

	TP/oneM2M/CSE/SUB/NTF/012_TWT/2
	2 (SLIDINGWINDOW)



TP/oneM2M/CSE/SUB/NTF/013
	TP Id
	TP/oneM2M/CSE/SUB/NTF/013

	Test objective
	Check that the IUT does not send a cross-resource notification to the notificationURI when a
notification from resource in regularResourcesAsTarget is not received within required TIME_LIMIT
window

	Reference
	TS-0001 [1], clause 9.6.58, TS-0004 [2], clause 7.5.1.2.18

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1 containing
a container resource on CONTAINER_RESOURCE_ADDRESS_1
a container resource on CONTAINER_RESOURCE_ADDRESS_2
and the IUThaving created a <crossResourceSubsription> resource on
CROSS_RESOURCE_SUBS_ADDRESS containing
regularResourcesAsTarget attribute containing
CONTAINER_RESOURCE_ADDRESS_1 and
CONTAINER_RESOURCE_ADDRESS_2 and
timeWindowType attribute set to TIME_WINDOW_TYPE and
timeWindowSize attribute set to DURATION and
notificationURI attribute set to AE2_RESOURCE_ADDRESS
and the IUT having registered the AE2
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |  |
                     | the IUT receives a valid UPDATE Request (Req1) from AE1contaning  |IUT <- AE1  |
                     | To set to CONTAINER_RESOURCE_ADDRESS_1 and  |  |
                     | From set to AE_ID and  |  |
                     | Content containing  |  |
                     | container resource containing  |  |
                     | valid labels attribute  |  |
                     | and the IUT receives a valid UPDATE Request (Req2) from AE1contaning  |IUT <- AE1 |
                     | To set to CONTAINER_RESOURCE_ADDRESS_2 and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid labels attribute  | |
                     | and timer has reached TIME_LIMIT  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE1  |
                     | the IUT sends a valid Response to AE1 for Req1  |IUT -> AE1  |
                     | and the IUT sends a valid Response to AE1 for Req2  | |
                     | and the IUT does not send a NOTIFY Request to AE2  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————–+————-+
	TP Id
	TIME_WINDOW_TYPE

	TP/oneM2M/CSE/SUB/NTF/013_TWT/1
	1 (PERIODICWINDOW)

	TP/oneM2M/CSE/SUB/NTF/013_TWT/2
	2 (SLIDINGWINDOW)



TP/oneM2M/CSE/SUB/NTF/014
	TP Id
	TP/oneM2M/CSE/SUB/NTF/014

	Test objective
	Check that the IUT sends a cross-resource notification to the notificationURI when notifications from
resources in regularResourcesAsTarget are received within required TIME_LIMIT window having
different NOTIFICATION_EVENT_TYPE values for each of the target resources

	Reference
	TS-0001 [1], clause 9.6.58, TS-0004 [2], clause 7.5.1.2.18

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1 containing
a container resource on CONTAINER_RESOURCE_ADDRESS_1
a container resource on CONTAINER_RESOURCE_ADDRESS_2
and the IUThaving created a <crossResourceSubsription> resource on
CROSS_RESOURCE_SUBS_ADDRESS containing
regularResourcesAsTarget attribute containing
CONTAINER_RESOURCE_ADDRESS_1 and
CONTAINER_RESOURCE_ADDRESS_2 and
timeWindowType attribute set to TIME_WINDOW_TYPE and
timeWindowSize attribute set to DURATION and
eventNotificationCriteriaSet containing
EVENT_NOTIFICATION_CRITERIA_1 set to 1 (Update_of_resource) and
EVENT_NOTIFICATION_CRITERIA_2 set to 3 (Create_of_Direct_Child_Resource)
and notificationURI attribute set to AE2_RESOURCE_ADDRESS
and the IUT having registered the AE2
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |  |  |
                     |when {  |  |
                     | the IUT receives a valid UPDATE Request (Req1) from AE1contaning  |IUT <- AE1  |
                     | To set to CONTAINER_RESOURCE_ADDRESS_1 and  |  |
                     | From set to AE_ID and  |  |
                     | Content containing  |  |
                     | container resource containing  |  |
                     | valid labels attribute  |  |
                     | and the IUT receives a valid CREATE Request (Req2) from AE1contaning  |IUT <- AE1 |
                     | To set to CONTAINER_RESOURCE_ADDRESS_2 and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | a valid container resource representation  | |
                     | and timer has not reached TIME_LIMIT  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response to AE1 for Req1  |IUT -> AE1  |
                     | and the IUT sends a valid Response to AE1 for Req2  |IUT -> AE1  |
                     | and the IUT sends a NOTIFY Request to AE2 generated from  |IUT -> AE2 |
                     | crossResourceSubscription CROSS_RESOURCE_SUBS_ADDRESS  | |
                     | containing  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | subscriptionReference attribute set to CROSS_SUBS_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	TIME_WINDOW_TYPE

	TP/oneM2M/CSE/SUB/NTF/014_TWT/1
	1 (PERIODICWINDOW)

	TP/oneM2M/CSE/SUB/NTF/014_TWT/2
	2 (SLIDINGWINDOW)



TP/oneM2M/CSE/SUB/NTF/015
	TP Id
	TP/oneM2M/CSE/SUB/NTF/015

	Test objective
	Check that the IUT successfully sends a cross-resource notification to the notificationURI when
notifications from resources in subscriptionResourcesAsTarget are received within required
TIME_LIMIT window

	Reference
	TS-0001 [1], clause 9.6.58, TS-0004 [2], clause 7.5.1.2.18

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1 containing
a container resource on CONTAINER_RESOURCE_ADDRESS_1 containing
a subscription resource on SUBS_RESOURCE_ADDRESS_1
a container resource on CONTAINER_RESOURCE_ADDRESS_2 containing
a subscription resource on SUBS_RESOURCE_ADDRESS_2
and the IUThaving created a <crossResourceSubscription> resource on
CROSS_RESOURCE_SUBS_ADDRESS containing
subscriptionResourcesAsTarget attribute containing
SUBS _RESOURCE_ADDRESS_1 and
SUBS _RESOURCE_ADDRESS_2 and
timeWindowType attribute set to TIME_WINDOW_TYPE and
timeWindowSize attribute set to DURATION and
notificationURI attribute set to AE2_RESOURCE_ADDRESS
and the IUT having registered the AE2
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |  |
                     | the IUT receives a valid UPDATE Request (Req1) from AE1contaning  |IUT <- AE1  |
                     | To set to AE1_RESOURCE_ADDRESS_1 and  |  |
                     | From set to AE_ID and  |  |
                     | Content containing  |  |
                     | AE resource containing  |  |
                     | valid labels attribute  |  |
                     | and the IUT receives a valid UPDATE Request (Req2) from AE1contaning  |IUT <- AE1 |
                     | To set to AE1_RESOURCE_ADDRESS_2 and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | valid labels attribute  | |
                     | and timer has not reached TIME_LIMIT  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response to AE1 for Req1  |IUT -> AE1  |
                     | and the IUT sends a valid Response to AE1 for Req2  |IUT -> AE1  |
                     | and the IUT sends a NOTIFY Request to AE1 generated from  |IUT -> AE1  |
                     | SUBS_RESOURCE_ADDRESS_1  |  |
                     | and the IUT sends a NOTIFY Request to AE1 generated from  |IUT -> AE1  |
                     | SUBS_RESOURCE_ADDRESS_2  |  |
                     | and the IUT sends a NOTIFY Request to AE2 generated from  |IUT -> AE2 |
                     | crossResourceSubscription CROSS_RESOURCE_SUBS_ADDRESS  | |
                     | containing  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | subscriptionReference attribute set to  | |
                     | CROSS_SUBS_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————+————-+
	TP Id
	TIME_WINDOW_TYPE

	TP/oneM2M/CSE/SUB/NTF/015_TWT/1
	1 (PERIODICWINDOW)

	TP/oneM2M/CSE/SUB/NTF/015_TWT/2
	2 (SLIDINGWINDOW)



TP/oneM2M/CSE/SUB/NTF/016
	TP Id
	TP/oneM2M/CSE/SUB/NTF/016

	Test objective
	Check that the IUT does not send a cross-resource notification to the notificationURI when a
notification from resource in subscriptionResourcesAsTarget is not received within required
TIME_LIMIT window

	Reference
	TS-0001 [1], clause 9.6.58, TS-0004 [2], clause 7.5.1.2.18

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1 containing
a container resource on CONTAINER_RESOURCE_ADDRESS_1 containing
a subscription resource on SUBS_RESOURCE_ADDRESS_1
a container resource on CONTAINER_RESOURCE_ADDRESS_2 containing
a subscription resource on SUBS_RESOURCE_ADDRESS_2
and the IUThaving created a <crossResourceSubscription> resource on
CROSS_RESOURCE_SUBS_ADDRESS containing
subscriptionResourcesAsTarget attribute containing
SUBS _RESOURCE_ADDRESS_1 and
SUBS _RESOURCE_ADDRESS_2 and
timeWindowType attribute set to TIME_WINDOW_TYPE and
timeWindowSize attribute set to DURATION and
notificationURI attribute set to AE2_RESOURCE_ADDRESS
and the IUT having registered the AE2
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |  |
                     | the IUT receives a valid UPDATE Request (Req1) from AE1contaning  |IUT <- AE1  |
                     | To set to AE1_RESOURCE_ADDRESS_1 and  |  |
                     | From set to AE_ID and  |  |
                     | Content containing  |  |
                     | AE resource containing  |  |
                     | valid labels attribute  |  |
                     | and the IUT receives a valid UPDATE Request (Req2) from AE1contaning  |IUT <- AE1 |
                     | To set to AE1_RESOURCE_ADDRESS_2 and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | valid labels attribute  | |
                     | and timer has reached TIME_LIMIT  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response to AE1 for Req1  |IUT -> AE1  |
                     | and the IUT sends a valid Response to AE1 for Req2  |IUT -> AE1  |
                     | and the IUT sends a NOTIFY Request to AE1 generated from  |IUT -> AE1  |
                     | SUBS_RESOURCE_ADDRESS_1  |  |
                     | and the IUT sends a NOTIFY Request to AE1 generated from  |IUT -> AE1 |
                     | SUBS_RESOURCE_ADDRESS_2  | |
                     | and the IUT does not send a NOTIFY Request to AE2  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————-+————-+
	TP Id
	TIME_WINDOW_TYPE

	TP/oneM2M/CSE/SUB/NTF/016_TWT/1
	1 (PERIODICWINDOW)

	TP/oneM2M/CSE/SUB/NTF/016_TWT/2
	2 (SLIDINGWINDOW)



TP/oneM2M/CSE/SUB/NTF/017
	TP Id
	TP/oneM2M/CSE/SUB/NTF/017

	Test objective
	Check that the IUT successfully sends notification request to the notificationURI when an
update request is received for the target subscribed-to resource with notificationEventType set
to "Blocking_Update"

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME set to VALUE_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE2  |
                     | the IUT sends a NOTIFY Request to AE2 contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | All attributes  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/018
	TP Id
	TP/oneM2M/CSE/SUB/NTF/018

	Test objective
	Check that the IUT successfully sends notification request to the notificationURI when an
update request is received for the target subscribed-to resource with notificationEventType set
to "Blocking_Update" when the attribute condition tag matches the modified attributes

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
attribute set to ATTRIBUTE_NAME
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME set to VALUE_2  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE2  |
                     | the IUT sends a NOTIFY Request to AE2 contaning  | |
                     | Content containing  | |
                     | notification message containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | All attributes  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SUB/NTF/019
	TP Id
	TP/oneM2M/CSE/SUB/NTF/019

	Test objective
	Check that the IUT does not send notification request to the notificationURI when an update
request is received for the target subscribed-to resource with notificationEventType set to
"Blocking_Update" but the attribute condition tag does not match the modified attributes

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME_1 set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
attribute set to ATTRIBUTE_NAME_2
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to
resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME_1 set to VALUE_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   | |
                     | the IUT does not send a NOTIFY Request to AE2_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/020
	TP Id
	TP/oneM2M/CSE/SUB/NTF/020

	Test objective
	Check that the IUT blocks update request for the target subscribed-to resource when an
previous update request is received with notificationEventType set to "Blocking_Update" and
notification process is still not completed

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to
resource
and the IUT having received a valid UPDATE Request from AE1_RESOURCE_ADDRESS
to SUBSCRIBED_TO_RESOURCE_ADDRESS
and the IUT having sent a valid NOTIFY Request to AE2_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESSand  | |
                     | From set to AE1_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | <subscribed‑to type> resourcecontaining  | |
                     | ATTRIBUTE_NAME set to VALUE_2  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   | |
                     | the IUT does not update SUBSCRIBED_TO_RESOURCE_ADDRESS  | |
                     | and the IUT does not send a NOTFIY Request to  | |
                     |AE2_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/021
	TP Id
	TP/oneM2M/CSE/SUB/NTF/021

	Test objective
	Check that the IUT successfully performs update request to the target subscribed-to resource
with notificationEventType set to "Blocking_Update"

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to
resource
and the IUT having received a valid UPDATE Request from AE1_RESOURCE_ADDRESS
to SUBSCRIBED_TO_RESOURCE_ADDRESS
and the IUT having sent the NOTIFY Request to the AE2_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE2 |
                     | the IUT receives a valid NOTIFY Response from AE2 containing  | |
                     | ResponseStatusCode set to OK (2000)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE1  |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/022
	TP Id
	TP/oneM2M/CSE/SUB/NTF/022

	Test objective
	Check that the IUT rejects update request to the target subscribed-to resource when
notificationEventType is set to "Blocking_Update" and the IUT have received the Notify
response containing Response Status Code indicating TARGET_NOT_REACHABLE

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to
resource
and the IUT having received a valid UPDATE Request from AE1_RESOURCE_ADDRESS
to SUBSCRIBED_TO_RESOURCE_ADDRESS
and the IUT having sent a NOTIFY Request to AE2_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE2 |
                     | the IUT receives a valid NOTIFY Response from AE2 containing  | |
                     | ResponseStatusCode set to TARGET_NOT_REACHABLE (5103)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE1  |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5107 (REMOTE_ENTITY_NOT_REACHABLE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SUB/NTF/023
	TP Id
	TP/oneM2M/CSE/SUB/NTF/023

	Test objective
	Check that the IUT rejects update request to the target subscribed-to resource when
notificationEventType is set to "Blocking_Update" and the IUT have received the Notify
response containing Response Status Code indicating OPERATION_NOT_ALLOWED

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
ATTRIBUTE_NAME set to VALUE_1 and
subscription child resource containing
notificationURI attribute set to AE2_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to
resource
and the IUT having received a valid UPDATE Request from AE1_RESOURCE_ADDRESS
to SUBSCRIBED_TO_RESOURCE_ADDRESS
and the IUT having sent a NOTIFY Request to AE2_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE2 |
                     | the IUT receives a valid NOTIFY Response from AE2 containing  | |
                     | ResponseStatusCode set to OPERATION_NOT_ALLOWED (4005)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE1  |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4127 (OPERATION_DENIED_BY_REMOTE_ENTITY)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SUB/NTF/024
	TP Id
	TP/oneM2M/CSE/SUB/NTF/024

	Test objective
	Check that the IUT rejects the creation of a subscription resource with notificationEventType set
to "Blocking_Update" when the subscribed-to resource has already a subscription resource
with this notificationEventType

	Reference
	TS-0004 [1], clause 7.5.1.2.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a <subscribed-to type> resource containing
subscription child resource containing
eventNotificationCriteria attribute containing
notificationEventType set to 7 (Blocking_Update)
and the AE1 having privileges to perform RETRIEVE operation on the subscribed-to resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE1 |
                     | the IUT receives a valid CREATE Request from AE1 containing  | |
                     | To set to SUBSCRIBED_TO_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | a subscription resource containing  | |
                     | eventNotificationCriteria attribute containing  | |
                     | notificationEventType set to 7 (Blocking_Update)   | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE1  |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4124  | |
                     |(BLOCKING_SUBSCRIPTION_ALREADY_EXISTS)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————+————-+
7.2.2.5	Group Management (GMG)
7.2.2.5.1	CREATE Operation
TP/oneM2M/CSE/GMG/CRE/001
	TP Id
	TP/oneM2M/CSE/GMG/CRE/001

	Test objective
	Check that the IUT rejects the creation of the group resource when member ID exceed max number of members

	Reference
	TS-0001 [1], clause 10.2.7.2, TS-0004 [2], clause 7.3.13

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE to perform CREATE operation
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to | |
                     | LIST_OF_MEMBER_RESOURCE_IDS and  | |
                     | maxNrOfMembers attribute set to MAX_NR_MEMBERS less  | |
                     | than the number of memerIDs set in memberIDs attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 6010  | |
                     | (MAX_NUMBER_OF_MEMBER_EXCEEDED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/GMG/CRE/002
	TP Id
	TP/oneM2M/CSE/GMG/CRE/002

	Test objective
	Check that the IUT rejects the creation of the group resource when the memberType cannot be
retrieved due to lack of privilege

	Reference
	TS-0001 [1], clause 10.2.7.2, TS-0004 [2], clause 7.3.13

	Parent Release
	Release 1

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and IUT registered with remote CSE CSE1
and the AE having created a resource at MEMBER_RESOURCE_ADDRESS_1 at another
CSE1 containing
resourceType set to RESOURCE_TYPE
and the IUT not having privileges to perform RETRIEVE operation on the
MEMBER_RESOURCE_ADDRESS_1
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberType attribute set to RESOURCE_TYPE and  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the group resource  | |
                     | and the IUT sends a valid valid Response containing  | |
                     | Response Status Code set to 5105  | |
                     |(RECEIVER_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/GMG/CRE/003
	TP Id
	TP/oneM2M/CSE/GMG/CRE/003

	Test objective
	Check that the IUT detects the presence of duplicate member IDs during the creation of the
<group> resource and removes the duplicate member IDs prior to creation of the <group>
resource

	Reference
	TS-0001 [1], clause 10.2.7.2

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource at TARGET_RESOURCE_ADDRESS allowing
a child resource type group
and the AE having privileges to perform CREATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having created a resource at MEMBER_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives an valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS,  | |
                     | MEMBER_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT creates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS  | |
                     |} | |
	Note: TARGET_RESOURCE_ADDRESS : <CSEBase>, <remoteCSE>
MEMBER_RESOURCE_ADDRESS : any oneM2M resource type



TP/oneM2M/CSE/GMG/CRE/004
	TP Id
	TP/oneM2M/CSE/GMG/CRE/004

	Test objective
	Check that the IUT validates the resource type during the creation of the <group> resource
when memberType attribute is not 'mixed'

	Reference
	TS-0001 [1], clause 10.2.7.2, TS-0004 [2], clause 7.4.14.2.1

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource at TARGET_RESOURCE_ADDRESS allowing
a child resource type group
and the AE having privileges to perform CREATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS
having resourceType attribute RESOURCE_TYPE
}



·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to MEMBER_RESOURCE_ADDRESS  | |
                     | and  | |
                     | memberType attribute set to RESOURCE_TYPE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT creates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to TRUE  | |
                     |} | |
	Note: TARGET_RESOURCE_ADDRESS : <CSEBase>, <remoteCSE>
MEMBER_RESOURCE_ADDRESS : any oneM2M resource type



TP/oneM2M/CSE/GMG/CRE/005
	TP Id
	TP/oneM2M/CSE/GMG/CRE/005

	Test objective
	Check that the IUT handles unsuccessful validation of the resource type during the creation of
the <group> resource when memberType attribute is not 'mixed' and the consistencyStrategy
attribute is SET_MIXED

	Reference
	TS-0001 [1], clause 10.2.7.2, TS-0004 [2], clause 7.4.14.2.1

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource at TARGET_RESOURCE_ADDRESS allowing
a child resource type group
and the AE having privileges to perform CREATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS having resourceType attribute RESOURCE_TYPE_1
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS  | |
                     | and memberType attribute set to RESOURCE_TYPE_2  | |
                     | and consistencyStrategy attribute set to SET_MIXED  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT creates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to TRUE and  | |
                     | memberType attribute set to MIXED  | |
                     |} | |
	Note: TARGET_RESOURCE_ADDRESS : <CSEBase>, <remoteCSE>
MEMBER_RESOURCE_ADDRESS : any oneM2M resource type



TP/oneM2M/CSE/GMG/CRE/006
	TP Id
	TP/oneM2M/CSE/GMG/CRE/006

	Test objective
	Check that the IUT handles unsuccessful validation of the resource type during the creation of
the <group> resource when memberType attribute is not 'mixed' and the consistencyStrategy
attribute is ABANDON_MEMBER

	Reference
	TS-0001 [1], clause 10.2.7.2, TS-0004 [2], clause 7.4.14.2.1

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource at TARGET_RESOURCE_ADDRESS allowing
a child resource type group
and the AE having privileges to perform CREATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1
having resourceType attribute RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2
having resourceType attribute RESOURCE_TYPE_2
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing   | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2 and  | |
                     | memberType attribute set to RESOURCE_TYPE_1 and | |
                     | consistencyStrategy attribute set to ABANDON_MEMBER  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT creates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to TRUE and  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1  | |
                     |} | |
	Note: TARGET_RESOURCE_ADDRESS : <CSEBase>, <remoteCSE>
MEMBER_RESOURCE_ADDRESS : any oneM2M resource type



TP/oneM2M/CSE/GMG/CRE/007
	TP Id
	TP/oneM2M/CSE/GMG/CRE/007

	Test objective
	Check that the IUT handles unsuccessful validation of the resource type during the creation of
the group resource when memberType attribute is not 'mixed' and the consistencyStrategy
attribute is ABANDON_GROUP

	Reference
	TS-0001 [1], clause 10.2.7.2, TS-0004 [2], clause 7.4.14.2.1

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource at TARGET_RESOURCE_ADDRESS allowing
a child resource type <group>
and the AE having privileges to perform CREATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2 having
resourceType attribute RESOURCE_TYPE_2
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2 and  | |
                     | memberType attribute set to RESOURCE_TYPE_1 and | |
                     | consistencyStrategy attribute set to ABANDON_GROUP  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not create the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4110  | |
                     |(GROUP_MEMBER_TYPE_INCONSISTENT)  | |
                     |} | |
	Note: TARGET_RESOURCE_ADDRESS : <CSEBase>, <remoteCSE>
MEMBER_RESOURCE_ADDRESS : any oneM2M resource type



TP/oneM2M/CSE/GMG/CRE/008
	TP Id
	TP/oneM2M/CSE/GMG/CRE/008

	Test objective
	Check that the IUT creates a <group> resource with empty memberIDs attribute.

	Reference
	TS-0001 [1], clause 9.6.13, 10.2.7.2, TS-0004 [2], clause 7.4.14.2.1

	Parent Release
	Release 3

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE to perform CREATE operation
}



·                  +---------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 9 (group) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to empty  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | group resource representation  | |
                     |} | |
+———————-+—————————————————————————————————+————-+
7.2.2.5.2	UPDATE Operation
TP/oneM2M/CSE/GMG/UPD/001
	TP Id
	TP/oneM2M/CSE/GMG/UPD/001

	Test objective
	Check that the IUT rejects the update of the group resource when the memberType cannot be
retrieved due to lack of privilege.

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.3.13

	Parent Release
	Release 1

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and IUT registered with remote CSE CSE1
and the IUThaving a resource at MEMBER_RESOURCE_ADDRESS_1 containing
resourceType set to RESOURCE_TYPE
and the IUT having created a <group> resource at GROUP_RESOURCE_ADDRESS
containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1 and
memberType attribute set to RESOURCE_TYPE
and the AE having privileges to perform UPDATE operation on the
GROUP_RESOURCE_ADDRESS
and the AEhaving created a resource at MEMBER_RESOURCE_ADDRESS_2 at another
CSE1
and the IUT not having privileges to perform RETRIEVE operation on
MEMBER_RESOURCE_ADDRESS_2
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid valid Response containing  | |
                     | Response Status Code set to 5105  | |
                     |(RECEIVER_HAS _NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/GMG/UPD/002
	TP Id
	TP/oneM2M/CSE/GMG/UPD/002

	Test objective
	Check that the IUT detects the presence of duplicate member IDs during an update of the
<group> resource and removes the duplicate member IDs prior to updating the <group>
resource

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1
and the IUT having created a <group> resource at GROUP_RESOURCE_ADDRESS
containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1
and the AE having privileges to perform UPDATE operation on the
GROUP_RESOURCE_ADDRESS
and the IUT having created a resource at MEMBER_RESOURCE_ADDRESS_2
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to GROUP_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_2,  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT updates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/GMG/UPD/003
	TP Id
	TP/oneM2M/CSE/GMG/UPD/003

	Test objective
	Check that the IUT validates the resource type during an UPDATE of the <group>
resource when memberType attribute is not 'mixed'.

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1
memberType attribute set to RESOURCE_TYPE_1
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2having
resourceType attribute RESOURCE_TYPE_1
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT updates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to TRUE  | |
                     |} | |
+———————-+——————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/GMG/UPD/004
	TP Id
	TP/oneM2M/CSE/GMG/UPD/004

	Test objective
	Check that the IUT handles unsuccessful validation of the resource type during an UPDATE of
the < group_>_ resource when memberType attribute is not 'mixed' and the consistencyStrategy
attribute is SET_MIXED

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1 and
memberType attribute set to RESOURCE_TYPE_1 and
memberTypeValidated attribute set to TRUE and
consistencyStrategy attribute set to SET_MIXED
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2* *having
resourceType attribute RESOURCE_TYPE_2
}**



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT updates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to TRUE and  | |
                     | memberType attribute set to MIXED  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/GMG/UPD/005
	TP Id
	TP/oneM2M/CSE/GMG/UPD/005

	Test objective
	Check that the IUT handles unsuccessful validation of the resource type during an UPDATE of
the group resource when memberType attribute is not 'mixed' and the consistencyStrategy
attribute is ABANDON_MEMBER

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1 and
memberType attribute set to RESOURCE_TYPE_1 and
memberTypeValidated attribute set to TRUE and
consistencyStrategy attribute set to ABANDON_MEMBER
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2having
resourceType attribute RESOURCE_TYPE_2
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT updates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to TRUE and  | |
                     | memberIDs attribute set to | |
                     | MEMBER_RESOURCE_ADDRESS_1  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/GMG/UPD/006
	TP Id
	TP/oneM2M/CSE/GMG/UPD/006

	Test objective
	Check that the IUT handles unsuccessful validation of the resource type during the update of
the group resource when memberType attribute is not 'mixed' and the consistencyStrategy
attribute is ABANDON_GROUP

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1 and
memberType attribute set to RESOURCE_TYPE_1 and
memberTypeValidated attribute set to TRUE and
consistencyStrategy attribute set to ABANDON_GROUP
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2having
resourceType attribute RESOURCE_TYPE_2
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT does not update the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4110  | |
                     |(GROUP_MEMBER_TYPE_INCONSISTENT)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/GMG/UPD/007
	TP Id
	TP/oneM2M/CSE/GMG/UPD/007

	Test objective
	Check that the IUT detects when the number of memberIDs exceeds the limitation of
maxNrOfMembers

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1,
MEMBER_RESOURCE_ADDRESS_2 and
maxNrOfMembers attribute set to 2
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute set to RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2having
resourceType attribute set to RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_3having
resourceType attributeset to RESOURCE_TYPE_1
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2,  | |
                     | MEMBER_RESOURCE_ADDRESS_3  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not update the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 6010  | |
                     |(MAX_NUMBER_OF_MEMBER_EXCEEDED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/GMG/UPD/008
	TP Id
	TP/oneM2M/CSE/GMG/UPD/008

	Test objective
	Check that the IUT detects when the value provided for maxNrOfMembers attribute is less than
the value of the currentNrOfMembers attribute

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1,
MEMBER_RESOURCE_ADDRESS_2 and
maxNrOfMembers attribute set to 2
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1having
resourceType attribute set to RESOURCE_TYPE_1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_2having
resourceType attribute set to RESOURCE_TYPE_1
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing group resource containing  | |
                     | maxNrOfMembers attribute set to 1  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT does not update the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 6010  | |
                     |(MAX_NUMBER_OF_MEMBER_EXCEEDED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/GMG/UPD/009
	TP Id
	TP/oneM2M/CSE/GMG/UPD/009

	Test objective
	Check that the IUT handles validation of the resource type during an UPDATE of the <group>
resource when memberIDs contains a sub-group on a temporarily unreachable Hosting CSE

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered to the remoteCSE
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1and
memberType attribute set to RESOURCE_TYPE_1 and
memberTypeValidated attribute set to TRUE and
consistencyStrategy attribute set to ABANDON_MEMBER
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute set to RESOURCE_TYPE_1
and the remoteCSE having a group
resource at MEMBER_RESOURCE_ADDRESS_2
containing
memberType attribute set to RESOURCE_TYPE_1
and the remoteCSE having onlineStatus set to False
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT updates the group resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to FALSE and  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/GMG/UPD/010
	TP Id
	TP/oneM2M/CSE/GMG/UPD/010

	Test objective
	Check that the IUT handles validation of the resource type during an UPDATE of the group
resource when memberIDs contains a sub-group on a a previously unreachable Hosting CSE
that has become reachable

	Reference
	TS-0001 [1], clause 10.2.7.4, TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered to the remoteCSE
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS_1,
MEMBER_RESOURCE_ADDRESS_2 and
memberType attribute set to RESOURCE_TYPE_1 and
memberTypeValidated attribute set to FALSE and
consistencyStrategy attribute set to ABANDON_MEMBER
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the AE having a subscription to TARGET_RESOURCE_ADDRESS
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS_1 having
resourceType attribute set to RESOURCE_TYPE_1
and the remoteCSE having a group resource at MEMBER_RESOURCE_ADDRESS_2
containing
memberType attribute set to RESOURCE_TYPE_2
and the remoteCSE having onlineStatus set to False
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid UPDATE Request from remoteCSE containing  | |
                     | To set to REMOTE_CSE_ADDRESS and  | |
                     | From set to CSE‑ID and  | |
                     | Content containing  | |
                     | remoteCSE resource containing  | |
                     | onlineStatus attribute set to TRUE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a NOTIFY Request containing  | |
                     | Content containing  | |
                     | group resource containing  | |
                     | memberTypeValidated attribute set to TRUE and  | |
                     | memberIDs attribute set to  | |
                     | MEMBER_RESOURCE_ADDRESS_1,  | |
                     | MEMBER_RESOURCE_ADDRESS_2  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————+————-+
7.2.2.5.3	RETRIEVE Operation
TP/oneM2M/CSE/GMG/RET/001
	TP Id
	TP/oneM2M/CSE/GMG/RET/001

	Test objective
	Check that the IUT performs a RETRIEVE request for each resource in memberIDs with a
relative address appended to fanOutPoint that includes a virtual resource

	Reference
	TS-0001 [1], clause 10.2.7.7

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to ACP_RESOURCE_ID indicating to
allow the AE privileges to perform RETRIEVE operation and
memberType attribute set to 3 (container) and
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS1,
MEMBER_RESOURCE_ADDRESS2
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1 containing
resourceType attribute set to container and
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2 containing
resourceType attribute set to container and
and MEMBER_RESOURCE_ADDRESS1 and MEMBER_RESOURCE_ADDRESS2
containing
a child resource containing
resourceType attribute set to contentInstance
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt/la and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | TaggregatedResponse message containing  | |
                     | Response for MEMBER_RESOURCE_ADDRESS1/la,  | |
                     | Response for MEMBER_RESOURCE_ADDRESS2/la  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+


7.2.2.5.4	BASIC OPERATION
TP/oneM2M/CSE/GMG/001
	TP Id
	TP/oneM2M/CSE/GMG/001

	Test objective
	Check that the IUT allows a <group>/fopt OPERATION when the Originator has OPERATION
permission specified in membersAccessControlPolicyIDs attribute in the group resource

	Reference
	TS-0001 [1], clause 10.2.7.7

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to allow the AE to perform OPERATION
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing  | |
                     | Response for MEMBER_RESOURCE_ADDRESS1,  | |
                     | Response for MEMBER_RESOURCE_ADDRESS2  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/GMG/001_CRE
	CREATE

	TP/oneM2M/CSE/GMG/001_RET
	RETRIEVE

	TP/oneM2M/CSE/GMG/001_UPD
	UPDATE

	TP/oneM2M/CSE/GMG/001_DEL
	DELETE



TP/oneM2M/CSE/GMG/002
	TP Id
	TP/oneM2M/CSE/GMG/002

	Test objective
	Check that IUT denies a <group>/fopt OPERATION when the Originator does not have
OPERATION permission specified in membersAccessControlPolicyIDs in the group resource

	Reference
	TS-0001 [1], clause 10.2.7.7

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to ACP_RESOURCE_ID indicating to
allow the AE to perform all operations except OPERATION
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103  | |
                     | (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/GMG/002_CRE
	CREATE

	TP/oneM2M/CSE/GMG/002_RET
	RETRIEVE

	TP/oneM2M/CSE/GMG/002_UPD
	UPDATE

	TP/oneM2M/CSE/GMG/002_DEL
	DELETE



TP/oneM2M/CSE/GMG/003
	TP Id
	TP/oneM2M/CSE/GMG/003

	Test objective
	Check that the IUT allows a <group>/fopt OPERATION when the Originator has OPERATION
permission specified in accessControlPolicyIDs and the membersAccessControlPolicyIDs is
empty in the <group> resource

	Reference
	TS-0001 [1], clause 10.2.7.7

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to empty and
accessControlPolicyIDs attribute set to ACP_RESOURCE_ID indicating to allow the
AE privileges to perform OPERATION
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set 2000(OK)and  | |
                     | Content containing  | |
                     | aggregatedResponse message containing  | |
                     | Response for MEMBER_RESOURCE_ADDRESS1,  | |
                     | Response for MEMBER_RESOURCE_ADDRESS2  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/GMG/003_CRE
	CREATE

	TP/oneM2M/CSE/GMG/003_RET
	RETRIEVE

	TP/oneM2M/CSE/GMG/003_UPD
	UPDATE

	TP/oneM2M/CSE/GMG/003_DEL
	DELETE



TP/oneM2M/CSE/GMG/004
	TP Id
	TP/oneM2M/CSE/GMG/004

	Test objective
	Check that IUT rejects a <group>/fopt OPERATION when the Originator does not have
OPERATION permission specified in accessControlPolicyIDs and the
membersAccessControlPolicyIDs is empty in the group resource

	Reference
	TS-0001 [1], clause 10.2.7.7

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to empty and
accessControlPolicyIDs attribute set to ACP_RESOURCE_ID indicating to allow the
AE privileges to perform all operations except OPERATION
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103  | |
                     | (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/GMG/004_CRE
	CREATE

	TP/oneM2M/CSE/GMG/004_RET
	RETRIEVE

	TP/oneM2M/CSE/GMG/004_UPD
	UPDATE

	TP/oneM2M/CSE/GMG/004_DEL
	DELETE



TP/oneM2M/CSE/GMG/005
	TP Id
	TP/oneM2M/CSE/GMG/005

	Test objective
	Check that IUT performs an OPERATION request for each resource in memberIDs with no
relative address appended to it

	Reference
	TS-0001 [1], clause 10.2.7.7

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having a <group> resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to allow the AE privileges to perform
OPERATION and
memberType attribute set to AE AE and
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS1,
MEMBER_RESOURCE_ADDRESS2
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1 containing
resourceTypeset to AE
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2 containing
resourceTypeset to AE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse message containing  | |
                     | Response for MEMBER_RESOURCE_ADDRESS1 and  | |
                     | Response for MEMBER_RESOURCE_ADDRESS2  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/GMG/005_CRE
	CREATE

	TP/oneM2M/CSE/GMG/005_RET
	RETRIEVE

	TP/oneM2M/CSE/GMG/005_UPD
	UPDATE

	TP/oneM2M/CSE/GMG/005_DEL
	DELETE



TP/oneM2M/CSE/GMG/006
	TP Id
	TP/oneM2M/CSE/GMG/006

	Test objective
	Check that IUT perfomrs an OPERATION request for each resource in memberIDs with a
relative address appended to it

	Reference
	TS-0001 [1], clause 10.2.7.7

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having a <group> resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to allow the AE privileges to
perform CREATE and
memberType attribute set to AE and
memberIDs attribute set to MEMBER_RESOURCE_ADDRESS1,
MEMBER_RESOURCE_ADDRESS2
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1 containing
resourceType attribute set to AE
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2 containing
resourceType attribute set to AE
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS1 containing
a child resource containing
resourceType attribute set to container and
resourceName attribute set to NAME
and the IUT having a resource at MEMBER_RESOURCE_ADDRESS2 containing
a child resource containing
resourceType attribute set to container and
resourceName attribute set to NAME
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt/NAME and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse message containing  | |
                     | Response for MEMBER_RESOURCE_ADDRESS1 and  | |
                     | Response for MEMBER_RESOURCE_ADDRESS2  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/GMG/006_CRE
	CREATE

	TP/oneM2M/CSE/GMG/006_RET
	RETRIEVE

	TP/oneM2M/CSE/GMG/006_UPD
	UPDATE

	TP/oneM2M/CSE/GMG/006_DEL
	DELETE




TP/oneM2M/CSE/GMG/007
	TP Id
	TP/oneM2M/CSE/GMG/007

	Test objective
	Check that the IUT denies a <group>/fanOutPoint RETRIEVE when there is no memberID in
<group> resource

	Reference
	TS-0004 [2], clause 7.4.14.2.4

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a group resource at TARGET_RESOURCE_ADDRESS containing
membersAccessControlPolicyIDs attribute set to ACP_RESOURCE_ID indicating to
allow the AE to perform all operations and
no memberID attribute
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/fopt and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4109 (NO_MEMBER)  | |
                     |} | |
+———————-+———————————————————————————————————————————————+————-+


7.2.2.6	Discovery (DIS)
7.2.2.6.1	RETRIEVE Operation
TP/oneM2M/CSE/DIS/001
	TP Id
	TP/oneM2M/CSE/DIS/001

	Test objective
	Check that the IUT returns successfully a list all discovered resource addresses

	Reference
	TS-0001 [1], clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY operation
}



·                  +------------------------------------------------------------------------------+----------------------+

·                      |when {  | |
                     | the IUT receives a valid RETRIEVE Request from AE containing | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +------------------------------------------------------------------------------+----------------------+

·                      |then {  | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList representation  | |
                     |} | |
+———————-+——————————————————————————+———————-+
TP/oneM2M/CSE/DIS/002
	TP Id
	TP/oneM2M/CSE/DIS/002

	Test objective
	Check that the IUT returns successfully appropriate list of discovered resource when the filter
criteria is provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY operation on the child resource
}



·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList representation  | |
                     |} | |
+———————-+———————————————————————————————————————-+————-+
TP/oneM2M/CSE/DIS/003
	TP Id
	TP/oneM2M/CSE/DIS/003

	Test objective
	Check that the IUT returns the empty address list when no result matching with filter criteria is
discovered

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY operation on the child resource
and FILTER_CRITERIA_CONDITIONS not matching child resource
}



·                  +-----------------------------------------------------------------------------------------------+----------------------+

·                      |when {  | |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------+----------------------+

·                      |then {   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList element set to empty list  | |
                     |} | |
+———————-+———————————————————————————————–+———————-+
TP/oneM2M/CSE/DIS/004
	TP Id
	TP/oneM2M/CSE/DIS/004

	Test objective
	Check that the IUT returns successfully a list of discovered resource addresses with Non-
hierarchical addressing form when the Desired Identifier Result Type is provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   | |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Desired Identifier Result Type set to 2 (unstructured) and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList representation containing  | |
                     | unstructured addresses of discovered resources  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————+———————-+
TP/oneM2M/CSE/DIS/005
	TP Id
	TP/oneM2M/CSE/DIS/005

	Test objective
	Check that the IUT accepts a discovery requests to the resource
TARGET_RESOURCE_ADDRESS when AE has no privilege to perform the discovery
operation on the children/descendant of resource TARGET_RESOURCE_ADDRESS

	Reference
	TS-0001 [1], clause 10.2.6.2 and clause 7.2.3.14, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
child resources
and the AE having no privileges to perform DISCOVERY operation on the children/ descendant of resource
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUTreceives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList element set to empty list  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/DIS/006
	TP Id
	TP/oneM2M/CSE/DIS/006

	Test objective
	Check that the IUT responds with an error when the AE sends requests to discover the resource
TARGET_RESOURCE_ADDRESS which does not exist in the Hosting CSE

	Reference
	TS-0001 [1], clause 10.2.6.2, TS-0004 [2], clause 7.3.3.14

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having not yet created a resource TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   | |
                     | the IUTreceives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+———————-+
TP/oneM2M/CSE/DIS/007
	TP Id
	TP/oneM2M/CSE/DIS/007

	Test objective
	Check that the IUT responds the originator with an error when the originator sends a request
including an invalid format of filter criteria to discover the resource
TARGET_RESOURCE_ADDRESS

	Reference
	TS-0001 [1], clause 10.2.6, TS-0004 [2], clause 7.3.3.6

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the originator AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS not being  | |
                     |valid format  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————+———————-+
TP/oneM2M/CSE/DIS/008
	TP Id
	TP/oneM2M/CSE/DIS/008

	Test objective
	Check that the IUT responds the originator with a success response when the originator sends
a request to discover the resource TARGET_RESOURCE_ADDRESS including two conflicted
filter criteria of different type FILTER_CRITERIA_CONDITION_1 and
FILTER_CRITERIA_CONDITION_ 2 (E.G. createBefore < createdAfter )

	Reference
	TS-0001 [1], clause 6.2.5, TS-0004 [2], clause 7.3.3.17

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the originator AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY operation on the child resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 1 (Discovery Criteria)and  | |
                     | having conflict conditions   | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList element set to empty list  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	REQ Reference
	FILTER_CRITERIA_CONDITION_1
	FILTER_CRITERIA_CONDITION_2

	TP/oneM2M/CSE/DIS/008_CRB/CRA
	REQ-0004-07241
	createdBefore
	createdAfter

	TP/oneM2M/CSE/DIS/008_MS/US
	REQ-0004-07242
	unmodifiedSince
	modifiedSince

	TP/oneM2M/CSE/DIS/008_STS/STB
	REQ-0004-07243
	stateTagSmaller
	stateTagBigger

	TP/oneM2M/CSE/DIS/008_EXB/EXA
	REQ-0004-07244
	expireBefore
	expireAfter



TP/oneM2M/CSE/DIS/009
	TP Id
	TP/oneM2M/CSE/DIS/009

	Test objective
	Check that the IUT returns the empty address list when resources match the filter criteria but they do not include DISCOVERY permission

	Reference
	TS-0001 [1], clause 9.6.2.3 and clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource
and the AE not having privileges to perform DISCOVERY operation on the child resource
and FILTER_CRITERIA_CONDITIONS matching the child resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList element set to empty list  | |
                     |} | |
+———————-+————————————————————————————————————————–+————-+
TP/oneM2M/CSE/DIS/010
	TP Id
	TP/oneM2M/CSE/DIS/010

	Test objective
	Check that the IUT returns successfully a list of discovered resource addresses with hierarchical
addressing form when the Desired Identifier Result Type is provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY operation
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   |  |
                     | the IUT receives a valid RETRIEVE Request from AE containing  |  |
                     | To set to TARGET_RESOURCE_ADDRESS and  |  |
                     | From set to AE‑ID and  |  |
                     | Desired Identifier Result Type set to 1 (structured) and  |IUT <- AE |
                     | Filter Criteria containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {  |  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2000 (OK) and  |  |
                     | Content containing  |IUT -> AE |
                     | URIList representation containing  | |
                     | structured addresses of discovered resources  | |
                     |} | |
+———————-+————————————————————————————————————————————————————–+———————-+
TP/oneM2M/CSE/DIS/011
	TP Id
	TP/oneM2M/CSE/DIS/011

	Test objective
	Check that the IUT returns successfully a list of discovered resource addresses with hierarchical
addressing form when the Desired Identifier Result Type is not provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resourceand
the AE having privileges to perform DISCOVERY operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   |  |
                     | the IUT receives a valid RETRIEVE Request from AE containing  |  |
                     | To set to TARGET_RESOURCE_ADDRESS and  |  |
                     | From set to AE‑ID and  |  |
                     | no Desired Identifier Result Type parameter and  |IUT <- AE |
                     | Filter Criteria containing  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2000 (OK) and  |  |
                     | Contentcontaining  |IUT -> AE |
                     | URIList representation containing  | |
                     | structured addresses of discovered resources  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————+———————-+
TP/oneM2M/CSE/DIS/012
	TP Id
	TP/oneM2M/CSE/DIS/012

	Test objective
	Check that the IUT successfully performs a Discovery-based OPERATION

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS_1 and
a child resource at CONTAINER_RESOURCE_ADDRESS_2
and the AE having privileges to perform DISCOVERY and OPERATION on children
resources
}



·                  +-------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------+----------------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_1,  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_2  | |
                     |} | |
+———————-+————————————————————————————————-+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/012_CRE
	CREATE

	TP/oneM2M/CSE/DIS/012_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/012_DEL
	DELETE



TP/oneM2M/CSE/DIS/013
	TP Id
	TP/oneM2M/CSE/DIS/013

	Test objective
	Check that the IUT successfully performs a Discovery-based OPERATION when the filter
criteria is provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS_1 and
a child resource at CONTAINER_RESOURCE_ADDRESS_2
and the AE having privileges to perform DISCOVERY and OPERATION on children resources
and FILTER_CRITERIA_CONDITIONS matching child resource at CONTAINER_RESOURCE_ADDRESS_1
}



·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     |containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_1  | |
                     |} | |
+———————-+————————————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/013_CRE
	CREATE

	TP/oneM2M/CSE/DIS/013_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/013_DEL
	DELETE



TP/oneM2M/CSE/DIS/014
	TP Id
	TP/oneM2M/CSE/DIS/014

	Test objective
	Check that the IUT returns the empty content when no result matching with filter criteria is
discovered in a Discovery-based OPERATION

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource
and the AE having privileges to perform DISCOVERY and OPERATION on child resource
and FILTER_CRITERIA_CONDITIONS not matching child resource
}



·                  +------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |} | |
+———————-+——————————————————————————————————————+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/014_CRE
	CREATE

	TP/oneM2M/CSE/DIS/014_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/014_DEL
	DELETE



TP/oneM2M/CSE/DIS/015
	TP Id
	TP/oneM2M/CSE/DIS/015

	Test objective
	Check that the IUT successfully performs a Discovery-based OPERATION using Non-
hierarchical addressing form when the Result Content and Desired Identifier Result Type is
provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource
and the AE having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Result Content set to 11 (discovery result resource references) and  | |
                     | Desired Identifier Result Typeset to 2 (unstructured) and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | URIList containing  | |
                     | unstructured addresses of discovered resources  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————–+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/015_CRE
	CREATE

	TP/oneM2M/CSE/DIS/015_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/015_DEL
	DELETE



TP/oneM2M/CSE/DIS/016
	TP Id
	TP/oneM2M/CSE/DIS/016

	Test objective
	Check that the IUT accepts a Discovery-based OPERATION request to the resource
TARGET_RESOURCE_ADDRESS when AE has no privilege to perform the discovery
operation

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
child resources
and the AE having no privileges to perform DISCOVERY and OPERATION on children
resources
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUTreceives a valid Discovery‑based OPERATION Request from  | |
                     | AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |  | |
                     |} | |
+———————-+———————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/016_CRE
	CREATE

	TP/oneM2M/CSE/DIS/016_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/016_DEL
	DELETE



TP/oneM2M/CSE/DIS/017
	TP Id
	TP/oneM2M/CSE/DIS/017

	Test objective
	Check that the IUT accepts a Discovery-based OPERATION request to the resource
TARGET_RESOURCE_ADDRESS when AE has privilege to perform the discovery operation
but AE has no privilege to perform the OPERATION request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS_1 and
a child resource at CONTAINER_RESOURCE_ADDRESS_2
and the AE having privileges to perform DISCOVERY on children resources
and the AE having no privileges to perform OPERATION on children resources
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUTreceives a valid Discovery‑based OPERATION Request from  | |
                     | AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT does not perform OPERATION  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK)  | |
                     | aggregatedResponse containing  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_1  | |
                     |containing  | |
                     | Response Status Code set to 4103(ACCESS_DENIED)  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_2  | |
                     |containing  | |
                     | Response Status Code set to 4103(ACCESS_DENIED)  | |
                     |  | |
                     |  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/017_CRE
	CREATE

	TP/oneM2M/CSE/DIS/017_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/017_DEL
	DELETE



TP/oneM2M/CSE/DIS/018
	TP Id
	TP/oneM2M/CSE/DIS/018

	Test objective
	Check that the IUT responds with an error when the AE sends Discovery-based OPERATION
requests to the resource TARGET_RESOURCE_ADDRESS which does not exist in the Hosting
CSE

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having not yet created a resource TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   |IUT <- AE |
                     | the IUTreceives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4(Discovery‑based Operation)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/018_CRE
	CREATE

	TP/oneM2M/CSE/DIS/018_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/018_DEL
	DELETE



TP/oneM2M/CSE/DIS/019
	TP Id
	TP/oneM2M/CSE/DIS/019

	Test objective
	Check that the IUT responds to the originator with an error when the originator sends a
Discovery-based OPERATION request including an invalid format of filter criteria to discover the
resource TARGET_RESOURCE_ADDRESS

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the originator AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from  | |
                     | AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS not being valid  | |
                     | format  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————-+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/019_CRE
	CREATE

	TP/oneM2M/CSE/DIS/019_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/019_DEL
	DELETE



TP/oneM2M/CSE/DIS/020
	TP Id
	TP/oneM2M/CSE/DIS/020

	Test objective
	Check that the IUT responds to the originator with a success response when the originator
sends a Discovery-based OPERATION including two conflicted filter criteria of different type
FILTER_CRITERIA_CONDITION_1 and FILTER_CRITERIA_CONDITION_ 2 (E.G.
createBefore < createdAfter )

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14 and clause 7.3.3.17

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the originator AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource
and the AE having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUTreceives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_IDand  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation) and  | |
                     | having conflict conditions   | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	COLSPAN
	FILTER_CRITERIA_CONDITION_1
	FILTER_CRITERIA_CONDITION_2
	OPERATION

	TP/oneM2M/CSE/DIS/020_CRB/CRA/CRE
	COLSPAN
	createdBefore
	createdAfter
	CREATE

	TP/oneM2M/CSE/DIS/020_MS/US/CRE
	COLSPAN
	unmodifiedSince
	modifiedSince
	CREATE

	TP/oneM2M/CSE/DIS/020_STS/STB/CRE
	COLSPAN
	stateTagSmaller
	stateTagBigger
	CREATE

	TP/oneM2M/CSE/DIS/020_EXB/EXA/CRE
	COLSPAN
	expireBefore
	expireAfter
	CREATE

	TP/oneM2M/CSE/DIS/020_CRB/CRA/UPD
	COLSPAN
	createdBefore
	createdAfter
	UPDATE

	TP/oneM2M/CSE/DIS/020_MS/US/UPD
	COLSPAN
	unmodifiedSince
	modifiedSince
	UPDATE

	TP/oneM2M/CSE/DIS/020_STS/STB/UPD
	COLSPAN
	stateTagSmaller
	stateTagBigger
	UPDATE

	TP/oneM2M/CSE/DIS/020_EXB/EXA/UPD
	COLSPAN
	expireBefore
	expireAfter
	UPDATE

	TP/oneM2M/CSE/DIS/020_CRB/CRA/DEL
	createdBefore
	createdAfter
	DELETE
	

	TP/oneM2M/CSE/DIS/020_MS/US/DEL
	unmodifiedSince
	modifiedSince
	DELETE
	

	TP/oneM2M/CSE/DIS/020_STS/STB/DEL
	stateTagSmaller
	stateTagBigger
	DELETE
	

	TP/oneM2M/CSE/DIS/020_EXB/EXA/DEL
	expireBefore
	expireAfter
	DELETE
	



TP/oneM2M/CSE/DIS/021
	TP Id
	TP/oneM2M/CSE/DIS/021

	Test objective
	Check that the IUT returns the empty content when resources match the filter criteria but they
do not include Discovery-based OPERATION permission.

	Reference
	TS-0001 [1], clause 9.6.2.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource
and the AE not having privileges to perform DISCOVERY on child resource
and the AE having privileges to perform OPERATION on child resource
and FILTER_CRITERIA_CONDITIONS matching the child resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |  | |
                     |} | |
+———————-+—————————————————————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/021_CRE
	CREATE

	TP/oneM2M/CSE/DIS/021_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/021_DEL
	DELETE



TP/oneM2M/CSE/DIS/022
	TP Id
	TP/oneM2M/CSE/DIS/022

	Test objective
	Check that the IUT successfully performs a Discovery-based OPERATION using hierarchical
addressing form when the Result Content and Desired Identifier Result Type is provided in the
request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   |  |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  |  |
                     | To set to TARGET_RESOURCE_ADDRESS and  |  |
                     | From set to AE‑ID and  |IUT <- AE |
                     | Result Content set to 11 (discovery result resource references) and  | |
                     | Desired Identifier Result Type set to 1 (structured) and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2000(OK) and  |  |
                     | Content containing  |IUT -> AE |
                     | URIList containing  | |
                     | structured addresses of discovered resources  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————-+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/022_CRE
	CREATE

	TP/oneM2M/CSE/DIS/022_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/022_DEL
	DELETE



TP/oneM2M/CSE/DIS/023
	TP Id
	TP/oneM2M/CSE/DIS/023

	Test objective
	Check that the IUT successfully performs a Discovery-based OPERATION using hierarchical
addressing form when the Desired Identifier Result Type is not provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6, TS-0004 [2], clause 7.2.3.13

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource and
the AE having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {   |  |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  |  |
                     | To set to TARGET_RESOURCE_ADDRESS and  |  |
                     | From set to AE‑ID and  |IUT <- AE |
                     | Result Content set to 11 (discovery result resource references) and  | |
                     | no Desired Identifier Result Type parameter and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |  |
                     | the IUT sends a valid Response containing  |  |
                     | Response Status Code set to 2000(OK) and  |  |
                     | Content containing  |IUT -> AE |
                     | URIList containing  | |
                     | structured addresses of discovered resources  | |
                     |} | |
+———————-+———————————————————————————————————————————————————-+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/023_CRE
	CREATE

	TP/oneM2M/CSE/DIS/023_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/023_DEL
	DELETE



TP/oneM2M/CSE/DIS/024
	TP Id
	TP/oneM2M/CSE/DIS/024

	Test objective
	Check that the IUT responds to the originator with an error when resources match the filter
criteria in a Discovery-based OPERATION request but including an invalid Content

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource
and the AE having privileges to perform DISCOVERY and OPERATION on child resource
and FILTER_CRITERIA_CONDITIONS matching the child resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from  | |
                     | AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content not being valid and  | |
                     | Filter Criteria set to FILTER_CRITERIA_CONDITIONS containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK)  | |
                     | aggregatedResponse containing  | |
                     | Response for child resource containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/024_CRE
	CREATE

	TP/oneM2M/CSE/DIS/024_UPD
	UPDATE



TP/oneM2M/CSE/DIS/025
	TP Id
	TP/oneM2M/CSE/DIS/025

	Test objective
	Check that the IUT successfully performs a Discovery-based OPERATION when resources
match the filter criteria containing geoQuery condition provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS_1 containing
location attribute not set to LOCATIONand
a child resource at CONTAINER_RESOURCE_ADDRESS_2 containing
location attribute set to LOCATION
and the AE having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteriacontaining  | |
                     | geoQuery set to LOCATION and  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_2  | |
                     |} | |
+———————-+——————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/025_CRE
	CREATE

	TP/oneM2M/CSE/DIS/025_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/025_DEL
	DELETE



TP/oneM2M/CSE/DIS/026
	TP Id
	TP/oneM2M/CSE/DIS/026

	Test objective
	Check that the IUT returns the empty content when no result matching with filter criteria
containing geoQuery condition provided in a Discovery-based OPERATION

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource containing
location attribute set to LOCATION
and the AE having privileges to perform DISCOVERY and OPERATION on child resource
and FILTER_CRITERIA_CONDITIONS not matching child resource location attribute
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteriaset to FILTER_CRITERIA_CONDITIONS containing  | |
                     | geoQuery not matching LOCATION and  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |} | |
+———————-+——————————————————————————————————————————————-+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/026_CRE
	CREATE

	TP/oneM2M/CSE/DIS/026_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/026_DEL
	DELETE



TP/oneM2M/CSE/DIS/027
	TP Id
	TP/oneM2M/CSE/DIS/027

	Test objective
	Check that the IUT responds to the originator with an error when the originator sends a
Discovery-based OPERATION request including an invalid format of filter criteria containing
geoQuery condition to discover the resource TARGET_RESOURCE_ADDRESS

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the originator AE
and the IUT having a container resource TARGET_RESOURCE_ADDRESS containing
a child resource containing
location attribute set to LOCATION
and the AE having privileges to perform DISCOVERY and_OPERATION_ on child resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | geoQuery not being valid format  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————-+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/027_CRE
	CREATE

	TP/oneM2M/CSE/DIS/027_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/027_DEL
	DELETE



TP/oneM2M/CSE/DIS/028
	TP Id
	TP/oneM2M/CSE/DIS/028

	Test objective
	Check that the IUT returns the empty content when the originator sends a Discovery-based
OPERATION request including filter criteria containing geQuery condition but resources do not
have location attribute

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource containing
no location attribute
and the AE having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteriacontaining  | |
                     | geoQuery set to LOCATION and  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————+———————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/028_CRE
	CREATE

	TP/oneM2M/CSE/DIS/028_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/028_DEL
	DELETE



TP/oneM2M/CSE/DIS/029
	TP Id
	TP/oneM2M/CSE/DIS/029

	Test objective
	Check that the IUT accepts Discovery-based OPERATION requests to the resource
TARGET_RESOURCE_ADDRESS when AE has privilege to perform the discovery operation
on the children/descendant but AE has no privilege to perform discovery operation of parent
resource TARGET_RESOURCE_ADDRESS

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS_1 and
a child resource at CONTAINER_RESOURCE_ADDRESS_2
and the AE having privileges to perform DISCOVERY and OPERATION on children
resources
and the AE having no privileges to perform DISCOVERY on parent resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     | | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_1,  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_2  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/029_CRE
	CREATE

	TP/oneM2M/CSE/DIS/029_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/029_DEL
	DELETE



TP/oneM2M/CSE/DIS/030
	TP Id
	TP/oneM2M/CSE/DIS/030

	Test objective
	Check that the IUT returns the empty content in a Discovery-based OPERATION when
resource has status marked as INACTIVE

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 1

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2 and
registrationStatus set t o 2 (INACTIVE)
and the AE2 having a resource TARGET_RESOURCE_ADDRESS containing
a child resource
and the AE1 having privileges to perform DISCOVERY and OPERATION on child resource
}



·                  +------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <- AE |
                     | the IUTreceives a valid OPERATION Request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID and  | |
                     | Filter Criteria containing  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |  | |
                     |} | |
+———————-+————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/030_CRE
	CREATE

	TP/oneM2M/CSE/DIS/030_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/030_DEL
	DELETE



TP/oneM2M/CSE/DIS/031
	TP Id
	TP/oneM2M/CSE/DIS/031

	Test objective
	Check that the IUT returns successfully appropriate list of discovered resources when resources
match the filter criteria containing geoQuery condition provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS containing
location attribute set to LOCATIONand
and the AE having privileges to perform DISCOVERY on child resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based RETRIEVE Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteriacontaining  | |
                     | geoQuery set to LOCATION and  | |
                     | filterUsageset to 1 (Discovery Criteria)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList representation  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/DIS/032
	TP Id
	TP/oneM2M/CSE/DIS/032

	Test objective
	Check that the IUT returns the empty content when no result matching with filter
criteria containing geoQuery condition provided in the request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS containing
location attribute set to LOCATION1 and
and the AE having privileges to perform DISCOVERY on child resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based RETRIEVE Request from AE  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteriacontaining  | |
                     | geoQuery set to LOCATION2 and  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList element set to empty list  | |
                     |} | |
+———————-+———————————————————————————————————————————-+————-+

TP/oneM2M/CSE/DIS/033
	TP Id
	TP/oneM2M/CSE/DIS/033

	Test objective
	Check that the IUT returns the empty address list when resources match the geoQuery filter
criteria but they do not include DISCOVERY permission

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS containing
location attribute set to LOCATIONand
and the AE not h aving privileges to perform DISCOVERY on child resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteriacontaining  | |
                     | geoQuery set to LOCATION and  | |
                     | filterUsage set to 1 (Discovery Criteria)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | URIList element set to empty list  | |
                     |} | |
+———————-+———————————————————————————————————————————–+————-+

TP/oneM2M/CSE/DIS/034
	TP Id
	TP/oneM2M/CSE/DIS/034

	Test objective
	Check that the IUT accepts a Discovery-based OPERATION request containing geoQuery filter
criteria when AE has privilege to perform the discovery operation but AE has no privilege to
perform the OPERATION request

	Reference
	TS-0001 [1], clause 8.1.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14 and clause 6.6.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS_1 containing
location attribute set to LOCATION
a child resource at CONTAINER_RESOURCE_ADDRESS_2 containing
location attribute set to LOCATION
and the AE having privileges to perform DISCOVERY on children resources
and the AE not h aving privileges to perform OPERATION on children resources
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from  | |
                     | AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria containing  | |
                     | geoQuery set to LOCATION  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT -> AE |
                     | the IUT does not perform OPERATION  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK)  | |
                     | aggregatedResponse containing  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_1  | |
                     | containing  | |
                     | Response Status Code set to 4103 (ACCESS_DENIED)  | |
                     | Response for CONTAINER_RESOURCE_ADDRESS_2  | |
                     | containing  | |
                     | Response Status Code set to 4103 (ACCESS_DENIED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/034_CRE
	CREATE

	TP/oneM2M/CSE/DIS/034_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/034_DEL
	DELETE



TP/oneM2M/CSE/DIS/035
	TP Id
	TP/oneM2M/CSE/DIS/035

	Test objective
	Check that the IUT returns the empty content when resources match the geoQuery filter criteria
but they do not include Discovery-based OPERATION permission.

	Reference
	TS-0001 [1], clause 9.6.2.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
a child resource at CONTAINER_RESOURCE_ADDRESS_1 containing
location attribute set to LOCATION
and the AE not having privileges to perform DISCOVERY on child resource
and the AE having privileges to perform OPERATION on child resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria containing  | |
                     | geoQuery set to LOCATION  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |  | |
                     |} | |
+———————-+————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/035_CRE
	CREATE

	TP/oneM2M/CSE/DIS/035_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/035_DEL
	DELETE



TP/oneM2M/CSE/DIS/036
	TP Id
	TP/oneM2M/CSE/DIS/036

	Test objective
	Check that the IUT accepts a Discovery-based OPERATION request to the resource
TARGET_RESOURCE_ADDRESS when AE has no privilege to perform the discovery
operation

	Reference
	TS-0001 [1], clause 9.6.2.3 and clause 10.2.6.4, TS-0004 [2], clause 7.3.3.14

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource TARGET_RESOURCE_ADDRESS containing
child resources
and the AE not having privileges to perform DISCOVERY on child resources
and the AE not having privileges to perform OPERATION on child resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <- AE |
                     | the IUT receives a valid Discovery‑based OPERATION Request from  | |
                     | AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria containing  | |
                     | geoQuery set to LOCATION  | |
                     | filterUsage set to 4 (Discovery‑based Operation)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT -> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | aggregatedResponse containing empty list  | |
                     |  | |
                     |} | |
+———————-+———————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/DIS/036_CRE
	CREATE

	TP/oneM2M/CSE/DIS/036_UPD
	UPDATE

	TP/oneM2M/CSE/DIS/036_DEL
	DELETE



7.2.2.7	Location (LOC)
7.2.2.7.1	CREATE Operation
TP/oneM2M/CSE/LOC/CRE/001
	TP Id
	TP/oneM2M/CSE/LOC/CRE/001

	Test objective
	Check that the IUT rejects the creation of the locationPolicy resource when locationSource attribute is set by Network Based and Location Server is not reachable

	Reference
	TS-0001 [1], clause 8.5 and clause 10.2.9, TS-0004 [2], clause 7.4.10

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUThaving no connection to Location Server
and the IUT having a CSEBase resource allowing
the AE to perform CREATE operation and
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid CREATE Request from AE containing
To set to CSEBASE_RESOURCE_ADDRESS and
From set to AE-ID and
Content containing
locationPolicy resource representation
}
	IUT <= AE

	
	then {
the IUT does not create the locationPolicy resource
and the IUT sends a valid Response containing
Response Status Code set to 4000 (BAD_REQUEST)
}
	IUT => AE



TP/oneM2M/CSE/LOC/CRE/002
	TP Id
	TP/oneM2M/CSE/LOC/CRE/002

	Test objective
	Check that the IUT accepts the creation of locationPolicy resource with locationSource attribute and locationUpdatePeriod attribute provided

	Reference
	TS-0001 [1], clause 10.2.9.2, TS-0004 [2], clause 7.4.11.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 10 (locationPolicy) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |locationSource attributeset to 1 (Network_based) and  | |
                     |valid locationUpdatePeriod attribute and  | |
                     |valid locationTargetID attributeand  | |
                     |valid locationServer attribute   | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT c reates the locationPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+———————————————————————————————————————————+————-+
TP/oneM2M/CSE/LOC/CRE/003
	TP Id
	TP/oneM2M/CSE/LOC/CRE/003

	Test objective
	Check that the IUT rejects the creation of locationPolicy resource when AE has no privilege to perform the creation request for the locationPolicy resource

	Reference
	TS-0001 [1], clause 10.2.9.2, TS-0004 [2], clause 7.4.10.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the originator AE
and the AE having no privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     |the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 10 (locationPolicy) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |locationSource attribute set to 1 (Network_based) and  | |
                     |valid locationUpdatePeriod attribute and  | |
                     |valid locationTargetID attributeand  | |
                     |valid locationServer attribute  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the locationPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/LOC/CRE/004
	TP Id
	TP/oneM2M/CSE/LOC/CRE/004

	Test objective
	Check that the IUT responds with an error when receiving a creation request of locationPolicy resource target to the TARGET_RESOURCE_ADDRESS which does not exist in the Hosting CSE

	Reference
	TS-0001 [1], clause 10.2.9.2, TS-0004 [2], clause 7.4.10.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the originator AE
and the IUT having not yet created a resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     |the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 10 (locationPolicy) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |locationSource attributeset to 1 (Network_based) and  | |
                     |valid locationUpdatePeriod attribute and  | |
                     |valid locationTargetID attributeand  | |
                     |valid locationServer attribute  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the locationPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/LOC/CRE/005
	TP Id
	TP/oneM2M/CSE/LOC/CRE/005

	Test objective
	Check that the IUT creates a container resource with CONTAINER_NAME included in the associated locationPolicy create request

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.10.2.1, TS-0004 [2], clause 7.3.3.3 and clause 7.4.11.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having no created container having
resourceName set to CONTAINER_NAME
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | ResourceType set to 10 (locationPolicy) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | locationContainerName attribute set to CONTAINER_NAME  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT creates the container resource with Content containing  | |
                     | container resource representation containing  | |
                     | resourceName attribute set to CONTAINER_NAME and  | |
                     | locationID attribute set to resourceID of the associated locationPolicy resource  | |
                     |and the IUT c reates the locationPolicy resource with Content containing  | |
                     | locationPolicy resource representation containing  | |
                     | locationContainerName attribute set to CONTAINER_NAME  | |
                     | and locationContainerId attribute set to resourceID of the created container resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
	Note that the IUT sets the locationContainerID attribute in locationPolicy resource to the resourceID of the created <container> resource



TP/oneM2M/CSE/LOC/CRE/006
	TP Id
	TP/oneM2M/CSE/LOC/CRE/006

	Test objective
	Check that the IUT creates a subscription resource with SUBSCRIPTION_NAME provided by the originator as a child resource of the container linked with a locationPolicy resource

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.9.2, TS-0004 [2], clause 7.3.3.3 and clause 7.4.10.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
resourceID set to NOTI_URI_ADDRESS
and the IUThaving created a resource LOCATIONPOLICY_ADDRESS of type <locationPolicy > containing
locationUpdatePeriod set to POSITIVE_UPDATE_PERIOD and
locationSource set to 1 (Network_based) and
locationTargetID set to LOCATION_TARGET_ID and
locationServer set to LOCATION_SERVER_ADDRESS and
locationContainerID set to CONTAINER_ADDRESSand
and the IUT having created a resource CONTAINER_ADDRESS of type <container > containing
locationID set to LOCATIONPOLICY_ADDRESS
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS

}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | ResourceType set to 23 (subscription) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |notificationURI attribute set to NOTI_URI_ADDRESS and  | |
                     |eventNotificationCriteria attribute containing  | |
                     | notificationEventType element set to 3 (Create_of_Direct_Child_Resource)  | |
                     | and notificationContentType attribute set to 1 (All Attributes)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT creates the subscription resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED) and  | |
                     |Content containing  | |
                     | subscription resource representation  | |
                     |} | |
	Note that the IUT sets the locationContainerID attribute in <locationPolicy> resource to the resourceID of the created <container> resource



TP/oneM2M/CSE/LOC/CRE/007
	TP Id
	TP/oneM2M/CSE/LOC/CRE/007

	Test objective
	Check that IUT accepts the creation of a locationPolicy resource with attribute locationSource set to Device-based and locationUpdatePeriod set to POSITIVE_UPDATE_PERIOD

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.9.2, TS-0004 [2], clause 7.3.3.3 and clause 7.4.10.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having location positioning modules
and the originator being a PX_ASN_AE
and the IUT being a PX_ASN_CSE
and the IUT having registered the PX_ASN_AE
and the ASN-AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= ASN‑AE|
                     |the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 10 (locationPolicy) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |locationSource attributeset to 2 (Device_based) and  | |
                     |locationUpdatePeriod attribute set to POSITIVE_UPDATE_PERIOD  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => ASN‑AE|
                     | the IUT creates the locationPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | locationPolicy resource representation  | |
                     |} | |
+———————-+————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/LOC/CRE/008
	TP Id
	TP/oneM2M/CSE/LOC/CRE/008

	Test objective
	Check that the IUT accepts the creation of a locationPolicy resource with attribute locationSource set to Sharing-based

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.9.2, TS-0004 [2], clause 7.3.3.3 and clause7.4.10.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the originator being a PX_ADN_AE
and the IUT being a PX_MN_CSE
and the ADN-AE being no location positioning modules deployed
and the ADN-AE being no Network-based positioning capabilities
and the IUT having registered the PX_ADN_AE
and the ADN-AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= ADN‑AE|
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 10 (locationPolicy) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |locationSource attributeset to 3 (Sharing_based)  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => ADN‑AE|
                     | the IUT creates the locationPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | locationPolicy resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————————-+————-+
TP/oneM2M/CSE/LOC/CRE/009
	TP Id
	TP/oneM2M/CSE/LOC/CRE/009

	Test objective
	Check that the IUT rejects the creation of the locationPolicy resource when locationSource attribute is set to Network-Based and neither locationTargetID nor locationServer is provided.

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.9.2, TS-0004 [2], clause 7.3.3.3 and clause7.4.10.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 10 (locationPolicy) and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     |locationSource attributeset to 1 (Network_based)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the locationPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————+————-+
7.2.2.7.2	UPDATE Operation
TP/oneM2M/CSE/LOC/UPD/001
	TP Id
	TP/oneM2M/CSE/LOC/UPD/001

	Test objective
	Check that the IUT rejects AE to update the locationPolicy resource identified with LOCATION_ID when receiving an update request containing an invalid attribute

	Reference
	TS-0001 [1], clause 10.2.9.4, TS-0004 [2], clause 7.3.3.4 and clause 7.4.10.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type locationPolicy containing
an optional RW attribute locationUpdatePeriod
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives an UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |Content containing  | |
                     |locationUpdatePeriod attribute set to INVALID_LOCATION_UPDATE_PERIOD  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not update the locationPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————-+————-+
7.2.2.7.3	RETRIEVE Operation
TP/oneM2M/CSE/LOC/RET/001
	TP Id
	TP/oneM2M/CSE/LOC/RET/001

	Test objective
	Check that the IUT responds with a container resource containing attribute locationID set to resourceID of the associated locationPolicy resource

	Reference
	TS-0001 [1], clause 10.2.9.3, TS-0004 [2], clause 7.4.10.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUThaving created a resource LOCATIONPOLICY_ADDRESS of type locationPolicy containing
locationContainerID attribute set to TARGET_RESOURCE_ADDRESSand
locationSource attribute set to 1 (Network_based) and
locationTargetID attributeset to LOCATION_TARGET_ID and
locationServer attribute set to LOCATION_SERVER_ADDRESS
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type container containing
locationID attribute set to LOCATIONPOLICY_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2000 (OK) and  | |
                     |Content containing  | |
                     | container resource containing  | |
                     | locationID attribute set to LOCATIONPOLICY_ADDRESS  | |
                     |} | |
+———————-+————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/LOC/RET/002
	TP Id
	TP/oneM2M/CSE/LOC/RET/002

	Test objective
	Check that the IUT sends a notification message including the location Information to the originator when the originator sends a retrieve request target to the <latest> resource of CONTAINER_ADDRESS container associated with a <locationPolicy> resource

	Reference
	TS-0001 [1], clause 8.5.2,clause 10.2.9.3 and clause 10.2.10.2.2, TS-0004 [2], clause 7.4.10.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUThaving created a resource LOCATIONPOLICY_ADDRESS of type locationPolicy containing
locationContainerID attribute set to CONTAINER_ADDRESSand
locationUpdatePeriod attribute set to ZERO (or NULL) and
locationSource attribute set to LOCATION_SOURCE

and the IUT having created a resource CONTAINER_ADDRESS of type <container > containing
locationID attribute set to LOCATIONPOLICY_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource CONTAINER_ADDRESS
and the AE having created a resource of type subscription as a child of the resource CONTAINER_ADDRESS of type container
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a RETRIEVE Request from AE containing  | |
                     | To set to CONTAINER_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid NOTIFY Response containing  | |
                     |Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | notification attribute containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | contentInstance resource containing location information  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	Reference
	LOCATION_SOURCE

	TP/oneM2M/CSE/LOC/RET/002_LOS/1
	TS-0001 [1], clause 9.6.10 and 10.2.9TS-0004 [2], clause 7.4.10 and 6.3.4.2.3
	1 (Network_based)

	TP/oneM2M/CSE/LOC/RET/002_LOS/2
	ROWSPAN
	2 (Device_based)

	TP/oneM2M/CSE/LOC/RET/002_LOS/3
	ROWSPAN
	3 (Sharing_based)



TP/oneM2M/CSE/LOC/RET/003
	TP Id
	TP/oneM2M/CSE/LOC/RET/003

	Test objective
	Check that the IUT responds with a <locationPolicy> resource containing attribute locationContainerID set to resourceID of the associated <container> resource

	Reference
	TS-0001 [1], clause 10.2.9.3, TS-0004 [2], clause 7.4.10.2.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUThaving created a resource TARGET_RESOURCE_ADDRESS of type locationPolicy containing
locationContainerID attribute set to CONTAINER_ADDRESSand
locationSource attribute set to 1 (Network_based) and
locationTargetID attributeset to LOCATION_TARGET_ID and
locationServer attribute set to LOCATION_SERVER_ADDRESS
and the IUT having created a resource CONTAINER_ADDRESS of type container containing
locationID attribute set to TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS

}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2000 (OK) and  | |
                     |Content containing  | |
                     | locationPolicy representation containing  | |
                     |locationContainerID attribute set to CONTAINER_ADDRESS  | |
                     |} | `|
+———————-+———————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/LOC/RET/004
	TP Id
	TP/oneM2M/CSE/LOC/RET/004

	Test objective
	Check that the IUT sets the locationStatus attribute with the error status code in the locationPolicy resource when the location information of the requested node is failed to be retrieved due to NSE

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.9.3, TS-0004 [2], clause 7.4.10.2.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUThaving created a resource TARGET_RESOURCE_ADDRESS of type locationPolicy
and the AE having privileges to perform RETRIEVE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2000 (OK) and  | |
                     |Content containing  | |
                     | locationPolicy representationcontaining  | |
                     | locationStatus attribute set to LOCATION_PROTOCOL_SPECIFIC_RESULT_CODE  | |
                     |} | |
	Note: the error status code LOCATION_PROTOCOL_SPECIFIC_RESULT_CODE is location protocol specific, e.g. in OMA Mobile Location Protocol the reslt code is set to 6 indicating POSITION METHOD FAILURE.
Note that the failure is caused by the NSE such as location server.



TP/oneM2M/CSE/LOC/RET/005
	TP Id
	TP/oneM2M/CSE/LOC/RET/005

	Test objective
	Check that the IUT responds with an error message "NOT_FOUND" when receiving a retrieve request target to an non-existing locationPolicy resource

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.9.3, TS-0004 [2], clause 7.3.3.2 and clause 7.4.10.2.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUThaving not created LOCATIONPOLICY_ADDRESS of type locationPolicy under the AE a resource
and the IUT having privileges to perform RETRIEVE operation on locationPolicy resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a RETRIEVE Request from AE containing  | |
                     | To set to LOCATIONPOLICY_ADDRESSand  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4004 (NOT_FOUND)  | |
                     |} | |
+———————-+————————————————————————————————————————————–+————-+
7.2.2.7.4	NOTIFY Operation
TP/oneM2M/CSE/LOC/NTF/001
	TP Id
	TP/oneM2M/CSE/LOC/NTF/001

	Test objective
	Check that the IUT sends a notification message including the location Information to the originator with frequency of POSITIVE_UPDATE_PERIOD set in field of_locationUpdatePeriod_

	Reference
	TS-0001 [1], clause 8.5.2 and clause 10.2.10.1.1, TS-0004 [2], clause 7.3.3.3 and clause 7.4.11.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the originator being a ADN-AE
and the IUT being a MN-CSE
and the ADN-AE being no location positioning modules deployed
and the ADN-AE being no Network-based positioning capabilities

and the IUT having registered the ADN-AE
and the IUT having created ORIGINATOR_LOCATIONPOLICY_ADDRESS of type locationPolicy containing
locationContainerID attribute set to ORIGINATOR_CONTAINER_ADDRESS
and locationUpdatePeriod attribute set to POSITIVE_UPDATE_PERIOD
and locationSource attribute set to 3 (Sharing-based)
and the IUThaving created ORIGINATOR_CONTAINER_ADDRESS of type container containing
locationID attribute set to ORIGINATOR_LOCATIONPOLICY_ADDRESS
and the IUThaving created a resource of type subscription as a child resource of ORIGINATOR_CONTAINER_ADDRESS of type container
and the IUT having registered a Node
being a minimum hop with the originator compared to other nodes registered with the hosting CSE
and the IUThaving created under the Node a child resource CLOSEST_NODE_CONTAINER_ADDRESS of type <container> containing
a latest contentInstance resource containing
the latest location information
and the IUT having privileges to perform RETRIEVE operation on the resource CLOSEST_NODE_CONTAINER_ADDRESS of type of container

}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a latest resource of container from the CLOSEST_NODE_CONTAINER_ADDRESS containing  | |
                     | latest location information  | |
                     |and the IUT creates a contentInstance as a child resource of ORIGINATOR_CONTAINER_ADDRESS of type <container> containing  | |
                     |the location information that retrieved  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => ADN‑AE|
                     |the IUT sends a valid Response containing  | |
                     |Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | notification representation containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | contentInstance resource containing  | |
                     |location information  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/LOC/NTF/002
	TP Id
	TP/oneM2M/CSE/LOC/NTF/002

	Test objective
	Check that the IUT sends a notification message including the location Information to the originator with frequency of POSITIVE_UPDATE_PERIOD set in field of locationUpdatePeriod

	Reference
	TS-0001 [1], clause 8.5.2, clause 10.2.10.1.1 and clause 10.2.10.2.2, TS-0004 [2], clause 7.4.11.2

	Parent Release
	Release 3

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUThaving created a resource LOCATIONPOLICY_ADDRESS of type locationPolicy containing
locationContainerID attribute set to CONTAINER_ADDRESSand
locationUpdatePeriod attribute set to POSITIVE_UPDATE_PERIOD and
locationSource attribute set to LOCATION_SOURCE
and the IUT having created a resource CONTAINER_ADDRESS of type container containing
locationID attribute set to LOCATIONPOLICY_ADDRESS
and the AE having created a resource of type subscription as a child of the resource CONTAINER_ADDRESS of type container
and the IUT having privileges to retrieve the location information from the NSE
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= NSE |
                     | the IUT receives a valid Response from NSE containing  | |
                     | location‑protocol‑specific‑result‑code of positioning procedure execution and  | |
                     |location‑response containing  | |
                     |location information  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     |the IUT transforms the location‑response into a oneM2M Response primitive and sends a valid NOTIFY Response containing  | |
                     |Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | notification representation containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | contentInstance representation  | |
                     |} | |
	Note that: the attribute location-protocol-specific-result-code and location-response are location acquisition protocol specific and the exact name of these two attributes have to follow the specification of corresponding location protocol e.g. OMA Mobile Location Protocol.



Table Referenced values for parameter LOCATION_SOURCE
	TP Id
	Reference
	LOCATION_SOURCE

	TP/oneM2M/CSE/LOC/NTF/010_LOS/1
	TS-0001 [1], clause 9.6.10 and 10.2.10TS-0004 [2], clause 7.4.11 and 6.3.4.2.3
	1 (Network_based)

	TP/oneM2M/CSE/LOC/NTF/010_LOS/2
	ROWSPAN
	2 (Device_based)

	TP/oneM2M/CSE/LOC/NTF/010_LOS/3
	ROWSPAN
	3 (Sharing_based)



Table Referenced values for parameter location-protocol-specific-result-code and location-response
	location-protocol-specific-result-code
	location-response
	Location protocol
	Reference

	[Result code]
	[Content]
	OMA Mobile Location Protocol
	Not Present

	[HTTP Response code]
	<TerminalLocation > representation containingattributes address indicating the address of targeted node where location information is retrieved_, locationRetrievalStatus_ indicating the status of retrieval of the location information for the target node , and_currentLocation_ containing the actual location data of the target node
	OMA RESTful NetAPI
	TS-0004 [2], Annex G

	[HTTP Response code]
	<SubscriptionNotification > representation
	OMA RESTful NetAPI
	Location Server Open RESTful API Specification



7.2.2.8	Device Management (DMG)
7.2.2.8.1	Resource timeSeries (TS)
TP/oneM2M/CSE/TS/001
	TP Id
	TP/oneM2M/CSE/TS/001

	Test objective
	Check that the IUT inserts the dataGenerationTime informantion of a missing data point and increases the missingDataCurrentNr attribute when a missing data point is detected

	Reference
	TS-0001 [1], clause 10.2.39, TS-0004 [2], clause 7.5.1.2.9

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having created a timeSeries resource containing
missingDataDetect attribute set to true and
a valid periodicInterval attribute
and the AE having privileges to perform RETRIEVE operation on the timeSeries resource
and the IUT having detected a missing data point
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TIMESERIES_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | timeSeries resourcecontaining  | |
                     | missingDataList attribute containing  | |
                     | dataGenerationTime element of the missing data point and  | |
                     | missingDataCurrentNr attributeset to one  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/TS/002
	TP Id
	TP/oneM2M/CSE/TS/002

	Test objective
	Check that the IUT removes the oldest element in MissingDataList when MissingDataCurrentNr reaches MissingDataMaxNr to enable insertion of a new missing data point

	Reference
	TS-0001 [1], clause 10.2.39, TS-0004 [2], clause 7.5.1.2.9

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having created a timeSeries resource containing
missingDataDetect attribute set to true and
a valid periodicInterval attribute
missingDataMaxNr attributeset to one
and the AE having privileges to perform RETRIEVE operation on the timeSeries resource
and the IUT having detected a missing data point
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUTdetects a new missing data pointand   | |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TIMESERIES_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | timeSeries resourcecontaining  | |
                     | missingDataList attribute containing  | |
                     | dataGenerationTime element of the new missing data point and  | |
                     | missingDataCurrentNr attributeset to one  | |
                     |} | |
+———————-+——————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/TS/003
	TP Id
	TP/oneM2M/CSE/TS/003

	Test objective
	Check that the IUT sends a notification with missing data points information when the number of missing data points detected becomes equal to the minimum specified missing number of the Time Series Data specified in missingData condition of the subscription resource

	Reference
	TS-0001 [1], clause 10.2.39, TS-0004 [2], clause 7.5.1.2.9

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a timeSeries resource containing
missingDataDetect attribute set to true and
a valid periodicInterval attribute and
a subscription resource containing
notificationURI attribute set to AE1_RESOURCE_ADDRESS and
eventNotificationCriteria attribute containing
missingData element containing
number element set to MISSING_DATA_POINT_NR and
duration element set to MISSING_DATA_POINT_DURATION
and the AE1 having privileges to perform RETRIEVE operation on the timeSeries resource
and the AE2 having privileges to perform CREATE operation on the timeSeries resource
and the IUT having detected MISSING_DATA_POINT_NR-1 missing data points from AE2
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT detects a new missing data point within MISSING_DATA_POINT_DURATION timer  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid NOTIFY request containing  | |
                     | Content containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | timeSeries resourcecontaining  | |
                     | missingDataList attributecontaining  | |
                     | dataGenerationTime of missing data points and  | |
                     | currentMissingDataNr attributeset to MISSING_DATA_POINT_NR  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/TS/004
	TP Id
	TP/oneM2M/CSE/TS/004

	Test objective
	Check that the IUT does not send notification when the total number of missing data points does not exceed the minimum specified missing number of the Time Series Data specified in missingData condition of the subscription resource during the window duration specified in the same missingData condition

	Reference
	TS-0001 [1], clause 10.2.39, TS-0004 [2], clause 7.5.1.2.9

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a timeSeries resource containing
missingDataDetect attribute set to true and
a valid periodicInterval attribute and
a subscription resource containing
notificationURI attribute set to AE1_RESOURCE_ADDRESS and
eventNotificationcriteria attribute containing
missingData element containing
number element set to MISSING_DATA_POINT_NR and
duration element set to MISSING_DATA_POINT_DURATION
and the AE1 having privileges to perform RETRIEVE operation on the timeSeries resource
and the AE2 having privileges to perform CREATE operation on the timeSeries resource
and the IUT having detected MISSING_DATA_POINT_NR-1 missing data points from AE2
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT does not detect a new missing data point within MISSING_DATA_POINT_DURATION timer  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT does not sends a NOTIFY request and  | |
                     | the IUT restarts missing data point counter and timer  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————————————————-+————-+ Editor's Note: This test case is not available on the ATS. Currently no idea to implementate internal timer, but will try to find a way to solve this problem.
TP/oneM2M/CSE/TS/005
	TP Id
	TP/oneM2M/CSE/TS/005

	Test objective
	Check that the IUT sends a final notification with the missing data points information when subscription is terminated

	Reference
	TS-0001 [1], clause 10.2.39, TS-0004 [2], clause 7.5.1.2.9

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having created a timeSeries resource containing
missingDataDetect attribute set to true and
a valid periodicInterval attribute and
a subscription resource containing
notificationURI attribute set to AE1_RESOURCE_ADDRESS and
eventNotificationcriteria attribute containing
missingData element containing
number element set to MISSING_DATA_POINT_NR and
duration element set to MISSING_DATA_POINT_DURATION
and the AE1 having privileges to perform RETRIEVE operation on the timeSeries resource
and the AE1 having privileges to perform DELETE operation on the subscription resource
and the AE2 having privileges to perform CREATE operation on the timeSeries resource
and the IUT having detected MISSING_DATA_POINT_NR-1 missing data points from AE2
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid DELETE Request from AE1 containing  | |
                     | To set to SUBSCRIPTION_RESOURCE_ADDRESS and  | |
                     | From set to AE1‑ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |  |
                     | the IUT sends a valid Response containing  |IUT => AE1  |
                     | Response Status Code set to 2000 (OK) and  |  |
                     | and the IUT sends a NOTIFY Request contaning  |IUT => AE2  |
                     | Content containing  |  |
                     | notificationEvent attribute containing  |  |
                     | representation attribute containing  |  |
                     | timeSeries resourcecontaining  |  |
                     | missingDataList attributecontaining  |  |
                     | dataGenerationTime of missing data points and  |  |
                     | currentMissingDataNr attributeset to MISSING_DATA_POINT_NR - 1  | |
                     |} | |
+———————-+———————————————————————————————————————————————-+————-+

7.2.2.9	Communication Management and Delivery Handling(CMDH)
7.2.2.9.1	Resource pollingChannel (PCH)
TP/oneM2M/CSE/PCH/001
	TP Id
	TP/oneM2M/CSE/PCH/001

	Test objective
	Check that the IUT which hosts <pollingChannel> resource forwards a Notify request successfully to a target AE, once the IUT receives a polling request from AE (retrieve request to <pollingChannelURI> resource)
See the Note below.

	Reference
	TS-0001 [1], clause 10.2.13.6, TS-0004 [2], clause 7.4.22.2.2

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having register ed an AE1
and the AE having a child <pollingChannel> resource
and the IUT having re ceived a retrieve request from the AE containing
To set to POLLINGCHANNELURI_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a NOTIFY Request from the CSE containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID } | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT send s a RETRIEVE Response to the AE containing  | |
                     |Response Status Code set to 2000 (OK)  | |
                     |Contentcontaining  | |
                     | the request re ceived from the CSE  | |
                     |} | |
	Note: Based on figure 10.2.5.12-1 in TS-0001[1] step 001, 002 and 003 in order.
In this case, IUT is pending AE's polling request since there was no request to AE



TP/oneM2M/CSE/PCH/002
	TP Id
	TP/oneM2M/CSE/PCH/002

	Test objective
	Check that the IUT which hosts <pollingChannel> resource forwards a Notify request successfully to a target AE, once the IUT receives a polling request from the AE

	Reference
	TS-0001 [1], clause 10.2.13.6, TS-0004 [2], clause 7.4.22.2.2

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having register ed an AE
and the AE having a child <pollingChannel> resource
and the IUT having receive d a NOTIFY Request from CSE containing
To set to AE_RESOURCE_ADDRESS and
From set to CSE_ID
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a retrieve Request from the AE containing  | |
                     | To set to POLLINGCHANNELURI _RESOURCE_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT send s a Response to the AE containing  | |
                     |Response Status Code set to 2000 (OK)  | |
                     |Contentcontaining  | |
                     | the Request re ceived from the CSE  | |
                     |} | |
	Note: Based on figure 10.2.13.1-1 in TS-0001[1] step 002 is followed by 001 and 003
The CSE's request to AE is pended and will be sent as soon as AE sends polling request to CSE.



TP/oneM2M/CSE/PCH/003
	TP Id
	TP/oneM2M/CSE/PCH/003

	Test objective
	Check that the IUT performs both forwarding the response to the CSE and sending response to AE after receiving a Notify Request from the AE sent to the <pollingChannelURI> resource

	Reference
	TS-0001 [1], clause 10.2.13.8, TS-0004 [2], clause 7.4.22.2.2

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having register ed an AE
and the AE1 having a child <pollingChannel> resource
and the IUT having re ceived a retrieve Request from the AE containing
To set to POLLINGCHANNELURI_RESOURCE_ADDRESS
and the IUT having re ceived a NOTIFY Request from the CSE containing
To set to AE_RESOURCE_ADDRESS and
From set to CSE_ID
and the IUT send s a Response to the AE containing
Response Status Code set to 2000 (OK)
Contentcontaining
the Request re ceived from the CSE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a NOTIFY Request from the AE containing  | |
                     | To set to POLLINGCHANNELURI_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE  |
                     | the IUT sends a Response to the CSE  |IUT => AE |
                     |Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |the IUT sends the valid NOTIFY Response to the AE  | |
                     |} | |
	Note: Based on figure 10.2.13.1-1 in TS-0001[1] step 005 and 006



TP/oneM2M/CSE/PCH/004
	TP Id
	TP/oneM2M/CSE/PCH/004

	Test objective
	Check that the IUT which performs polling sends the Notify request to <pollingChannelURI> Hosting CSE after receiving response using polling channel

	Reference
	TS-0001 [1], clause 10.2.13.8, TS-0004 [2], clause 7.4.22.2.5

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered to a CSE
and the IUT having a <pollingChannel> resource
and the IUT having sent a retrieve Request to the CSE
To set to POLLINGCHANNELURI_RESOURCE_ADDRESS
and the CSE having re ceived the Request containing
To set to CSE_RESOURCE_ADDRESS and
From set to ORIGINATOR_ID
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE1 |
                     | the IUT receives a polling Response from the CSE containing  | |
                     |Response Status Code set to 2000 (OK)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a NOTIFY Request to the CSE containing  | |
                     | To set to POLLINGCHANNELURI_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
	Note: Based on figure 10.2.13.1-1 in TS-0001[1] step 004 and 005



TP/oneM2M/CSE/PCH/005
	TP Id
	TP/oneM2M/CSE/PCH/005

	Test objective
	Check that the IUT rejects a <pollingChannel> OPERATION of the AE when AE-ID is not same as the AE-ID of the parent resource

	Reference
	TS-0001 [1], clause 10.2.13.2, TS-0004 [2], clause 7.4.21

	Config Id
	CF01

	Parent Release

	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having register ed an AE1
and the IUT having registered an AE2
and the IUThaving created a pollingChannel resource on the AE1
}



·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE2 |
                     |the IUT receives a valid OPERATION Request from the AE2 containing  | |
                     | To set to POLLING_CHANNEL_RESOURCE_ADDRESS and  | |
                     | From set to AE2_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE2 |
                     | the IUT send s a valid Response containing  | |
                     |Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+——————————————————————————————————————–+————-+
	TP Id
	Reference
	OPERATION

	TP/oneM2M/CSE/PCH/005_RET
	TS-0001 10.2.13.3
	RETRIEVE

	TP/oneM2M/CSE/PCH/005_UPD
	TS-0001 10.2.13.4
	UPDATE

	TP/oneM2M/CSE/PCH/005_DEL
	TS-0001 10.2.13.5
	DELETE



TP/oneM2M/CSE/PCH/006
	TP Id
	TP/oneM2M/CSE/PCH/006

	Test objective
	Check that the IUT sends the response with a status to the CSE1 when the request expires according to its Request Expiration Timestamp

	Reference
	TS-0001 [1], clause 10.2.13.6

	Config Id
	CF02

	Parent Release
	Release 2

	PICS Selection
	PICS_PCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having register ed an AE
and the AE having a child <pollingChannel> resource
and the IUT having receive d a RETRIEVE Request from AE containing
To set to POLLINGCHANNELURI_RESOURCE_ADDRESS and Request Expiration Timestamp set to VALUE
}



·                  +-------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | Request Expiration Timestamp expires  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | and the IUT sends a Response to the AE containing  | |
                     |Response Status Code set to 4008 (REQUEST_TIMEOUT)  | |
                     |} | |
+———————-+————————————————————————————————————————-+————-+
7.2.2.9.2	Response Type (RT)
7.2.2.9.2.1	nonBlockingRequestSynch (NBS)
TP/oneM2M/CSE/RT/NBS/001
	TP Id
	TP/oneM2M/CSE/RT/NBS/001

	Test objective
	Check that the IUT rejects a Non-Blocking Synchronous Request OPERATION if the IUT does not support the <request> resource

	Reference
	TS-0001 [1], clause 8.2.2.2

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_SYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}




·                  +------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | Resource Type set to 3 (container)and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | ResponseType set to 1 (nonBlockingRequestSynch)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5206 (NON_BLOCKING_REQUEST_NOT_SUPPORTED)  | |
                     |} | |
+———————-+——————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/RT/NBS/001_CRE
	CREATE

	TP/oneM2M/CSE/RT/NBS/001_UPD
	UPDATE

	TP/oneM2M/CSE/RT/NBS/001_RET
	RETRIEVE

	TP/oneM2M/CSE/RT/NBS/001_DEL
	DELETE



Editor's Note: Need to be clarified that does it make sense to have such TPs on the NBR group when no support of NBR from the IUT is required.
TP/oneM2M/CSE/RT/NBS/002
	TP Id
	TP/oneM2M/CSE/RT/NBS/002

	Test objective
	Check that the IUT responds to a Non-Blocking Synchronous Request OPERATION with the reference of a <request> resource provided within the Content parameter of the Response

	Reference
	TS-0001 [1], clause 8.2.2.1

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_SYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS
}




·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | Resource Type set to 3 (container)and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | ResponseType set to 1 (nonBlockingRequestSynch)  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 1001 (ACCEPTED for n onBlockingRequestSynch) and  | |
                     | Content containing  | |
                     | URI attribute set to REQUEST_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/RT/NBS/002_CRE
	CREATE

	TP/oneM2M/CSE/RT/NBS/002_UPD
	UPDATE

	TP/oneM2M/CSE/RT/NBS/002_RET
	RETRIEVE

	TP/oneM2M/CSE/RT/NBS/002_DEL
	DELETE



TP/oneM2M/CSE/RT/NBS/003
	TP Id
	TP/oneM2M/CSE/RT/NBS/003

	Test objective
	Check that the IUT returns successfully the <request> resource after receiving a Non-Blocking Synchronous Request OPERATION and it contains the expected result in operationResult attribute

	Reference
	TS-0001 [1], clause 8.2.2.2

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_SYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having received a Non-Blocking Synchronous Request OPERATION
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type <request> under the AE resource
}




·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | ResponseTypeset to 3 (blockingRequest)  | |
                     |no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | request resource representation containing  | |
                     | operationResult attribute containing  | |
                     | expected response to OPERATION  | |
                     |  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/RT/NBS/003_CRE
	CREATE

	TP/oneM2M/CSE/RT/NBS/003_UPD
	UPDATE

	TP/oneM2M/CSE/RT/NBS/003_RET
	RETRIEVE

	TP/oneM2M/CSE/RT/NBS/003_DEL
	DELETE



7.2.2.9.2.2	nonBlockingRequestAsynch (NBA)
TP/oneM2M/CSE/RT/NBA/001
	TP Id
	TP/oneM2M/CSE/RT/NBA/001

	Test objective
	Check that the IUT responds to a Non-Blocking Asynchronous Request OPERATION without a reference to a resource containing the context of the request if the IUT does not support the <request> resource

	Reference
	TS-0001 [1], clause 8.2.2.3

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_ASYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS
}




·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | Resource Type set to 3 (container)and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | ResponseType set to 2 (nonBlockingRequestAsynch)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     |the IUT sends a valid Response containing  | |
                     | Response Status Code set to 1002 (ACCEPTED for nonBlockingRequestAsynch) and  | |
                     | no Content  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/RT/NBA/001_CRE
	CREATE

	TP/oneM2M/CSE/RT/NBA/001_UPD
	UPDATE

	TP/oneM2M/CSE/RT/NBA/001_RET
	RETRIEVE

	TP/oneM2M/CSE/RT/NBA/001_DEL
	DELETE



Editor's Note: Need to be clarified that does it make sense to have such TPs on the NBR group when no support of NBR from the IUT is required.
TP/oneM2M/CSE/RT/NBA/002
	TP Id
	TP/oneM2M/CSE/RT/NBA/002

	Test objective
	Check that the IUT responds to a Non-Blocking Asynchronous Request OPERATION with the reference of a <request> resource provided within the Content parameter of the Response

	Reference
	TS-0001 [1], clause 8.2.2.2

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_ASYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS
}




·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | Resource Type set to 3 (container)and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | ResponseType set to 2 (nonBlockingRequestAsynch)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 1002 (ACCEPTED for nonBlockingRequestAsynch) and  | |
                     | Content containing  | |
                     | URI attribute set to REQUEST_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/RT/NBA/002_CRE
	CREATE

	TP/oneM2M/CSE/RT/NBA/002_UPD
	UPDATE

	TP/oneM2M/CSE/RT/NBA/002_RET
	RETRIEVE

	TP/oneM2M/CSE/RT/NBA/002_DEL
	DELETE



TP/oneM2M/CSE/RT/NBA/003
	TP Id
	TP/oneM2M/CSE/RT/NBA/003

	Test objective
	Check that the IUT sends the result of the requested Non-Blocking Asynchronous OPERATION as notification to the Originator when no notification target list is provided

	Reference
	TS-0001 [1], clause 8.1.2, 8.2.2.2

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_ASYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS
}




·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | Resource Type set to 3 (container)and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | ResponseType set to 2 (nonBlockingRequestAsynch)  | |
                     | NotificationURI not set   | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     |the IUT sends a valid Response (Ack)  | |
                     | and the IUT sends a valid NOTIFY Request containing  | |
                     | Content containing  | |
                     | ResponsePrimitive representation indicating the response of the original Non‑Blocking Asynchronous OPERATION containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/RT/NBA/003_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/RT/NBA/003_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/RT/NBA/003_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/RT/NBA/003_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/RT/NBA/004
	TP Id
	TP/oneM2M/CSE/RT/NBA/004

	Test objective
	Check that the IUT does not send the result of the requested Non-Blocking Asynchronous OPERATION as notification to the Originator when an empty notification target list is provided

	Reference
	TS-0001 [1], clause 8.1.2, 8.2.2.2

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_ASYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the Originator having privileges to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS
}




·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | Resource Type set to 3 (container)and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | ResponseType set to 2 (nonBlockingRequestAsynch) and  | |
                     | NotificationURI set to empty list  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     |the IUT sends a valid Response (Ack)  | |
                     | and the IUT does not send a NOTIFY Response  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/RT/NBA/004_CRE
	CREATE

	TP/oneM2M/CSE/RT/NBA/004_UPD
	UPDATE

	TP/oneM2M/CSE/RT/NBA/004_RET
	RETRIEVE

	TP/oneM2M/CSE/RT/NBA/004_DEL
	DELETE



TP/oneM2M/CSE/RT/NBA/005
	TP Id
	TP/oneM2M/CSE/RT/NBA/005

	Test objective
	Check that the IUT sends the result of the requested Non-Blocking Asynchronous OPERATION as notification to the notification targets indicated in responseType/notificationURI attribute of the request

	Reference
	TS-0001 [1], clause 8.1.2, 8.2.2.2

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_NON_BLOCKING_REQUEST_ASYNCH

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the AE1 having privileges to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | Resource Type set to 3 (container)and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Response Type parameter containing  | |
                     | responseTypeValue set to 2 (nonBlockingRequestAsynch) and  | |
                     | NotificationURI set to AE1_RESOURCE_ADDRESS and AE2_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE1  |
                     | the IUT sends a valid Response (Ack)  |  |
                     | and the IUT sends a valid NOTIFY Request containing to AE1  |  |
                     | Content containing  |IUT => AE1  |
                     | ResponsePrimitive representation indicating the response of the original Non‑Blocking Asynchronous OPERATION containing  |  |
                     | Response Status Code set to RESPONSE_STATUS_CODE  |  |
                     | and the IUT sends a valid NOTIFY Request containing to AE2  |  |
                     | Content containing  |  |
                     | ResponsePrimitive representation indicating the response of the original Non‑Blocking Asynchronous OPERATION containing  |IUT => AE2 |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/RT/NBA/005_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/RT/NBA/005_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/RT/NBA/005_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/RT/NBA/005_DEL
	DELETE
	2002 (DELETED)



7.2.2.10	Security(SEC)
7.2.2.10.1	CREATE Operation
TP/oneM2M/CSE/SEC/ACP/CRE/001
	TP Id
	TP/oneM2M/CSE/SEC/ACP/CRE/001

	Test objective
	Check that the IUT accepts the creation of a accessControlPolicy resource with privileges attribute having multiple access control rules

	Reference
	TS-0001 [1], clause 9.6.2-2 and clause, 10.2.21

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_IDand  | |
                     | Content containing  | |
                     | accessControlPolicy resource containing  | |
                     | privileges attribute containing  | |
                     | accessControlRule attribute containing  | |
                     | ACCESS_CONTROL_RULE_1 and  | |
                     | ACCESS_CONTROL_RULE_2  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT creates the accessControlPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+—————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ACP/CRE/002
	TP Id
	TP/oneM2M/CSE/SEC/ACP/CRE/002

	Test objective
	Check that the IUT accepts the creation of a accessControlPolicy resource with selfPrivileges attribute having multiple access control rules

	Reference
	TS-0001 [1], clause 9.6.2-2 and clause 10.2.21

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_IDand  | |
                     | Content containing  | |
                     | accessControlPolicy resource containing  | |
                     | selfPrivileges attribute containing  | |
                     | accessControlRule attribute containing  | |
                     | ACCESS_CONTROL_RULE_1 and  | |
                     | ACCESS_CONTROL_RULE_2  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT creates the accessControlPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+——————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEC/ACP/CRE/003
	TP Id
	TP/oneM2M/CSE/SEC/ACP/CRE/003

	Test objective
	Check that the IUT accepts the creation of a accessControlPolicy resource with privileges attribute having empty rules

	Reference
	TS-0001 [1], clause 9.6.2 and clause 10.2.21

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_IDand  | |
                     | Content containing  | |
                     | accessControlPolicy resource containing  | |
                     | privileges attribute set to empty list  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT creates the accessControlPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+———————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ACP/CRE/004
	TP Id
	TP/oneM2M/CSE/SEC/ACP/CRE/004

	Test objective
	Check that the IUT responds with an error when the creation of a accessControlPolicy resource with selfPrivileges attribute having empty rules

	Reference
	TS-0001 [1], clause 9.6.2and clause 10.2.21

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_IDand  | |
                     | Content containing  | |
                     | accessControlPolicy resource containing  | |
                     | selfPrivileges attribute set to empty list  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the accessControlPolicy resource  | |
                     | and the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+———————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ACP/CRE/005
	TP Id
	TP/oneM2M/CSE/SEC/ACP/CRE/005

	Test objective
	Check that the IUT responds successfully when an AE creates an accessControlPolicy resource having accessControlOriginators element set to a group resource identifier which contains AE resource as member

	Reference
	TS-0001 [1], clause 9.6.2

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the AE1 having privileges to perform CREATE operation on the resource TARGET_RESOURCE_ADDRESS
and the IUT having registered the AE2
and the IUT having created a group resource at GROUP_RESOURCE_ADDRESS containing
memberIDs set to AE2_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid CREATE Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | accessControlPolicy resource containing  | |
                     | privileges containing  | |
                     | accessControlRule element containing  | |
                     | accessControlOriginators element set to GROUP_RESOURCE_ADDRESS  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————+————-+
7.2.2.10.2	UPDATE Operation
TP/oneM2M/CSE/SEC/ACP/UPD/001
	
TP Id
	TP/oneM2M/CSE/SEC/ACP/UPD/001

	Test objective
	Check that the IUT updates successfully the accessControlPolicyIDs attribute of the <AE> resource when the AE has privileges for UPDATE operation in any selfPrivileges of the <accessControlPolicy> resources which this attribute originally indicates

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
accessControlPolicyID attribute set to ACP_ID_1
and the AE having privileges to perform UPDATE operation on the AE_RESOURCE_ADDRESS in selfPrivileges
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | accessControlPolicyIDs attribute set to ACP_ID_2  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT updates the accessControlPolicyIDs attribute of AE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | AE resourcecontaining  | |
                     | accessControlPolicyID attribute set to ACP_ID_2  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ACP/UPD/002
	
TP Id
	TP/oneM2M/CSE/SEC/ACP/UPD/002

	Test objective
	Check that the IUT responds with an error when the AE tries an UPDATE operation on the accessControlPolicyIDs attribute without having privileges for such operation in any selfPrivileges of the <accessControlPolicy> resources which this attribute originally indicates

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
accessControlPolicyID attribute set to ACP_ID_1
and the AE having no privileges to perform UPDATE operation on the AE_RESOURCE_ADDRESS in selfPrivileges
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | AE resource containing  | |
                     | accessControlPolicyID attribute set to ACP_ID_2  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not update the accessControlPolicyIDs attribute of AE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————————-+————-+
7.2.2.10.3	BASIC OPERATION
TP/oneM2M/CSE/SEC/ACP/001
	TP Id
	TP/oneM2M/CSE/SEC/ACP/001

	Test objective
	Check that the IUT responds with an error when an ORIGINATOR tries an OPERATION without having privileges for performing the OPERATION on the TARGET_RESOURCE_TYPE resource

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the ORIGINATOR having no privileges to perform an OPERATION on the resource TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |when {   |IUT <= ORIGINATOR|
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to ORIGINATOR_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |then {   |IUT => ORIGINATOR|
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+—————–+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SEC/ACP/001_CRE
	CREATE

	TP/oneM2M/CSE/SEC/ACP/001_RET
	RETRIEVE

	TP/oneM2M/CSE/SEC/ACP/001_UPD
	UPDATE

	TP/oneM2M/CSE/SEC/ACP/001_DEL
	DELETE



TP/oneM2M/CSE/SEC/ACP/002
	TP Id
	TP/oneM2M/CSE/SEC/ACP/002

	Test objective
	Check that the IUT responds successfully when the AE tries an OPERATION on its <AE> resource which has multiple accessControlPolicyID attribute

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1 and clause 9.6.2.1-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having a child <Container> resource containing
accessControlPolicyID attribute containing
ACP_ID_1 and
ACP_ID_2
and the AE having privileges to perform an OPERATION on itself given by ACP_ID_2 only
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/002_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/002_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/002_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/002_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/003
	TP Id
	TP/oneM2M/CSE/SEC/ACP/003

	Test objective
	Check that the IUT responds successfully when an allowed DOMAIN tries an OPERATION on a AE_RESOURCE_TYPE resource.

	Reference
	TS-0001 [1], clause 9.6.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the DOMAIN having privileges to perform an OPERATION on the resource AE_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= DOMAIN|
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to DOMAIN  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => DOMAIN|
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+———————————————————————————————————+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/003_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/003_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/003_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/003_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/004
	TP Id
	TP/oneM2M/CSE/SEC/ACP/004

	Test objective
	Check that the IUT responds successfully when any ORIGINATOR tries an OPERATION on a AE_RESOURCE_TYPE resource for which all originators are allowed

	Reference
	TS-0001 [1], clause 9.6.2.1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and any originator (*) having privileges to perform an OPE RATION on the resource AE_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |when {   |IUT <= ORIGINATOR|
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to ORIGINATOR  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |then {   |IUT => ORIGINATOR|
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————+—————–+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/004_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/004_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/004_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/004_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/005
	TP Id
	TP/oneM2M/CSE/SEC/ACP/005

	Test objective
	Check that the IUT responds successfully when the AE tries an OPERATION on a AE_RESOURCE_TYPE resource and that the request is within accessControlTimeWindow context

	Reference
	TS-0001 [1], clause 9.6.2.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AEhaving privileges to perform OPERATION on the AE_RESOURCE_ADDRESSwithin TIME_WINDOW
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | within TIME_WINDOW  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/005_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/005_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/005_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/005_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/006
	TP Id
	TP/oneM2M/CSE/SEC/ACP/006

	Test objective
	Check that the IUT responds with an error when the AE tries an_OPERATION_ on a AE_RESOURCE_TYPE resource out of accessControlTimeWindow context

	Reference
	TS-0001 [1], clause 9.6.2.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AEhaving privileges to perform OPERATION on the AE_RESOURCE_ADDRESSwithin TIME_WINDOW
}



·                  +------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | out of TIME_WINDOW  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SEC/ACP/006_CRE
	CREATE

	TP/oneM2M/CSE/SEC/ACP/006_RET
	RETRIEVE

	TP/oneM2M/CSE/SEC/ACP/006_UPD
	UPDATE

	TP/oneM2M/CSE/SEC/ACP/006_DEL
	DELETE



TP/oneM2M/CSE/SEC/ACP/007
	TP Id
	TP/oneM2M/CSE/SEC/ACP/007

	Test objective
	Check that the IUT responds successfully when the AE tries an OPERATION on a AE_RESOURCE_TYPE resource and that the request is within accessControlLocationRegion context

	Reference
	TS-0001 [1], clause 9.6.2.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a child locationPolicy resource containing
locationContainerID attribute set to CONTAINER_ID
and a child container resource containing
locationID attribute set to LOCATION_POLICY_ID and
contentInstance resource containing
content attribute set to LOCATION
and the AEhaving privileges to perform OPERATION on the AE_RESOURCE_ADDRESSwithin LOCATION_RESTRICTION
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | and LOCATION within LOCATION_RESTRICTION  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+


	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/007_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/007_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/007_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/007_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/008
	TP Id
	TP/oneM2M/CSE/SEC/ACP/008

	Test objective
	Check that the IUT responds with an error when the AE tries an OPERATION on a AE_RESOURCE_TYPE resource out of accessControlLocationRegion context

	Reference
	TS-0001 [1], clause 9.6.2.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AEhaving privileges to perform OPERATION on the AE_RESOURCE_ADDRESSwithin LOCATION_RESTRICTION

}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | out of LOCATION_RESTRICTION  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SEC/ACP/008_CRE
	CREATE

	TP/oneM2M/CSE/SEC/ACP/008_RET
	RETRIEVE

	TP/oneM2M/CSE/SEC/ACP/008_UPD
	UPDATE

	TP/oneM2M/CSE/SEC/ACP/008_DEL
	DELETE



TP/oneM2M/CSE/SEC/ACP/009
	TP Id
	TP/oneM2M/CSE/SEC/ACP/009

	Test objective
	Check that the IUT responds successfully when the AE tries an OPERATION on a TARGET_RESOURCE_TYPE resource and that the request is within accessControlIpAddresses context

	Reference
	TS-0001 [1], clause 9.6.2.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AEhaving privileges to perform OPERATION on the AE_RESOURCE_ADDRESSwithin IP_ADDRESS_RESTRICTION
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | and AE_IP_ADDRESSwithin IP_ADDRESS_RESTRICTION  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/009_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/009_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/009_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/009_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/010
	TP Id
	TP/oneM2M/CSE/SEC/ACP/010

	Test objective
	Check that the IUT responds with an error when the AE tries an OPERATION on a AE_RESOURCE_TYPE resource out of accessControlIpAddresses context

	Reference
	TS-0001 [1], clause 9.6.2.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AEhaving privileges to perform OPERATION on the AE_RESOURCE_ADDRESSwithin IP_ADDRESS_RESTRICTION
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | and AE_IP_ADDRESS out of IP_ADDRESS_RESTRICTION  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SEC/ACP/010_CRE
	CREATE

	TP/oneM2M/CSE/SEC/ACP/010_RET
	RETRIEVE

	TP/oneM2M/CSE/SEC/ACP/010_UPD
	UPDATE

	TP/oneM2M/CSE/SEC/ACP/010_DEL
	DELETE



TP/oneM2M/CSE/SEC/ACP/011
	TP Id
	TP/oneM2M/CSE/SEC/ACP/011

	Test objective
	Check that the IUT responds successfully when the AE tries an OPERATION on its child <container> resource whose accessControlPolicyID attribute is not set and AE has privileges for such OPERATION on its associated accessControlPolicy resource

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having a child <Container> resource containing
no accessControlPolicyID attribute
and the AE having privileges to perform an OPERATION on the resource CONTAINER_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/011_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/011_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/011_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/011_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/012
	TP Id
	TP/oneM2M/CSE/SEC/ACP/012

	Test objective
	Check that the IUT responds with an error when an ORIGINATOR tries an OPERATION on a <Container> resource with no accessControlPolicyID associated and such ORIGINATOR having no privileges for performing the OPERATION on the <Container> resource

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE, PICS_ACP_SUPPORT

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having a child <Container> resource containing
no accessControlPolicyID attribute
and the ORIGINATOR having no privileges to perform an OPERATION on the <Container> resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |when {   |IUT <= ORIGINATOR|
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to ORIGINATOR_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-----------------+

·                      |then {   |IUT => ORIGINATOR|
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————–+—————–+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SEC/ACP/012_CRE
	CREATE

	TP/oneM2M/CSE/SEC/ACP/012_RET
	RETRIEVE

	TP/oneM2M/CSE/SEC/ACP/012_UPD
	UPDATE

	TP/oneM2M/CSE/SEC/ACP/012_DEL
	DELETE



TP/oneM2M/CSE/SEC/ACP/013
	TP Id
	TP/oneM2M/CSE/SEC/ACP/013

	Test objective
	Check that the IUT responds successfully when the creator AE tries an OPERATION on the AE resource whose accessControlPolicyIDs attribute is not set

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1

	Config Id
	CF01

	Parent release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the <AE> resource having no accessControlPolicyIDs attribute
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/013_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/013_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/013_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/013_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/014
	TP Id
	TP/oneM2M/CSE/SEC/ACP/014

	Test objective
	Check that the IUT responds with an error when an AE2 tries an OPERATION on the AE1 resource whose accessControlPolicyIDs attribute is not set

	Reference
	TS-0001 [1], clause 9.6.1.3.2-1

	Config Id
	CF01

	Parent release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the <AE> resource of AE1 having no accessControlPolicyIDs attribute
}



·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE2 |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE1_RESOURCE_ADDRESS and  | |
                     | From set to AE2_ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE2 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SEC/ACP/014_CRE
	CREATE

	TP/oneM2M/CSE/SEC/ACP/014_RET
	RETRIEVE

	TP/oneM2M/CSE/SEC/ACP/014_UPD
	UPDATE

	TP/oneM2M/CSE/SEC/ACP/014_DEL
	DELETE



TP/oneM2M/CSE/SEC/ACP/015
	TP Id
	TP/oneM2M/CSE/SEC/ACP/015

	Test objective
	Check that the IUT responds successfully when an AE tries an OPERATION on the AE1 resource whose accessControlPolicyIDs attribute is set

	Reference
	TS-0001 [1], clause 9.6.2

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having <group> resource GRP1 having AE2 as memberIds
and the <AE> resource of AE1 having accessControlPolicyIDs attribute set and this referenced <accessControlPolicy> having atleast single ACR accessControlOriginators attribute having resourceID of <group> resource GRP1 and accessControlOperations to OPERATION
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE2 |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE1_RESOURCE_ADDRESS and  | |
                     | From set to AE2_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE2 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/015_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SEC/ACP/015_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/015_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/015_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SEC/ACP/016
	TP Id
	TP/oneM2M/CSE/SEC/ACP/016

	Test objective
	Check that the IUT responds with an error when an AE tries an OPERATION on the AE1 resource whose accessControlPolicyIDs attribute is set

	Reference
	TS-0001 [1], clause 9.6.2

	Config Id
	CF01

	Parent release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having registered the AE3
and the IUT having <group> resource GRP1 having AE3 as member only
and the <AE> resource of AE1 having accessControlPolicyIDs attribute set and this referenced <accessControlPolicy> having at least single ACR accessControlOriginators attribute having resourceID of <group> resource GRP1 and accessControlOperations to OPERATION
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE2 |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to AE1_RESOURCE_ADDRESS and  | |
                     | From set to AE2_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE2 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SEC/ACP/016_CRE
	CREATE

	TP/oneM2M/CSE/SEC/ACP/016_RET
	RETRIEVE

	TP/oneM2M/CSE/SEC/ACP/016_UPD
	UPDATE

	TP/oneM2M/CSE/SEC/ACP/016_DEL
	DELETE



TP/oneM2M/CSE/SEC/ACP/017
	TP Id
	TP/oneM2M/CSE/SEC/ACP/017

	Test objective
	Check that the IUT accepts the OPERATION request on <accessControlPolicy> resource when at least one of the access control rules defined in the selfPrivileges attribute allows the operation

	Reference
	TS-0001 [1], clause 10.2.3.1, TS-0004 [2], clause 7.4.2.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a Hosting CSE
and the IUT having registered the AE as ORIGINATOR
and the IUT having an <accessControlPolicy> resource at
TARGET_RESOURCE_ADDRESS containing
selfPrivileges attribute containing
access control rule(s) to allow the OPERATION
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SEC/ACP/017_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SEC/ACP/017_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SEC/ACP/017_DEL
	DELETE
	2002 (DELETED)



7.2.2.10.4	Authentication
7.2.2.10.4.1	ESPrim (ESP)
7.2.2.10.4.1.1	NOTIFY Operation
TP/oneM2M/CSE/SEC/ESP/NTF/001
	TP Id
	TP/oneM2M/CSE/SEC/ESP/NTF/001

	Test objective
	Check that the IUT sends a new ESPrimRandObject when requested

	Reference
	TS-0003 8.4.2 - step B.2C.2, TS-0004 7.5.1.2.11

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT having established a pairwiseESPrimKey with the Originator (AE1)
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid NOTIFY request from AE1 containing To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE1_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 3 (receiverESPrimRandObject  | |
                     | Request)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid NOTIFY Response containing  | |
                     | To set to TARGET_ORIGINATOR_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 4 (receiverESPrimRandObject  | |
                     | Response) and  | |
                     | esprimRandObject element containing  | |
                     | receiverESPrimRandObject  | |
                     |} | |
+———————-+————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ESP/NTF/002
	TP Id
	TP/oneM2M/CSE/SEC/ESP/NTF/002

	Test objective
	Check that the IUT responds with a valid ESPrim object when it receives a request

	Reference
	TS-0003 8.4.2 - step C.9, TS-0004 7.6.2

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT having established a sessionESPrimKey with the Originator (AE1)
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid NOTIFY Request from AE1 containing To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to AE1_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 5 (ESPrim Object) and  | |
                     | valid esprimObject element  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid NOTIFY Response containing  | |
                     | To set to RECEIVER_RECEIVER_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 5 (ESPrim Object) and  | |
                     | valid esprimObject element  | |
                     |} | |
+———————-+————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ESP/NTF/003
	TP Id
	TP/oneM2M/CSE/SEC/ESP/NTF/003

	Test objective
	Check that the IUT successfully detects AE impersonation in an End-to-End Security of Primitives

	Reference
	TS-0003 7.2.2 - step 4, TS-0004 7.6.2

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT having established a sessionESPrimKey with with the Originator (AE1)
}



·                  +-------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE1 |
                     | the IUT receives a valid NOTIFY Request from AE1 containing   | |
                     | To set to CSE_ID and  | |
                     | From set to a value other than AE1_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 5 (ESPrim Object) and  | |
                     | valid esprimObject element  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response containing  | IUT => AE1 |
                     | Response Status Code set to  | |
                     | 4116 (ESPRIM_IMPERSONATION_ERROR)  | |
                     |} | |
+———————-+————————————————————————————-+————-+
7.2.2.10.4.1.2	RETRIEVE Operation
TP/oneM2M/CSE/SEC/ESP/RET/001
	TP Id
	TP/oneM2M/CSE/SEC/ESP/RET/001

	Test objective
	Check that the IUT sends a valid request for e2eSecInfo attribute of the Receiver's <remoteCSE> resource in the CSE Registered with Receiver CSE

	Reference
	TS-0003 8.4.2 - step B.2A, TS-0004 7.5.1.2.11

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUThaving established a pairwiseESPrimKey with the Receiver CSE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing  | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE <= IUT |
                     | the IUT sends a valid RETRIEVE Request to Target CSE containing  | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | remoteCSE resourcecontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
+———————-+————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEC/ESP/RET/002
	TP Id
	TP/oneM2M/CSE/SEC/ESP/RET/002

	Test objective
	Check that the IUT sends a notification containing an inner "receiverESPrimRandObject request" to the Receiver if the sharedReceiverESPrimRandObject parameter is not present in the <remoteCSE> resource in the CSE Registered with Receiver CSE

	Reference
	TS-0003 8.4.2 - step B.2D, TS-0004 7.5.1.2.11

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered and
and the IUT being switched on
a nd the IUT having established a pairwiseESPrimKey with the Originator
and the <remoteCSE> resource at TARGET_REMOTE_CSE_ADDRESS containing e2eSecInfo attribute with no sharedReceiverESPrimRandObject parameter
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing   | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFICATION Request containing  | |
                     | To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 3 (receiverESPrimRandObject  | |
                     | Request)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ESP/RET/003
	TP Id
	TP/oneM2M/CSE/SEC/ESP/RET/003

	Test objective
	Check that the IUT sends a notification containing an inner "receiverESPrimRandObject request" to the Receiver if the sharedReceiverESPrimRandObject in the <remoteCSE> resource is expired

	Reference
	TS-0003 8.4.2 - step B.2B, TS-0004 7.5.1.2.11

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT having established a pairwiseESPrimKey with the Originator and
and the <remoteCSE> resource at TARGET_REMOTE_CSE_ADDRESS contain ing
e2eSecInfo attribute with an expired sharedReceiverESPrimRandObject parameter
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid RETRIEVE Request containing   | |
                     | To set to TARGET_REMOTE_CSE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | attributeList elementcontaining  | |
                     | e2eSecInfo attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFICATION Request containing  | |
                     | To set to TARGET_RECEIVER_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 3 (receiverESPrimRandObject  | |
                     | Request)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————+————-+
7.2.2.10.4.2	Roles (ROL)
7.2.2.10.4.2.1	CREATE Operation
TP/oneM2M/CSE/SEC/ROL/CRE/001
	TP Id
	TP/oneM2M/CSE/SEC/ROL/CRE/001

	Test objective
	Check that the IUT sends a CREATE <role> resource request to the Role Repository (CSE1) when triggered

	Reference
	TS-0003 7.4.2.2 - step 3

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT acting as an Authorization Authority
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to ROLE_REPOSITORY_ADDRESS (CSE1) and  | |
                     | Resource Type set to 31 (role) and  | |
                     | Content containing  | |
                     | < role> resource representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid CREATE Request to CSE1 containing  | IUT => CSE1 |
                     | To set to ROLE_REPOSITORY_ADDRESS and  | |
                     | Resource Type set to 31 (role) and  | |
                     | Content containing  | |
                     | <role> resource representation  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
TP/oneM2M/CSE/SEC/ROL/CRE/002
	TP Id
	TP/oneM2M/CSE/SEC/ROL/CRE/002

	Test objective
	Check that the IUT successfully creates the <role> resource requested by the Authorization Authority

	Reference
	TS-0003 7.4.2.2 - step 4 and 5

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered and
and the IUT being switched on and
and the IUT acting as a Role Repository
}



·                  +------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE1 |
                     | the IUT receives a valid CREATE Request from CSE1 (AA) containing   | |
                     | From set to CSE1_ID and  | |
                     | To set to ROLE_REPOSITORY_ADDRESS and  | |
                     | Resource Type set to 31 (role) and  | |
                     | Content containing  | |
                     | <role> resource representation  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT creates the <role> resource  | IUT => CSE1 |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | <role> resource representation  | |
                     |} | |
+———————-+——————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ROL/CRE/003
	TP Id
	TP/oneM2M/CSE/SEC/ROL/CRE/003

	Test objective
	Check that the IUT sends a CREATE <token> resource request to the Token Repository when triggered

	Reference
	TS-0003 7.4.2.3 - step 2

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT acting as an Authorization Authority
and the IUT having assigned a role for the Originator
}



·                  +---------------------------------------------------------------------------------------+-------------+

·                      |when {  |NA |
                     | the IUT is triggered to send a valid CREATE Request containing  | |
                     | To set to TOKEN_REPOSITORY_ADDRESS (CSE1) and  | |
                     | Resource Type set to 32 (token) and  | |
                     | Content containing  | |
                     | <token> resource representation  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid CREATE Request to CSE containing  | IUT => CSE1 |
                     | To set to TOKEN _REPOSITORY_ADDRESS and  | |
                     | Resource Type set to 32 (token) and  | |
                     | Content containing  | |
                     | <token> resource representation  | |
                     |} | |
+———————-+—————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ROL/CRE/004
	TP Id
	TP/oneM2M/CSE/SEC/ROL/CRE/004

	Test objective
	Check that the IUT successfully creates the <token> resource requested by the Authorization Authority

	Reference
	TS-0003 7.4.2.3 - step 3 and 4

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT acting as a Token Repository
and the Authorization Authority having assigned a role for the Originator
}



·                  +-------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE1 |
                     | the IUT receives a valid CREATE Request from CSE1 (AA) containing   | |
                     | From set to CSE1_ID and  | |
                     | To set to TOKEN_REPOSITORY_ADDRESS and  | |
                     | Resource Type set to 32 (token) and  | |
                     | Content containing  | |
                     | <token> resource representation  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT creates the <token> resource  | IUT => CSE1 |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | <token> resource representation  | |
                     |} | |
+———————-+——————————————————————————————-+————-+
7.2.2.10.4.2.2	RETRIEVE Operation
TP/oneM2M/CSE/SEC/ROL/RET/001
	TP Id
	TP/oneM2M/CSE/SEC/ROL/RET/001

	Test objective
	Check that the IUT returns the <role> resource of the Originator

	Reference
	TS-0003 7.4.2.2 - step 8

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT acting as a Role Repository
and the Authorization Authority having assigned a role for the Originator at
ROLE_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE1 |
                     | the IUT receives a RETRIEVE Request containing   | |
                     | From set to CSE1_ID and  | |
                     | To set to ROLE_RESOURCE_ADDRESS and   | |
                     | no Content  | |
                     |} | |
·                  +-----------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response containing  | IUT => CSE1 |
                     | Response Status Code set to 2000 (OK) and   | |
                     | Content containing  | |
                     | valid <role> resource representation  | |
                     |} | |
+———————-+—————————————————————————–+————-+
TP/oneM2M/CSE/SEC/ROL/RET/002
	TP Id
	TP/oneM2M/CSE/SEC/ROL/RET/002

	Test objective
	Check that the IUT returns the <token> resource of the Originator

	Reference
	TS-0003 7.4.2.3 - step 8

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT acting as a Token Repository
and the Authorization Authority having assigned a role for the Originator
and the IUT having a token associated to the role of the Originator at
TOKEN_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE1 |
                     | the IUT receives a RETRIEVE Request containing   | |
                     | From set to CSE1_ID and  | |
                     | To set to TOKEN_RESOURCE_ADDRESS and   | |
                     | no Content  | |
                     |} | |
·                  +--------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response containing  | IUT => CSE1 |
                     | Response Status Code set to 2000 (OK) and   | |
                     | Content containing  | |
                     | valid <token> resource representation  | |
                     |} | |
+———————-+————————————————————————–+————-+
TP/oneM2M/CSE/SEC/ROL/RET/003
	TP Id
	TP/oneM2M/CSE/SEC/ROL/RET/003

	Test objective
	Check that the IUT sends a <role> Retrieve request to the Role Repository after receiving a request on a resource protected by role based access control

	Reference
	TS-0003 7.4.3 - step 2

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
a nd the Authorization Authority having assigned a role for the Originator
a nd the Authorization Authority having created a token associated to the role of the Originator
a nd the IUT having a <container> resource at RESOURCE_TARGET_ADDRESS protected by role based access control
a nd the IUThaving granted the Originator access to the <container> resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE1 |
                     | the IUT receives a valid RETRIEVE Request containing   | |
                     | From set to AE1_ID and  | |
                     | To set to RESOURCE_TARGET_ADDRESS and   | |
                     | Role ID parameter set to address the <role> resource assigned to the Originator  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid RETRIEVE Request to CSE1 containing  | IUT => CSE1 |
                     | From set to CSE_ID and  | |
                     | To set to Role ID and   | |
                     | no Content  | |
                     |} | |
+———————-+———————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEC/ROL/RET/004
	TP Id
	TP/oneM2M/CSE/SEC/ROL/RET/004

	Test objective
	Check that the IUT sends a <token> Retrieve request to the Token Repository after receiving a request on a resource protected by role based access control

	Reference
	TS-0003 7.4.3 - step 2

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the Authorization Authority having assigned a role for the Originator
and the Authorization Authority having created a token associated to the role of the Originator
and the IUT having a <container> resource at RESOURCE_TARGET_ADDRESS protected by role based access control procedure
an d the IUThaving granted the Originator access to the <container> resource
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE1 |
                     | the IUT receives a valid RETRIEVE Request containing   | |
                     | From set to AE1_ID and  | |
                     | To set to RESOURCE_TARGET_ADDRESS and   | |
                     | Role ID parameter set to address the <role> resource assigned to the Originator  | |
                     | Token ID parameter set to address the <token> resource assigned to the role of the Originator  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid RETRIEVE Request to CSE1 containing  | IUT => CSE1 |
                     | From set to CSE_ID and  | |
                     | To set to Token_ID and   | |
                     | no Content  | |
                     |} | |
+———————-+————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ROL/RET/005
	TP Id
	TP/oneM2M/CSE/SEC/ROL/RET/005

	Test objective
	Check that the IUT returns the result of a requeston a resource protected by role based access control, when the appropriate credentials are provided in the request

	Reference
	TS-0003 7.4.3 - step 7

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the Authorization Authority having assigned a role for the Originator
and the Authorization Authority having created a token associated to the role of the Originator
and the IUT having a <container> resource at RESOURCE_TARGET_ADDRESS protected by role based access control procedure
and the IUThaving granted the Originator access to the <container> resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE1 |
                     | the IUT receives a valid RETRIEVE Request containing   | |
                     | From set to AE1_ID and  | |
                     | To set to RESOURCE_TARGET_ADDRESS and   | |
                     | Role ID parameter set to address the <role> resource assigned to the Originator  | |
                     | Token ID parameter set to address the <token> resource assigned to the role of the Originator  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a RETRIEVE Response containing  | IUT => AE1 |
                     | Response Status Code set to 2000 (OK) and   | |
                     | Content containing  | |
                     | <container> resource  | |
                     |} | |
+———————-+——————————————————————————————————————————————————-+————-+
7.2.2.10.4.2.3	UPDATE Operation
TP/oneM2M/CSE/SEC/ROL/UPD/001
	TP Id
	TP/oneM2M/CSE/SEC/ROL/UPD/001

	Test objective
	Check that the IUT updates the tokenLink attribute of the <role> resource after creating its associated <token> resource

	Reference
	TS-0003 7.4.2.3 - step 5

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on
and the IUT acting as an Authorization Authority
and the IUT having assigned a role for the Originator
and the IUT having created a token associated to the role of the Originator at
TOKEN_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE2 |
                     | the IUT receives a valid CREATE Response from CSE2 (TR) containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | <token> resource representation  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid UPDATE Request to CSE1 (RR) containing  | IUT => CSE1 |
                     | To set to ROLE_REPOSITORY_ADDRESS and  | |
                     | Resource Type set to 32 (token) and  | |
                     | Content containing  | |
                     | <token> resource representation containing  | |
                     | tokenLink attribute set to TOKEN_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+—————————————————————————————————————–+————-+
7.2.2.10.4.2.4	NOTIFY Operation
TP/oneM2M/CSE/SEC/ROL/NTF/001
	TP Id
	TP/oneM2M/CSE/SEC/ROL/NTF/001

	Test objective
	Check that the IUT notifies the Originator about a token issuance associated to its role

	Reference
	TS-0003 7.4.2.3 - step 6

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being switched on the IUT being in the "initial state"
and the IUT acting as an Authorization Authority
and the IUT having assigned a role for the Originator
and the IUT having created a token associated to the role of the Originator
}



·                  +---------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= CSE2 |
                     | the IUT receives a valid CREATE Response from CSE2 (TR) containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | <token> resource representation  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid NOTIFY Request to CSE1 (Originator) containing | IUT => CSE1 |
                     | Content containing  | |
                     | notificationEvent attribute containing  | |
                     | representation attribute containing  | |
                     | <token> resource representation  | |
                     |} | |
+———————-+—————————————————————————————+————-+
7.2.2.10.4.3	DAS (DAS)
7.2.2.10.4.3.1	NOTIFY Operation
7.2.2.10.4.4	ESCertKE (ESC)
7.2.2.10.4.4.1	NOTIFY Operation
TP/oneM2M/CSE/SEC/ESC/NTF/001
	TP Id
	TP/oneM2M/CSE/SEC/ESC/NTF/001

	Test objective
	Check that the IUT sends a notify request with ESCertKE message 1 when triggered

	Reference
	TS-0003 8.7.2.2 - step C.1.a, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Terminating End-Point's Certificate Info & Identity
}



·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |NA |
                     | the IUT is triggered to send a valid NOTIFY Request containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 1 (TLS Message: Client Hello)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Request to CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE1 ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 1 (TLS Message: Client Hello)  | |
                     |} | |
+———————-+———————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ESC/NTF/002
	TP Id
	TP/oneM2M/CSE/SEC/ESC/NTF/002

	Test objective
	Check that the IUT sends a notify response with ESCertKE message 2 when it receives a notify request with ESCertKE message 1

	Reference
	TS-0003 8.7.2.2 - step C.1.b, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Initiating End-Point's Certificate Info & Identity
}



·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE1 |
                     | the IUT receives a valid NOTIFY Request from CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE1_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 1 (TLS  | |
                     | Message: Client Hello)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Response to CSE1 containing  | |
                     | To set to INITIATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 2 (TLS  | |
                     | Messages: Server Hello, Certificate*,  | |
                     | ServerKeyExchange, CertificateRequest, ServerHelloDone)  | |
                     |} | |
+———————-+———————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ESC/NTF/003
	TP Id
	TP/oneM2M/CSE/SEC/ESC/NTF/003

	Test objective
	Check that the IUT sends a notify request with ESCertKE message 3 when it receives a notify response with ESCertKE message 2

	Reference
	TS-0003 8.7.2.2 - step C.1.c, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Terminating End-Point's Certificate Info & Identity
and the IUT having sent a notify request to the Terminating End-Point with ESCertKE
Message 1
}



·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE1 |
                     | the IUT receives a valid NOTIFY Response from CSE1 containing  | |
                     | To set to INITIATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE1_ID and  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 2 (TLS  | |
                     | Messages: Server Hello, Certificate*,  | |
                     | ServerKeyExchange, CertificateRequest,  | |
                     | ServerHelloDone)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Request to CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 3 (TLS  | |
                     | Messages: Certificate*, ClientKeyExchange,  | |
                     | CertificateVerify*, [ChangeCipherSpec], Finished)  | |
                     |} | |
+———————-+—————————————————————————————————————+————-+
TP/oneM2M/CSE/SEC/ESC/NTF/004
	TP Id
	TP/oneM2M/CSE/SEC/ESC/NTF/004

	Test objective
	Check that the IUT sends a notify response with ESCertKE message 4 when it receives a notify request with ESCertKE message 3

	Reference
	TS-0003 8.7.2.2 - step C.1.d, TS-0001 11.4.3, TS-0004 6.3.5.48

	Config Id
	CF04

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT is being registered
and the IUT being switched on
and the IUT having been provisioned with the corresponding private key and certificate
and the IUT having configured Initiating End-Point's Certificate Info & Identity
and the IUT having sent a notify request to the Initiating End-Point with ESCertKE Message 2
}



·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE1 |
                     | the IUT receives a valid NOTIFY Request from CSE1 containing  | |
                     | To set to TERMINATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE1_ID and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 3 (TLS  | |
                     | Messages: Certificate*, ClientKeyExchange,  | |
                     | CertificateVerify*, [ChangeCipherSpec], Finished)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE1 |
                     | the IUT sends a valid NOTIFY Response to CSE containing  | |
                     | To set to INITIATING_ENDPOINT_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Contentcontaining  | |
                     | securityInfo element containing  | |
                     | securityInfoType element set to 6 (ESCertKE Message) and  | |
                     | escertkeMessage element containing  | |
                     | base64 representation of ESCertKE Message 4 (TLS  | |
                     | Messages: [ChangeCipherSpec], Finished)  | |
                     |} | |
+———————-+—————————————————————————————————————+————-+
7.2.2.11	Resource Announcement (ANNC)
7.2.2.11.1	BASIC Operation
TP/oneM2M/CSE/ANNC/001
	TP Id
	TP/oneM2M/CSE/ANNC/001

	Test objective
	Check that the IUT provides confirmation of the announcement of a resource to the originator of the initiating request after a successful resource announcement procedure

	Reference
	TS-0001 [1], clause 10.2.18.1, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the remoteCSE
and the IUT having created the PARENT_RESOURCE resource containing
RESOURCE_TYPE resource
and the IUT having announced the PARENT_RESOURCE resource
and the AE having privileges to perform an OPERATION operation on the resource TARGET_RESOURCE_ADDRESS
and the IUT having received a valid OPERATION Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
Content containing
RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ADDRESS
and The IUT having sent a valid CREATE Request containing
To set REMOTE_CSE_RESOURCE_ADDRESSand
Content containing
RESOURCE_TYPE announced variant resourcecontaining
MA (mandatory) attributes
}

	Expected behaviour
	Test events
	Direction

	
	when {
the IUT receives a valid Response from ANNC_TARGET_CSE containing
Response Status Code set to 2001 (CREATED) containing
valid RESOURCE_TYPE announced variant resource representation
}
	IUT <= CSE

	
	then {
The IUT sends a valid Response containing
Response Status Code set to RESPONSE_STATUS_CODE and
Content containing
RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_RESOURCE_ADDRESS
}
	IUT => AE



	TP Id
	RESOURCE_TYPE
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/ANNC/001_ACP/UPD
	1 (accesControlPolicy)
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/ANNC/001_ACP/CRE
	1 (accesControlPolicy)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_CNT/UPD
	3 (container)
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/ANNC/001_CNT/CRE
	3 (container)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_GRP/UPD
	9 (group)
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/ANNC/001_GRP/CRE
	9 (group)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_LCP/UPD
	10 (locationPolicy)
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/ANNC/001_LCP/CRE
	10 (locationPolicy)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_MGO/UPD
	13 (mgmtObj)
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/ANNC/001_MGO/CRE
	13 (mgmtObj)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_NOD/UPD
	14 (node)
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/ANNC/001_NOD/CRE
	14 (node)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_SCH/UPD
	18 (schedule)
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/ANNC/001_SCH/CRE
	18 (schedule)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_CIN/CRE
	4 (contentInstance)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_TS/UPD
	29 (timeSeries)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_TS/CRE
	29 (timeSeries)
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/ANNC/001_TSI/CRE
	30 (timeSeriesInstance)
	CREATE
	2001 (CREATED)



7.2.2.11.2	CREATE Operation
TP/oneM2M/CSE/ANNC/CRE/001
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/001

	Test objective
	Check that the accessControlPolicyIDs attribute is announced when accessControlPolicyIDs attribute of the original resource is not present

	Reference
	TS-0001 [1], clause 10.2.18.4 and clause 9.6.26.3-1, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created and announced the PARENT_RESOURCE to the announcement target CSE
and the AE having privileges to perform CREATE operation on the resource
PARENT_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | no accessControlPolicyIDs attribute and  | |
                     | no anouncedAttribute attribute and  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to ANNC_PARENT_RESOURCE and  | |
                     | Content containing  | |
                     | containerAnnc resource containing  | |
                     | MA (mandatory) attributes and  | |
                     | valid accessControlPolicyIDs attribute  | |
                     |} | |
+———————-+—————————————————————————————————————————–+————-+
TP/oneM2M/CSE/ANNC/CRE/002
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/002

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource when a new CSE-ID is provided in announcedTo optional attribute and IUT having not been announced to announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created the RESOURCE_TYPE resource
and the IUT having not been announced nor registered to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
and the IUT having received a valid UPDATE Request containing
Content containing
RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ID
and the IUT having sent a valid CREATE Request containing
To set to ANNC_TARGET_CSE_ID and
Content containing
CSEBaseAnnc resource
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT => CSE |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |CSE => IUT |
                     | and the IUT sends a valid CREATE Request containing  | |
                     | To set to CSE_BASE_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/CRE/002_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/CRE/002_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/CRE/002_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/CRE/002_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/CRE/002_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/CRE/002_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/CRE/002_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/CRE/002_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/CRE/003
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/003

	Test objective
	Host CSE of original resource removes an announcement target CSE from the announceTo attribute if it does not return successful CREATE response for the announced resource (for a CREATE initiating resource announcement)

	Reference
	TS-0001 [1], clause 10.2.18.4

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created and announced the container resource
and the AE having privileges to perform CREATE operation on the resource
CONTAINER_RESOURCE_ADDRESS
and the IUT having received a valid CREATE Request from AE containing
To set to CONTAINER_RESOURCE_ADDRESS and
From set to AE-ID and
Content containing
contentInstance resource containing
announceTo attribute set to ANNC_TARGET_CSE_ID
and The IUT having sent a valid CREATE Request containing
To set to REMOTE_CSE_RESOURCE_ADDRESS and
Content containing
contentInstanceAnnc resource containing
MA (mandatory) attributes
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid Response from ANNC_TARGET_CSE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     |The IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)and  | |
                     | Content containing  | |
                     | contentInstance resourcecontaining  | |
                     | announceTo attribute set to EMPTH  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/ANNC/CRE/004
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/004

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource during its creation when announceTo optional attribute is provided and its parent resource having been announced to the announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created and announced the PARENT_RESOURCE resource
and the AE having privileges to perform CREATE operation on the resource
PARENT_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to REMOTE_CSE_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/CRE/004_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/CRE/004_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/CRE/004_CIN
	4 (contentInstance)

	TP/oneM2M/CSE/ANNC/CRE/004_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/CRE/004_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/CRE/004_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/CRE/004_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/CRE/004_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/CRE/004_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/CRE/005
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/005

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource during its creation when announceTo optional attribute is provided and IUT having been already announced to announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT not having registered to the CSE
and the IUT having created the PARENT_RESOURCE resource
and the IUT having been announced to the announcement target CSE
and the AE having privileges to perform CREATE operation on the resource
PARENT_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to CSE_BASE_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resourcecontaining  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/CRE/005_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/CRE/005_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/CRE/005_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/CRE/005_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/CRE/005_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/CRE/005_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/CRE/005_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/CRE/005_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/CRE/006
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/006

	Test objective
	Check that the IUT removes successfully an entry from announceTo attribute of the RESOURCE_TYPE resource during its creation when announceTo optional attribute is provided when parent has not been announced at the announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created the PARENT_RESOURCE resource
and the AE having privileges to perform CREATE operation on the resource
PARENT_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | The IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)and  | |
                     | Content containing  | |
                     | contentInstance resourcecontaining  | |
                     | announceTo attribute set to EMPTY  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/CRE/006_CIN
	4 (contentInstance)

	TP/oneM2M/CSE/ANNC/CRE/006_TSI
	30 (timeSeriesInstance)



TP/oneM2M/CSE/ANNC/CRE/007
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/007

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource during its creation when announceTo optional attribute is provided and IUT having not been announced to announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having create d the PARENT_RESOURCE resource
and the IUT having not been announced nor registered to the announcement target CSE
and the AE having privileges to perform CREATE operation on the resource
PARENT_RESOURCE_ADDRESS
and the IUT having received a valid CREATE Request containing
To set to PARENT_RESOURCE_ADDRESS
Content containing
RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ID
and the IUT having sent a valid CREATE Request containing
To set to ANNC_TARGET_CSE_ID and
Content containing
CSEBaseAnnc resource representation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to CSE_BASE_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/CRE/007_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/CRE/007_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/CRE/007_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/CRE/007_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/CRE/007_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/CRE/007_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/CRE/007_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/CRE/007_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/CRE/008
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/008

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource during its creation when announceTo and announcedAttribute optional attributes are provided and its parent resource having been announced to the announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.6, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created and announced the PARENT_RESOURCE to the announcement target CSE
and the AE having privileges to perform CREATE operation on the resource
PARENT_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | OA_ATTRIBUTE attribute set to VALUE and  | |
                     | announcedAttribute attribute set to OA_ATTRIBUTE and  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to REMOTE_CSE_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | MA (mandatory) attributes and  | |
                     | OA_ATTRIBUTE attribute set to VALUE  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE
	OA_ATTRIBUTE

	TP/oneM2M/CSE/ANNC/CRE/008_CNT/MBS
	3 (container)
	maxByteSize

	TP/oneM2M/CSE/ANNC/CRE/008_CIN/CNF
	4 (contentInstance)
	contentInfo

	TP/oneM2M/CSE/ANNC/CRE/008_GRP/MT
	9 (group)
	memberType

	TP/oneM2M/CSE/ANNC/CRE/008_LCP/LOI
	10 (locationPolicy)
	locationContainerID

	TP/oneM2M/CSE/ANNC/CRE/008_MGO/DC
	13 (mgmtObj)
	description

	TP/oneM2M/CSE/ANNC/CRE/008_NOD/HCL
	14 (node)
	hostCSELink

	TP/oneM2M/CSE/ANNC/CRE/008_SCH/SE
	18 (schedule)
	scheduleElement

	TP/oneM2M/CSE/ANNC/CRE/008_TS/MBS
	29 (timeSeries)
	maxByteSize

	TP/oneM2M/CSE/ANNC/CRE/008_TSI/DGT
	30 (timeSeriesInstance)
	dataGenerationTime



TP/oneM2M/CSE/ANNC/CRE/009
	TP Id
	TP/oneM2M/CSE/ANNC/CRE/009

	Test objective
	Check that the labels attribute is announced when such attribute is present in the original resource

	Reference
	TS-0001 [1], clause 10.2.18.4 and 9.6.26.3-1, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created and announced the PARENT_RESOURCE to the announcement target CSE
and the AE having privileges to perform CREATE operation on the resource
PARENT_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | no anouncedAttribute attribute and  | |
                     | labels attribute set to VALUE and  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to ANNC_PARENT_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | containerAnnc resource containing  | |
                     | MA (mandatory) attributes and  | |
                     | labels attribute set to VALUE  | |
                     |} | |
+———————-+———————————————————————————————————+————-+
7.2.2.11.3	RETRIEVE Operation
TP/oneM2M/CSE/ANNC/RET/001
	TP Id
	TP/oneM2M/CSE/ANNC/RET/001

	Test objective
	Host of <resourceAnnc> returns the <resourceAnnc> representation in a RETRIEVE response

	Reference
	TS-0001 [1], clause 10.2.18.2

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having RESOURCE_TYPE announced variant resource containing
link attribute set to ORIGINAL_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the TARGET_RESOURCE_ANNC_ADDRESS
}



·                  +-----------------+--------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ANNC_ADDRESS and  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +-----------------+--------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource representation  | |
                     |} | |
+———————-+—————–+——————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/RET/001_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/RET/001_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/RET/001_CIN
	4 (contentInstance)

	TP/oneM2M/CSE/ANNC/RET/001_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/RET/001_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/RET/001_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/RET/001_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/RET/001_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/RET/001_TS
	29 (timeSeries)

	TP/oneM2M/CSE/ANNC/RET/001_TSI
	30 (timeSeriesInstance)



TP/oneM2M/CSE/ANNC/RET/002
	TP Id
	TP/oneM2M/CSE/ANNC/RET/002

	Test objective
	Host of <resourceAnnc> returns the original <resource> representation from the original resource hosting CSE in a RETRIEVE response when result content is set to "original-resource"

	Reference
	TS-0001 [1], clause 10.2.18.2

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the CSE having created RESOURCE_TYPE
and the IUT having RESOURCE_TYPE announced variant resource containing
link attribute set to ORIGINAL_RESOURCE_ADDRESS
and the AE having privileges to perform RETRIEVE operation on the TARGET_RESOURCE_ANNC_ADDRESS
and the IUT having received a valid RETRIEVE Request from AE containing
To set to TARGET_RESOURCE_ANNC_ADDRESS and
From set to AE-ID and
Result Content set to 7 (original-resource)
and the IUT having sent a a valid RETRIEVE Request to CSE containing
To set to ORIGINAL_RESOURCE_ADDRESS and
From set to AE-ID
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource representation  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/RET/002_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/RET/002_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/RET/002_CIN
	4 (contentInstance)

	TP/oneM2M/CSE/ANNC/RET/002_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/RET/002_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/RET/002_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/RET/002_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/RET/002_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/RET/002_TS
	29 (timeSeries)

	TP/oneM2M/CSE/ANNC/RET/002_TSI
	30 (timeSeriesInstance)




7.2.2.11.4	UPDATE Operation
TP/oneM2M/CSE/ANNC/UPD/001
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/001

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource when a new CSE-ID is provided in announcedTo optional attribute and its parent resource having been announced to the announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the remoteCSE
and the IUT having created and announce d the PARENT_RESOURCE resource to the announcement target CSE
and the IUT having created a RESOURCE_TYPE resource at TARGET_RESOURCE_ADDRESS containing
announceTo attribute set to NULL
and the AE having privileges to perform UPDATE operation on the resource TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ADDRESS  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set REMOTE_CSE_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resourcecontaining  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/UPD/001_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/UPD/001_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/UPD/001_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/UPD/001_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/UPD/001_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/UPD/001_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/UPD/001_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/UPD/001_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/UPD/002
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/002

	Test objective
	Check that the IUT initiates de-announcement of the RESOURCE_TYPE resource when a CSE-ID is deleted from the announceTo optional attribute

	Reference
	TS-0001 [1], clause 10.2.18.5, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the remoteCSE
and the IUT having created a RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ADDRESS
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to NULL  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid DELETE Request containing  | |
                     | To set to TARGET_ANNC_RESOURCE_ADDRESS  | |
                     |} | |
+———————-+——————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/UPD/002_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/UPD/002_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/UPD/002_GRP
	4 (group)

	TP/oneM2M/CSE/ANNC/UPD/002_LCP
	9 (locationPolicy)

	TP/oneM2M/CSE/ANNC/UPD/002_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/UPD/002_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/UPD/002_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/UPD/002_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/UPD/003
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/003

	Test objective
	Check that the IUT provides confirmation of resource de-announcement to the originator of the initiating request after a successful resource de-announcement procedure originator (for an UPDATE initiating resource de-announcement)

	Reference
	TS-0001 [1], clause 10.2.18.3, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
and the IUT having registered the AE
and the IUT having registered to the remoteCSE
and the IUT having created a RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ADDRESS
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
and the IUT having received a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
Content attribute containing
RESOURCE_TYPE resourcecontaining
announceTo attribute set to NULL
and the IUT having sent a valid DELETE Request containing
To set to TARGET_ANNC_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid Response from ANNC_TARGET_CSE containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT updates RESOURCE_TYPE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resourcecontaining  | |
                     | announceTo attribute set to NULL  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/UPD/003_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/UPD/003_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/UPD/003_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/UPD/003_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/UPD/003_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/UPD/003_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/UPD/003_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/UPD/003_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/UPD/004
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/004

	Test objective
	HOST CSE of original resource returns a valid response where value in announcedAttributes is removed if such attribute is not marked OA

	Reference
	TS-0001 [1], clause 10.2.18.1 and clause 10.2.18.4, TS-0004 [2], clause 7.3.1.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered to the CSE
and the IUT having registered the AE
and the IUT having a resource of type RESOURCE_TYPE at
TARGET_RESOURCE_ADDRESS
containing
announceTo attribute set to NULL
announcedAttribute attribute set to NULL
parentId attribute set to PARENT_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
and the resource at PARENT_RESOURCE_ADDRESS
containing
announceTo attribute set to ANNOUNCED_PARENT_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing RESOURCE_TYPE resource  | |
                     | containing  | |
                     | announceTo set to ANNC_TARGET_CSE_ID and  | |
                     | announcedAttributes attribute set to pi  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | announceTo attribute set to ANNOUNCED_RESOURCE_ADDRESS and  | |
                     | announcedAttributes set to empty  | |
                     |} | |
+———————-+————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/UPD/004_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/UPD/004_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/UPD/004_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/UPD/004_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/UPD/004_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/UPD/004_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/UPD/004_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/UPD/005
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/005

	Test objective
	Check that the labels attribute is de-announced when such attribute is deleted from the original resource

	Reference
	TS-0001 [1], clause 10.2.18.4 and clause 9.6.26.3-1, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the remoteCSE
and the IUT having created a container resource containing
announceTo attribute set to ANNC_TARGET_CSE_ADDRESS and
valid labels attribute
and the IUT having announced the container resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
CONTAINER_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | labels attribute set to NULL   | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | The IUT sends a valid UPDATE Request containing  | |
                     | To set to CONTAINER_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | containerAnnc resource containing  | |
                     | labels attribute set to NULL  | |
                     |} | |
+———————-+—————————————————————————————————————-+————-+
TP/oneM2M/CSE/ANNC/UPD/006
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/006

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource when a new CSE-ID is provided in announcedTo optional attribute and IUT having been already announced to announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT not having registered to the CSE
and the IUT having been announced to the announcement target CSE
and the IUT having created the RESOURCE_TYPE resource
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to CSE_BASE_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resourcecontaining  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/UPD/006_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/UPD/006_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/UPD/006_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/UPD/006_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/UPD/006_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/UPD/006_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/UPD/006_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/UPD/006_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/UPD/007
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/007

	Test objective
	Check that the IUT announces successfully the RESOURCE_TYPE resource when a new CSE-ID is provided in announcedTo optional attribute and IUT has registered and created a <remoteCSE> resource to the announcement target CSE

	Reference
	TS-0001 [1], clause 10.2.18.4, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created the RESOURCE_TYPE resource
and the IUT having registered and created a CSE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announceTo attribute set to ANNC_TARGET_CSE_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | The IUT sends a valid CREATE Request containing  | |
                     | To set to REMOTE_ANNC_TARGET_CSE_ID and  | |
                     | Content containing  | |
                     | CSEBaseAnnc resourcecontaining  | |
                     | MA (mandatory) attributes  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/UPD/007_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/UPD/007_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/UPD/007_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/UPD/007_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/UPD/007_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/UPD/007_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/UPD/007_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/UPD/007_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/UPD/008
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/008

	Test objective
	Check that the IUT provides confirmation of the announcement of an attribute to the originator of the initiating request after a successful attribute announcement procedure

	Reference
	TS-0001 [1], clause 10.2.18.6, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created a RESOURCE_TYPE resource containing
OA_ATTRIBUTE attribute set to VALUE and
announceTo attribute set to ANNC_TARGET_CSE_ID and
announcedAttribute attribute set to NULL
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
and the IUT having received a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
Content containing
RESOURCE_TYPE resource containing
announcedAttribute attribute set to OA_ATTRIBUTE
and the IUT having sent a valid UPDATE Request containing
To set to TARGET_ANNC_RESOURCE_ADDRESS and
Content containing
RESOURCE_TYPE announced variant resourcecontaining
OA_ATTRIBUTE attribute set to VALUE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid Response from CSE containing  | |
                     | Response Status Code set to 2004 (UPDATED) containing  | |
                     | valid RESOURCE_TYPE announced variant resource representation  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT updates the RESOURCE_TYPE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announcedAttribute attribute set to OA_ATTRIBUTE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE
	OA_ATTRIBUTE

	TP/oneM2M/CSE/ANNC/UPD/008_CNT/MBS
	3 (container)
	maxByteSize

	TP/oneM2M/CSE/ANNC/UPD/008_GRP/MNM
	9 (group)
	maxNrOfMembers

	TP/oneM2M/CSE/ANNC/UPD/008_LCP/LOI
	10 (locationPolicy)
	locationContainerID

	TP/oneM2M/CSE/ANNC/UPD/008_MGO/DC
	13 (mgmtObj)
	description

	TP/oneM2M/CSE/ANNC/UPD/008_NOD/HCL
	14 (node)
	hostedCSELink

	TP/oneM2M/CSE/ANNC/UPD/008_SCH/SE
	18 (schedule)
	scheduleElement

	TP/oneM2M/CSE/ANNC/UPD/008_TS/MBS
	29 (timeSeries)
	maxByteSize



TP/oneM2M/CSE/ANNC/UPD/009
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/009

	Test objective
	Check that the IUT updates successfully RESOURCE_TYPE announced variant resource when a new OA attribute is provided to announcedAttribute attribute of the original resource

	Reference
	TS-0001 [1], clause 10.2.18.8, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created a RESOURCE_TYPE resource containing
OA_ATTRIBUTE attribute set to VALUE and
announceTo attribute set to ANNC_TARGET_CSE_ID and
announcedAttribute attribute set to NULL
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announcedAttribute attribute set to OA_ATTRIBUTE  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid UPDATE Request containing  | |
                     | To set to TARGET_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | OA_ATTRIBUTE attribute set to VALUE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE
	OA_ATTRIBUTE

	TP/oneM2M/CSE/ANNC/UPD/009_CNT/MBS
	3 (container)
	maxByteSize

	TP/oneM2M/CSE/ANNC/UPD/009_GRP/MNM
	9 (group)
	maxNrOfMembers

	TP/oneM2M/CSE/ANNC/UPD/009_LCP/LOI
	10 (locationPolicy)
	locationContainerID

	TP/oneM2M/CSE/ANNC/UPD/009_MGO/DC
	13 (mgmtObj)
	description

	TP/oneM2M/CSE/ANNC/UPD/009_NOD/HCL
	14 (node)
	hostedCSELink

	TP/oneM2M/CSE/ANNC/UPD/009_SCH/SE
	18 (schedule)
	scheduleElement

	TP/oneM2M/CSE/ANNC/UPD/009_TS/MBS
	29 (timeSeries)
	maxByteSize



TP/oneM2M/CSE/ANNC/UPD/010
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/010

	Test objective
	Check that the IUT updates successfully the RESOURCE_TYPE announced variant resource when a MA attribute of its original resource is updated

	Reference
	TS-0001 [1], clause 10.2.18.10, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created a RESOURCE_TYPE resource containing
expirationTime attribute set to VALUE_1 and
announceTo attribute set to ANNC_TARGET_CSE_ID
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | expirationTime attribute set to VALUE_2  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid UPDATE Request containing  | |
                     | To set to TARGET_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | expirationTime attribute set to VALUE_2  | |
                     |} | |
+———————-+———————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/UPD/010_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/UPD/010_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/UPD/010_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/UPD/010_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/UPD/010_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/UPD/010_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/UPD/010_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/UPD/010_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/UPD/011
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/011

	Test objective
	Check that the IUT updates successfully the RESOURCE_TYPE announced variant resource when a optional attribute present in the announcedAttribute attribute of its original resource is updated

	Reference
	TS-0001 [1], clause 10.2.18.10, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created a RESOURCE_TYPE resource containing
OA_ATTRIBUTE attribute set to VALUE_1 and
announceTo attribute set to ANNC_TARGET_CSE_ID and
announcedAttribute attribute set to OA_ATTRIBUTE
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | OA_ATTRIBUTE attribute set to VALUE_2  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid UPDATE Request containing  | |
                     | To set to TARGET_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | OA_ATTRIBUTE attribute set to VALUE_2  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE
	OA_ATTRIBUTE

	TP/oneM2M/CSE/ANNC/UPD/011_CNT/MBS
	3 (container)
	maxByteSize

	TP/oneM2M/CSE/ANNC/UPD/011_GRP/MNM
	9 (group)
	maxNrOfMembers

	TP/oneM2M/CSE/ANNC/UPD/011_LCP/LOI
	10 (locationPolicy)
	locationContainerID

	TP/oneM2M/CSE/ANNC/UPD/011_MGO/DC
	13 (mgmtObj)
	description

	TP/oneM2M/CSE/ANNC/UPD/011_NOD/HCL
	14 (node)
	hostedCSELink

	TP/oneM2M/CSE/ANNC/UPD/011_SCH/SE
	18 (schedule)
	scheduleElement

	TP/oneM2M/CSE/ANNC/UPD/011_TS/MBS
	29 (timeSeries)
	maxByteSize



TP/oneM2M/CSE/ANNC/UPD/012
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/012

	Test objective
	Check that the IUT de-announces successfully an announced attribute when such attribute is deleted from announcedAttribute attribute

	Reference
	TS-0001 [1], clause 10.2.18.9, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created a RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ID and
announcedAttribute attribute set to OA_ATTRIBUTE and
valid OA_ATTRIBUTE attribute
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | announcedAttribute attribute set to NULL  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid UPDATE Request containing  | |
                     | To set to TARGET_ANNC_RESOURCE_ADDRESS and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | OA_ATTRIBUTE attribute set to NULL  | |
                     |} | |
+———————-+———————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE
	OA_ATTRIBUTE

	TP/oneM2M/CSE/ANNC/UPD/012_CNT/MBS
	3 (container)
	maxByteSize

	TP/oneM2M/CSE/ANNC/UPD/012_GRP/MT
	9 (group)
	memberType

	TP/oneM2M/CSE/ANNC/UPD/012_LCP/LOI
	10 (locationPolicy)
	locationContainerID

	TP/oneM2M/CSE/ANNC/UPD/012_MGO/DC
	13 (mgmtObj)
	description

	TP/oneM2M/CSE/ANNC/UPD/012_NOD/HCL
	14 (node)
	hostedCSELink

	TP/oneM2M/CSE/ANNC/UPD/012_SCH/SE
	18 (schedule)
	scheduleElement

	TP/oneM2M/CSE/ANNC/UPD/012_TS/MBS
	29 (timeSeries)
	maxByteSize



TP/oneM2M/CSE/ANNC/UPD/013
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/013

	Test objective
	Check that the IUT provides confirmation of the de-announcement of an attribute to the originator of the initiating request after a successful attribute de-announcement procedure

	Reference
	TS-0001 [1], clause 10.2.18.7, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created a RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ID and
announcedAttribute attribute set to OA_ATTRIBUTE and
valid OA_ATTRIBUTE attribute
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
and the IUT having received a valid UPDATE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS and
Content containing
RESOURCE_TYPE resource containing
announcedAttribute attribute set to NULL
and The IUT having sent a valid UPDATE Request containing
To set to TARGET_ANNC_RESOURCE_ADDRESS and
Content containing
RESOURCE_TYPE announced variant resource containing
OA_ATTRIBUTE attribute set to NULL
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid Response from CSE containing  | |
                     | Response Status Code set to 2004 (UPDATED) containing  | |
                     | RESOURCE_TYPE announced variant resource containing  | |
                     | no OA_ATTRIBUTE attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT updates the RESOURCE_TYPE resource  | |
                     | and the IUT sends valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | RESOURCE_TYPE resource containing  | |
                     | no announcedAttribute attribute  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE
	OA_ATTRIBUTE
	PICS

	TP/oneM2M/CSE/ANNC/UPD/013_CNT/MBS
	3 (container)
	maxByteSize
	PICS_IN_PROFILE

	TP/oneM2M/CSE/ANNC/UPD/013_GRP/MNM
	9 (group)
	maxNrOfMembers
	

	TP/oneM2M/CSE/ANNC/UPD/013_LCP/LOI
	10 (locationPolicy)
	locationContainerID
	

	TP/oneM2M/CSE/ANNC/UPD/013_MGO/DC
	13 (mgmtObj)
	description
	

	TP/oneM2M/CSE/ANNC/UPD/013_NOD/HCL
	14 (node)
	hostedCSELink
	

	TP/oneM2M/CSE/ANNC/UPD/013_SCH/SE
	18 (schedule)
	scheduleElement
	

	TP/oneM2M/CSE/ANNC/UPD/013_TS/MBS
	29 (timeSeries)
	maxByteSize
	



TP/oneM2M/CSE/ANNC/UPD/014
	TP Id
	TP/oneM2M/CSE/ANNC/UPD/014

	Test objective
	Check that the IUT removes an announcement target CSE from the announceTo attribute if it does not return successful CREATE response for the announced resource (for an UPDATE initiating resource announcement)

	Reference
	TS-0001 [1], clause 10.2.18.4

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the CSE
and the IUT having created the container resource
and the AE having privileges to perform UPDATE operation on the resource
CONTAINER_RESOURCE_ADDRESS
and the IUT having received a valid UPDATE Request from AE containing
To set to CONTAINER_RESOURCE_ADDRESS and
From set to AE-ID and
Content containing
container resource containing
announceTo attribute set to ANNC_TARGET_CSE_ID
and the IUT having created a CSEBaseAnnc at CSE_BASE_ANNC_RESOURCE_ADDRESS
and The IUT having sent a valid CREATE Request containing
To set to CSE_BASE_ANNC_RESOURCE_ADDRESS and
Content containin g
containerAnnc resource containing
MA (mandatory) attributes
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid Response from CSE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT updates the container resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)and  | |
                     | Content containing  | |
                     | container resourcecontaining  | |
                     | announceTo attribute empty  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————+————-+
7.2.2.11.5	DELETE Operation
TP/oneM2M/CSE/ANNC/DEL/001
	TP Id
	TP/oneM2M/CSE/ANNC/DEL/001

	Test objective
	Check that the IUT provides confirmation of resource de-announcement to the originator of the initiating request after a successful resource de-announcement procedure (for a DELETE initiating resource de-announcement)

	Reference
	TS-0001 [1], clause 10.2.18.3, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
and the IUT having registered the AE
and the IUT having registered to the remoteCSE
and the IUT having created a RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ADDRESS
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform DELETE operation on the resource
TARGET_RESOURCE_ADDRESS
and the IUT having received a valid DELETE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS
and the IUT having sent a valid DELETE Request containing
To set to TARGET_ANNC_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE |
                     | the IUT receives a valid Response from ANNC_TARGET_CSE  | |
                     | containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT deletes the RESOURCE_TYPE resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/DEL/001_ACP
	1 (accesControlPolicy)

	TP/oneM2M/CSE/ANNC/DEL/001_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/DEL/001_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/DEL/001_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/DEL/001_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/DEL/001_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/DEL/001_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/DEL/001_TS
	29 (timeSeries)



TP/oneM2M/CSE/ANNC/DEL/002
	TP Id
	TP/oneM2M/CSE/ANNC/DEL/002

	Test objective
	Check that the IUT deletes all announced resources when the original resource is deleted

	Reference
	TS-0001 [1], clause 9.6.26.1 and clause 10.2.18.5, TS-0004 [2], clause 7.3.3.10

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having registered to the remoteCSE
and the IUT having created a RESOURCE_TYPE resource containing
announceTo attribute set to ANNC_TARGET_CSE_ADDRESS
and the IUT having announced the RESOURCE_TYPE resource to the announcement target CSE
and the AE having privileges to perform DELETE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => CSE |
                     | The IUT sends a valid DELETE Request containing  | |
                     | To set to TARGET_RESOURCE_ANNC_ADDRESS  | |
                     |} | |
+———————-+————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/ANNC/DEL/002_ACP
	1(accesControlPolicy)

	TP/oneM2M/CSE/ANNC/DEL/002_CNT
	3 (container)

	TP/oneM2M/CSE/ANNC/DEL/002_GRP
	9 (group)

	TP/oneM2M/CSE/ANNC/DEL/002_LCP
	10 (locationPolicy)

	TP/oneM2M/CSE/ANNC/DEL/002_MGO
	13 (mgmtObj)

	TP/oneM2M/CSE/ANNC/DEL/002_NOD
	14 (node)

	TP/oneM2M/CSE/ANNC/DEL/002_SCH
	18 (schedule)

	TP/oneM2M/CSE/ANNC/DEL/002_TS
	29 (timeSeries)



7.2.2.12	3GPP interworking (3GPP)
7.2.2.12.1	BASIC Operation
TP/oneM2M/CSE/3GPP/TRIG/001
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/001

	Test objective
	Check that the IUT sends an explicit 3GPP Device Trigger Request when it receives a valid <triggerRequest> from an A

	Reference
	TS-0026 [5], clause 7.5.1, step 3a

	Parent Release
	Release 3

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE1
and the AE1being hosted on a 3GPP UE
and the IUT allowing to register an AE2
}



·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid CREATE request from AE2 containing  | |
                     | To set to AE2_RESOURCE_ADDRESS and  | |
                     | From set to AE2_ID and  | |
                     | Resource Type set to 38 (triggerRequest) and  | |
                     | Content containing  | |
                     | triggerRequest resource containing  | |
                     | triggerPurpose set to TRIGGER_PURPOSE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT send s a Request to the SCEF containing  | |
                     | 3GPP Device Trigger Request message containing  | |
                     | A valid 3GPP Device Trigger Request containing  | |
                     | triggerPayload attribute  | |
                     |} | |
+———————-+———————————————————————————————————-+————-+
	TP Id
	TRIGGER_PURPOSE

	TP/oneM2M/CSE/3GPP/TRIG/001_CON
	establishConnection

	TP/oneM2M/CSE/3GPP/TRIG/001_REQ
	registrationRequest

	TP/oneM2M/CSE/3GPP/TRIG/001_EXE
	executeCRUD

	TP/oneM2M/CSE/3GPP/TRIG/001_ENR
	enrolmentRequest



TP/oneM2M/CSE/3GPP/TRIG/002
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/002

	Test objective
	Check that the IUT sends an implicit 3GPP Device Trigger Request when it receives a valid <notification> from an AE

	Reference
	TS-0026 [5], clause 7.5.1

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE1
and the AE1being hosted on a 3GPP UE
and the AE1 having subscribed to CONTAINER_RESOURCE_ADDRESS
and the AE1 being not reachable
and the IUT allowing to register an AE2
}



·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives the UPDATE request from the AE2 containing  | |
                     | To set to CONTAINER_RESOURCE_ADDRESS containing  | |
                     | From set to AE2_ID and  | |
                     | Content containing  | |
                     | container resource containing  | |
                     | valid labels attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT send s a Request to the SCEF containing  | |
                     | 3GPP Device Trigger Request message containing  | |
                     | A valid 3GPP Device Trigger Requestcontaining  | |
                     | triggerPayload_ attribute set to NULL  | |
                     |} | |
+———————-+———————————————————————————————————+————-+
TP/oneM2M/CSE/3GPP/TRIG/003
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/003

	Test objective
	Check that the IUT sets the triggerStatus attribute of the <triggerRequest> to ERROR_NSE_NOT_FOUND when the SCEF does not respond to the Device Trigger Request prior to the timeout period

	Reference
	TS-0026 [5], clause 7.5.1, step 3

	Parent Release
	Release 3

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE1
and the AE1being hosted on a 3GPP UE
and the IUT allowing to register an AE2
and the AE2 having created a <triggerRequest> resource
and the IUT having sent a 3GPP Device Trigger Request
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT does not receive a reponse from SCEF  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT |
                     | the IUT updates <triggerRequest> resource containing  | |
                     | triggerStatus attribute set to ERROR_NSE_NOT_FOUND  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/3GPP/TRIG/004
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/004

	Test objective
	Check that the IUT sets the triggerStatus attribute of the <triggerRequest> to the proper value when the SCEF responds to the Device Trigger Request

	Reference
	TS-0026 [5], clause 7.5.1, step 3b

	Parent Release
	Release 3

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE1
and the AE1being hosted on a 3GPP UE
and the IUT allowing to register an AE2
and AE2 having created a TRIGGER_REQUEST
and the IUT having sent a POST 3GPP Device Trigger Request
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= SCEF |
                     | the IUT receives a valid Device Triggering response from SCEF | |
                     | containing  | |
                     | deliveryResult set to SCEF_RESULT  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT sets triggerStatus attribute of TRIGGER_REQUEST to | |
                     | TRIGGER_RESULT  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+
	TP Id
	SCEF_RESULT
	TRIGGER_RESULT

	TP/oneM2M/CSE/3GPP/TRIG/004_1
	SUCCESS
	TRIGGER-DELIVERED

	TP/oneM2M/CSE/3GPP/TRIG/004_2
	UNKNOWN
	TRIGGER-FAILED

	TP/oneM2M/CSE/3GPP/TRIG/004_3
	FAILURE
	TRIGGER-FAILED

	TP/oneM2M/CSE/3GPP/TRIG/004_4
	TRIGGERED
	TRIGGER-TRIGGERED

	TP/oneM2M/CSE/3GPP/TRIG/004_5
	EXPIRED
	TRIGGER-EXPIRED

	TP/oneM2M/CSE/3GPP/TRIG/004_6
	UNCONFIRMED
	TRIGGER-UNCONFIRMED

	TP/oneM2M/CSE/3GPP/TRIG/004_7
	REPLACED
	TRIGGER-FAILED

	TP/oneM2M/CSE/3GPP/TRIG/004_8
	TERMINATE
	TRIGGER-TERMINATED



TP/oneM2M/CSE/3GPP/TRIG/005
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/005

	Test objective
	Check that the IUT returns a HTTP response when it receives a valid DeviceTriggeringDeliveryReportNotification Report message

	Reference
	TS-0026 [5], clause 7.5.1, step 6 and 7

	Parent Release
	Release 3

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE1
and the AE1being hosted on a 3GPP UE
and the IUT allowing to register an AE2
and AE2 having created a TRIGGER_REQUEST
and the IUT having sent a POST 3GPP Device Trigger Request
}



·                  +--------+----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= SCEF |
                     | the IUT receives a valid DeviceTriggeringDeliveryReportNotification  | |
                     | request from SCEF containing  | |
                     | deliveryResult set to SCEF_RESULT  | |
                     |} | |
·                  +--------+----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT sets triggerStatus attribute of TRIGGER_REQUEST to  | |
                     | TRIGGER_RESULT  | |
                     | and the IUT sends a valid HTTP response containing  | |
                     | Response Code set to 204 (NO_CONTENT)  | |
                     |} | |
+———————-+——–+—————————————————————————————————————-+————-+
	TP Id
	SCEF_RESULT
	TRIGGER_RESULT

	TP/oneM2M/CSE/3GPP/TRIG/005_1
	SUCCESS
	TRIGGER-DELIVERED

	TP/oneM2M/CSE/3GPP/TRIG/005_2
	UNKNOWN
	TRIGGER-FAILED

	TP/oneM2M/CSE/3GPP/TRIG/005_3
	FAILURE
	TRIGGER-FAILED

	TP/oneM2M/CSE/3GPP/TRIG/005_4
	TRIGGERED
	TRIGGER-TRIGGERED

	TP/oneM2M/CSE/3GPP/TRIG/005_5
	EXPIRED
	TRIGGER-EXPIRED

	TP/oneM2M/CSE/3GPP/TRIG/005_6
	UNCONFIRMED
	TRIGGER-UNCONFIRMED

	TP/oneM2M/CSE/3GPP/TRIG/005_7
	REPLACED
	TRIGGER-FAILED

	TP/oneM2M/CSE/3GPP/TRIG/005_8
	TERMINATE
	TRIGGER-TERMINATED



TP/oneM2M/CSE/3GPP/TRIG/006
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/006

	Test objective
	Check that the IUT sends an explicit Device Trigger Replace Request when it receives a valid Device Trigger Replace Request from an AE

	Reference
	TS-0001 [1], clause 8.3.3.2.2 and clause 9.6.49, TS-0026 [5], clause 7.5.2

	Parent Release
	Release 4

	Config Id
	CF05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE2
and the AE2being hosted on a 3GPP UE
and the IUT allowing to register an AE1
and AE1 having created a TRIGGER_REQUEST
and the IUT having a <triggerRequest> resource at TARGET_RESOURCE_ADDRESS
and the IUT having sent a POST 3GPP Device Trigger Request containing
triggerReference
and the IUT having not received a Response for Device Trigger Request
}



·                  +-------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid UPDATE request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => SCEF |
                     | the IUT assigns a new triggerReference for the new trigger  | |
                     | message  | |
                     | and the IUT sends a HTTP PUT 3GPP Request to the SCEF  | |
                     | targeting the correct transactionID containing  | |
                     | 3GPP Device Trigger Request message containing  | |
                     | a valid 3GPP Device Replace Request with updated  | |
                     | triggerReference  | |
                     |} | |
+———————-+————————————————————————————————————————-+————-+
TP/oneM2M/CSE/3GPP/TRIG/007
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/007

	Test objective
	Check that the IUT sends an explicit Device Trigger Recall Request when it receives a valid Device Trigger Recall Request from an AE

	Reference
	TS-0001 [1], clause 8.3.3.2 and clause 9.6.49, TS-0026 [5], clause 7.5.2

	Parent Release
	Release 4

	Config Id
	CF05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE2
and the AE2being hosted on a 3GPP UE
and the IUT allowing to register an AE1
and AE1 having created a TRIGGER_REQUEST
and the IUT having a <triggerRequest> resource at TARGET_RESOURCE_ADDRESS
and the IUT having sent a POST 3GPP Device Trigger Request
and the IUT having not received a Response for Device Trigger Request
}



·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid DELETE request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT sends a HTTP DELETE 3GPP Request to the SCEF  | |
                     | targeting the correct transactionID with NULL payload  | |
                     |} | |
+———————-+———————————————————————————————————————–+————-+
TP/oneM2M/CSE/3GPP/TRIG/008
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/008

	Test objective
	Check that the IUT sends an implicit (initiated by IN-CSE) Device Trigger Replace Request when it determines there is a need for a Replace based on internal policies

	Reference
	TS-0001 [1], clause 8.3.3.2.2 and clause 9.6.49, TS-0026 [5], clause 7.5.2

	Parent Release
	Release 4

	Config Id
	CF05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and IUT having created a TRIGGER_REQUEST for TARGET_RESOURCE
and TARGET_RESOURCE (AE/MN-CSE/ADN-AE)being hosted on a 3GPP UE
and the IUT having a <triggerRequest> resource
and the IUT having sent a POST 3GPP Device Trigger Request for
TARGET_RESOURCE containing triggerReference
and the IUT having not received a Response for Device Trigger Request
}



·                  +-----+--------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT generates a UPDATE <triggerRequest> message after  | |
                     | determining a need for a Trigger Request Replace based on internal  | |
                     | policies  | |
                     |} | |
·                  +-----+--------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT assigns a new triggerReference for the new trigger  | |
                     | message  | |
                     | and the IUT sends a HTTP PUT 3GPP Request to the SCEF  | |
                     | targeting the correct transactionID containing  | |
                     | 3GPP Device Trigger Request message containing  | |
                     | a valid 3GPP Device Replace Request with updated  | |
                     | triggerReference  | |
                     |} | |
+———————-+—–+——————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/3GPP/TRIG/009
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/009

	Test objective
	Check that the IUT sends an implicit (initiated by IN-CSE) Device Trigger Recall Request when it determines there is a need for a Recall based on internal policies

	Reference
	TS-0001 [1], clause 8.3.3.2 and clause 9.6.49, TS-0026 [5], clause 7.5.2

	Parent Release
	Release 4

	Config Id
	CF05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and IUT having created a TRIGGER_REQUEST for TARGET_RESOURCE
and TARGET_RESOURCE (AE/MN-CSE/ADN-AE) being hosted on a 3GPP UE
and the IUT having a <triggerRequest> resource
and the IUT having sent a POST 3GPP Device Trigger Request for
TARGET_RESOURCE containing triggerReference
and the IUT having not received a Response for Device Trigger Request
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT generates a DELETE <triggerRequest> message after  | |
                     | determining a need for a Trigger Request Recall based on  | |
                     | internal policies  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT sends a HTTP DELETE 3GPP Request to the  | |
                     | SCEF targeting the correct transactionID with NULL payload  | |
                     |} | |
+———————-+——————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/3GPP/TRIG/010
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/010

	Test objective
	Check that the IUT sets the triggerStatus attribute of the <triggerRequest> to ERROR_NSE_NOT_FOUND when the SCEF does not respond to the Device Trigger Recall/Replace Request prior to the timeout period

	Reference
	TS-0026 [5], clause 7.5.2, step 3

	Parent Release
	Release 4

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and IUT having created a TRIGGER_REQUEST for TARGET_RESOURCE
and TARGET_RESOURCE (AE/MN-CSE/ADN-AE) being hosted on a 3GPP UE
and the IUT having a <triggerRequest> resource
and the IUT having sent a 3GPP Device Trigger Replace/Recall Request
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT does not receive a response from SCEF for the 3GPP  | |
                     | Device Trigger Replace/Recall Request  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT |
                     | the IUT updates <triggerRequest> resource containing  | |
                     | triggerStatus attribute set to ERROR_NSE_NOT_FOUND  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/3GPP/TRIG/011
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/011

	Test objective
	Check that the IUT sets the triggerStatus attribute of the <triggerRequest> to the proper value and generates an appropriate response to AE when the SCEF responds to the Device Trigger Replace Request

	Reference
	TS-0004 [2], clause 6.6.3 and clause 7.4.57.2.3, TS-0026 [5], clause 7.5.2 and clause 8.3.1

	Parent Release
	Release 4

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE2
and the AE2being hosted on a 3GPP UE
and the IUT allowing to register an AE1
and AE1 having initiated a TRIGGER_REQUEST
and the IUT having a <triggerRequest> resource
and the IUT having sent a PUT 3GPP Device Trigger Replace Request
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= SCEF |
                     | the IUT receives a valid Device Triggering response from SCEF  | |
                     | containing  | |
                     | SCEF_RESULT_RESPONSE_CODE  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sets triggerStatus attribute of a <triggerRequest> resource  | |
                     | to TRIGGER_RESULT  | |
                     | and the IUT sends a valid response to AE1  | |
                     | containing  | |
                     | Response Status Code set to TRIGGER_RESPONSE_CODE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————+————-+
	TP Id
	SCEF_RESULT_RESPONSE_CODE
	TRIGGER_RESULT
	TRIGGER_RESPONSE_CODE

	TP/oneM2M/CSE/3GPP/TRIG/011_1
	200 OK( deliveryResult set to REPLACED)
	TRIGGER-REPLACED
	2004 (UPDATED)

	TP/oneM2M/CSE/3GPP/TRIG/011_2
	400 Bad Request
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_3
	401 Unauthorized
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_4
	403 Forbidden
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_5
	404 Not Found
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_6
	411 Length Required
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_7
	413 Payload Too Large
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_8
	415 Unsupported Media Type
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_9
	429 Too Many Requests
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_10
	500 Internal Server Error
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/011_11
	503 Service Unavailable
	TRIGGER-FAILED
	5219 (UNABLE_TO_REPLACE_REQUEST)



TP/oneM2M/CSE/3GPP/TRIG/012
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/012

	Test objective
	Check that the IUT deletes the <triggerRequest> resource and generates an appropriate response to AE when it receives a successful trigger recall response from SCEF

	Reference
	TS-0004 [2], clause 6.6.3 and clause 7.4.57.2.4, TS-0026 [5], clause 7.5.2

	Parent Release
	Release 4

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE2
and the AE2being hosted on a 3GPP UE
and the IUT allowing to register an AE1
and AE1 having created a TRIGGER_REQUEST
and the IUT having a <triggerRequest> resource
and the IUT having sent a POST 3GPP Device Trigger Request
and the IUT having not received a Response for Device Trigger Request
and the AE1 having sent a DELETE <triggerRequest> request to the IUT
and the IUT having sent a DELETE 3GPP Device Trigger Recall Request
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= SCEF |
                     | the IUT receives a valid Device Triggering response from SCEF/ | |
                     | containing  | |
                     | Response Status Code set to 204 (NO CONTENT)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT deletes the <triggerRequest> resource  | |
                     | and the IUT sends a valid response to AE1  | |
                     | containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/3GPP/TRIG/013
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/013

	Test objective
	Check that the IUT does not delete the <triggerRequest> resource and generates an appropriate response to AE when it receives an unsuccessful trigger recall response from SCEF

	Reference
	TS-0004 [2], clause 6.6.3 and clause 7.4.57.2.4, TS-0026 [5], clause 7.5.2, 8.3.1

	Parent Release
	Release 4

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE2
and the AE2being hosted on a 3GPP UE
and the IUT allowing to register an AE1
and AE1 having created a TRIGGER_REQUEST
and the IUT having a <triggerRequest> resource
and the IUT having sent a POST 3GPP Device Trigger Request
and the IUT having not received a Response for Device Trigger Request
and the AE1 having sent a DELETE <triggerRequest> request to the IUT
and the IUT having sent a DELETE 3GPP Device Trigger Recall Request
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= SCEF |
                     | the IUT receives a valid Device Triggering response from SCEF  | |
                     | containing  | |
                     | Response Status Code set to SCEF_ERROR_CODE  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid response to AE1  | |
                     | containing  | |
                     | Response Status Code set to TRIGGER RESPONSE_CODE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————+————-+
	TP Id
	SCEF _ERROR_CODE
	TRIGGER_RESPONSE_CODE

	TP/oneM2M/CSE/3GPP/TRIG/013_1
	400 Bad Request
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_2
	401 Unauthorized
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_3
	403 Forbidden
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_4
	404 Not Found
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_5
	411 Length Required
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_6
	413 Payload Too Large
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_7
	415 Unsupported Media Type
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_8
	429 Too Many Requests
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_9
	500 Internal Server Error
	5220 (UNABLE_TO_RECALL_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/013_10
	503 Service Unavailable
	5220 (UNABLE_TO_RECALL_REQUEST)



TP/oneM2M/CSE/3GPP/TRIG/014
	TP Id
	TP/oneM2M/CSE/3GPP/TRIG/014

	Test objective
	Check that the IUT does not accept the request for Trigger Replace and Recall operation if the original Device Trigger request has already been processed and responds with an error

	Reference
	TS-0001 [1], clause 9.6.49, TS-0004 [2], clause 6.6.3.6 and clause 7.4.57.2, TS-0026 [5], clause 7.5.2 and clause 8.3.1

	Parent Release
	Release 4

	Config Id
	CFG05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT allowing to register an AE2
and the AE2being hosted on a 3GPP UE
and the IUT allowing to register an AE1
and AE1 having created a TRIGGER_REQUEST
and the IUT having a <triggerRequest> resource at TARGET_RESOURCE_ADDRESS
containing triggerStatus not set to PROCESSING
and the IUT having sent a POST 3GPP Device Trigger Request
and the IUT having received a Response for Device Trigger Request
and the IUT having processed the Device Trigger Request
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid OPERATION request from AE1  | |
                     | containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid response to AE1  | |
                     | containing  | |
                     | Response Status Code set to ERROR_RESPONSE_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION
	ERROR_RESPONSE_CODE

	TP/oneM2M/CSE/3GPP/TRIG/014_1
	UPDATE
	5219 (UNABLE_TO_REPLACE_REQUEST)

	TP/oneM2M/CSE/3GPP/TRIG/014_2
	DELETE
	5220 (UNABLE_TO_RECALL_REQUEST)



7.2.2.12.2	SCEF-based NIDD
TP/oneM2M/CSE/3GPP/NIDD/001
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/001

	Test objective
	Check that the IUT sends NIDD configuration request when it receives create request of <serviceSubscribedNode> resource associated with a UE hosting an ADN-AE with niddRequired attribute set to TRUE.

	Reference
	TS-0026 [5], clause 7.1.1.1

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_IN_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE request from AE  | |
                     | containing To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Typeset to 20(serviceSubscribedNode) and  | |
                     | Content containing valid serviceSubscribedNode resource  | |
                     | representation containing niddRequired attribute set to TRUE  | |
                     |and nodeID attribute set to M2M‑Ext‑ID of UE hosting an AND‑AE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT sends a valid Request to the SCEF  | |
                     | containing NIDD configuration Request message containing  | |
                     | a valid NIDD configuration Request  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/3GPP/NIDD/002
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/002

	Test objective
	Check that the IUT issues NIDD configuration request when it receives update request of <serviceSubscribedNode> resource associated with a UE hosting an ADN-AE to set niddRequired attribute TRUE.

	Reference
	TS-0026 [5], clause 7.1.1.1

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <serviceSubscribedNode> resource at
TARGET_RESOURCE_ADDRESS containing niddRequired attribute set to False
and nodeID attribute set to M2M-Ext-ID of UE hosting an AND-AE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE request from AE  | |
                     | containing To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing valid serviceSubscribedNode resource  | |
                     | representation containing niddRequired attribute set to TRUE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT send s a valid Request to the SCEF  | |
                     | containing NIDD configuration Request message containing  | |
                     | A NIDD configuration Request  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/3GPP/NIDD/003
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/003

	Test objective
	Check that the IUT issues NIDD configuration delete request when it receives update request of <serviceSubscribedNode> resource associated with a UE hosting an ADN-AE to set niddRequired attribute False.

	Reference
	TS-0026 [5], clause 7.1.1.1

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_IN_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <serviceSubscribedNode> resource at
TARGET_RESOURCE_ADDRESS containing niddRequired_ attribute set to True
and nodeID attribute set to M2M-Ext-ID of UE hosting an AND-AE
and the AE having privileges to perform UPDATE operation on the resource
TARGET_RESOURCE_ADDRESS and
IUT having established NIDD configuration for M2M-Ext-ID
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE request from AE  | |
                     | containing To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing valid serviceSubscribedNode resource  | |
                     | representation containing niddRequired attribute set to  | |
                     | FALSE  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT send s a valid Request to the SCEF  | |
                     | containing  | |
                     | NIDD configuration delete Request message containing  | |
                     | A NIDD configuration delete Request  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/3GPP/NIDD/004
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/004

	Test objective
	Check that the IUT issues NIDD configuration delete request when it receives delete request of <serviceSubscribedNode> resource associated with a UE hosting an ASN/MN-CSE or ADN-AE.

	Reference
	TS-0026 [5], clause 7.1.1.1

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_IN_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <serviceSubscribedNode> resource at
TARGET_RESOURCE_ADDRESS containing niddRequired attribute set to True
and nodeID attribute set to M2M-Ext-ID of UE hosting an AND-AE
and the AE having privileges to perform DELETE operation on the resource
TARGET_RESOURCE_ADDRESS
IUT having established NIDD configuration for M2M-Ext-ID
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE request from AE  | |
                     | containing To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT send s a valid Request to the SCEF  | |
                     | containing  | |
                     | NIDD configuration delete Request message containing  | |
                     | A NIDD configuration delete Request  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/3GPP/NIDD/005
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/005

	Test objective
	Check that the IUT issues SCEF-based Mobile Terminated (MT) NIDD Downlink Data Transfer Request if the size of the oneM2M request primitive to be sent in the MT NIDD Request is less than or equal to the maximumPacketSize defined in the NIDD Configuration response.

	Reference
	TS-0026 [5], clause 7.1.1.2

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_IN_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having done successful NIDD Configuration Request for the targeted
ADN-AE hosted on a UE
and size of the oneM2M request primitive to be sent in the MT NIDD Request is less than or equal to the maximumPacketSize defined in the NIDD Configuration response.
and the IUT having registered the IN-AE
and the IUT having registered the AE1 hosted on AND-AE containing valid M2M-Ext-ID attribute
and the IN-AE having created the container resource
CONTAINER_RESOURCE_ADDRESS containing
subscription child resource containing notificationURI attribute set to AE1
and notificationEventType attribute set to 3
and the IN-AE having privileges to perform CREATE operation on the resource
CONTAINER_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= IN‑AE |
                     | the IUT receives a valid CREATE request from IN‑AE  | |
                     | containing To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to IN‑AE and  | |
                     | Content containing valid contentInstance resource  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT send s a valid MT NIDD Downlink Data Transfer Request to  | |
                     |the SCEF  | |
                     | containing   | |
                     |Non‑IP data containing oneM2M request primitive containing Content containing valid Notification  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/3GPP/NIDD/006
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/006

	Test objective
	Check that the IUT does not issue SCEF-based Mobile Terminated (MT) NIDD Downlink Data Transfer Request if the size of the oneM2M request primitive to be sent in the MT NIDD Request is more than the maximumPacketSize defined in the NIDD Configuration response.

	Reference
	TS-0026 [5], clause 7.1.1.2

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_IN_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having done successful NIDD Configuration Request for the targeted
ADN-AE hosted on a UE
and size of the oneM2M request primitive to be sent in the MT NIDD Request is more than the maximumPacketSize defined in the NIDD Configuration response.
and the IUT having registered the IN-AE
and the IUT having registered the AE1 hosted on AND-AE containing valid M2M-Ext-ID attribute
and the IN-AE having created the container resource
CONTAINER_RESOURCE_ADDRESS containing
subscription child resource containing notificationURI attribute set to AE1
and notificationEventType attribute set to 3
and the IN-AE having privileges to perform CREATE operation on the resource
CONTAINER_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= IN‑AE |
                     | the IUT receives a valid CREATE request from IN‑AE  | |
                     | containing To set to CONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to IN‑AE and  | |
                     | Content containing valid contentInstance resource  | |
                     | } | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   | |
                     | the IUT does not send a MT NIDD Downlink Data Transfer Request to the SCEF  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/3GPP/NIDD/007
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/007

	Test objective
	Check that the IUT issues SCEF-based Mobile Terminated (MT) NIDD Downlink Data Transfer Request if the size of the oneM2M response primitive to be sent in the MT NIDD Request is less than or equal to the maximumPacketSize defined in the NIDD Configuration response.

	Reference
	TS-0026 [5], clause 7.1.1.2

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_IN_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having done successful NIDD Configuration Request for the targeted
ADN-AE hosted on a UE
and size of the oneM2M response primitive to be sent in the MT NIDD Request is less
than or equal to the maximumPacketSize defined in the NIDD Configuration response.
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE1 |
                     | the IUT receives a valid MO(Mobile Originated) request from AE1  | |
                     | containing Non‑IP data containing valid oneM2M request containing To set to AE1 and  | |
                     | From set to AE1 and  | |
                     | Content containing valid AE resource  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT send s a valid MT NIDD Downlink Data Transfer  | |
                     | Request to the SCEF  | |
                     | containing   | |
                     |Non‑IP data containing valid oneM2M response primitive  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/3GPP/NIDD/008
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/008

	Test objective
	Check that IUT responds with a 204 NO CONTENT acknowledging the notification when SCEF sends MT NIDD Downlink Data Delivery Status Notification.

	Reference
	TS-0026 [5], clause 7.1.1.2, step 7

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered AE1 hosted on a 3GPP UE
and the IUT having sent a MT Downlink data transfer request
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= SCEF |
                     | the IUT receives a valid MT NIDD Downlink Data Delivery  | |
                     | Status Notificationfrom SCEF containing valid  | |
                     | NiddDownlinkDataDeliveryStatusNotification  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT sends a 204 NO CONTENT acknowledging the  | |
                     | notification  | |
                     |} | |
+———————-+———————————————————————————————————————————–+————-+
TP/oneM2M/CSE/3GPP/NIDD/009
	TP Id
	TP/oneM2M/CSE/3GPP/NIDD/009

	Test objective
	Check that IUT responds with a 204 NO CONTENT acknowledging the notification when SCEF sends MO NIDD Uplink Data Notification.

	Reference
	TS-0026 [5], clause 7.1.1.2, step 7

	Parent Release
	Release 3

	Config Id
	CF05

	PICS Selection
	PICS_IN_CSE, PICS_3GPP

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having register an AE1 hosted on a 3GPP UE
}



·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= SCEF |
                     | the IUT receives a valid MO NIDD Uplink Data  | |
                     | Notificationfrom SCEF  | |
                     | containing NiddUplinkDataNotification  | |
                     | containing Non_IP data containing a valid oneM2M  | |
                     | response primitive  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => SCEF |
                     | the IUT sends a 204 NO CONTENT acknowledging the  | |
                     | notification  | |
                     |} | |
+———————-+—————————————————————————————————————–+————-+
7.2.2.13	FlexContainer (FLXC)
7.2.2.13.1	CREATE Operation
TP/oneM2M/CSE/FLXC/CRE/001
	TP Id
	TP/oneM2M/CSE/FLXC/CRE/001

	Test objective
	Check that the IUT rejects the creation of the <flexContainer> resource when the resource representation does not comply with the schema definition.

	Reference
	TS-0001 [1], clause 3, 10.2.4.16, TS-0004 [2], clause 7.4.29.2.1

	Parent Release
	Release 2

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource
AE_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives an invalid CREATE request from AE containing  | |
                     | To set to AE_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Resource Type set to 28 (flexContainer) and  | |
                     | Content containing  | |
                     | an invalid resource representation  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the flexContainer resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+
TP/oneM2M/CSE/FLXC/CRE/002
	TP Id
	TP/oneM2M/CSE/FLXC/CRE/002

	Test objective
	Check that the IUT rejects the CREATE request of <flexContainer> resource when the containerDefinition attribute does not include the schema value to validate the received resource representation

	Reference
	TS-0001 [1], clause 10.1.2 and 10.2.4.16, TS-0004 [2], clause 7.4.37.2.1

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
the AEhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | flexContainer resource containing  | |
                     | containerDefinition set to UNAVAILABLE_SCHEMA  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT does not create the flexContainer resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4125 (SPECIALIZATION_SCHEMA_NOT_FOUND)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/FLXC/CRE/003
	TP Id
	TP/oneM2M/CSE/FLXC/CRE/003

	Test objective
	Check that the IUT rejects the CREATE request of <flexContainer> resource when value of contentSize attribute is greater than maxByteSize attribute

	Reference
	TS-0001 [1], clause 10.1.2 and 10.2.4.16, TS-0004 [2], clause 7.4.37.2.1

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
the AEhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | flexContainer resource containing  | |
                     | maxNrOfInstances set to non‑zero value and  | |
                     | a valid maxByteSizeand  | |
                     | a valid CUSTOM_ATTRIBUTE_1, and CUSTOM_ATTRIBUTE_2 with total byte sizegreater than maxByteSize  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT does not create the flexContainer resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/FLXC/CRE/004
	TP Id
	TP/oneM2M/CSE/FLXC/CRE/004

	Test objective
	Check that the IUT successfully creates the <flexContainer> resource and its child <flexcontainerInstance> resource when ATTRIBUTE attribute of <flexContainer> resource is present with a non-zero value in the request

	Reference
	TS-0001 [1], clause 10.1.2 and 10.2.4.16, TS-0004 [2], clause 7.4.37.2.1

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
and the AEhaving privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | flexContainer resource containing  | |
                     | a valid ATTRIBUTE attribute set to non‑zero value  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT creates the <flexContainer> resource  | |
                     | and the IUT creates the child <flexContainerInstance> resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/FLXC/CRE/004/MNI
	maxNrOfInstances

	TP/oneM2M/CSE/FLXC/CRE/004/MBS
	maxByteSize

	TP/oneM2M/CSE/FLXC/CRE/004/MIA
	maxInstanceAge



7.2.2.13.2	UPDATE Operation
TP/oneM2M/CSE/FLXC/UPD/001
	TP Id
	TP/oneM2M/CSE/FLXC/UPD/001

	Test objective
	Check that the IUT increments the field value of attribute stateTag in the <flexContainer> resource when a custom attribute of the resource is modified

	Reference
	TS-0001 [1], clause 9.6.35

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource FLEXCONTAINER_RESOURCE_ADDRESS containing
stateTag attribute
and the AE having privileges to perform UPDATE operation on the resource
FLEXCONTAINER_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to FLEXCONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Contentcontaining  | |
                     | flexContainer resourcecontaining  | |
                     | ATTRIBUTE_NAME attribute set to VALUE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT increments the stateTag attribute of FLEXCONTAINER_RESOURCE_ADDRESS resource   | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————+————-+
TP/oneM2M/CSE/FLXC/UPD/002
	TP Id
	TP/oneM2M/CSE/FLXC/UPD/002

	Test objective
	Check that the IUT does not increment the field value of attribute stateTag in the <flexContainer> resource when a common attribute of the resource is modified

	Reference
	TS-0001 [1], clause 9.6.35

	Config Id
	CF01

	Parent Release
	Release 2

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
a container resource FLEXCONTAINER_RESOURCE_ADDRESS containing
stateTag attribute
and the AE having privileges to perform UPDATE operation on the resource
FLEXCONTAINER_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to FLEXCONTAINER_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | flexContainer resource containing  | |
                     | ATTRIBUTE_NAME attribute set to VALUE  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not increment the stateTag attribute of FLEXCONTAINER resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/FLXC/UPD/003
	TP Id
	TP/oneM2M/CSE/FLXC/UPD/003

	Test objective
	Check that the IUT rejects the update of the <flexContainer> resource when the resource representation does not comply with the schema definition.

	Reference
	TS-0001 [1], clause 10.2.4.18, TS-0004 [2], clause 7.4.29.2.3

	Parent Release
	Release 2

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform UPDATE operation on the resource
FLXC_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives an invalid UPDATE request from AE  | |
                     | containing  | |
                     | To set to FLXC_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | flexContainer resource containing  | |
                     | an invalid resource representation  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not update the flexContainer resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/FLXC/UPD/004
	TP Id
	TP/oneM2M/CSE/DMR/UPD/004

	Test objective
	Check that the IUT rejects the UPDATE request of <flexContainer> resource when the size value of the customAttributes exceeds the value specified in the maxByteSize attribute

	Reference
	TS-0001 [1], clause 10.1.4 and 10.2.4.18, TS-0004 [2], clause 7.4.37.2.3

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
a valid maxByteSize attribute
and the AEhaving privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | flexcontainer resource containing  | |
                     | a valid CUSTOM_ATTRIBUTE_1, and CUSTOM_ATTRIBUTE_2 with total byte size greater than maxByteSize  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/FLXC/UPD/005
	TP Id
	TP/oneM2M/CSE/FLXC/UPD/005

	Test objective
	Check that IUT updates the <flexContainer> resource and creates its new child <flexContainerInstance> resource when request contains a custom attribute of the targeted <flexContainer> resource

	Reference
	TS-0001 [1], clause 10.1.4 and 10.2.4.18, TS-0004 [2], clause 7.4.37.2.3

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
a valid ATTRIBUTE attribute
and the AE having privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | flexcontainer resource containing  | |
                     | a valid CUSTOM_ATTRIBUTE attribute  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT updates the <flexContainer> resource  | |
                     | and the IUT creates the child <flexContainerInstance> resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————–+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/FLXC/UPD/005/MNI
	maxNrOfInstances

	TP/oneM2M/CSE/FLXC/UPD/005/MBS
	maxByteSize

	TP/oneM2M/CSE/FLXC/UPD/005/MIA
	maxInstanceAge



TP/oneM2M/CSE/FLXC/UPD/006
	TP Id
	TP/oneM2M/CSE/FLXC/UPD/006

	Test objective
	Check that IUT updates the <flexContainer> resource and creates its new child <flexContainerInstance> resource when request contains no custom attribute of the targeted <flexContainer> resource

	Reference
	TS-0001 [1], clause 10.1.4 and 10.2.4.18, TS-0004 [2], clause 7.4.37.2.3

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
a valid ATTRIBUTE attribute
and the AEhaving privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT updates the <flexContainer> resource  | |
                     | and the IUT creates the child <flexContainerInstance> resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/FLXC/UPD/006/MNI
	maxNrOfInstances

	TP/oneM2M/CSE/FLXC/UPD/006/MBS
	maxByteSize

	TP/oneM2M/CSE/FLXC/UPD/006/MIA
	maxInstanceAge



TP/oneM2M/CSE/FLXC/UPD/007
	TP Id
	TP/oneM2M/CSE/FLXC/UPD/007

	Test objective
	Check that the IUT updates the currentNrOfInstances and currentByteSize attributes of the <flexContainer> resource when the UPDATE request creates, modifies or deletes the ATTRIBUTE attribute of the <flexContainer> resource

	Reference
	TS-0001 [1], clause 10.1.4 and 10.2.4.18, TS-0004 [2], clause 7.4.37.2.3

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
children <flexContainerInstance> resources
and the AEhaving privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | flexContainer resource containing  | |
                     | a valid ATTRIBUTE attribute  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT updates the set of <flexContainerInstances> resources according to the modified <flexContainer> attributes  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | Content containing  | |
                     | flexContainer resource containing  | |
                     | currentNrOfInstances and currentByteSize attributes indicating modified values  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/FLXC/UPD/007/MNI
	maxNrOfInstances

	TP/oneM2M/CSE/FLXC/UPD/007/MBS
	maxByteSize

	TP/oneM2M/CSE/FLXC/UPD/007/MIA
	maxInstanceAge



TP/oneM2M/CSE/FLXC/UPD/008
	TP Id
	TP/oneM2M/CSE/FLXC/UPD/008

	Test objective
	Check that the IUT deletes all child <flexContainerInstance> resources and the currentNrOfInstances, currentByteSize, maxNrOfInstances, maxByteSize and maxInstanceAge attributes of the <flexContainer> when UPDATE request updates ATTRIBUTE of the <flexContainer> resource with a value of zero

	Reference
	TS-0001 [1], clause 10.1.4 and 10.2.4.18, TS-0004 [2], clause 7.4.37.2.3

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT being a hosting CSE
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
children <flexContainerInstance> resources
and the AEhaving privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Resource Type set to 28 (flexContainer)  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | <flexContainer> resource containing  | |
                     | ATTRIBUTE attribute set to ZERO  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT deletes all <flexContainerInstance> resources  | |
                     | and the IUT deletes currentNrOfInstances, currentByteSize, maxNrOfInstances, maxByteSize and maxInstanceAge attributes of <flexContainer>  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/FLXC/UPD/008/MNI
	maxNrOfInstances

	TP/oneM2M/CSE/FLXC/UPD/008/MBS
	maxByteSize

	TP/oneM2M/CSE/FLXC/UPD/008/MIA
	maxInstanceAge



7.2.2.13.3	RETRIEVE Operation
TP/oneM2M/CSE/FLXC/RET/001
	TP Id
	TP/oneM2M/CSE/FLXC/RET/001

	Test objective
	Check that the IUT performs the RETRIEVE request for the latest <flexContainerInstance> resource

	Reference
	TS-0001 [1], clause 10.1.3, 10.2.4.17, TS-0004 [2], clause 7.4.37.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_1
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_2
and creationTime attribute of FLEX_CONTAINER_INSTANCE_1 is less than creationTime attribute of FLEX_CONTAINER_INSTANCE_2
and the AEhaving privileges to perform RETRIEVE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | Resource Type set to 58 (flexContainerInstance) and  | |
                     | Toset to TARGET_RESOURCE_ADDRESS/la and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +---------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | flexContainerInstance resource containing  | |
                     | resourceName attribute set to FLEX_CONTAINER_INSTANCE_2  | |
                     |} | |
+———————-+—————————+—————————————————————————————————-+————-+
TP/oneM2M/CSE/FLXC/RET/002
	TP Id
	TP/oneM2M/CSE/FLXC/RET/002

	Test objective
	Check that the IUT performs the RETRIEVE request for the oldest <flexContainerInstance> resource

	Reference
	TS-0001 [1], clause 10.1.3, 10.2.4.17, TS-0004 [2], clause 7.4.37.2.2

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_1
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_2
and creationTime attribute of FLEX_CONTAINER_INSTANCE_1 is less than creationTime attribute of FLEX_CONTAINER_INSTANCE_2
and the AEhaving privileges to perform RETRIEVE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | Resource Type set to 58 (flexContainerInstance) and  | |
                     | To set to TARGET_RESOURCE_ADDRESS/ol and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +---------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | flexContainerInstance resource containing  | |
                     | resourceName attribute set to FLEX_CONTAINER_INSTANCE_1  | |
                     |} | |
+———————-+—————————+—————————————————————————————————-+————-+
7.2.2.13.4	DELETE Operation
TP/oneM2M/CSE/FLXC/DEL/001
	TP Id
	TP/oneM2M/CSE/FLXC/DEL/001

	Test objective
	Check that the IUT performs the DELETE request for the latest <flexContainerInstance> resource

	Reference
	TS-0001 [1], clause 10.1.5, 10.2.4.19, TS-0004 [2], clause 7.4.37.2.4

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_1
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_2
and creationTime attribute of FLEX_CONTAINER_INSTANCE_1 is less than creationTime attribute of FLEX_CONTAINER_INSTANCE_2
and the AEhaving privileges to perform RETRIEVE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | Resource Type set to 58 (flexContainerInstance)  | |
                     | To set to TARGET_RESOURCE_ADDRESS/la and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-----------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT deletes the FLEX_CONTAINER_INSTANCE_2 resource  | |
                     | the IUT updates the currentNrOfInstances, currentByteSize and contentSize attributes of the <flexContainer> resource | |
                     |and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+—————————–+—————————————————————————————————-+————-+
TP/oneM2M/CSE/FLXC/DEL/002
	TP Id
	TP/oneM2M/CSE/FLXC/DEL/002

	Test objective
	Check that the IUT performs the DELETE request for the oldest <flexContainerInstance> resource

	Reference
	TS-0001 [1], clause 10.1.5, 10.2.4.19, TS-0004 [2], clause 7.4.37.2.4

	Config Id
	CF01

	Parent Release
	Release 1

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE containing
and the IUT having a <flexContainer> resource at
TARGET_RESOURCE_ADDRESS containing
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_1
a child <flexContainerInstance> resource as FLEX_CONTAINER_INSTANCE_2
and creationTime attribute of FLEX_CONTAINER_INSTANCE_1 is less than creationTime attribute of FLEX_CONTAINER_INSTANCE_2
and the AEhaving privileges to perform RETRIEVE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | Resource Type set to 58 (flexContainerInstance)  | |
                     | To set to TARGET_RESOURCE_ADDRESS/ol and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-----------------------------+----------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT deletes the FLEX_CONTAINER_INSTANCE_1 resource  | |
                     | the IUT updates the currentNrOfInstances, currentByteSize and contentSize attributes of the <flexContainer> resource | |
                     |and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+—————————–+—————————————————————————————————-+————-+
7.2.2.14	Dynamic Authorization (DAU)
7.2.1.14.1	NOTIFY Operation
TP/oneM2M/CSE/DAU/NOT/001
	TP Id
	TP/oneM2M/CSE/DAU/NOT/001

	Test objective
	Check that the IUT starts the Dynamic Authorization for an incoming request and sends a Notify Request to DAS including all mandatory fields

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF06

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the <container> resource having a dynamicAuthorizationConsultationID
attribute and corresponding <dynamicAuthorizationConsultation> not set to FALSE
}



·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid RETRIEVE request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID and  | |
                     | no Content  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |DAS <= IUT |
                     | the IUT sends a valid NOTIFY Request to DAS containing  | |
                     | To set to DAS_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Notification datacontaining  | |
                     | securityInfo containing  | |
                     | securityInfoType set to 1 (Dynamic Authorization Request) and  | |
                     | dasRequest containing  | |
                     | originator set to AE_ID and  | |
                     | targetedResourceType set to 3 (container) and  | |
                     | operation set to 2 (Retrieve)  | |
                     |} | |
+———————-+——————————————————————————————————————————-+————-+ Editor's Note: Config Id will be newly proposed to cover this test purpose.
TP/oneM2M/CSE/DAU/NOT/002
	TP Id
	TP/oneM2M/CSE/DAU/NOT/002

	Test objective
	Check that the IUT starts the Dynamic Authorization for an incoming request and sends a Notify Request including all mandatory fields and one ore more optional fields

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF06

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the <container> resource has a dynamicAuthorizationConsultationID attribute and
corresponding <dynamicAuthorizationConsultation> not set to FALSE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid RETRIEVE request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID and  | |
                     | no Content  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |DAS <= IUT |
                     | the IUT sends a valid NOTIFY Request to DAS containing  | |
                     | To set to DAS_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Notification datacontaining  | |
                     | securityInfo containing  | |
                     | securityInfoType set to 1 (Dynamic Authorization Request) and  | |
                     | dasRequest containing  | |
                     | originator set to AE_ID and  | |
                     | targetedResourceType set to 3 (container) and  | |
                     | operation set to 2 (Retrieve)  | |
                     | originatorIP set to AE_IP  | |
                     | originatorLocation set to location of originator of the received   | |
                     | request  | |
                     | originatorRole set to role of originator of the received request  | |
                     | requestTimestamp set to time of receipt of request  | |
                     | targetedResourceID set to identifier of the targeted resource  | |
                     | proposedPrivilegesLifetime set to time duration of requested   | |
                     | privileges  | |
                     | rolesFromACPs set to list of roles of requested resource  | |
                     | tokenIdDs set to list of token identifiers from the received request  | |
                     | authorSignIndicator set to value specified by the received request  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/DAU/NOT/003
	TP Id
	TP/oneM2M/CSE/DAU/NOT/003

	Test objective
	Check that the IUT does not start the Dynamic Authorization for an incoming request and rejects that incoming request if the dynamicAuthorizationConsultationID attribute and corresponding <dynamicAuthorizationConsultation> resource can not be found

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the <container> resource does not have a dynamicAuthorizationConsultationID attribute
nor corresponding <dynamicAuthorizationConsultation>
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid RETRIEVE request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID and  | |
                     | no Content  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE1 <= IUT |
                     | the IUT rejects the incoming request from the AE1  | |
                     | containing Response Status Code set to   | |
                     | "ORIGINATOR_HAS_NO_PRIVILEGE"  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/DAU/NOT/004
	TP Id
	TP/oneM2M/CSE/DAU/NOT/004

	Test objective
	Check that the IUT does not start the Dynamic Authorization for an incoming request and rejects that incoming request if the dynamicAuthorizationEnabled of a <dynamicAuthorizationConsultation> is set to FALSE

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the <container> resource has <dynamicAuthorizationConsultation> with
dynamicAuthorizationEnabled set to FALSE
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid RETRIEVE request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1_ID and  | |
                     | no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE1 <= IUT |
                     | the IUT rejects the incoming request from the AE1  | |
                     | containing Response Status Code set to   | |
                     | "ORIGINATOR_HAS_NO_PRIVILEGE"  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/DAU/NOT/005
	TP Id
	TP/oneM2M/CSE/DAU/NOT/005

	Test objective
	Check that the IUT correctly processes a Notify response received in response to a Notify request that started Dynamic Authorization

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF06

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the AE1 having sent a Retrieve request for the resource at
TARGET_RESOURCE_ADDRESS
and the AE1 having no privileges to perform RETRIEVE operation on the resource
and the IUT having sent a NOTIFY Request to DAS to start Dynamic Authorization
}



·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |DAS => IUT |
                     | the IUT receives a valid NOTIFY Response containing  | |
                     | Notification datacontaining  | |
                     | securityInfo containing  | |
                     | securityInfoType set to 2 (Dynamic Authorization Response)  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE1 <= IUT |
                     | the IUT sends a valid Response to AE1 containing  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Content containing  | |
                     | <container> representation  | |
                     |} | |
+———————-+———————————————————————————————————————–+————-+
TP/oneM2M/CSE/DAU/NOT/006
	TP Id
	TP/oneM2M/CSE/DAU/NOT/006

	Test objective
	Check that the IUT correctly processes a Notify response including a dynamicACPInfo element received in response to a Notify request that started Dynamic Authorization

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF06

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the AE1 having sent a Retrieve request for the resource at
TARGET_RESOURCE_ADDRESS
and the AE1 having no privileges to perform RETRIEVE operation on the resource
and the IUT having sent a NOTIFY Request to DAS to start Dynamic Authorization
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |DAS => IUT |
                     | the IUT receives a valid NOTIFY Response containing  | |
                     | Notification datacontaining  | |
                     | securityInfo containing  | |
                     | securityInfoType set to 2 (Dynamic Authorization Response) and  | |
                     | dynAuthDasResponse containing dynamicACPInfo  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE1 <= IUT |
                     | the IUT creates  | |
                     | <accesscontrolPolicy> child resource and  | |
                     | configures the privileges, expirationTime and selfPrivileges attributes  | |
                     | based on the data received in the dynamicACPInfo,  | |
                     | and the IUT sends a valid Response to AE1 containing  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Content containing  | |
                     | <container> representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/DAU/NOT/007
	TP Id
	TP/oneM2M/CSE/DAU/NOT/007

	Test objective
	Check that the IUT correctly processes a Notify response including a tokens element received in response to a Notify request that started Dynamic Authorization

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF06

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the AE1 having sent a Retrieve request for the resource at
TARGET_RESOURCE_ADDRESS
and the AE1 having no privileges to perform RETRIEVE operation on the resource
and the IUT having sent a NOTIFY Request to DAS to start Dynamic Authorization
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |DAS => IUT |
                     | the IUT receives a valid NOTIFY Response containing  | |
                     | Notification datacontaining  | |
                     | Tokens element  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE1 <= IUT |
                     | the IUT sends a valid Response to AE1 containing  | |
                     | ResponseStatusCode set to OK (2000) and  | |
                     | Content containing  | |
                     | <container> representation  | |
                     |} | |
+———————-+————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/DAU/NOT/008
	TP Id
	TP/oneM2M/CSE/DAU/NOT/008

	Test objective
	

	Reference
	TS-0001 [1], clause 10.1.6 and 10.2.10.6, TS-0004 [2], clause 7.2.2.1 and 7.5.1.2.10

	Config Id
	CF06

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being registered
and the IUT being a hosting CSE
and the IUT having registered AE1
and the IUT having registered the DAS
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and the AE1 having sent a Retrieve request for the resource at
TARGET_RESOURCE_ADDRESS
and the AE1 having no privileges to perform RETRIEVE operation on the resource
and the IUT having sent a NOTIFY Request to DAS to start Dynamic Authorization
}



·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |DAS => IUT |
                     | the IUT receives a valid NOTIFY Response NOT containing  | |
                     | Notification datacontaining  | |
                     | securityInfo containing  | |
                     | securityInfoType set to 2 (Dynamic Authorization Response)  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE1 <= IUT |
                     | the IUT rejects the incoming request from the AE1containing  | |
                     | Response Status Code set to   | |
                     | "ORIGINATOR_HAS_NO_PRIVILEGE"  | |
                     |} | |
+———————-+——————————————————————————————————————-+————-+
7.2.2.15	Semantic (SEM)
7.2.2.15.1	CREATE Operation
TP/oneM2M/CSE/SEM/CRE/001
	TP Id
	TP/oneM2M/CSE/SEM/CRE/001

	Test objective
	Check that the IUT rejects the creation request of a <semanticDescriptor> resource which descriptor attribute does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.1.2, and TS-0004 [2], clause 7.4.34.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a parent resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | descriptor attributeset to a value that does not conform to  | |
                     | the RDF/XML syntax  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the <semanticDescriptor> resource and  | |
                     | the IUT sends a valid Response containing  | |
                     | failure information with additional error information  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/CRE/002
	TP Id
	TP/oneM2M/CSE/SEM/CRE/002

	Test objective
	Check that the IUT generates a Response Status Code indicating a "ONTOLOGY_NOT_AVAILABLE" error when referenced ontology cannot be retrieved during a semantic validation process

	Reference
	TS-0004 [2], clause 7.4.34.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | ontologyRef attribute set to a non‑resolvable URI  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4118 (ONTOLOGY_NOT_AVAILABLE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/CRE/003
	TP Id
	TP/oneM2M/CSE/SEM/CRE/003

	Test objective
	Check that the IUT generates a Response Status Code indicating a "LINKED_SEMANTICS_NOT_AVAILABLE" error when local linked <semanticDescriptor> resources cannot be retrieved during a semantic validation process

	Reference
	TS-0004 [2], clause 7.4.34.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | relatedSemantics attribute set to a non‑resolvable URI  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4119  | |
                     | (LINKED_SEMANTICS_NOT_AVAILABLE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/CRE/004
	TP Id
	TP/oneM2M/CSE/SEM/CRE/004

	Test objective
	Check that the IUT retrieves the referenced ontology from the ontology hosting CSE when performing a semantic validation as a result of a creation of a stand-alone <semanticDescriptor> resource

	Reference
	TS-0034 [6], clauses 6.1.2 and 7.10.3, and TS-0004 [2], clause 7.4.34.2.1

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
and the ontology hosting CSE having an <ontology> resource at
REFERENCED_ONTOLOGY_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | descriptor attribute and  | |
                     | ontologyRef attribute set to  | |
                     | REFERENCED_ONTOLOGY_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid RETRIEVE Request containing  | |
                     | To set to REFERENCED_ONTOLOGY_ADDRESS and  | |
                     | Content containing  | |
                     | <ontology> resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/CRE/005
	TP Id
	TP/oneM2M/CSE/SEM/CRE/005

	Test objective
	Check that the IUT sends a valid response when performing a semantic validation as a result of a creation of a stand-alone <semanticDescriptor> resource

	Reference
	TS-0034 [6], clauses 6.1.2 and 7.10.3, and TS-0004 [2], clause 7.4.34.2.1

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
and the ontology hosting CSE having an <ontology> resource at
REFERENCED_ONTOLOGY_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | descriptor attribute and  | |
                     | ontologyRef attribute set to  | |
                     | REFERENCED_ONTOLOGY_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code indicating success of validation  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/CRE/006
	TP Id
	TP/oneM2M/CSE/SEM/CRE/006

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupInstance> resource, indicating a "BAD_REQUEST" error, when the <semanticMashupJobProfile> resource referenced in its smjpID attribute does not exist

	Reference
	TS-0034 [6], clause 6.4.2, and TS-0004 [2], clause 7.4.50.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 41 (semanticMashupInstance) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticMashupInstance> resource representation containing  | |
                     | smjpID attributeset to a reference to a non‑existent  | |
                     | <semanticMashupJobProfile> resource  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupInstance> resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/CRE/007
	TP Id
	TP/oneM2M/CSE/SEM/CRE/007

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupInstance> resource, indicating a "BAD_REQUEST" error, when its smjpInputParameter attribute value does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.4.2, and TS-0004 [2], clause 7.4.50.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
CREATE operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 41 (semanticMashupInstance) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticMashupInstance> resource representation containing  | |
                     | smjpID attribute set to a reference to the  | |
                     | <semanticMashupJobProfile> resource at  | |
                     | TARGET_RESOURCE_ADDRESS  | |
                     | smjpInputParameter set to a value that does not conform to  | |
                     | the RDF/XML syntax  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupInstance> resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/CRE/008
	TP Id
	TP/oneM2M/CSE/SEM/CRE/008

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupInstance> resource, indicating a "BAD_REQUEST" error, when its smjpInputParameter attribute value does not meet the input parameter requirement specified by the inputDescriptor attribute of the corresponding <semanticMashupJobProfile> resource

	Reference
	TS-0034 [6], clause 6.4.2, and TS-0004 [2], clause 7.4.50.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
CREATE operation
inputDescriptor attribute set to a valid value
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 41 (semanticMashupInstance) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticMashupInstance> resource representation containing  | |
                     | smjpID attribute set to a reference to the  | |
                     | <semanticMashupJobProfile> resource at  | |
                     | TARGET_RESOURCE_ADDRESS  | |
                     | smjpInputParameter set to a value of a type not allowed  | |
                     | according to the inputDescriptor attribute of the  | |
                     | <semanticMashupJobProfile> resource at  | |
                     | TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupInstance> resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/CRE/009
	TP Id
	TP/oneM2M/CSE/SEM/CRE/009

	Test objective
	Check that the IUT returns a "MASHUP_MEMBER_NOT_FOUND" error when creating a <semanticMashupInstance> when a required mashup member resource cannot be identified

	Reference
	TS-0034 [6], clause 6.4.2, and TS-0004 [2], clause 7.4.50.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
CREATE operation
memberFilter attribute set to a SPARQL query to discover an unidentified mashup
member
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 41 (semanticMashupInstance) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticMashupInstance> resource representation containing  | |
                     | smjpID attributeset to a reference to the  | |
                     | <semanticMashupJobProfile> resource at  | |
                     | TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4121  | |
                     | (MASHUP_MEMBER_NOT_FOUND)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/CRE/010
	TP Id
	TP/oneM2M/CSE/SEM/CRE/010

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupJobProfile> resource, indicating a "BAD_REQUEST" error, when its inputDescriptor attribute value does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.3.2, and TS-0004 [2], clause 7.4.49.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {  |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing inputDescriptor attribute set to a  | |
                     | value that does not conform to the RDF/XML syntax  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/CRE/011
	TP Id
	TP/oneM2M/CSE/SEM/CRE/011

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupJobProfile> resource, indicating a "BAD_REQUEST" error, when its outputDescriptor attribute value does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.3.2, and TS-0004 [2], clause 7.4.49.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the AE having privileges to perform CREATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing outputDescriptor attributeset to  | |
                     | a value that does not conform to the RDF/XML syntax  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/CRE/012
	TP Id
	TP/oneM2M/CSE/SEM/CRE/012

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupJobProfile> resource, indicating a "BAD_REQUEST" error, when its functionDescriptor attribute value does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.3.2, and TS-0004 [2], clause 7.4.49.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the AE having privileges to perform CREATE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing functionDescriptor attributeset  | |
                     | to a value that does not conform to the RDF/XML syntax  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/CRE/013
	TP Id
	TP/oneM2M/CSE/SEM/CRE/013

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupJobProfile> resource, indicating a "BAD_REQUEST" error, when its memberFilter attribute value does not conform to a valid SPARQL query request

	Reference
	TS-0034 [6], clause 6.3.2, and TS-0004 [2], clause 7.4.49.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
CREATE operation
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and Resource  | |
                     | Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing memberFilter attributeset to  | |
                     | a value that does not conform to a valid SPARQL query  | |
                     | request  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/CRE/014
	TP Id
	TP/oneM2M/CSE/SEM/CRE/014

	Test objective
	Check that the IUT creates successfully the <semanticMashupInstance> resource

	Reference
	TS-0001 [1], clause 9.6.54, TS-0004 [2], clause 7.4.50.2.1, TS-0034 [6], clause 6.4.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
CREATE operation
}



·              +----------------------------------------------------------------------------------------------------------------------------------------------+---------+

·                  |when {   |IUT <= AE|
                 | the IUT receives a valid CREATE Request from AE containing  | |
                 | To set to TARGET_RESOURCE_ADDRESS and  | |
                 | Resource Type set to 41 (semanticMashupInstance) and  | |
                 | From set to AE‑ID and  | |
                 | Content containing <semanticMashupInstance> resource  | |
                 | representation containing  | |
                 | smjpID attribute set to a reference to the  | |
                 | <semanticMashupJobProfile> resource at  | |
                 | TARGET_RESOURCE_ADDRESS  | |
                 | smjpInputParameter set to a value that does conform to  | |
                 | the RDF/XML syntax  | |
                 |} | |
·              +----------------------------------------------------------------------------------------------------------------------------------------------+---------+

·                  |then {   |IUT => AE|
                 | the IUT creates the semanticMashupInstance resource  | |
                 | and the IUT sends a valid Response containing  | |
                 | Response Status Code set to 2001 (CREATED)  | |
                 |} | |
+——————+———————————————————————————————————————————————-+———+
TP/oneM2M/CSE/SEM/CRE/015
	TP Id
	TP/oneM2M/CSE/SEM/CRE/015

	Test objective
	Check that the IUT creates successfully the <semanticMashupInstance> resource with resultGenType set to WHEN_SMI_IS_CREATED


	Reference
	TS-0001 [1], clause 9.6.54, TS-0004 [2], clause 7.4.50.2.1, TS-0034 [6], clause 6.4.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
CREATE operation
}



·              +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------------------------------------------------------------------------------------------------------------------------------+---------+

·                  |when {   |IUT <= AE|
                 | the IUT receives a valid CREATE Request from AE containing  | |
                 | To set to TARGET_RESOURCE_ADDRESS and  | |
                 | Resource Type set to 41 (semanticMashupInstance) and  | |
                 | From set to AE‑ID and  | |
                 | Content containing <semanticMashupInstance> resource  | |
                 | representation containing smjpID attributeset to a reference to  | |
                 | the <semanticMashupJobProfile> resource at  | |
                 | TARGET_RESOURCE_ADDRESS smjpInputParameter set to a  | |
                 | value that does conform to the RDF/XML syntaxand  | |
                 | resultGenType is set to WHEN_SMI_IS_CREATED  | |
                 |} | |
·              +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+----------------------------------------------------------------------------------------------------------------------------------------------+---------+

·                  |then {  |IUT => AE|
                 | the IUT creates the semanticMashupInstance resource  | |
                 | and the IUT sends a valid Response containing  | |
                 | Response Status Code set to 2001 (CREATED)  | |
                 |} | |
+——————+———————————————————————————————————————————————————————————————————————————————————-+———————————————————————————————————————————————-+———+
TP/oneM2M/CSE/SEM/CRE/016
	TP Id
	TP/oneM2M/CSE/SEM/CRE/016

	Test objective
	Check that the IUT creates successfully the <semanticMashupInstance> resource with resultGenType set to PERIODICALLY


	Reference
	TS-0001 [1], clause 9.6.54, TS-0004 [2], clause 7.4.50.2.1, TS-0034 [6], clause 6.4.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 41 (semanticMashupInstance) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupInstance> resource  | |
                     | representation containing smjpID attributeset to a reference to  | |
                     | the <semanticMashupJobProfile> resource at  | |
                     | TARGET_RESOURCE_ADDRESS smjpInputParameter set to  | |
                     | a value that does conform to the RDF/XML syntax and  | |
                     | resultGenType is set to PERIODICALLY with a period of t1  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT creates a new semanticMashupInstance resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+——————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/CRE/017
	TP Id
	TP/oneM2M/CSE/SEM/CRE/017

	Test objective
	Check that the IUT rejects the creation request of a <semanticDescriptor> resource in which descriptorRepresentation attribute is set to "IRI".

	Reference
	TS-0034 [6], clause 6.1.2, and TS-0004 [2], clause 7.4.34.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a parent resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | descriptorRepresentation attribute is set to "IRI"  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticDescriptor> resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————-+————-+
7.2.2.15.2	UPDATE Operation
TP/oneM2M/CSE/SEM/UPD/001
	TP Id
	TP/oneM2M/CSE/SEM/UPD/001

	Test objective
	Check that the IUT rejects the update request of a <semanticDescriptor> resource indicating a "NOT_ACCEPTABLE" error when the request contains both semanticOpExec and descriptor attributes

	Reference
	TS-0004 [2], clause 7.4.34.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation at TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | descriptor attributeset to a valid value  | |
                     | semanticOpExec attribute set to a valid value  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not update the <semanticDescriptor> resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/002
	TP Id
	TP/oneM2M/CSE/SEM/UPD/002

	Test objective
	Check that the IUT rejects the update request of a <semanticDescriptor> resource indicating a "NOT_ACCEPTABLE" error when the request contains a semanticOpExec attribute which does not contain a valid SPARQL query request

	Reference
	TS-0004 [2], clause 7.4.34.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | no descriptor attributeand  | |
                     | semanticOpExec attributeset to a non‑valid SPARQL query request  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not update the <semanticDescriptor> resource and  | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/003
	TP Id
	TP/oneM2M/CSE/SEM/UPD/003

	Test objective
	Check that the IUT rejects the update request of a <semanticDescriptor> resource when the request contains a descriptor attribute which does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0004 [2], clause 7.4.34.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | no semanticOpExec attributeand  | |
                     | descriptor attributeset to a value that does not conform to  | |
                     | the RDF/XML syntax  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not update the <semanticDescriptor> resource and  | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/004
	TP Id
	TP/oneM2M/CSE/SEM/UPD/004

	Test objective
	Check that the IUT retrieves the referenced ontology from the ontology hosting CSE when performing a semantic validation as a result of an update of a stand-alone <semanticDescriptor> resource

	Reference
	TS-0034 [6], clauses 6.1.4 and 7.10.3, and TS-0004 [2], clause 7.4.34.2.3

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
and the ontology hosting CSE having an <ontology> resource at
REFERENCED_ONTOLOGY_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | descriptor attribute and  | |
                     | ontologyRef attribute set to  | |
                     | REFERENCED_ONTOLOGY_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid RETRIEVE Request containing  | |
                     | To set to REFERENCED_ONTOLOGY_ADDRESS and  | |
                     | Content containing  | |
                     | <ontology> resource representation  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/005
	TP Id
	TP/oneM2M/CSE/SEM/UPD/005

	Test objective
	Check that the IUT sends a valid response when performing a semantic validation as a result of an update of a stand-alone <semanticDescriptor> resource

	Reference
	TS-0034 [6], clauses 6.1.4 and 7.10.3, and TS-0004 [2], clause 7.4.34.2.3

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
and the ontology hosting CSE having an <ontology> resource at
REFERENCED_ONTOLOGY_ADDRESS
**}*



·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | descriptor attribute and  | |
                     | ontologyRef attribute set to  | |
                     | REFERENCED_ONTOLOGY_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (UPDATED)and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource  | |
                     |} | |
+———————-+———————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/UPD/006
	TP Id
	TP/oneM2M/CSE/SEM/UPD/006

	Test objective
	Check that the IUT retrieves the linked <semanticDescriptor> resource from the hosting CSE when performing a semantic validation as a result of an update of the <semanticValidation> virtual resource

	Reference
	TS-0034 [6], clauses 6.9.4 and 7.10.3, and TS-0004 [2], clause 7.4.48.2.3

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <ontologyRepositoy> resource at TARGET_RESOUCE ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
and the IUThaving a <ontology> resource at REFERENCED_ONTOLOGY_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
and the hosting CSE having a <semanticDescriptor> resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to the TARGET_RESOURCE_ADDRESS/smv and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | descriptor attribute and  | |
                     | ontologyRef attribute set to  | |
                     | REFERENCED_ONTOLOGY_ADDRESS and  | |
                     | relatedSemantics attributeset to  | |
                     | LINKED_SEMANTIC_DESCRIPTOR_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid RETRIEVE Request containing  | |
                     | To set to LINKED_SEMANTIC_DESCRIPTOR_ADDRESS and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/007
	TP Id
	TP/oneM2M/CSE/SEM/UPD/007

	Test objective
	Check that the IUT sends a valid response when performing a semantic validation a semantic validation as a result of an update of the <semanticValidation> virtual resource

	Reference
	TS-0034 [6], clauses 6.9.4 and 7.10.3, and TS-0004 [2], clause 7.4.48.2.3

	Parent Release
	Release 3

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <ontologyRepositoy> resource at TARGET_RESOUCE_ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
and the IUT having a <ontology> resource at REFERENCED_ONTOLOGY_ADDRESS
and the IUT having a local policy that allows semantic validation procedures
and the hosting CSE having a <semanticDescriptor> resource
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to the TARGET_RESOURCE_ADDRESS/smv and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | descriptor attribute and  | |
                     | ontologyRef attribute set to  | |
                     | REFERENCED_ONTOLOGY_ADDRESS and  | |
                     | relatedSemantics attributeset to  | |
                     | LINKED_SEMANTIC_DESCRIPTOR_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid response containing  | |
                     | Response Status Code indicating success of validation  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/008
	TP Id
	TP/oneM2M/CSE/SEM/UPD/008

	Test objective
	Check that the IUT rejects the update request of a <semanticMashupJobProfile> resource, indicating a "NOT_ACCEPTABLE" error, when its inputDescriptor attribute value does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.3.4, and TS-0004 [2], clause 7.4.49.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
UPDATE operation
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing inputDescriptor attribute set to a  | |
                     | value that does not conform to the RDF/XML syntax  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource andg   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/009
	TP Id
	TP/oneM2M/CSE/SEM/UPD/009

	Test objective
	Check that the IUT rejects the update request of a <semanticMashupJobProfile> resource, indicating a "NOT_ACCEPTABLE" error, when its outputDescriptor attribute value does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.3.4, and TS-0004 [2], clause 7.4.49.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing accessControlPolicyIDs attribute set to
allow the AE privileges to perform UPDATE operation
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing outputDescriptor attribute set to  | |
                     | a value that does not conform to the RDF/XML syntax  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/UPD/010
	TP Id
	TP/oneM2M/CSE/SEM/UPD/010

	Test objective
	Check that the IUT rejects the update request of a <semanticMashupJobProfile> resource, indicating a "NOT_ACCEPTABLE" error, when its functionDescriptor attribute value does not conform to the RDF/XML syntax as defined in RDF 1.1 XML Syntax

	Reference
	TS-0034 [6], clause 6.3.4, and TS-0004 [2], clause 7.4.49.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing accessControlPolicyIDs attribute set to
allow the AE privileges to perform UPDATE operation
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing functionDescriptor attribute set  | |
                     | to a value that does not conform to the RDF/XML syntax  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource and  | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/011
	TP Id
	TP/oneM2M/CSE/SEM/UPD/011

	Test objective
	Check that the IUT rejects the creation request of a <semanticMashupJobProfile> resource, indicating a "NOT_ACCEPTABLE" error, when its memberFilter attribute value does not conform to a valid SPARQL query request

	Reference
	TS-0034 [6], clause 6.3.4, and TS-0004 [2], clause 7.4.49.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
UPDATE operation
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 40 (semanticMashupJobProfile) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing <semanticMashupJobProfile> resource  | |
                     | representation containing memberFilter attribute set to  | |
                     | a value that does not conform to a valid SPARQL query  | |
                     | request  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not create the <semanticMashupJobProfile>  | |
                     | resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/012
	TP Id
	TP/oneM2M/CSE/SEM/UPD/012

	Test objective
	Check that the IUT creates a new sematicMashupResult when the parameter smjpInputParameter is updated

	Reference
	TS-0034 [6], clause 6.3.4, and TS-0004 [2], clause 7.4.49.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticMashupInstance> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
UPDATE operation
}



·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |When {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 41 (semanticMashupInstance) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing smjpInputParameter attribute set  | |
                     | to a valid value  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT creates a new <sematicMashupResult>  | |
                     | resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+——————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/013
	TP Id
	TP/oneM2M/CSE/SEM/UPD/013

	Test objective
	Check that the IUT changes the mashupMember attribute of sematicMashupInstance when the parameter memberStoreType is updated

	Reference
	TS-0034 [6], clause 6.4.4, and TS-0004 [2], clause 7.4.50.2.3, TS-0001 [1], clause 9.6.54

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticMashupInstance> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
UPDATE operation
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |When {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 41 (semanticMashupInstance) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing memberStoreType attribute set  | |
                     | to a new valid value  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT updates mashupMember attribute of resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/UPD/014
	TP Id
	TP/oneM2M/CSE/SEM/UPD/014

	Test objective
	Check that the IUT rejects the update request of a <semanticDescriptor> resource in which descriptorRepresentation attribute is set to "IRI".

	Reference
	TS-0034 [6], clause 6.1.4, and TS-0004 [2], clause 7.4.34.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------+-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource representation containing  | |
                     | descriptorRepresentation attribute is set to "IRI"  | |
                     |} | |
·                  +-------------------------------------------+-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not update the <semanticDescriptor> resource and   | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————-+———————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/UPD/015
	TP Id
	TP/oneM2M/CSE/SEM/UPD/015

	Test objective
	Check that the IUT generates a Response Status Code indicating a "SPARQL_UPDATE_ERROR" error to a update request of a <semanticDescriptor> resource in which semanticOpExec attribute contains a valid SPARQL update request and request cannot be executed by the Hosting CSE.

	Reference
	TS-0034 [6], clause 6.1.4, and TS-0004 [2], clause 7.4.34.2.3

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing semanticOpExec attribute set  | |
                     | to a SPARQL update request and  | |
                     | SPARQL update request cannot be executed by IUT  | |
                     |}  | |
                     | | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not update the <semanticDescriptor> resource and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5212 (SPARQL_UPDATE_ERROR)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————–+————-+
7.2.2.15.3	RETRIEVE Operation
TP/oneM2M/CSE/SEM/RET/001
	TP Id
	TP/oneM2M/CSE/SEM/RET/001

	Test objective
	Check that the IUT generates a Response Status Code indicating a "NOT_ACCEPTABLE" error to a retrieve request of a <semanticFanOutPoint> resource when the request contains a semanticsFilter condition set to a non-valid SPARQL query request

	Reference
	TS-0004 [2], clause 7.4.35.2.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <group> resource at TARGET_RESOURCE_ADDRESS containing
semanticSupportIndicator attribute set to "True" and
accessControlPolicyIDs attribute set to allow the AE privileges to perform
RETRIEVE operation and
<semanticFanOutPoint> virtual resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/sfop and  | |
                     | From set to AE‑ID and  | |
                     | Semantic Query Indicator set to "True" and  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter conditionset to a non‑valid SPARQL query request  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/RET/002
	TP Id
	TP/oneM2M/CSE/SEM/RET/002

	Test objective
	Check that the IUT generates a <semanticMashupResult> resource as a child of a <semanticMashupInstance> when a retrieve operation is sent to its <mashup> virtual resource

	Reference
	TS-0004 [2], clause 7.4.51.2.2, and TS-0034 [6], clause 6.5.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupInstance> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform
RETRIEVE operation and
<mashup> virtual resource
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/msp and  | |
                     | From set to AE‑ID and  | |
                     | Content set to void  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUTcreates a child <semanticMashupResult> resource at  | |
                     | TARGET_RESOURCE_ADDRESS and  | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/RET/003
	TP Id
	TP/oneM2M/CSE/SEM/RET/003

	Test objective
	Check that the IUT generates a Response Status Code indicating a "NOT_ACCEPTABLE" error to a retrieve request of a <semanticFanOutPoint> resource when the request addresses a group resource with semanticSupportIndicator attribute set to "False"

	Reference
	TS-0004 [2], clause 7.4.35.2.2, and TS-0001 [1], clause 10.2.7.12

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <group> resource at TARGET_RESOURCE_ADDRESS containing
semanticSupportIndicator attributeset to "False" and
accessControlPolicyIDs attribute set to allow the AE privileges to perform
RETRIEVE operation and
<semanticFanOutPoint> virtual resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS/sfop and  | |
                     | From set to AE‑ID and  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter conditionset to a valid SPARQL query request  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 5207 (NOT_ACCEPTABLE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/RET/004
	TP Id
	TP/oneM2M/CSE/SEM/RET/004

	Test objective
	Check that the IUT accepts a valid semantic discovery request for target resource other than <semanticFanOutPoint>

	Reference
	TS-0034 [6], clause 7.4, TS-0001 [1] clauses 8.1.2 and 10.2.14

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a AE resource containing
<semanticDescriptor>
and no restrictions from ACPs
}



·                  +--------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter conditionset to a valid SPARQL query request  | |
                     | not containing <Semantic Query Indicator> parameter  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Semantic resource discovery result containing  | |
                     | URI (of child resource with target semanticDescriptor)  | |
                     |} | |
+———————-+——————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/RET/005
	TP Id
	TP/oneM2M/CSE/SEM/RET/005

	Test objective
	Check that the IUT accepts a valid semantic discovery request for group members

	Reference
	TS-0001 [1], clauses 8.1.2, 9.6.14a, 10.2.7.12 and 10.2.14, and TS-0034 [6], clauses 6.2.2 and 7.4

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having <semanticSupportIndicator> set to TRUE
and the IUT having registered the AE
and the IUT having a AE <group> resource containing
<semanticDescriptor>
and no restrictions from ACPs
}



·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS containing   | |
                     | <semanticFanOutPoint> and  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter conditionset to a valid SPARQL query request  | |
                     | not containing <Semantic Query Indicator> parameter  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Semantic resource discovery result containing  | |
                     | URI (of child resource with target semanticDescriptor)  | |
                     |} | |
+———————-+———————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/RET/006
	TP Id
	TP/oneM2M/CSE/SEM/RET/006

	Test objective
	Check that the IUT accepts a valid semantic discovery request for group members hosted at other CSE and sends a discovery request to the remote CSE

	Reference
	TS-0034 [6], clauses 6.2.2 and 7.4

	Config Id
	CF02

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <semanticDescriptor> having linked semantic resource at remote CSE
and no restrictions from ACPs
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS containing   | |
                     | <semanticFanOutPoint> and  | |
                     | not containing <Semantic Query Indicator> parameter  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE2 |
                     | the IUT sends a valid RETRIEVE Request containing  | |
                     | To set to address of linked semantic resource at remote CSE  | |
                     |} | |
+———————-+————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/RET/007
	TP Id
	TP/oneM2M/CSE/SEM/RET/007

	Test objective
	Check that the IUT accepts a valid semantic discovery response for group members hosted at other CSE and sends a discovery response to the originating AE

	Reference
	TS-0001 [1], clauses 8.1.2, 9.6.14a, 10.2.7.12 and 10.2.14, and TS-0034 [6], clauses 6.2.2 and 7.4

	Config Id
	CF02

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticDescriptor> resource having linked semantic resource at remote CSE
and no restrictions from ACPs
and the IUT having receive d a valid RETRIEVE Request from AE containing
To set to TARGET_RESOURCE_ADDRESS containing
<semanticFanOutPoint> and
Filter Criteria containing
semanticsFilter conditionset to a valid SPARQL query request
not containing <Semantic Query Indicator> parameter
and the IUT having sent a valid RETRIEVE Request containing
To set to address of linked semantic resource at remote CSE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= CSE2 |
                     | the IUT receives a valid Response from CSE2 containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | containing Semantic resource from remote CSE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Semantic resource discovery result containing  | |
                     | URI (of child resource with target semanticDescriptor)  | |
                     |} | |
+———————-+——————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/RET/008
	TP Id
	TP/oneM2M/CSE/SEM/RET/008

	Test objective
	Check that the IUT retrieves relatedSemantics in a valid semantic discovery request

	Reference
	TS-0034 [6], clauses 7.4, 7.4.3, and TS-0001 [1] clauses 8.1.2, 10.2.14

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a AE resource containing
<semanticDescriptor> containing
relatedSemantics attribute
and no restrictions from ACPs
}



·                  +------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter conditionset to a valid SPARQL query request  | |
                     | not containing <Semantic Query Indicator> parameter  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Semantic resource discovery result containing  | |
                     | URI (of child resource with target semanticDescriptor) and  | |
                     | URI (of resources from relatedSemantics)  | |
                     |} | |
+———————-+——————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/RET/009
	TP Id
	TP/oneM2M/CSE/SEM/RET/009

	Test objective
	Check that the IUT retrieves content-related semantics in a valid semantic discovery request

	Reference
	TS-0034 [6], clauses 7.4, 7.6, and TS-0001 [1] clauses 8.1.2, 10.2.14

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a AE resource containing
<semanticDescriptor> and
<contentInstance> present
and no restrictions from ACPs
}



·                  +----------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter conditionset to a valid SPARQL query request and  | |
                     | content‑related semantics  | |
                     | not containing <Semantic Query Indicator> parameter  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Semantic resource discovery result containing  | |
                     | URI (of child resource with target semanticDescriptor)  | |
                     |} | |
+———————-+—————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/RET/010
	TP Id
	TP/oneM2M/CSE/SEM/RET/010

	Test objective
	Check that the IUT returns successfully the attributes of the <semanticMashupJobProfile> resource


	Reference
	TS-0004 [2], clause 7.4.49.2.2, TS-0034 [6], clause 6.3.3, TS-0001 [1], clause 9.6.53

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to
perform RETRIEVE operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | attributes of resource representation  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/RET/011
	TP Id
	TP/oneM2M/CSE/SEM/RET/011

	Test objective
	Check that the IUT returns successfully the attributes of the <semanticMashupInstance> resource


	Reference
	TS-0004 [2], clause 7.4.50.2.2, TS-0034 [6], clause 6.4.3, TS-0001 [1], clause 9.6.54

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupInstance> resource at
TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform RETRIEVE operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | attributes of resource representation  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/RET/012
	TP Id
	TP/oneM2M/CSE/SEM/RET/012

	Test objective
	Check that the IUT returns successfully the attributes of the <semanticMashupResult> resource


	Reference
	TS-0004 [2], clause 7.4.52.2.2, TS-0034 [6], clause 6.6.2, TS-0001 [1], clause 9.6.56

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupResult> resource at TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform RETRIEVE operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | attributes of resource representation  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/RET/013
	TP Id
	TP/oneM2M/CSE/SEM/RET/013

	Test objective
	Check that the IUT rejects a semantic query request with semanticsFilter condition set to a non-valid SPARQL query request

	Reference
	TS-0034 [6], clause 7.5, TS-0004 [1] clauses 7.3.3.19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource at TARGET_RESOURCE_ADDRESS containing
<semanticDescriptor> resource as direct child or as a descendent with accessControlPolicyIDs attribute set to allow the AE privileges to perform RETRIEVE operation
}



·                  +---------------------------------------------------------+-------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     |the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Semantic Query Indicator set to "True" and  | |
                     | Result Content shall be set to "semantic content"  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter condition set to a non‑valid SPARQL query request  | |
                     |} | |
·                  +---------------------------------------------------------+-------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+———————————————————+————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/RET/014
	TP Id
	TP/oneM2M/CSE/SEM/RET/014

	Test objective
	Check that the IUT accepts a valid semantic query request for target resource and returns a valid query result

	Reference
	TS-0034 [6], clause 7.5, TS-0004 [1] clauses 7.3.3.19

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource at TARGET_RESOURCE_ADDRESS containing
<semanticDescriptor> resource as direct child or as a descendent with accessControlPolicyIDs attribute set to allow the AE privileges to perform RETRIEVE operation
}



·                  +---------------------------------------------------------------------+-------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     |the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Semantic Query Indicator set to "True" and  | |
                     | Result Content shall be set to "semantic content"  | |
                     | Filter Criteria containing  | |
                     | semanticsFilter condition set to a valid SPARQL query request  | |
                     |} | |
·                  +---------------------------------------------------------------------+-------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing string representing Semantic query result  | |
                     |} | |
+———————-+———————————————————————+————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/RET/015
	TP Id
	TP/oneM2M/CSE/SEM/RET/015

	Test objective
	Check that the IUT returns successfully the attributes of the <semanticDescriptor> resource except the semanticOpEx attribute

	Reference
	TS-0004 [2], clause 7.4.34.2.2,, TS-0001 [1], clause 9.6.30

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	
with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticDescriptor> resource at TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform RETRIEVE operation
}



·                  +----------+------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +----------+------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000 (OK) and  | |
                     | Content containing  | |
                     | attributes of resource representation ensuring that the semanticOpExec attribute is never returned in the response.  | |
                     |} | |
+———————-+———-+————————————————————————————————————————+————-+
TP/oneM2M/CSE/SEM/CRE/016
	TP Id
	TP/oneM2M/CSE/SEM/CRE/016

	Test objective
	Check that the IUT generates a Response Status Code indicating a "ONTOLOGY_NOT_AVAILABLE" error when referenced ontology of the local linked <semanticDescriptor> resources cannot be retrieved during a semantic validation process

	Reference
	TS-0004 [2], clause 7.4.34.2.1

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE, PICS_SEMANTIC_VALIDATION

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
and the IUT having privileges to perform RETRIEVE operation on <semanticDescriptor>
resource at SEMANTIC_DESCRIPTOR_RESOURCE_ADDRESS containing
ontologyRef attribute set to an invalid URI
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | relatedSemantics attribute set to SEMANTIC_DESCRIPTOR_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4118 (ONTOLOGY_NOT_AVAILABLE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/CRE/017
	TP Id
	TP/oneM2M/CSE/SEM/CRE/017

	Test objective
	Check that the IUT generates a Response Status Code indicating a "INVALID_SEMANTICS" error when any aspect of the semantic validation process fails (according to clause 7.10.3.7.10.4 in TS-0034[6])

	Reference
	TS-0004 [2], clause 7.4.34.2.1, TS-0034 [6], clause 7.10.3, 7.10.4

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE, PICS_SEMANTIC_VALIDATION

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |iIUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 24 (semanticDescriptor) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticDescriptor> resource containing  | |
                     | validationEnable attribute set to "True" and  | |
                     | descriptor attribute set to invalid RDF triples  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4120  | |
                     | (INVALID_SEMANTICS)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————+————-+


7.2.2.15.4	DELETE Operation
TP/oneM2M/CSE/SEM/DEL/001
	TP Id
	TP/oneM2M/CSE/SEM/DEL/001

	Test objective
	Check that the IUT delete all <semanticMashupInstance> child resources when their parent <semanticMashupJobProfile> receives a delete request

	Reference
	TS-0034 [6], clause 6.3.5

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform DELETE operation and
<semanticMashupInstance> resource and
<semanticMashupInstance> resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticMashupJobProfile> resource representation  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2002 (DELETED) and  | |
                     | the IUT deletes the <semanticMashupJobProfile> resource and  | |
                     | the IUTdeletes thetwo <semanticMashupInstance> child resources  | |
                     |} | |
+———————-+————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SEM/DEL/002
	TP Id
	TP/oneM2M/CSE/SEM/DEL/002

	Test objective
	Check that the IUT notifies all <semanticMashupInstance> resources referenced in the smiID attribute when the corresponding <semanticMashupJobProfile> receives a delete request

	Reference
	TS-0034 [6], clause 6.3.5

	Config Id
	CF02

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a <semanticMashupJobProfile> resource at TARGET_RESOURCE_ADDRESS containing
accessControlPolicyIDs attribute set to allow the AE privileges to perform DELETE operation and
smiID attribute set to a list of two <semanticMashupInstance> resources located in
hosting CSE
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | <semanticMashupJobProfile> resource representation  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT notifies each referenced <semanticMashupJobProfile> resource  | |
                     | located in the hosting CSE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SEM/DEL/003
	TP Id
	TP/oneM2M/CSE/SEM/DEL/003

	Test objective
	Check that the IUT deletes successfully <semanticMashupResult> resource


	Reference
	TS-0004 [2], clause 7.4.52.2.4, TS-0034 [6], clause 6.6.3, TS-0001 [1], clause 9.6.56

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <semanticMashupResult> resource at TARGET_RESOURCE_ADDRESS containing accessControlPolicyIDs attribute set to allow the AE privileges to perform
DELETE operation
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_IDand  | |
                     | no content  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT deletes the TARGET_RESOURCE_ADDRESS resource and   | |
                     | the IUT sends a Response message containing  | |
                     | Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————–+————-+
7.2.2.16	Initial Service Provisioning (ISP)
7.2.2.16.1	BASIC Operation
TP/oneM2M/CSE/ISP/001
	TP Id
	TP/oneM2M/CSE/ISP/001

	Test objective
	Check that the IUT accepts a valid M2M node subscription

	Reference
	TS-0001 [1], clauses 9.6.19, 9.6.20,11.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_IN_CSE, PICS_REMOTE_PROVISIONING

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having completed the enrolment function procedure with the AE
and the IUT having completed the security provisioning procedure
and the IUT having a <m2mserviceSubscriptionProfile > at
PARENT_RESOURCE_ADDRESS

}



·                  +----------------------------------------+-------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 20_(_ serviceSubscribedNode ) and  | |
                     | Contentcontaining valid serviceSubscribedNode resource   | |
                     |representation  | |
                     |} | |
·                  +----------------------------------------+-------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED)  | |
                     |} | |
+———————-+—————————————-+————————————————-+————-+
TP/oneM2M/CSE/ISP/002
	TP Id
	TP/oneM2M/CSE/ISP/002

	Test objective
	Check that the IUT rejects a non-authorized M2M node subscription

	Reference
	TS-0001 [1], clauses 9.6.19, 9.6.20, 11.2

	Config Id
	CF01

	Parent Release
	Release 3

	PICS Selection
	PICS_IN_CSE, PICS_REMOTE_PROVISIONING

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having completed the enrolment function procedure with the AE
and the IUT having completed the security provisioning procedure
and the IUT not containing a <m2m serviceSubscriptionProfile >
}



·                  +---------------------------------+----------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 20_(_ serviceSubscribedNode ) and  | |
                     | Content containing valid serviceSubscribedNode resource  | |
                     |} | |
·                  +---------------------------------+----------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)and  | |
                     | no Content  | |
                     |} | |
+———————-+———————————+—————————————————-+————-+
7.2.2.17	Service Charging and Accounting (CSA)
7.2.2.17.1	Event Based Charging (EBC)
TP/oneM2M/CSE/SCA/EBC/001
	TP Id
	TP/oneM2M/CSE/SCA/EBC/001

	Test objective
	Check that the IUT successfully generates the statistics collection record and send to target AE once the IUT receives an event collection trigger from AE when the eventType attribute is TIMERBASED in the stat collection configuration

	Reference
	TS-0001 [1], clause 10.2.11, clause 9.6.24, TS004 [2], clause 7.4.24

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE, PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource containing
a child eventConfig resource containing
eventType attribute set to TIMERBASED and
eventID attribute having value EVENT_ID
and the IUT having a statsCollect resource containing
eventID attributeset to EVENT_ID
and the AE having privileges to perform Create operation
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT is triggered to send statistic collection record  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Notify Request containing  | |
                     | Content (see note) containing  | |
                     | Statistic collection representation  | |
                     |} | |
	NOTE: Content value is not specified.



TP/oneM2M/CSE/SCA/EBC/002
	TP Id
	TP/oneM2M/CSE/SCA/EBC/002

	Test objective
	Check that the IUT successfully generates the statistics collection record and send to target AE once the IUT receives an event collection trigger from AE when the eventType attribute is TIMERBASED in the stat collection configuration

	Reference
	TS-0001 [1], clause 10.2.11, clause 9.6.24, TS004 [2], clause 7.4.24

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE, PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource containing
a child eventConfig resource containing
eventType attribute set to TIMERBASED and
eventID attribute having value EVENT_ID
and the IUT having a statsCollect resource containing
eventID attributeset to EVENT_ID
and the AE having privileges to perform Update operation
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT is triggered to send statistic collection record  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Notify Request containing  | |
                     | Content (see note) containing  | |
                     | statistic collection representation  | |
                     |} | |
	NOTE: Content value is not specified.



TP/oneM2M/CSE/SCA/EBC/003
	TP Id
	TP/oneM2M/CSE/SCA/EBC/003

	Test objective
	Check that the IUT successfully generates the statistics collection record and send to target AE once the IUT receives an event collection trigger from AE when the eventType attribute is STORAGEBASED in the stat collection configuration

	Reference
	TS-0001 [1], clause 10.2.11, clause 9.6.24, TS004 [2], clause 7.4.24

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE, PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource containing
a child eventConfig resource containing
eventType attribute set to STORAGEBASED and
eventID attribute having value EVENT_ID
and the IUT having a statsCollect resource containing
eventID attributeset to EVENT_ID
and the AE having privileges to perform Create operation
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT is triggered to send statistic collection record  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Notify Request containing   | |
                     | Content (see note) containing  | |
                     | statistic collection resource representation  | |
                     |} | |
	NOTE: Content value is not specified.



TP/oneM2M/CSE/SCA/EBC/004
	TP Id
	TP/oneM2M/CSE/SCA/EBC/004

	Test objective
	Check that the IUT successfully generates the statistics collection record and send to target AE once the IUT receives an event collection trigger from AE when the eventType attribute is DataOperation in the stat collection configuration

	Reference
	TS-0001 [1], clause 10.2.11, clause 9.6.24, TS004 [2], clause 7.4.24

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE, PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource containing
a child eventConfig resource containing
eventType attribute set to DataOperation and
eventID attribute having value EVENT_ID
and the IUT having a statsCollect resource containing
eventID attributeset to EVENT_ID
and the AE having privileges to perform Create operation
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT is triggered to send statistic collection record  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Notify Request containing   | |
                     | Content (see note) containing  | |
                     | statistic collection resource representation  | |
                     |} | |
	NOTE: Content value is not specified.




TP/oneM2M/CSE/SCA/EBC/005
	TP Id
	TP/oneM2M/CSE/SCA/EBC/005

	Test objective
	Check that the IUT does not accept eventEnd time less than eventStart time

	Reference
	TS-0001 [1], clause 10.2.11.6, clause 9.6.24, TS004 [2], clause 7.4.24.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE, PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource
and the AE having privileges to perform Create operation
}



·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE request containing  | |
                     | eventConfig resource containing  | |
                     | eventEnd time less than eventStart time  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————-+————-+
TP/oneM2M/CSE/SCA/EBC/006
	TP Id
	TP/oneM2M/CSE/SCA/EBC/006

	Test objective
	Check that the IUT verifies dataSize attribute when eventType is set to "Storage based"

	Reference
	TS-0001 [1], clause 10.2.11.6, clause 9.6.24, TS004 [2], clause 7.4.24.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE,PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource
and the AE having privileges to perform Create operation
}



·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE request containing  | |
                     | eventConfig resource containing  | |
                     | eventType set to STORAGEBASED and  | |
                     | dataSize attribute not set   | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————-+————-+
TP/oneM2M/CSE/SCA/EBC/007
	TP Id
	TP/oneM2M/CSE/SCA/EBC/007

	Test objective
	Check that the IUT generates statistic collection records when multiple <statsCollect> resources are defined

	Reference
	TS-0001 [1], clause 10.2.11.10, clause 9.6.24, clause 9.6.25, TS004 [2], clause 7.4.24.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE, PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource containing
a child eventConfig resource containing
eventType attribute set to TIMERBASED and
eventID attribute having value EVENT_ID
and the IUT having a statsCollect resource containing
eventID attributeset to EVENT_ID and
collectingEntity attribute set to AE
and the IUT having a statsCollect resource containing
eventID attributeset to EVENT_ID and
collectingEntity attribute set to AE
}



·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT is triggered to send statistic collection record  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Notify Request containing  | |
                     | Content (see note) containing  | |
                     | statistic collection representation1 and  | |
                     | statistic collection representation2  | |
                     |} | |
	NOTE: Content value is not specified.



TP/oneM2M/CSE/SCA/EBC/008
	TP Id
	TP/oneM2M/CSE/SCA/EBC/008

	Test objective
	Check that the IUT sends a CDR in an Accounting-Request message when sending to an external charging service

	Reference
	TS-0001 [1], clause 12.2.4.2, clause 9.6.24, clause 9.6.25, TS004 [2], clause 7.4.24.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE, PICS_SCA

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a statsConfig resource containing
a child eventConfig resource containing
eventType attribute set to TIMERBASED and
eventID attribute having value EVENT_ID
and the IUT having a statsCollect resource containing
eventID attributeset to EVENT_ID
and the charging messages are sent to an external Charging Server
}



·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT is triggered to send statistic collection record  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |AE <= IUT |
                     | the IUT sends a valid Notify Request containing  | |
                     | Content (see note) containing  | |
                     | statistic collection representation  | |
                     |} | |
+———————-+———————————————————————————————————————+————-+
7.2.2.18	Service Subscription Management(SSM)
7.2.2.18.1	Service Subscription User Profile(SSUP)
TP/oneM2M/CSE/SSM/SSUP/001
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/001

	Test objective
	Check that the IUT successfully performs operations on resource serviceSubscribedUserProfile for authorized M2M Service User

	Reference
	TS-0001 [1], clauses 9.6.68

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having m2mServiceSubscriptionProfile at TARGET_RESOURCE_ADDRESS
containing a child resource
and the AE having privileges to perform OPERATION on TARGET_RESOURCE_ADDRESS
and the IUThaving an authorized M2M Service User AE-ID
}



·                  +--+---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized M2M Users AE‑ID and  | |
                     |} | |
·                  +--+---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status set to RESPONSE_STATUS_CODE and  | |
                     | Content containing  | |
                     | serviceSubscribedUserProfile resource representation (when required)  | |
                     |} | |
+———————-+–+—————————————————————————————————————+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SSM/SSUP/001_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSUP/001_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SSM/SSUP/001_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SSM/SSUP/002_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SSM/SSUP/002
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/002

	Test objective
	Check that the IUT rejects the operation on serviceSubscribedUserProfile resource when the attributes violate the limits specified in the parent resource

	Reference
	TS-0001 [1], clauses 9.6.68

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUThaving registered an AE
and the IUT having serviceSubscribedUserProfile at TARGET_RESOURCE_ADDRESS and the AE having privileges to perform OPERATION on TARGET_RESOURCE and the IUThaving an authorized M2M Service User AE-ID

}



·                  +---------------------------------------------------------------------------------------+--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized M2M Users AE‑ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------+--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4102 (CONTENTS_UNACCEPTABLE)  | |
                     |} | |
+———————-+—————————————————————————————+——————————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SSM/SSUP/002_CRE
	CREATE

	TP/oneM2M/CSE/SSM/SSUP/002_UPD
	UPDATE




TP/oneM2M/CSE/SSM/SSUP/003
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/003

	Test objective
	Check that the IUT successfully restricts the usage of services by a M2M Service User

	Reference
	TS-0001 [1], clauses 9.6.68

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUThaving registered an AE
and the IUT having m2mServiceSubscriptionProfile at TARGET_RESOURCE_ADDRESS containing a child resource
containing a child resource
the AE having privileges to perform OPERATION on TARGET_RESOURCE_ADDRESS
and the IUThaving an authorized M2M Service User
}



·                  +-----------------------------------------+------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to an authorized M2M Service User AE‑ID  | |
                     |} | |
·                  +-----------------------------------------+------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUSs_CODE and  | |
                     | Content containing  | |
                     | serviceSubscribedUserProfile resource representation  | |
                     |} | |
+———————-+—————————————–+————————————————————————+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SSM/SSUP/003_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSUP/003_UPD
	UPDATE
	2004 (UPDATED)




TP/oneM2M/CSE/SSM/SSUP/004
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/004

	Test objective
	Check that the IUT rejects the OPERATION when the associated services of a M2M Service User reach limits provided in the serviceSubscribedUserProfile resource

	Reference
	TS-0001 [1], clauses 9.6.68

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUThaving registered an AE
and the IUT having serviceSubscribedUserProfile at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform OPERATION on
}



·                  +----------------------+---------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to an authorized M2M Service User AE‑ID  | |
                     |} | |
·                  +----------------------+---------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4102 (CONTENTS_UNACCEPTABLE)  | |
                     |} | |
+———————-+———————-+—————————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SSM/SSUP/004_CRE
	CREATE

	TP/oneM2M/CSE/SSM/SSUP/004_UPD
	UPDATE




TP/oneM2M/CSE/SSM/SSUP/005
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/005

	Test objective
	Check that IUT rejects the request when the values of ATTRIBUTE in request exceed the actual resources associated with the Service user

	Reference
	TS-0001 [1], clauses 9.6.68

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUThaving registered an AE
and the IUT having serviceSubscribedUserProfile at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE on TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------+----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to an authorized M2M Service User AE‑ID  | |
                     |} | |
·                  +--------------------------------------------+----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4102 (CONTENTS_UNACCEPTABLE)  | |
                     |} | |
+———————-+——————————————–+—————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/SSM/SSUP/005_MNA
	maxNumAEs

	TP/oneM2M/CSE/SSM/SSUP/005_MNN
	maxNumNodes

	TP/oneM2M/CSE/SSM/SSUP/005_MNC
	maxNumContainers

	TP/oneM2M/CSE/SSM/SSUP/005_MNI
	maxNumInstancesPerContainer




TP/oneM2M/CSE/SSM/SSUP/006
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/006

	Test objective
	Check that IUT accepts the request when the values of ATTRIBUTE in request do not exceed the actual resources associated with the Service user

	Reference
	TS-0001 [1], clauses 9.6.68

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS _CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUThaving registered an AE
and the IUT having serviceSubscribedUserProfile at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform UPDATE on TARGET_RESOURCE**_** ADDRESS
}



·                  +--------------------------------------+-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     |} | |
·                  +--------------------------------------+-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     |} | |
+———————-+————————————–+———————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/SSM/SSUP/006_MNA
	maxNumAEs

	TP/oneM2M/CSE/SSM/SSUP/006_MNN
	maxNumNodes

	TP/oneM2M/CSE/SSM/SSUP/006_MNC
	maxNumContainers

	TP/oneM2M/CSE/SSM/SSUP/006_MNI
	maxNumInstancesPerContainer




TP/oneM2M/CSE/SSM/SSUP/007
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/007

	Test objective
	Check that IUT successfully accepts the request with the default access control policies when the accessControlPolicyIDs attribute of a resource serviceSubscribedUserProfile created by this M2M Service User is not configured

	Reference
	TS-0001 [1], clauses 9.6.68

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS _CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having m2mServiceSubscriptionProfile at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform OPERATION on TARGET_RESOURCE_ADDRESS
and the IUT having an authorized M2M Service User AE-ID
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to an authorized M2M Service User AE‑ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SSM/SSUP/007_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSUP/007_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SSM/SSUP/007_UPD
	UPDATE
	2004 (UPDATED)




TP/oneM2M/CSE/SSM/SSUP/008
	TP Id
	TP/oneM2M/CSE/SSM/SSUP/008

	Test objective
	Check that IUT rejects OPERATION request if service subscription profile associated with the M2M service user/AE is not available

	Reference
	TS-0004 [2], clauses 7.3.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT not having a <serviceSubscribedUserProfile_>_ associated with the M2M service user at
TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform operation on
TARGET_RESOURCE_ADDRESS
}



·                  +---------------+----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from an AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | a valid content  | |
                     |} | |
·                  +---------------+----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41xx (UNAUTHORIZED_USER)  | |
                     |} | |
+———————-+—————+———————————————————————————————————————-+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SSM/SSUP/008_RET
	RETRIEVE

	TP/oneM2M/CSE/SSM/SSUP/008_UPD
	UPDATE

	TP/oneM2M/CSE/SSM/SSUP/008_DEL
	DELETE



7.2.2.18.2	Service Subscription Profile(SSP)
7.2.2.18.2.1	Basic Operation
TP/oneM2M/CSE/SSM/SSP/001
	TP Id
	TP/oneM2M/CSE/SSM/SSP/001

	Test objective
	Check that the IUT successfully performs operations on resource m2mServiceSubscriptionProfile for authorized AE

	Reference
	TS-0001 [1], clauses 9.6.19

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform OPERATION on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+————————————————————————————————–+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SSM/SSP/001_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/001_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SSM/SSP/001_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SSM/SSP/001_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/SSM/SSP/002
	TP Id
	TP/oneM2M/CSE/SSM/SSP/002

	Test objective
	Check that the IUT responds with an error when the AE not having service subscription tries to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS

	Reference
	TS-0004 [2], clause 7.3.2.1, clause 7.3.2.7

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT not having a m2mServiceSubscriptionProfile resource For the AE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4128  | |
                     |(SERVICE_SUBSCRIPTION_NOT_ESTABLISHED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SSM/SSP/002_CRE
	CREATE

	TP/oneM2M/CSE/SSM/SSP/002_RET
	RETRIEVE

	TP/oneM2M/CSE/SSM/SSP/002_UPD
	UPDATE

	TP/oneM2M/CSE/SSM/SSP/002_DEL
	DELETE



TP/oneM2M/CSE/SSM/SSP/003
	TP Id
	TP/oneM2M/CSE/SSM/SSP/003

	Test objective
	Check that the IUT responds with an error when the AE having inactive service subscription tries to perform a request

	Reference
	TS-0004 [2], clause 7.3.2.1, clause 7.3.2.7

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having a m2mServiceSubscriptionProfile resource For the AE
containing
status attribute set to INACTIVE
}



·                  +----+--------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE To set to  | |
                     |TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----+--------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4139  | |
                     |(SERVICE_SUBSCRIPTION_NOT_ACTIVE)  | |
                     |} | |
+———————-+—-+——————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SSM/SSP/003_CRE
	CREATE

	TP/oneM2M/CSE/SSM/SSP/003_RET
	RETRIEVE

	TP/oneM2M/CSE/SSM/SSP/003_UPD
	UPDATE

	TP/oneM2M/CSE/SSM/SSP/003_DEL
	DELETE



TP/oneM2M/CSE/SSM/SSP/004
	TP Id
	TP/oneM2M/CSE/SSM/SSP/004

	Test objective
	Check that the IUT processes the request when the AE having an active service subscription tries to perform a request

	Reference
	TS-0004 [2], clause 7.3.2.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a m2mServiceSubscriptionProfile resource For the AE
containing
status attribute set to ACTIVE
}



·                  +--------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request from AE  | |
                     | To set to TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK)  | |
                     |} | |
+———————-+——————————————————————————————————–+————-+
TP/oneM2M/CSE/SSM/SSP/005
	TP Id
	TP/oneM2M/CSE/SSM/SSP/005

	Test objective
	Check that the IUT responds with an error when the authorized AE exceeds the request rate limit specified in its service subscription profile

	Reference
	TS-0004 [2], clause 7.3.2.x

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a m2mServiceSubscriptionProfile resource For the AE
containing
maxRequestRate attribute set to MAX_REQUEST_RATE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request  | |
                     | at a rate higher than MAX_REQUEST_RATE  | |
                     | from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 413x  | |
                     |(SERVICE_SUBSCRIPTION_LIMITS_EXCEEDED)  | |
                     |} | |
+———————-+——————————————————————————————————————————–+————-+
	TP Id
	OPERATION

	TP/oneM2M/CSE/SSM/SSP/005_CRE
	CREATE

	TP/oneM2M/CSE/SSM/SSP/005_RET
	RETRIEVE

	TP/oneM2M/CSE/SSM/SSP/005_UPD
	UPDATE

	TP/oneM2M/CSE/SSM/SSP/005_DEL
	DELETE



TP/oneM2M/CSE/SSM/SSP/006
	TP Id
	TP/oneM2M/CSE/SSM/SSP/006

	Test objective
	Check that the IUT processes the request when the authorized AE sends requests within the request rate limit specified in its service subscription profile

	Reference
	TS-0004 [2], clause 7.3.2.x

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a m2mServiceSubscriptionProfile resource For the AE
containing
maxRequestRate attribute set to MAX_REQUEST_RATE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid RETRIEVE Request  | |
                     | at a rate less than MAX_REQUEST_RATE  | |
                     | from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2000(OK)  | |
                     |} | |
+———————-+———————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SSM/SSP/007
	TP Id
	TP/oneM2M/CSE/SSM/SSP/007

	Test objective
	Check that the IUT responds with an error when the authorized AE tries to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS and it exceeds the limit for ATTRIBUTE_NAME in its m2mServiceSubscriptionProfile resource

	Reference
	TS-0004 [2], clause 7.3.3.x

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a m2mServiceSubscriptionProfile resource For the AE
containing
ATTRIBUTE_NAME attribute set to MAX_VALUE
and the IUT having the current limit with CURRENT_VALUE corresponding to this
ATTRIBUTE_NAME_ equal MAX_VALUE
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request  | |
                     | from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 413x (SERVICE_SUBSCRIPTION_LIMITS_EXCEEDED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE_NAME
	OPERATION

	TP/oneM2M/CSE/SSM/SSP/007_MAE
	maxNumAEs
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MND
	maxNumNodes
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MNB
	maxNumBytes
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MNU
	maxNumUsers
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MNC
	maxNumContainers
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MIC_CRE
	maxNumInstancesPerContainer
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MIC_UPD
	maxNumInstancesPerContainer
	UPDATE

	TP/oneM2M/CSE/SSM/SSP/007_MNT
	maxNumTimeSeries
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MMG_CRE
	maxMembersPerGroup
	CREATE

	TP/oneM2M/CSE/SSM/SSP/007_MMG_UPD
	maxMembersPerGroup
	UPDATE

	TP/oneM2M/CSE/SSM/SSP/007_MNF
	maxNumFlexContainers
	CREATE



TP/oneM2M/CSE/SSM/SSP/008
	TP Id
	TP/oneM2M/CSE/SSM/SSP/008

	Test objective
	Check that the IUT processes the request when the authorized AE having not exceeded the limit for ATTRIBUTE_NAME in its m2mServiceSubscriptionProfile resource tries to perform OPERATION on the resource TARGET_RESOURCE_ADDRESS

	Reference
	TS-0004 [2], clause 7.3.3.x

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a m2mServiceSubscriptionProfile resource For the AE
containing
ATTRIBUTE_NAME_ attribute set to MAX_VALUE
and the IUT having the current limit corresponding to this ATTRIBUTE_NAME with
CURRENT_VALUE less than MAX_VALUE
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request  | |
                     | from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => CSE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE   | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SSM/SSP/008_MAE
	maxNumAEs
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MND
	maxNumNodes
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MNB
	maxNumBytes
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MNU
	maxNumUsers
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MNC
	maxNumContainers
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MIC_CRE
	maxNumInstancesPerContainer
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MIC_UPD
	maxNumInstancesPerContainer
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SSM/SSP/008_MNT
	maxNumTimeSeries
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MMG_CRE
	maxMembersPerGroup
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSP/008_MMG_UPD
	maxMembersPerGroup
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SSM/SSP/008_MNF
	maxNumFlexContainers
	CREATE
	2001 (CREATED)



7.2.2.18.2.2	UPDATE
TP/oneM2M/CSE/SSM/SSP/UPD/001
	TP Id
	TP/oneM2M/CSE/SSM/SSP/UPD/001

	Test objective
	Check that the IUT updates the value of the attributes activationTime , status , deactivationTime in <m2mserviceSubscriptionProfile> resource when activate attribute is set to TRUE in resource representation of UPDATE request

	Reference
	TS-0001 [1], clauses 9.6.19, TS-0004[2], clauses 7.4.19.2.3

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform UPDATE on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resource containing  | |
                     | activate_ attribute set to TRUE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT updates the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resourcecontaining  | |
                     | activate attribute set to TRUE  | |
                     | activation Time attribute set to Current Time  | |
                     | deactivationTime_ attribute set to Null  | |
                     | status attribute set to ACTIVE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SSM/SSP/UPD/002
	TP Id
	TP/oneM2M/CSE/SSM/SSP/UPD/002

	Test objective
	Check that the IUT updates the value of the attributes de_activationTime_ , status when activate attribute is set to FALSE in resource representation of UPDATE request

	Reference
	TS-0001 [1], clauses 9.6.19, TS-0004[2], clauses 7.4.19.2.3

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform UPDATE on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resource containing  | |
                     | activate attribute set to FALSE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT updates the TARGET_RESOURCE_ADDRESS resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resourcecontaining  | |
                     | activate attribute set to FALSE  | |
                     | deactivation Time attribute set to Current Time  | |
                     | status attribute set to INACTIVE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SSM/SSP/UPD/003
	TP Id
	TP/oneM2M/CSE/SSM/SSP/UPD/003

	Test objective
	Check that the IUT overrides the value of the attribute ATTRIBUTE_NAME with the current limit when the value provided in the resource representation of the UPDATE request is less than the current limit.

	Reference
	TS-0001 [1], clauses 9.6.19, TS-0004[2], clauses 7.4.19.2.3

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a <m2mServiceSubscriptionProfile> resource at
TARGET_RESOURCE_ADDRESS
containing
ATTRIBUTE_NAME attribute set to MAX_VALUE
and the IUT having the current limit VALUE_1 corresponding to this
ATTRIBUTE_NAME
and the AE having privileges to perform UPDATE on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resource containing  | |
                     | ATTRIBUTE_NAME attribute set to value less than  | |
                     | VALUE_1.  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resource containing  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_1  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————–+————-+
	TP Id
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MAE
	maxNumAEs

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MND
	maxNumNodes

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MNB
	maxNumBytes

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MNU
	maxNumUsers

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MRR
	maxRequestRate

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MNC
	maxNumContainers

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MIC
	maxNumInstancesPerContainer

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MNT
	maxNumTimeSeries

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MIT
	maxNumInstancesPerTimeSeries

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MMG
	maxMembersPerGroup

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MNR
	maxNotificationRate

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MNF
	maxNumFlexContainers

	TP/oneM2M/CSE/SSM/SSP/UPD/003_MIF
	maxNumInstancesPerFlexContainer



TP/oneM2M/CSE/SSM/SSP/UPD/004
	TP Id
	TP/oneM2M/CSE/SSM/SSP/UPD/004

	Test objective
	Check that the IUT updates successfully the value of the attribute ATTRIBUTE_NAME of the TARGET_RESOURCE_ADDRESS resource, when the value provided in the resource representation of the UPDATE request is more than the current limit.

	Reference
	TS-0001 [1], clauses 9.6.19, TS-0004[2], clauses 7.4.19.2.3

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a m2mServiceSubscriptionProfile resource at
TARGET_RESOURCE_ADDRESS
containing
ATTRIBUTE_NAME attribute set to MAX_VALUE
and the IUT having the current limit with CURRENT_VALUE corresponding to this
ATTRIBUTE_NAME
and the AE having privileges to perform UPDATE on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resource containing  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_1 more than  | |
                     | CURRENT_VALUE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED) and  | |
                     | Content containing  | |
                     | m2mServiceSubscriptionProfile resource containing  | |
                     | ATTRIBUTE_NAME attribute set to VALUE_1  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	ATTRIBUTE_NAME

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MAE
	maxNumAEs

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MND
	maxNumNodes

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MNB
	maxNumBytes

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MNU
	maxNumUsers

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MRR
	maxRequestRate

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MNC
	maxNumContainers

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MIC
	maxNumInstancesPerContainer

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MNT
	maxNumTimeSeries

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MIT
	maxNumInstancesPerTimeSeries

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MMG
	maxMembersPerGroup

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MNR
	maxNotificationRate

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MNF
	maxNumFlexContainers

	TP/oneM2M/CSE/SSM/SSP/UPD/004_MIF
	maxNumInstancesPerFlexContainer



7.2.2.18.3	Service Subscribed App Rule(SSAR)
TP/oneM2M/CSE/SSM/SSAR/001
	TP Id
	TP/oneM2M/CSE/SSM/SSAR/001

	Test objective
	Check that the IUT successfully performs operations on resource seriviceSubscribedAppRule for authorized AE

	Reference
	TS-0001 [1], clauses 9.6.29, TS-0004, clauses 7.4.29

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform OPERATION on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+———————————————————————————————-+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SSM/SSAR/001_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSAR/001_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SSM/SSAR/001_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SSM/SSAR/001_DEL
	DELETE
	2002 (DELETED)



7.2.2.18.4	Service Subscribed Node(SSN)
7.2.2.18.4.1	Basic Operation
TP/oneM2M/CSE/SSM/SSN/001
	TP Id
	TP/oneM2M/CSE/SSM/SSN/001

	Test objective
	Check that the IUT successfully performs operations on resource seriviceSubscribedNode for authorized AE

	Reference
	TS-0001 [1], clauses 9.6.20, TS-0004, clauses 7.4.20

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform OPERATION on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+——————————————————————————————-+————-+
	TP Id
	OPERATION
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/SSM/SSN/001_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/SSM/SSN/001_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/SSM/SSN/001_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/SSM/SSN/001_DEL
	DELETE
	2002 (DELETED)



7.2.2.18.4.2	CREATE Operation
TP/oneM2M/CSE/SSM/SSN/CRE/001
	TP Id
	TP/oneM2M/CSE/SSM/SSN/CRE/001

	Test objective
	Check that the IUT rejects CREATE request If the ruleLinks attribute is present in the resource representation, but the CSE-ID attribute is not present in the resource representation of <serviceSubscribedNode> resource

	Reference
	TS-0001 [1], clauses 9.6.20, TS-0004 [2], clause 7.4.20.2.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_IN_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE OPERATION on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to authorized AE‑ID  | |
                     | Content containing  | |
                     | serviceSubscribedNode resource containing  | |
                     | ruleLinks attribute set to valid value and  | |
                     | CSE‑ID attribute Not set  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD Request)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————+————-+
7.2.2.19	Primitive Profile (PP)
7.2.2.19.1	Basic Operation
TP/oneM2M/CSE/PP/001
	
TP Id
	TP/oneM2M/CSE/PP/001

	Test objective
	Check that IUT applies the referenced <primitiveProfile> over the request messages by adding the applicable parameters/attributes when the request message contains a valid Primitive Profile Identifier parameter and the referenced profile is accessible to the Hosting CSE

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a target resource at TARGET_RESOURCE_ADDRESS
and the AE having the privilege to perform OPERATION on
TARGET_RESOURCE_ADDRESS
and the IUT having a <primitiveProfile> resource at PRIMITIVE_PROFILE_ADDRESS
containing
additions attribute having list of attributes to be added
and AE having Retrieve privileges for the <primitiveProfile> resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | The IUT applies the profile by adding attributes defined in additions  | |
                     |attribute  | |
                     | and the IUT sends a valid Response to the AE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/PP/001_CRE
	CREATE

	TP/oneM2M/CSE/PP/001_RET
	RETRIEVE

	TP/oneM2M/CSE/PP/001_UPD
	UPDATE

	TP/oneM2M/CSE/PP/001_DEL
	DELETE



TP/oneM2M/CSE/PP/002
	
TP Id
	TP/oneM2M/CSE/PP/002

	Test objective
	Check that IUT applies the referenced < primitiveProfile_>_ over the request messages by deleting the applicable parameters/attributes when the request message contains a valid PrimitiveProfileIdentifier parameter and the referenced profile is accessible to the Hosting CSE

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a target resource at TARGET_RESOURCE_ADDRESS
and the AE having the privilege to perform OPERATION on
TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ at PRIMITIVE_PROFILE_ADDRESS containing
deletions attribute having list of attributes to be deleted
and AE having Retrieve privileges for the <primitiveProfile> resource
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | The IUT applies the profile by deleting attributes defined in deletions  | |
                     | and the IUT sends a valid Response to the AE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/PP/002_CRE
	CREATE

	TP/oneM2M/CSE/PP/002_RET
	RETRIEVE

	TP/oneM2M/CSE/PP/002_UPD
	UPDATE

	TP/oneM2M/CSE/PP/002_DEL
	DELETE



TP/oneM2M/CSE/PP/003
	
TP Id
	TP/oneM2M/CSE/PP/003

	Test objective
	Check that IUT applies the referenced < primitiveProfile_>_ over the request messages by replacing the applicable parameters/attributes when the request message contains a valid PrimitiveProfileIdentifier parameter and the referenced profile is accessible to the Hosting CSE

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a target resource at TARGET_RESOURCE_ADDRESS
and the AE having the privilege to perform OPERATION on
TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ at PRIMITIVE_PROFILE_ADDRESS containing
additions attribute having list of attributes to be replaced
and AE having Retrieve privileges for the <primitiveProfile> resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | the IUT receives a valid OPERATION Request from AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | The IUT applies the profile by replacing attributes defined in additions  | |
                     |attribute  | |
                     | and the IUT sends a valid Response to the AE  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/PP/003_CRE
	CREATE

	TP/oneM2M/CSE/PP/003_RET
	RETRIEVE

	TP/oneM2M/CSE/PP/003_UPD
	UPDATE

	TP/oneM2M/CSE/PP/003_DEL
	DELETE



TP/oneM2M/CSE/PP/004
	
TP Id
	TP/oneM2M/CSE/PP/004

	Test objective
	Check that the IUT rejects the request when the < primitiveProfile_>_ resource referenced by the PrimitiveProfileIdentifier parameter is not present

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a target resource at TARGET_RESOURCE_ADDRESS
and the AE having the retrieve privilege for <primitiveProfile> resource to perform
OPERATION_ on TARGET_RESOURCE_ADDRESS
and the IUT not having <primitiveProfile> resource
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | The IUT receives a valid OPERATION Request from AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not apply the primitive profile  | |
                     | and the IUTsends a valid Response containing  | |
                     | Response Status Code set to 41XX  | |
                     |(PRIMITIVE_PROFILE_NOT_ACCESSIBLE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/PP/004_CRE
	CREATE

	TP/oneM2M/CSE/PP/004_RET
	RETRIEVE

	TP/oneM2M/CSE/PP/004_UPD
	UPDATE

	TP/oneM2M/CSE/PP/004_DEL
	DELETE



TP/oneM2M/CSE/PP/005
	
TP Id
	TP/oneM2M/CSE/PP/005

	Test objective
	Check that the IUT rejects the request when the originator does not have retrieve privileges for < primitiveProfile_>_ resource referenced by the PrimitiveProfileIdentifier parameter

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2] 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a < primitiveProfile_>_ at PRIMITIVE_PROFILE_ADDRESS
and the AE not having the retrieve privilege for <primitiveProfile> resource to perform
OPERATION_ on TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | The IUT receives a valid OPERATION Request from AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not apply the primitive profile  | |
                     | and the IUTsends a valid Response containing  | |
                     | Response Status Code set to 41XX  | |
                     |(PRIMITIVE_PROFILE_NOT_ACCESSIBLE)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/PP/005_CRE
	CREATE

	TP/oneM2M/CSE/PP/005_RET
	RETRIEVE

	TP/oneM2M/CSE/PP/005_UPD
	UPDATE

	TP/oneM2M/CSE/PP/005_DEL
	DELETE



TP/oneM2M/CSE/PP/006
	
TP Id
	TP/oneM2M/CSE/PP/006

	Test objective
	Check that the IUT successfully processes the request without applying the profile when the attributes in the request do not match with the referenced < primitiveProfile_>_ resource attributes

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 6.6.3.5, 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a target resource at TARGET_RESOURCE_ADDRESS
and the AE having the retrieve privilege for resource <primitiveProfile> to perform
OPERATION_ on TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource at PRIMITIVE_PROFILE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | The IUT receives a valid OPERATION Request from AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | not matching with the <primitiveProfile> resource attributes  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT does not apply the primitive profile  | |
                     | and sends the request to TARGET_RESOURCE_ADDRESS  | |
                     | when the process is completed  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/PP/006_CRE
	CREATE

	TP/oneM2M/CSE/PP/006_RET
	RETRIEVE

	TP/oneM2M/CSE/PP/006_UPD
	UPDATE

	TP/oneM2M/CSE/PP/006_DEL
	DELETE



TP/oneM2M/CSE/PP/007
	
TP Id
	TP/oneM2M/CSE/PP/007

	Test objective
	Check that the IUT rejects the creation of <primitiveProfile> resource request when the request parameters or resource attributes defined in the additions and deletions attributes of the referenced <primitiveProfile> resource are not valid

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 60? (primitiveProfile)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code s et to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/PP/008
	
TP Id
	TP/oneM2M/CSE/PP/008

	Test objective
	Check that the IUT rejects the update request of <primitiveProfile> resource when the request parameters or resource attributes defined in the additions and deletions attributes of the referenced <primitiveProfile> resource are not valid

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform UPDATE operation on PRIMITIVE_PROFILE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource at PRIMITIVE_PROFILE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | The IUT receives a valid UPDATE Request from AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | To set to PRIMITIVE_PROFILE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT=> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/PP/009
	
TP Id
	TP/oneM2M/CSE/PP/009

	Test objective
	Check that the IUT rejects the creation of a <primitiveProfile> resource when a mutual exclusivity check is failed on the names of the attributes or parameters specified in the additions and, deletions attributes

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | The IUT receives a valid CREATE Request from AEcontaining | |
                     | Resource Type set to 60? (primitiveProfile) and  | |
                     | Content containing  | |
                     | primitiveProfile resource containing  | |
                     | additions attribute and  | |
                     | deletions attribute  | |
                     | not being mutually exclusive  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/PP/010
	
TP Id
	TP/oneM2M/CSE/PP/010

	Test objective
	Check that the IUT rejects the update request of <primitiveProfile> resource when a mutual exclusivity check is failed on the names of the attributes or parameters specified in the additions and deletions attributes

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource at PRIMITIVE_PROFILE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | The IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to PRIMITIVE_PROFILE_ADDRESS and  | |
                     | Content containing  | |
                     | additions attribute and  | |
                     | deletions attribute  | |
                     | not being mutually exclusive  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT=> AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/PP/011
	
TP Id
	TP/oneM2M/CSE/PP/011

	Test objective
	Check that the IUT rejects the creation of a <primitiveProfile > resource when a request contains non permissible or mandatory parameters specified in the additions and deletions attributes

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | The IUTreceives a valid CREATE Request from AE containing  | |
                     | To set to PRIMITIVE_PROFILE_ADDRESS and  | |
                     | Content containing  | |
                     | primitiveProfile resource containing  | |
                     | additions attribute indicating ADD_PARAMETER and  | |
                     | deletions attribute indicating DEL_PARAMETER   | |
                     | } | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | The IUT sends a valid Response containing  | |
                     | Response Status Code set to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/PP/012
	
TP Id
	TP/oneM2M/CSE/PP/012

	Test objective
	Check that the IUT rejects the UPDATE operation on resource <primitiveProfile> when a request contains non permissible or mandatory parameters specified in the additions and deletions attributes

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ at PRIMITIVE_PROFILE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | The IUTreceives a valid UPDATE Request from AE containing  | |
                     | To set to PRIMITIVE_PROFILE_ADDRESS and  | |
                     | Content containing  | |
                     | primitiveProfile resource containing  | |
                     | additions attribute indicating ADD_PARAMETER and  | |
                     | deletions attribute indicating DEL_PARAMETER   | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     | REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/PP/013
	
TP Id
	TP/oneM2M/CSE/PP/013

	Test objective
	Check that IUT successfully applies the < primitiveProfile_>_ to the notification (Notify request primitive) in case of nonBlockingRequestAsynch request having valid attribute PrimitiveProfileIdentifier

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS0004 [2], clause 7.5.1.2.5

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a resource representation at TARGET_RESOURCE_ADDRESS
and the IUT having received a valid nonBlockingRequestAsynch request containing
a valid Primitive Profile Identifier
and the IUT having a < primitiveProfile_>_ at PRIMITIVE_PROFILE_ADDRESS containing
additions attribute indicating ADD_PARAMETER and
deletions attribute indicating DEL_PARAMETER
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | The requested operation is completed  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | The IUT applies the < primitiveProfile_>_ to Notify request primitive by  | |
                     | adding ADD_PARAMETER  | |
                     | and deleting DEL_PARAMETER  | |
                     | and the IUT sends a valid NOTIFY request containing  | |
                     | content representation  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/PP/014
	
TP Id
	TP/oneM2M/CSE/PP/014

	Test objective
	Check that IUT successfully applies the < primitiveProfile_>_ to the response in case of nonBlockingRequestSynch request having valid Primitive Profile Identifier

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS0004 [2], clause 7.2.2.2

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
The IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having the <request> resource at REQUEST_RESOURCE_ADDRESS
and the IUT having received a valid nonBlockingRequestSynch request containing
a valid Primitive Profile Identifier
and the IUT having a < primitiveProfile_>_ at PRIMITIVE_PROFILE_ADDRESS containing
additions attribute indicating ADD_PARAMETER and
deletions attribute indicating DEL_PARAMETER
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | The IUTreceives a valid RETRIEVE Request from AE containing  | |
                     | To set to REQUEST_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT |
                     | the IUT applies the referenced < primitiveProfile_>_ to the response by  | |
                     | adding ADD_PARAMETER  | |
                     | and deleting DEL_PARAMETER  | |
                     | and the IUT sends a valid Response containing  | |
                     | Content containing  | |
                     | Response Status Codeset to 2XXXand Response Primitive  | |
                     |representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/PP/015
	
TP Id
	TP/oneM2M/CSE/PP/015

	Test objective
	Check that IUT successfully applies the < primitiveProfile_>_ to the notification request generated for the <subscription> resource

	Reference
	TS-0001 [1], clause 9.6.8, clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF03

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a valid < subscription_>_ resource containing
a primitiveProfileID attribute set to PRIMITIVE_PROFILE_ID
and AE having subscribed to the < subscription_>_ resource
and the IUT having a valid < primitiveProfile_>_ resource containing
resourceID attribute set to PRIMITIVE_PROFILE_IDand
additions attribute indicating ADD_PARAMETER and
deletions attribute indicating DEL_PARAMETER
}



·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | The IUT generates a valid notification request for a the _<subscription>  | |
                     |resource containing primitiveProfileID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT |
                     | The IUT applies the < primitiveProfile_>_ resource referenced in the  | |
                     | primitiveProfileID attribute to the generated notification by  | |
                     | adding ADD_PARAMETER  | |
                     | and deleting DEL_PARAMETER  | |
                     | and the IUT sends a valid NOTIFY request containing  | |
                     | content representation  | |
                     |} | |
+———————-+——————————————————————————————————————————–+————-+
TP/oneM2M/CSE/PP/016
	
TP Id
	TP/oneM2M/CSE/PP/016

	Test objective
	Check that the IUT retargets the request to the hosting CSE without applying the < primitiveProfile_>_ when the To parameter contains the hosting CSE-ID which is known by the IUT

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered to a Hosting CSE (H-CSE)
and the IUT having registered the AE
and the Hosting CSE having create a RESOURCE on TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform OPERATION on the Hosting CSE
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | the IUT receives a valid OPERATION Request from the AE containing  | |
                     | a valid Primitive Profile Identifier and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => H‑CSE |
                     | The IUT forwards the OPERATION Request to Hosting CSE without  | |
                     | applying the < primitiveProfile_>_ resource referenced in the  | |
                     | Primitive Profile Identifier  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/PP/016_CRE
	CREATE

	TP/oneM2M/CSE/PP/016_RET
	RETRIEVE

	TP/oneM2M/CSE/PP/016_UPD
	UPDATE

	TP/oneM2M/CSE/PP/016_DEL
	DELETE



TP/oneM2M/CSE/PP/017
	
TP Id
	TP/oneM2M/CSE/PP/017

	Test objective
	Check that IUT applies the referenced < primitiveProfile_>_ over the response messages by adding the applicable parameters/attributes when the originating AE specified a valid PrimitiveProfileIdentifier parameter in the corresponding request

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.12

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a RESOURCE at TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource containing
resourceID attribute set to PRIMITIVE_PROFILE_IDand
a valid additions attribute having list of attributes to be added
and AE having the privilege to perform OPERATION on TARGET_RESOURCE_ADDRESS
and the IUThaving received a valid OPERATION Request from the AE containing
a valid Primitive Profile Identifier and
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT receives a valid response from a resource containing  | |
                     | To set to AE_ID and  | |
                     | Fromset to TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT applies the referenced primitive profile by adding attributes  | |
                     |defined in additions attribute  | |
                     | and the IUTsends a valid Response to the AE  | |
                     | containing valid RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/PP/017_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/PP/017_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/PP/017_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/PP/017_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/PP/018
	
TP Id
	TP/oneM2M/CSE/PP/018

	Test objective
	Check that IUT applies the referenced < primitiveProfile_>_ over the response messages by deleting the applicable parameters/attributes when the originating AE specified a valid PrimitiveProfileIdentifier parameter in the corresponding request

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
The IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a RESOURCE at TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource containing
resourceID attribute set to PRIMITIVE_PROFILE_IDand
deletions attribute having list of attributes to be deleted
and AE having the privilege to perform OPERATION on TARGET_RESOURCE_ADDRESS
and the IUT having received a valid OPERATION Request from the AE containing
a valid Primitive Profile Identifier and
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT receives a valid response from a resource containing  | |
                     | To set to AE_ID and  | |
                     | Fromset to TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT applies the referenced primitive profile by deleting attributes defined in deletions attribute  | |
                     | and the IUTsends a valid Response to the AE  | |
                     | containing valid RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/PP/018_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/PP/018_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/PP/018_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/PP/018_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/PP/019
	
TP Id
	TP/oneM2M/CSE/PP/019

	Test objective
	Check that IUT applies the referenced < primitiveProfile_>_ over the response messages by replacing the applicable parameters/attributes when the originating AE specified a valid PrimitiveProfileIdentifier parameter in the corresponding request

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
The IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a RESOURCE at TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource containing
resourceID attribute set to PRIMITIVE_PROFILE_ID and
additions attribute having list of attributes to be replaced
and AE having the privilege to perform OPERATION on TARGET_RESOURCE_ADDRESS
and the IUT having received a valid OPERATION Request from the AE containing
a valid Primitive Profile Identifier and
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT receives a valid response from a resource containing  | |
                     | To set to AE_ID and  | |
                     | Fromset to TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT applies the referenced primitive profile by replacing attributes defined in additions attribute  | |
                     | and the IUTsends a valid Response to the AE  | |
                     | containing valid RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	RESOURCE_TYPE
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/PP/019_CRE
	CREATE
	2001 (CREATED)

	TP/oneM2M/CSE/PP/019_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/PP/019_UPD
	UPDATE
	2004 (UPDATED)

	TP/oneM2M/CSE/PP/019_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/PP/020
	
TP Id
	TP/oneM2M/CSE/PP/020

	Test objective
	Check that IUT successfully applies the <primitiveProfile> to the representation of the requested resource returned in the Content parameter of the response and If the Content parameter of the response includes nested representations of child resource(s) and their descendant(s), the Hosting CSE shall not apply the profile to these child resource(s) or descendant(s)

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.12

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
The IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the IUT having a RESOURCE at TARGET_RESOURCE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource containing
resourceID attribute set to PRIMITIVE_PROFILE_ID and
modifications attribute having list of attributes to be modified
and AE having the privilege to perform OPERATION on TARGET_RESOURCE_ADDRESS
and the IUT having received a valid OPERATION Request from the AE containing
a valid Primitive Profile Identifier and
To set to TARGET_RESOURCE_ADDRESS and
From set to AE_ID
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT |
                     | the IUT receives a valid response from a resource containing  | |
                     | To set to AE_ID and  | |
                     | Fromset to TARGET_RESOURCE_ADDRESS and  | |
                     | Result Content set to 4 (attributes and child resources) and  | |
                     | Content containing  | |
                     | Resource representation containing  | |
                     | nested representations of child resources and their descendants  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT applies the referenced primitive profile on the requested resource  | |
                     |representation and ignore the child resource(s) or descendant(s) of the  | |
                     |resource representation.  | |
                     | and the IUTsends a valid Response to the AE  | |
                     | containing valid RESPONSE_STATUS_CODE  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	RESOURCE_TYPE
	RESPONSE_STATUS_CODE

	TP/oneM2M/CSE/PP/020_RET
	RETRIEVE
	2000 (OK)

	TP/oneM2M/CSE/PP/020_DEL
	DELETE
	2002 (DELETED)



TP/oneM2M/CSE/PP/021
	
TP Id
	TP/oneM2M/CSE/PP/021

	Test objective
	Check that the IUT rejects the creation of <primitiveProfile> resource when the request parameters or resource attributes defined in the additions attribute have complex data type definition

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.2.1.2

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 60? (primitiveProfile)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | primitiveProfile resource containing   | |
                     | additions attribute indicating ADD_PARAMTER  | |
                     | having complex data type  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code s et to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/PP/022
	
TP Id
	TP/oneM2M/CSE/PP/022

	Test objective
	Check that the IUT rejects the creation of a <primitiveProfile> resource when any parameters specified in the additions attribute do not match the defined data types for the parameters

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | the IUTreceives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 60? (primitiveProfile) and  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing   | |
                     | primitiveProfile resource containing  | |
                     | additions attribute containing  | |
                     | an invalid ADD_PARAMETER attribute  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/PP/023
	
TP Id
	TP/oneM2M/CSE/PP/023

	Test objective
	Check that the IUT rejects the update request of a <primitiveProfile> resource when any parameters specified in the additions attribute do not match the defined data types for the parameters

	Reference
	TS-0001 [1], clause 9.6.73 and clause 10.2.25, TS-0004 [2], clause 7.3.3.1

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a hosting CSE
and the IUT having registered an AE
and the AE having the privilege to perform UPDATE operation on
PRIMITIVE_PROFILE_ADDRESS
and the IUT having a < primitiveProfile_>_ resource at PRIMITIVE_PROFILE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | the IUTreceives a valid UPDATE Request from AE containing  | |
                     | To set to PRIMITIVE_PROFILE_ADDRESSand  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | primitiveProfile resource containing   | |
                     | additions attribute containing  | |
                     | an invalid ADD_PARAMETER attribute  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41YY (PRIMITIVE_PROFILE_BAD  | |
                     |REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+————-+
7.2.2.20	Transaction Management(TMG)
7.2.2.20.1	CREATE Operation
TP/oneM2M/CSE/TMG/CRE/001
	TP Id
	TP/oneM2M/CSE/TMG/CRE/001

	Test objective
	Check that the IUT sets value of transactionControl to INITIAL during the creation of <transactionMgmt> resource

	Reference
	TS-0004 [2], clause 7.4.60.2.1 Recv-6.4 (a)

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE to perform CREATE operation
}



·                  +-+--------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 50 (transactionMgmt) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | transactionMgmt resource containing  | |
                     | requestPrimitives attribute set to  | |
                     | LIST_OF_REQUESTPRIMITIVES  | |
                     |} | |
·                  +-+--------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT creates the transactionMgmt resource  | |
                     | and the IUT sends Response Status Code set to 2001 (CREATED)  | |
                     | Content containing  | |
                     |transactionMgmt resource containing  | |
                     | transactionControl attribute set to  | |
                     | INITIAL  | |
                     |} | |
+———————-+-+——————————————————————————————————–+————-+
TP/oneM2M/CSE/TMG/CRE/002
	TP Id
	TP/oneM2M/CSE/TMG/CRE/002

	Test objective
	Check that the IUT rejects creation of <transactionMgmt> resource when From parameters contained in the requestPrimitives attribute of the received <transactionMgmt> resource is not AE1

	Reference
	TS-0004 [2], clause 7.4.60.2.1 Recv-6.4 (a)

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE1 to perform CREATE operation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 50 (transactionMgmt) and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transactionMgmt resource containing  | |
                     | requestPrimitives attribute set to LIST_OF_REQUESTPRIMITIVES containing  | |
                     | From set to AE2  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the transactionMgmt resource and  | |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/TMG/CRE/003
	TP Id
	TP/oneM2M/CSE/TMG/CRE/003

	Test objective
	Check that the IUT sets value of transactionControl to LOCK during the creation of <transaction> resource

	Reference
	TS-0004 [2], clause 7.4.61.2.1, Recv-6.4

	Parent Release
	Release 4

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource PARENT_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation
}



·                  +-------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 51 (transaction) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | transaction resource containing  | |
                     | requestPrimitive attribute set to REQUESTPRIMITIVE  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT creates the transaction resource  | |
                     | and the IUT sends Response Status Code set to 2001 (CREATED)  | |
                     | Content containing  | |
                     |transaction resource containing  | |
                     | transactionControl attribute set to  | |
                     | LOCK  | |
                     |} | |
+———————-+————————————————————————————————-+————-+
TP/oneM2M/CSE/TMG/CRE/004
	TP Id
	TP/oneM2M/CSE/TMG/CRE/004

	Test objective
	Check that the IUT rejects creation of <transaction> resource when From parameters contained in the requestPrimitive attribute of the received <transaction> resource is not AE1

	Reference
	TS-0004 [2], clause 7.4.60.2.1 Recv-6.4 (a)

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having registered the AE2
and the IUT having a resource PARENT_RESOURCE_ADDRESS allowing
the AE1 to perform CREATE operation
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 51 (transaction) and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transaction resource containing  | |
                     | requestPrimitive attribute set to REQUESTPRIMITIVE  | |
                     |containing  | |
                     | From set to AE2  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT does not create the transaction resource   | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/TMG/CRE/005
	TP Id
	TP/oneM2M/CSE/TMG/CRE/005

	Test objective
	Check that the IUT creates a <transaction> resource as child for each target resource contained in the requestPrimitives attribute when receiving a valid transactionMgmt create request

	Reference
	TS-0001 [2], clause 10.2.18.1

	Parent Release
	Release 4

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource PARENT_RESOURCE_ADDRESS
and the IUT having a resource TARGET_RESOURCE_ADDRESS
the AE having privileges to perform CREATE operation at
PARENT_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Contentcontaining  | |
                     | TransactionMgmt containing  | |
                     | requestPrimitives attribute containing  | |
                     | to set to TARGET_RESOURCE_ADDRESS  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | Valid transactionMgmt resource representation and IUT creates a  | |
                     |transaction resource as child of the target resource address  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————+————-+
7.2.2.20.2	UPDATE Operation
TP/oneM2M/CSE/TMG/UPD/001
	TP Id
	TP/oneM2M/CSE/TMG/UPD/001

	Test objective
	Check that the IUT rejects the update of transactionControl attribute of transactionMgmt resource when Originator of update request is not the creator of transactionMgmt resource

	Reference
	TS-0001 [4], clause 7.4.60.2.3, Recv-6.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE2
and the IUT having registered the AE1
and the IUT having a transactionMgmt resource at TARGET_RESOURCE_ADDRESS
containing
creator attribute set to AE2
and the AE1 having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transactionMgmt resource containing  | |
                     | transactionControl attribute set to TRANSACTION_CONTROL_VALUE  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103  | |
                     |(ORIGINATOR_HAS _NO_PRIVILEGE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————+————-+
TP/oneM2M/CSE/TMG/UPD/002
	TP Id
	TP/oneM2M/CSE/TMG/UPD/002

	Test objective
	Check that the IUT rejects update of transactionControl attribute of transactionMgmt resource when transactionMode is "CSE_CONTROLLED"

	Reference
	TS-0004 [4], clause 7.4.60.2.3, Recv-6.3

	Parent Release
	Release 4

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a transactionMgmt resource at TARGET_RESOURCE_ADDRESS
containing
creator attribute set to AE and
transactionMode set to "CSE_CONTROLLED"
}



·                  +--------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE and  | |
                     | Content containing  | |
                     | transactionMgmt resource containing  | |
                     | transactionControl attribute set to  | |
                     |TRANSACTION_CONTROL_VALUE_  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000  | |
                     |(BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————–+————-+
TP/oneM2M/CSE/TMG/UPD/003
	TP Id
	TP/oneM2M/CSE/TMG/UPD/003

	Test objective
	Check that the IUT rejects update of transactionMgmt resource when the transactionControl value in the request primitive does not transition to values specified in Table 10.2.18.1-1 of oneM2M TS-0001

	Reference
	TS-0001 [4], Table 10.2.18.1-1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having a transactionMgmt resource at TARGET_RESOURCE_ADDRESS containing
creator attribute set to AE1 and
transactionMode set to "CREATOR_CONTROLLED" and
transactionState set to TRANSACTION_STATE_VALUE
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transactionMgmt resource containing  | |
                     | transactionControl attribute set to  | |
                     | INVALID_CORRESPONDING_TRANSACTION_CONTROL_VALUE_  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4123  | |
                     |(ILLEGAL_TRANSACTION_STATE_TRANSITION_ATTEMPTED )  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————–+————-+
	TP Id
	TRANSACTION_STATE_VALUE
	INVALID_CORRESPONDING_TRANSACTION_CONTROL_VALUE

	TP/oneM2M/CSE/TMG/UPD/003_INI
	INITIAL
	EXECUTE, ABORT,COMMIT, INITIAL, ERROR

	TP/oneM2M/CSE/TMG/UPD/003_LOC
	LOCKED
	COMMIT, INITIAL, LOCK, ERROR

	TP/oneM2M/CSE/TMG/UPD/003_EXE
	EXECUTED
	INITIAL,LOCK, EXECUTE, ERROR

	TP/oneM2M/CSE/TMG/UPD/003_ERR
	ERROR
	LOCK, EXECUTE, COMMIT, ERROR

	TP/oneM2M/CSE/TMG/UPD/003_COM
	COMMITTED
	EXECUTE, ABORT,COMMIT, LOCK, ERROR

	TP/oneM2M/CSE/TMG/UPD/003_ABT
	ABORTED
	EXECUTE, ABORT,COMMIT, LOCK, ERROR



TP/oneM2M/CSE/TMG/UPD/004
	TP Id
	TP/oneM2M/CSE/TMG/UPD/004

	Test objective
	Check that the IUT successfully updates of transactionMgmt resource when transactionMode is "CREATOR_CONTROLLED" and the transactionControl value in the request primitive transitions to values specified in Table 10.2.18.1-1 of oneM2M TS-0001 and Originator of request matches creator attribute of transactionMgmt resource

	Reference
	TS-0001 [4], Table 10.2.18.1-1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having a transactionMgmt resource at TARGET_RESOURCE_ADDRESS
containing
creator attribute set to AE1 and
transactionMode set to "CREATOR_CONTROLLED" and
transactionState set to TRANSACTION_STATE_VALUE
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transactionMgmt resource containing  | |
                     | transactionControl attribute set to | |
                     | VALID_CORRESPONDING_TRANSACTION_CONTROL_VALUE_  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT updates the transactionMgmt resource  | |
                     | and the IUT sends a valid Response containing  | |
                     | Response Status Code set to 2004 (UPDATED)  | |
                     | Content containing  | |
                     | transactionMgmt resource containing  | |
                     | transactionControl attribute set to | |
                     |VALID_CORRESPONDING_TRANSACTION_CONTROL_VALUE  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	TRANSACTION_STATE_VALUE
	INVALID_CORRESPONDING_TRANSACTION_CONTROL_VALUE

	TP/oneM2M/CSE/TMG/UPD/004_INI
	INITIAL
	LOCK

	TP/oneM2M/CSE/TMG/UPD/004_LOC
	LOCKED
	EXECUTE, ABORT

	TP/oneM2M/CSE/TMG/UPD/004_EXE
	EXECUTED
	COMMIT, ABORT

	TP/oneM2M/CSE/TMG/UPD/004_ERR
	ERROR
	ABORT, INITIAL

	TP/oneM2M/CSE/TMG/UPD/004_COM
	COMMITTED
	INITIAL

	TP/oneM2M/CSE/TMG/UPD/004_ABT
	ABORTED
	INITIAL



TP/oneM2M/CSE/TMG/UPD/005
	TP Id
	TP/oneM2M/CSE/TMG/UPD/005

	Test objective
	Check that the IUT rejects the update of transactionControl attribute of transaction resource when Originator of update request is not the creator of transaction resource

	Reference
	TS-0001 [4], clause 7.4.61.2.3, Recv-6.3

	Parent Release
	Release 4

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE2
and the IUT having registered the AE1
and the IUT having a transaction resource at TARGET_RESOURCE_ADDRESS
containing
creator attribute set to AE2 and
the AE1 having privileges to perform UPDATE operation on the
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transaction resource containing  | |
                     | transactionControl attribute set to | |
                     |TRANSACTION_CONTROL_VALUE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS  | |
                     |_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/TMG/UPD/006
	TP Id
	TP/oneM2M/CSE/TMG/UPD/006

	Test objective
	Check that the IUT rejects update of transaction resource when the transactionControl value in the request primitive does not transition to values specified in Table 10.2.18.1-2 of oneM2M TS-0001

	Reference
	TS-0001 [4], Table 10.2.18.1-2

	Parent Release
	Release 4

	Config Id
	CF02

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having a transaction resource at TARGET_RESOURCE_ADDRESS
containing
creator attribute set to AE1 and
transactionState set to
TRANSACTION_STATE_VALUE
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transaction resource containing  | |
                     | transactionControl attribute set to  | |
                     |TRANSACTION_CONTROL_VALUE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS  | |
                     |_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————-+————-+
	TP Id
	TRANSACTION_STATE_VALUE
	INVALID_CORRESPONDING_TRANSACTION_CONTROL_VALUE

	TP/oneM2M/CSE/TMG/UPD/006_LOC
	LOCKED
	COMMIT, LOCK, ERROR

	TP/oneM2M/CSE/TMG/UPD/006_EXE
	EXECUTED
	INITIAL,LOCK, EXECUTE, ERROR

	TP/oneM2M/CSE/TMG/UPD/006_ERR
	ERROR
	EXECUTE,COMMIT, ERROR

	TP/oneM2M/CSE/TMG/UPD/006_COM
	COMMITTED
	EXECUTE, ABORT,COMMIT, ERROR

	TP/oneM2M/CSE/TMG/UPD/006_ABT
	ABORTED
	EXECUTE, ABORT,COMMIT, ERROR



TP/oneM2M/CSE/TMG/UPD/007
	TP Id
	TP/oneM2M/CSE/TMG/UPD/007

	Test objective
	Check that the IUT successfully updates of transaction resource when the transactionControl value in the request primitive transitions to values specified in Table 10.2.18.1-2 of oneM2M TS-0001 and Originator of request is matches creator attribute of transaction resource

	Reference
	TS-0001 [4], Table 10.2.18.1-1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE1
and the IUT having a transaction resource at TARGET_RESOURCE_ADDRESS
containing
creator attribute set to AE1 and
transactionState set to TRANSACTION_STATE_VALUE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE1 |
                     | the IUT receives a valid UPDATE Request from AE1 containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE1 and  | |
                     | Content containing  | |
                     | transaction resource containing  | |
                     | transactionControl attribute set to | |
                     |TRANSACTION_CONTROL_VALUE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE1 |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS  | |
                     |_NO_PRIVILEGE)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	TRANSACTION_STATE_VALUE
	INVALID_CORRESPONDING_TRANSACTION_CONTROL_VALUE

	TP/oneM2M/CSE/TMG/UPD/007_LOC
	LOCKED
	EXECUTE, ABORT

	TP/oneM2M/CSE/TMG/UPD/007_EXE
	EXECUTED
	COMMIT, ABORT

	TP/oneM2M/CSE/TMG/UPD/007_ERR
	ERROR
	ABORT, LOCK

	TP/oneM2M/CSE/TMG/UPD/007_COM
	COMMITTED
	LOCK

	TP/oneM2M/CSE/TMG/UPD/007_ABT
	ABORTED
	LOCK



7.2.2.20.3	DELETE Operation
TP/oneM2M/CSE/TMG/DEL/001
	TP Id
	TP/oneM2M/CSE/TMG/DEL/001

	Test objective
	Check that the IUT deletes RESOURCE_TYPE resource when transactionState is either "COMMITTED" or "ABORTED".

	Reference
	TS-0004 [2], clause 7.4.61.2.4 and 7.4.60.2.4

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having created a resource TARGET_RESOURCE_ADDRESS of type
RESOURCE_TYPE containing
transactionState set to "COMMITTED" or "ABORTED"
and the AE having privileges to perform DELETE operation on the resource
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------+-------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | no Content  | |
                     |} | |
·                  +--------------------------------------------------+-------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT deletes the RESOURCE_TYPE resource and sends a valid  | |
                     |Response containing Response Status Code set to 2002 (DELETED)  | |
                     |} | |
+———————-+————————————————–+————————————————————————————————-+————-+
	TP Id
	RESOURCE_TYPE

	TP/oneM2M/CSE/TMG/DEL/001_TRAM_COM
	50 (transactionMgmt)

	TP/oneM2M/CSE/TMG/DEL/001_TRAM_ABT
	50 (transactionMgmt)

	TP/oneM2M/CSE/TMG/DEL/001_TRAC_COM
	51 (transaction)

	TP/oneM2M/CSE/TMG/DEL/001_TRAC_ABT
	51 (transaction)



7.2.2.21	Resource Schedule (SCH)
7.2.2.21.1	BASIC Operation
TP/oneM2M/CSE/SCH/001
	TP Id
	TP/oneM2M/CSE/SCH/001

	Test objective
	Check that the IUT rejects the CREATE request for the <schedule> resource, with the networkCoordinated attribute set, when the parent resource is of type <subscription>

	Reference
	TS-0001 [1], clause 9.6.9, TS-0004 [2], clause 7.4.9.2

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a Hosting CSE
and the IUT having registered the AE
and the IUT having a <subscription> resource at TARGET_RESOURCE_ADDRESS
and AE having privileges to perform CREATE on TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid CREATE request from AE containing  | |
                     | Resource Type set to schedule  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID  | |
                     | Content containing  | |
                     | schedule resource containing  | |
                     | networkCoordinated attribute  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response to AE containing  |IUT => AE |
                     | Response Status Code set to 4102  | |
                     |(CONTENTS_UNACCEPTABLE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+


TP/oneM2M/CSE/SCH/002
	TP Id
	TP/oneM2M/CSE/SCH/002

	Test objective
	Check that the IUT rejects the UPDATE request for the <schedule> resource, with the networkCoordinated attribute set, when the parent resource is of type <subscription>

	Reference
	TS-0001 [1], clause 9.6.9, TS-0004 [2], clause 7.4.9.2

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a Hosting CSE
and the IUT having registered the AE
and the IUT having a <subscription> resource containing
a child resource <schedule> at TARGET_RESOURCE_ADDRESS
and AE having privileges to perform UPDATE on TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT <= AE |
                     | the IUT receives a valid UPDATE request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID  | |
                     | Content containing  | |
                     | schedule resource containing  | |
                     | networkCoordinated attribute  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid Response to AE containing  |IUT => AE  |
                     | Response Status Code set to 4102  | |
                     |(CONTENTS_UNACCEPTABLE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+


TP/oneM2M/CSE/SCH/003
	TP Id
	TP/oneM2M/CSE/SCH/003

	Test objective
	Check that the IUT delivers notifications for the subscribed-to events of the <subscription> resource according to the allowed time window specified in the scheduleElement of the associated child <schedule> resource

	Reference
	TS-0001 [1], clause 9.6.9, TS-0004 [2], clause 7.4.9.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT being a Hosting CSE
and the IUT having registered AE1 and AE2
and the IUT having a <container> resource at TARGET_RESOURCE_ADDRESS
and AE1 having privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
and AE2 having privileges to perform RETRIEVE operation on
TARGET_RESOURCE_ADDRESS
and AE2 having created a <subscription> resource for the <container> resource
and the IUT having a child resource <schedule> for the <subscription> resource containing
scheduleElement attribute set to SCHEDULE_TIME
and AE1 having UPDATED the <container> resource at
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |IUT |
                     | the SCHEDULE_TIME is reached  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     | the IUT sends a valid NOTIFY Request to the AE containing  |IUT => AE2  |
                     | Content containing  | |
                     | notification message containing  | |
                     | a valid notificationEvent attribute  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————-+————-+
7.2.2.22	Process Management(PMG)
7.2.2.22.1	CREATE Operation
TP/oneM2M/CSE/PMG/CRE/001
	TP Id
	TP/oneM2M/CSE/PMG/CRE/001

	Test objective
	Check that the IUT creates <processManagement> resource on the TARGET_RESOURCE_ADDRESS of type PARENT_RESOURCE_TYPE

	Reference
	TS-0004 [2] clause 7.4.XX.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to XX (processManagement) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 2001 (CREATED) and  | |
                     | Content containing  | |
                     | processManagement resource containing   | |
                     | processStatus attribute set to value "Disabled" and | |
                     |currentState set to NULL  | |
                     |} | |
+———————-+—————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/CRE/002
	TP Id
	TP/oneM2M/CSE/PMG/CRE/002

	Test objective
	Check that the IUT rejects create of <state> resource when processStatus attribute of parent <processManagement> has value not equal to "Disabled"

	Reference
	TS-0004 [2] clause 7.4.XX.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <processManagement> resource at TARGET_RESOURCE_ADDRESS
having processStatus attribute set to value not equal to "Disabled"
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +--------+-------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to XX (state) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource  | |
                     |} | |
·                  +--------+-------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+——–+——————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/CRE/003
	TP Id
	TP/oneM2M/CSE/PMG/CRE/003

	Test objective
	Check that the IUT rejects create of <state> resource when some referenced <state> resources in stateTransitions attribute don't exist

	Reference
	TS-0004 [2] clause 7.4.XX.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions



	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <processManagement> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                   +------------------------------------------------------+-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                       |when {   |IUT <= AE |
                      | the IUT receives a valid CREATE Request from AE containing  | |
                      | To set to TARGET_RESOURCE_ADDRESS and  | |
                      | Resource Type set to XX (state) and  | |
                      | From set to AE‑ID and  | |
                      | Content containing  | |
                      | state resource containing  | |
                      | stateTransitions attribute set to non‑existing state resources  | |
                      |} | |
·                   +------------------------------------------------------+-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                       |then {   |IUT => AE |
                      | the IUT sends valid Response to AE containing  | |
                      | Response Status Code set to 41xx  | |
                      |(INVALID_PROCESS_CONFIGURATION)  | |
                      |} | |
+———————–+——————————————————+——————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/CRE/004
	TP Id
	TP/oneM2M/CSE/PMG/CRE/004

	Test objective
	Check that the IUT rejects create of <state> resource when for some referenced <state> resources in stateTransitions attributes Originator don't have retrieve privilege

	Reference
	TS-0004 [2] clause 7.4.XX.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <processManagement> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to XX (state) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute set to state  | |
                     |resources on which Originator do not have retrieve privilege  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/CRE/005
	TP Id
	TP/oneM2M/CSE/PMG/CRE/005

	Test objective
	Check that the IUT rejects create of <state> resource when some referenced <state> resources in stateTransitions attributes are not child resources of parent <processManagement>

	Reference
	TS-0004 [2] clause 7.4.XX.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <processManagement> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to XX (state) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute set to some state resources not child  | |
                     |resources of TARGET_RESOURCE_ADDRESS resource  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 41xx | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/CRE/006
	TP Id
	TP/oneM2M/CSE/PMG/CRE/006

	Test objective
	Check that the IUT rejects create of <action> resource when resource referenced by ATTRIBUTE attribute doesn't exist

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | ATTRIBUTE set to not‑existing resourceID.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+———————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/CRE/006_SRI
	subjectResourceID

	TP/oneM2M/CSE/PMG/CRE/006_ORI
	objectResourceID




TP/oneM2M/CSE/PMG/CRE/007
	TP Id
	TP/oneM2M/CSE/PMG/CRE/007

	Test objective
	Check that the IUT rejects create of <action> resource when resource referenced by subjectResourceID attribute is not accessible to it

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | subjectResourceID set to non‑accessible resourceID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/CRE/009
	TP Id
	TP/oneM2M/CSE/PMG/CRE/009

	Test objective
	Check that the IUT rejects create of <action> resource when resource referenced by objectResourceID attribute is not accessible to it

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | objectResourceID set to non‑accessible resourceID  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/CRE/010
	TP Id
	TP/oneM2M/CSE/PMG/CRE/010

	Test objective
	Check that the IUT rejects create of <action> resource when From parameter in actionPrimitive attribute is not same as Originator of create request

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | valid value set in actionPrimitive containing  | |
                     | From parameter not same as Originator of create request  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/CRE/011
	TP Id
	TP/oneM2M/CSE/PMG/CRE/011

	Test objective
	Check that the IUT rejects create of <action> resource when evalMode attribute has value either "off" or "once" and evalControlParam attribute is also set

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | evalMode set to "off" or "once" and  | |
                     | evalControlParam also set.  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/CRE/012
	TP Id
	TP/oneM2M/CSE/PMG/CRE/012

	Test objective
	Check that the IUT rejects create of <action> resource when subject element of evalCriteria attribute is not an attribute of resource type referenced by subjectResourceID attribute

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having child <container> resource at CHILD_ADDRESS
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | subjectResourceID set to CHILD_ADDRESS  | |
                     | valid value set in evalCriteria attribute containing  | |
                     | subject element not matching CHILD_ADDRESS attributes  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/CRE/013
	TP Id
	TP/oneM2M/CSE/PMG/CRE/013

	Test objective
	Check that the IUT rejects create of <action> resource when subjectResourceID attribute not set and subject element of evalCriteria attribute is not an attribute of the parent resource type

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | subjectResourceID not set  | |
                     | valid value set in evalCriteria attribute containing  | |
                     | subject element not matching | |
                     |TARGET_RESOURCE_ADDRESS attributes  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/CRE/014
	TP Id
	TP/oneM2M/CSE/PMG/CRE/014

	Test objective
	Check that the IUT rejects create of <action> resource when threshold element of evalCriteria is outside value space of data type of subject element

	Reference
	TS-0004 [2] clause 7.4.73.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE operation on the resource a
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | evalCriteria attribute set and  | |
                     | subject element set and  | |
                     | threshold element set outside value space of data type of  | |
                     |subject attribute  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/CRE/015
	TP Id
	TP/oneM2M/CSE/PMG/CRE/015

	Test objective
	Check that the IUT rejects create of <action> resource when operator element of evalCriteria has invalid value

	Reference
	TS-0004 [2] clause 7.4.73.2.1, Table 6.3.4.2.86-1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the AE having privileges to perform CREATE on the resource at
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | Resource Type set to 63 (action) and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | evalCriteria attribute set and  | |
                     | operator set to invalid value  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/CRE/016
	TP Id
	TP/oneM2M/CSE/PMG/CRE/016

	Test objective
	Check that the IUT rejects create of <dependency> resource when resource defined by referencedResourceID attribute doesn't exist

	Reference
	TS-0004 [2] clause 7.4.74.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <action> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Resource Type set to 64 (dependency) and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | referencedResourceID set to not‑existing resourceID.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+———————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/CRE/017
	TP Id
	TP/oneM2M/CSE/PMG/CRE/017

	Test objective
	Check that the IUT rejects create of <dependency> resource when Originator doesn't have retrieve privilege on resource defined by referencedResourceID attribute

	Reference
	TS-0004 [2] clause 7.4.74.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <action> resource at TARGET_RESOURCE_ADDRESS
and the IUT having <container> resource at CHILD_ADDRESS not accessible to AE
and the AE having privileges to perform CREATE operation at TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Resource Type set to 64 (dependency) and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | referencedResourceID set to CHILD_ADDRESS.  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/CRE/018
	TP Id
	TP/oneM2M/CSE/PMG/CRE/018

	Test objective
	Check that the IUT rejects create of <dependency> resource when attribute referenced by subject element of evalCriteria attribute of request is not an attribute of resource type referenced by referencedResourceID attribute

	Reference
	TS-0004 [2] clause 7.4.74.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <action> resource at TARGET_RESOURCE_ADDRESS
and the IUT having <container> resource at CHILD_ADDRESS accessible to AE
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Resource Type set to 64 (dependency) and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | referencedResourceID set to CHILD_ADDRESS and  | |
                     | valid value set in evalCriteria containing  | |
                     | subject element set not to one of the attributes of CHILD_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/PMG/CRE/019
	TP Id
	TP/oneM2M/CSE/PMG/CRE/019

	Test objective
	Check that the IUT rejects create of <dependency> resource when value of threshold element of evalCriteria attribute is outside the value space of data type of subject element of evalCriteria

	Reference
	TS-0004 [2] clause 7.4.74.2.1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <action> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Resource Type set to 64 (dependency) and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | valid value set in evalCriteria containing  | |
                     | subject element set and  | |
                     | threshold element set to value outside value range of  | |
                     |referenced attribute data type of subject element  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/CRE/020
	TP Id
	TP/oneM2M/CSE/PMG/CRE/020

	Test objective
	Check that the IUT rejects create of <dependency> resource when value of operator element is invalid

	Reference
	TS-0004 [2] clause 7.4.74.2.1, Table 6.3.4.2.86

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having <action> resource at TARGET_RESOURCE_ADDRESS
and the AE having privileges to perform CREATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Resource Type set to 64 (dependency) and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | valid value set in evalCriteria containing  | |
                     | operator element set to invalid value  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends valid Response to AE containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————+————-+
7.2.2.22.2	DELETE Operation
TP/oneM2M/CSE/PMG/DEL/001
	TP Id
	TP/oneM2M/CSE/PMG/DEL/001

	Test objective
	Check that the IUT rejects delete of <processManagement> resource when the value of the processStatus attribute is not equal to "Disabled"

	Reference
	TS-0004 [2] clause 7.4.XX.2.4

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource <processManagement> at
TARGET_RESOURCE_ADDRESS, processStatus set not equal to "Disabled"
and the AE have privilege to perform DELETE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+——————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/DEL/002
	TP Id
	TP/oneM2M/CSE/PMG/DEL/002

	Test objective
	Check that the IUT rejects delete of <state> resource when the value of the stateActive attribute is equal to "true"

	Reference
	TS-0004 [2] clause 7.4.XX.2.4

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource <state> at TARGET_RESOURCE_ADDRESS, stateActive
set to "true"
and the AE have privilege to perform DELETE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+———————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/DEL/003
	TP Id
	TP/oneM2M/CSE/PMG/DEL/003

	Test objective
	Check that the IUT rejects delete of <state> resource when the value of the processStatus attribute of parent <processManagement> is not equal to "Disabled"

	Reference
	TS-0004 [2] clause 7.4.XX.2.4

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered the AE
and the IUT having a resource <processManagement> at PARENT_RESOURCE_ADDRESS, processStatus set not equal to "Disabled"
and the IUT having a resource <state> at TARGET _RESOURCE_ADDRESS
and the AE have privilege to perform DELETE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————–+————-+
7.2.2.22.3	UPDATE Operation
TP/oneM2M/CSE/PMG/UPD/001
	TP Id
	TP/oneM2M/CSE/PMG/UPD/001

	Test objective
	Check that the IUT rejects update of ATTRIBUTE attribute of <processManagement> resource when the processStatus attribute has value not equal to "Disabled"

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
and the IUT having a <processManagement> at TARGET_RESOURCE_ADDRESS having processStatus attribute set value not equal to "Disabled" and
the AE have privilege to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | ATTRIBUTE attribute containing valid value.  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/001_AC
	activateConditions

	TP/oneM2M/CSE/PMG/UPD/001_EC
	endConditions

	TP/oneM2M/CSE/PMG/UPD/001_IS
	InitialState




TP/oneM2M/CSE/PMG/UPD/002
	TP Id
	TP/oneM2M/CSE/PMG/UPD/002

	Test objective
	Check that the IUT rejects update of <processManagement> resource when originator does not have retrieve privilege on the resources or attributes referred by subject element of the evalCriteria of ATTRIBUTE attribute

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having < processManagement> resource at TARGET_RESOURCE_ADDRESS and
the AE having privileges to perform UPDATE operation at TARGET_RESOURCE_ADDRESS and
the IUT having a resource at SUBJECT_RESOURCE_ADDRESS and
the AE not having privileges to perform RETRIEVE operation at
SUBJECT_RESOURCE_ADDRESS.
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | ATTRIBUTE attribute containing  | |
                     | evalCriteria attribute containing  | |
                     | subject parameter set to SUBJECT_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code  | |
                     |set to 41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————–+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/002_AC
	activateConditions

	TP/oneM2M/CSE/PMG/UPD/002_EC
	endConditions




TP/oneM2M/CSE/PMG/UPD/003
	TP Id
	TP/oneM2M/CSE/PMG/UPD/003

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the resources or attributes referred by subject attribute of evalCriteria parameters of ATTRIBUTE attribute do not exist

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having <processManagement> resource at TARGET_RESOURCE_ADDRESS and
the AE having privileges to perform UPDATE operation at
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | ATTRIBUTE attribute containing  | |
                     | evalCriteria attribute containing  | |
                     | subject parameter set to UNAVAILABLE_RESOURCE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     |41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/003_AC
	activateConditions

	TP/oneM2M/CSE/PMG/UPD/003_EC
	endConditions




TP/oneM2M/CSE/PMG/UPD/004
	TP Id
	TP/oneM2M/CSE/PMG/UPD/004

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the evalCriteria of ATTRIBUTE has threshold element value not within the value space of the data type of the subject element

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <processManagement> resource at TARGET_RESOURCE_ADDRESS
and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS.
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | ATTRIBUTE attribute containing  | |
                     | evalCriteria element containing  | |
                     | threshold element set to invalid value  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     | 41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/004_AC
	activateConditions

	TP/oneM2M/CSE/PMG/UPD/004_EC
	endConditions




TP/oneM2M/CSE/PMG/UPD/005
	TP Id
	TP/oneM2M/CSE/PMG/UPD/005

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the evalCriteria of ATTRIBUTE has invalid value in operator attribute

	Reference
	TS-0004 [2] clause 7.4.XX.2.3, Table 6.3.4.2.86-1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource <processManagement> at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS.
}



·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | ATTRIBUTE attribute containing  | |
                     | evalCriteria attribute having  | |
                     | operator parameter set to invalid value.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     |41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+———————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/005_AC
	activateConditions

	TP/oneM2M/CSE/PMG/UPD/005_EC
	endConditions




TP/oneM2M/CSE/PMG/UPD/006
	TP Id
	TP/oneM2M/CSE/PMG/UPD/006

	Test objective
	Check that the IUT rejects update of initialState attribute of <processManagement> resource when referred <state> resource doesn't exist

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource <processManagement> at TARGET_RESOURCE_ADDRESS
and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS.
}



·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | initialState set to UNAVAILABLE STATE RESOURCE.  | |
                     |.  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to | |
                     |41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+———————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/007
	TP Id
	TP/oneM2M/CSE/PMG/UPD/007

	Test objective
	Check that the IUT rejects update of initialState attribute of <processManagement> resource when Originator does not have retrieve privilege on referenced <state> resource

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource <processManagement> at TARGET_RESOURCE_ADDRESS
and
the AE having privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS and
the IUT having a <state> resource at STATE_RESOURCE_ADDRESS and
the AE not having privileges to perform RETRIEVE operation at
STATE_RESOURCE_ADDRESS.

}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | initialState attribute set to STATE_RESOURCE_ADDRESS.  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to 41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/008
	TP Id
	TP/oneM2M/CSE/PMG/UPD/008

	Test objective
	Check that the IUT rejects update of initialState attribute of <processManagement> resource when the referred resource is not the child resource of <processManagement>

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource <processManagement> at TARGET_RESOURCE_ADDRESS and
the AE having privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS and
the IUT having a resource <processManagement> at TARGET_RESOURCE_ADDRESS2 and
the IUT having <state> resource at STATE_RESOURCE_ADDRESS as child resource of TARGET_RESOURCE_ADDRESS2.
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | initialState attribute set to STATE_RESOURCE_ADDRESS  | |
                     |.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to 41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/009
	TP Id
	TP/oneM2M/CSE/PMG/UPD/009

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the value of the processControl attribute in the request is equal to "Enable" and the value of the processStatus attribute of the <processManagement> resource is equal to _PROCESS_STATUS VALUE

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having resource <processManagement> at TARGET_RESOURCE_ADDRESS
having,processStatus set equal to "PROCESS_STATUS_VALUE and
the AE having privilege to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS.
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | processControl attribute set to value "Enable".  | |
                     |.  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     | 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	PROCESS_STATUS_VALUE

	TP/oneM2M/CSE/PMG/UPD/009_EN
	Enabled

	TP/oneM2M/CSE/PMG/UPD/009_AC
	Activated

	TP/oneM2M/CSE/PMG/UPD/009_PU
	Paused

	TP/oneM2M/CSE/PMG/UPD/009_CM
	Completed

	TP/oneM2M/CSE/PMG/UPD/009_AB
	Aborted




TP/oneM2M/CSE/PMG/UPD/010
	TP Id
	TP/oneM2M/CSE/PMG/UPD/010

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the value of the processControl attribute in the request is equal to "Disable" and the value of the processStatus attribute of the <processManagement> resource is equal to "Disabled"

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having resource <processManagement> at TARGET_RESOURCE_ADDRESS, processStatus set to "Disabled" and
the AE having privilege to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS.
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | processControl attribute set to value "Disable".  | |
                     |.  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     | 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/011
	TP Id
	TP/oneM2M/CSE/PMG/UPD/011

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the value of the processControl attribute in the request is equal to "Pause" and the value of the processStatus attribute of the <processManagement> resource is equal to "_PROCESS_STATUS VALUE

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource <processManagement> at TARGET_RESOURCE_ADDRESS,
processStatus attribute set equal to _PROCESS_STATUS VALUE and
the AE having privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS.
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | processControl attribute set to value "Pause".  | |
                     |.  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     |4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	PROCESS_STATUS_VALUE

	TP/oneM2M/CSE/PMG/UPD/011_EN
	Enabled

	TP/oneM2M/CSE/PMG/UPD/011_DS
	Disabled

	TP/oneM2M/CSE/PMG/UPD/011_PU
	Paused

	TP/oneM2M/CSE/PMG/UPD/011_CM
	Completed

	TP/oneM2M/CSE/PMG/UPD/011_AB
	Aborted




TP/oneM2M/CSE/PMG/UPD/012
	TP Id
	TP/oneM2M/CSE/PMG/UPD/012

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the value of the processControl attribute in the request is equal to "Reactivate" and the value of the processStatus attribute of the <processManagement> resource is equal to "_PROCESS_STATUS VALUE "

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource <processManagement> at TARGET_RESOURCE_ADDRESS,
processStatus set equal to "_PROCESS_STATUS VALUE " and
the AE having privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS.
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | processControl attribute set to value "Reactivate".  | |
                     |.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     |4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————————————-+————-+
	TP Id
	PROCESS_STATUS_VALUE

	TP/oneM2M/CSE/PMG/UPD/012_EN
	Enabled

	TP/oneM2M/CSE/PMG/UPD/012_DS
	Disabled

	TP/oneM2M/CSE/PMG/UPD/012_AC
	Activated

	TP/oneM2M/CSE/PMG/UPD/012_CM
	Completed

	TP/oneM2M/CSE/PMG/UPD/012_AB
	Aborted




TP/oneM2M/CSE/PMG/UPD/013
	TP Id
	TP/oneM2M/CSE/PMG/UPD/013

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the value of the processControl attribute in the request is equal to "Enable" and the value of the processStatus attribute of the <processManagement> resource is equal to "Disabled" when any of the referenced child resources is not available

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having resource <processManagement> at TARGET_RESOURCE_ADDRESS,
processStatus attribute set to "Disabled" and
the IUT having <state> resource as child resource of TARGET_RESOURCE_ADDRESS
and referenced in initialState attribute and
the resource referenced by stateAction attribute is not available and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS.
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | processControl attribute set to value "Enable".  | |
                     |.  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     | 41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/014
	TP Id
	TP/oneM2M/CSE/PMG/UPD/014

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the value of the processControl attribute in the request is equal to "Enable" and the value of the processStatus attribute of the <processManagement> resource is equal to "Disabled" but Originator does not have required privileges on any of the referenced child resources

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having resource <processManagement> at TARGET_RESOURCE_ADDRESS
containing
processStatus attribute set to "Disabled" and
initialState attribute set to child <state> resource at STATE_ADDRESS containing
stateAction attribute set to child <action> resource at ACTION_ADDRESS and
the AE having privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
and
but AE not having privilege on STATE_ADDRESS and ACTION_ADDRESS.
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | processControl set to value "Enable".  | |
                     |.  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing Response Status Code set to  | |
                     |41xx (INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/015
	TP Id
	TP/oneM2M/CSE/PMG/UPD/015

	Test objective
	Check that the IUT rejects update of <processManagement> resource when the value of the processControl attribute in the request is equal to "Enable" and the value of the processStatus attribute of the <processManagement> resource is equal to "Disabled" but any of referenced resources are not descendent resource of <processManagement>

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having <state> resource at STATE and
the IUT having <action> resource at ACTION and
the IUT having resource <processManagement> at TARGET_RESOURCE_ADDRESS
containing
processStatus set to "Disabled" and
initialState attribute set to STATE and
stateAction attribute set to ACTION

the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS.
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | processManagement resource containing  | |
                     | processControl set to value "Enable".  | |
                     |.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to  | |
                     |41xx(INVALID_PROCESS_CONFIGURATION).  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/016
	TP Id
	TP/oneM2M/CSE/PMG/UPD/016

	Test objective
	Check that the IUT rejects update of <state> resource when the processStatus attribute of parent <processManagement> has value not equal to "Disabled"

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
and the IUT having a <processManagement> resource at PARENT_RESOURCE_ ADDRESS containing
processStatus attribute set not equal to "Disabled" and
and the IUT having a child <state> resource at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | ATTRIBUTE attribute containing valid value.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+————————————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/016_STAC
	stateAction

	TP/oneM2M/CSE/PMG/UPD/016_STTRS
	stateTransitions




TP/oneM2M/CSE/PMG/UPD/017
	TP Id
	TP/oneM2M/CSE/PMG/UPD/017

	Test objective
	Check that the IUT rejects update of <state> resource when the resource referenced by stateAction attribute does not exist

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateAction attribute value set to NON EXISTENT ACTION RESOURCE.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/018
	TP Id
	TP/oneM2M/CSE/PMG/UPD/018

	Test objective
	Check that the IUT rejects update of <state> resource when the Originator does not have retrieve privilege on resource referenced by stateAction attribute

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at PARENT_RESOURCE_ADDRESS and
the IUT having a child <action> resource ACTION_ADDRESS Originator not having retrieve
privilege of and
the AE have privilege to perform UPDATE operation on PARENT_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateAction attribute value set to ACTION_ADDRESS.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/019
	TP Id
	TP/oneM2M/CSE/PMG/UPD/019

	Test objective
	Check that the IUT rejects update of <state> resource when the resource referenced by stateAction attribute is not a child resource

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at TARGET_RESOURCE_ADDRESS and
the IUT having created RESOURCE_TYPE resource containing a child <action> resource at
ACTION_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateAction attribute value set to ACTION_ADDRESS.  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/020
	TP Id
	TP/oneM2M/CSE/PMG/UPD/020

	Test objective
	Check that the IUT rejects update of <state> resource when the any of <state> resources referenced by stateTransitions attribute doesn't exist

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute set to NON EXISTENT STATE  | |
                     |RESOURCE.  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/021
	TP Id
	TP/oneM2M/CSE/PMG/UPD/021

	Test objective
	Check that the IUT rejects update of <state> resource when for any of <state> resources referenced by stateTransitions attribute Originator doesn't have retrieve privilege

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at STATE_ADDRESS1 and
the IUT having a <state> resource at STATE_ADDRESS2 and
the AE having privilege to perform UPDATE operation on STATE_ADDRESS1
AE not having privileges to perform RETRIEVE operation on STATE_ADDRESS2

}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to STATE_ADDRESS1and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute value set to STATE_ADDRESS2.  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/022
	TP Id
	TP/oneM2M/CSE/PMG/UPD/022

	Test objective
	Check that the IUT rejects update of <state> resource when any of <state> resources referenced by stateTransitions attribute is not child resource of parent <processManagement>

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <processManagement> resource at PARENT_ADDRESS having
a child <state> resource at STATE_ADDRESS and
the IUT having a <processManagement> resource at PARENT_ADDRESS2 having
a child <state> resource at STATE_ADDRESS2 and
the AE have privilege to perform UPDATE operation on STATE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to STATE_ADDRESS and  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute indicating  | |
                     | nextState element set to STATE_ADDRESS2  | |
                     | .  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/023
	TP Id
	TP/oneM2M/CSE/PMG/UPD/023

	Test objective
	Check that the IUT rejects update of <state> resource when any of resources and attributes referenced by subject element of evalCriteria of stateTransitions attribute doesn't exist

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute set having some  | |
                     | evalCriteria' subject element set to NON‑EXISTING RESOURCES  | |
                     |AND ATTRIBUTES.  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/024
	TP Id
	TP/oneM2M/CSE/PMG/UPD/024

	Test objective
	Check that the IUT rejects update of <state> resource when Originator doesn't have retrieve privilege on any of resources and attributes referenced by subject element of evalCriteria of stateTransitions attribute

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
and
the AE not having privileges to perform RETRIEVE operation at
SUBJECT_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute containing  | |
                     | evalCriteria' subject element set to  | |
                     |SUBJECT_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/025
	TP Id
	TP/oneM2M/CSE/PMG/UPD/025

	Test objective
	Check that the IUT rejects update of <state> resource when threshold element of evalCriteria of stateTransitions attribute have value outside the value spaces of the data type of subject element

	Reference
	TS-0004 [2] clause 7.4.XX.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute containing  | |
                     | evalCriteria' threshold element set to outside range spaces of the  | |
                     |data type of subject element.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/026
	TP Id
	TP/oneM2M/CSE/PMG/UPD/026

	Test objective
	Check that the IUT rejects update of <state> resource when operator element of evalCriteria of stateTransitions attribute have invalid value

	Reference
	TS-0004 [2] clause 7.4.XX.2.3, Table 6.3.4.2.86-1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <state> resource at PARENT_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on PARENT_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | state resource containing  | |
                     | stateTransitions attribute containing  | |
                     | evalCriteria' operator element set to invalid value.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 41xx  | |
                     |(INVALID_PROCESS_CONFIGURATION)  | |
                     |} | |
+———————-+———————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/027
	TP Id
	TP/oneM2M/CSE/PMG/UPD/027

	Test objective
	Check that the IUT rejects update of <action> resource when resource referenced by ATTRIBUTE attribute doesn't exist

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at PARENT_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on PARENT_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | ATTRIBUTE attribute set to non‑existing resourceID.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+———————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/027_SRI
	subjectResourceID

	TP/oneM2M/CSE/PMG/UPD/027_DEP
	dependencies

	TP/oneM2M/CSE/PMG/UPD/027_ORI
	objectResourceID




TP/oneM2M/CSE/PMG/UPD/028
	TP Id
	TP/oneM2M/CSE/PMG/UPD/028

	Test objective
	Check that the IUT rejects update of <action> resource when resource referenced by ATTRIBUTE attribute is not accessible by Originator

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at PARENT_RESOURCE_ADDRESS and
the IUT having child <container> at CHILD_ADDRESS not accessible by AE and
the AE have privilege to perform UPDATE operation on PARENT_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to PARENT_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | ATTRIBUTE attribute set to CHILD_ADDRESS.  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————-+————-+
	TP Id
	ATTRIBUTE

	TP/oneM2M/CSE/PMG/UPD/028_SRI
	subjectResourceID

	TP/oneM2M/CSE/PMG/UPD/028_DEP
	Dependencies

	TP/oneM2M/CSE/PMG/UPD/028_ORI
	objectResourceID




TP/oneM2M/CSE/PMG/UPD/029
	TP Id
	TP/oneM2M/CSE/PMG/UPD/029

	Test objective
	Check that the IUT rejects update of <action> resource when any of <dependency> resources referenced by dependencies attribute are not child resources of this <action> resource

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS and
the IUT having another <action> at TARGET_RESOURCE_ADDRESS2 and
and IUT having <dependency> resource at DEPENDENCY_RESOURCE_ADDRESS as child
resource of TARGET_RESOURCE_ADDRESS2.

}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | dependencies attribute set to  | |
                     |DEPENDENCY_RESOURCE_ADDRESS.  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/030
	TP Id
	TP/oneM2M/CSE/PMG/UPD/030

	Test objective
	Check that the IUT rejects update of <action> resource when From parameter contained in actionPrimitive attribute not equal to Originator

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | actionPrimitive attribute's From element not equal AE‑ID.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/031
	TP Id
	TP/oneM2M/CSE/PMG/UPD/031

	Test objective
	Check that the IUT rejects update of <action> resource when request evalMode attribute has value EVAL_MODE_VALUE " and request evalControlParam attribute is also present

	Reference
	TS-0004 [2] clause 7.4.73is .2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS containing
noevalControlParam attribute and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | evalMode set to EVAL_MODE_VALUE and  | |
                     | evalControlParam is present.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————-+————-+
	TP Id
	EVAL_MODE_VALUE

	TP/oneM2M/CSE/PMG/UPD/031_OFF
	OFF

	TP/oneM2M/CSE/PMG/UPD/031_ONCE
	ONCE




TP/oneM2M/CSE/PMG/UPD/032
	TP Id
	TP/oneM2M/CSE/PMG/UPD/032

	Test objective
	Check that the IUT rejects update of <action> resource when request evalMode attribute has value EVAL_MODE_VALUE ,request evalControlParam attribute not present but evalControlParam within <action> resource has value set

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS containing a valid evalControlParam attribute and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | evalMode set to EVAL_MODE_VALUE and  | |
                     | evalControlParam is not present  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————+————-+
	TP Id
	EVAL_MODE_VALUE

	TP/oneM2M/CSE/PMG/UPD/032_OFF
	OFF

	TP/oneM2M/CSE/PMG/UPD/032_ONCE
	ONCE




TP/oneM2M/CSE/PMG/UPD/033
	TP Id
	TP/oneM2M/CSE/PMG/UPD/033

	Test objective
	Check that the IUT rejects update of <action> resource when value of subject element of evalCriteria attribute of request is not one of the attribute of referenced resource of subjectResourceID attribute of request

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS, subjectResourceID not set
and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
and
IUT having a resource at RESOURCE_ADDRESS not having attribute ATTRIBUTE
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | subjectResourceID set to RESOURCE_ADDRESS and  | |
                     | evalCriteria attribute containing  | |
                     | subject element set to ATTRIBUTE.  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/034
	TP Id
	TP/oneM2M/CSE/PMG/UPD/034

	Test objective
	Check that the IUT rejects update of <action> resource when value of subject element of evalCriteria attribute of request is not one of the attribute of referenced resource of subjectResourceID attribute of <action>

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
IUT having a resource at RESOURCE_ADDRESS not having attribute ATTRIBUTE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS containing
subjectResourceID set to RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing   | |
                     | evalCriteria attribute containing  | |
                     | subject element set to ATTRIBUTE  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/035
	TP Id
	TP/oneM2M/CSE/PMG/UPD/035

	Test objective
	Check that the IUT rejects update of <action> resource when value of subject element of evalCriteria attribute of request is not one of the attribute of parent resource

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
AE not having attribute ATTRIBUTE and
the AE having a child <action> at TARGET_RESOURCE_ADDRESS and
havingsubjectResourceID not set and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | subjectResourceID not set and  | |
                     | valid value set in evalCriteria containing  | |
                     | subject element value set to ATTRIBUTE  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/PMG/UPD/036
	TP Id
	TP/oneM2M/CSE/PMG/UPD/036

	Test objective
	Check that the IUT rejects update of <action> resource when value of subject element of evalCriteria attribute of target <action> resource is not one of the attribute of resource referenced by request subjectResourceID attribute

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource at RESOURCE_ADDRESS not having attribute ATTRIBUTE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS containing evalCriteria
having subject element set to ATTRIBUTE and
the AE having privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | subjectResourceID set to RESOURCE_ADDRESS  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/037
	TP Id
	TP/oneM2M/CSE/PMG/UPD/037

	Test objective
	Check that the IUT rejects update of <action> resource when value of threshold element of evalCriteria is not within value space of the data type of subject element of evalCriteria attribute

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | valid value set in evalCriteria containing  | |
                     | subject element set to ATTRIBUTE and  | |
                     | threshold element value outside value range of ATTRIBUTE data type.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/038
	TP Id
	TP/oneM2M/CSE/PMG/UPD/038

	Test objective
	Check that the IUT rejects update of <action> resource when value of operator element of evalCriteria has invalid value

	Reference
	TS-0004 [2] clause 7.4.73.2.3 , Table 6.3.4.2.86-1

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <action> at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | action resource containing  | |
                     | valid value set in evalCriteria containing  | |
                     | operator element set to invalid value.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————-+————-+

TP/oneM2M/CSE/PMG/UPD/039
	TP Id
	TP/oneM2M/CSE/PMG/UPD/039

	Test objective
	Check that the IUT rejects update of <dependency> resource when value present in subject element of evalCriteria of request is not an attribute of resource type referenced by referencedResourceID attribute

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a resource at RESOURCE_ADDRESS not having attribute ATTRIBUTE and
the IUT having a <dependency> at TARGET_RESOURCE_ADDRESS, referencedResourceID set to RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | valid value set in evalCriteria containing  | |
                     | subject element set to ATTRIBUTE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/040
	TP Id
	TP/oneM2M/CSE/PMG/UPD/040

	Test objective
	Check that the IUT rejects update of <dependency> resource when value present in threshold element of evalCriteria attribute of request is not within value space of data type of subject element

	Reference
	TS-0004 [2] clause 7.4.73.2.3

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <dependency> at TARGET_RESOURCE_ADDRESS having referencedResourceID attribute set and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | valid value set in evalCriteria containing  | |
                     | subject element value set to ATTRIBUTE and  | |
                     | threshold element value set to value outside value range of data type of ATTRIBUTE.  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/PMG/UPD/041
	TP Id
	TP/oneM2M/CSE/PMG/UPD/041

	Test objective
	Check that the IUT rejects update of <dependency> resource when value of operator element of evalCriteria attribute of request is invalid

	Reference
	TS-0004 [2] clause 7.4.73.2.3 , Table 6.3.4.2.86

	Parent Release
	Release 4

	Config Id
	CF01

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state" and
the IUT having registered the AE and
the IUT having a <dependency> at TARGET_RESOURCE_ADDRESS and
the AE have privilege to perform UPDATE operation on TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | To set to TARGET_RESOURCE_ADDRESSand  | |
                     | From set to AE‑ID and  | |
                     | Content containing  | |
                     | dependency resource containing  | |
                     | evalCriteria attribute set containing  | |
                     | operator element set to invalid value.  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {   |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     |Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————-+————-+
7.2.2.23	Software Management(SM)
7.2.2.23.1	BASIC Operation
TP/oneM2M/CSE/SM/001
	TP Id
	TP/oneM2M/CSE/SM/001

	Test objective
	Check that the IUT rejects the creation request of <softwareCampaign> resource if target node referenced in softwareTargets attribute does not exist

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT not having the resource referenced in attribute softwareTargets
and the AE having the privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 61? (softwareCampaign)  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTargets attribute set to  | |
                     | INVALID_RESOURCE_ADDRESS  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+

TP/oneM2M/CSE/SM/002
	TP Id
	TP/oneM2M/CSE/SM/002

	Test objective
	Check that the IUT rejects creation of <softwareCampaign> resource when the AE does not have the privilege to perform operation on the resource referenced in softwareTargets attribute

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the AE not having the privileges to create [software] specialization child resource on the
resource referenced in softwareTargets attribute
and the AE having the privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 61? (softwareCampaign)  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTargets attribute set to  | |
                     | UNACCESSIBLE_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SM/003
	TP Id
	TP/oneM2M/CSE/SM/003

	Test objective
	Check that the IUT rejects creation of <softwareCampaign> resource if the resource referenced in softwareTriggerCriteria attribute does not exist

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT not having the resource referenced in attribute softwareTriggerCriteria
and the AE having the privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 61? (softwareCampaign)  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTriggerCriteria attribute containing  | |
                     | resources set to INVALID_RESOURCE_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SM/004
	TP Id
	TP/oneM2M/CSE/SM/004

	Test objective
	Check that the IUT rejects creation of <softwareCampaign> resource if the resource referenced in softwareTriggerCriteria attribute is not accessible by the AE

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the AE not having the privileges to perform CREATE operation on the resource
referenced in softwareTriggerCriteria attribute
and the AE having the privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 61? (softwareCampaign)  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTriggerCriteria attribute containing  | |
                     | resources set to UNACCESSIBLE_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SM/005
	TP Id
	TP/oneM2M/CSE/SM/005

	Test objective
	Check that the IUT rejects creation of <softwareCampaign> resource if it conflicts with any existing <softwareCampaign> resource in the hosting CSE

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT having a valid <softwareCampaign> resource containing
softwareTargets attribute set to SOFTWARE_TARGETS and
campaignEnabled set to TRUE
and the AE having the privileges to perform CREATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid CREATE Request from AE containing  | |
                     | Resource Type set to 61? (softwareCampaign)  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and   | |
                     | Content containing  | |
                     | softwareCompaign resource representation containing  | |
                     | softwareTargets attribute set to SOFTWARE_TARGETS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4105 (CONFLICT)  | |
                     |} | |
+———————-+——————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SM/006
	TP Id
	TP/oneM2M/CSE/SM/006

	Test objective
	Check that the IUT rejects UPDATE of <softwareCampaign> resource when the campaignStatus attribute is set to CANCELLING

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT having a <softwareCampaign> resource at TARGET_RESOURCE_ADDRESS
containing campaignStatus attribute set to CANCELLING
and the AE having the privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | Valid <softwareCampaign> resource representation} | |
·                  +-------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+————————————————————————————————————-+————-+
TP/oneM2M/CSE/SM/007
	TP Id
	TP/oneM2M/CSE/SM/007

	Test objective
	Check that the IUT rejects UPDATE of <softwareCampaign> resource when the campaignEnabled attribute is set to TRUE and attributes mentioned in the request do not match with the attribute values of existing targeted <softwareCampaign> resource

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT having a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE
and the AE having the privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | <softwareCampaign> resource representation containing  | |
                     | MANDATORY_ATTR not matching with the existing <softwareCampaign> attribute values  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
	Note: MANDATORY_ATTR can be softwareVersion, softwareName, softwareURL, softwareTargets, softwareTriggerCriteria, or softwareOperation.




TP/oneM2M/CSE/SM/008
	TP Id
	TP/oneM2M/CSE/SM/008

	Test objective
	Check that the IUT rejects the UPDATE request of <softwareCampaign> resource if target node referenced in softwareTargets attribute does not exist

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT having a <softwareCampaign> resource at TARGET_RESOURCE_ADDRESS
containing campaignEnabled attribute set to TRUE
and the AE having the privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTargets attribute set to INVALID_RESOURCE_ADDRESS  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+—————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/SM/009
	TP Id
	TP/oneM2M/CSE/SM/009

	Test objective
	Check that the IUT rejects UPDATE of <softwareCampaign> resource when the AE does not have the privilege to perform operation on the resource referenced in softwareTargets attribute

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUT having a <softwareCampaign> resource at TARGET_RESOURCE_ADDRESS

and the AE having the privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
and the AE not having the privileges to perform CREATE operation on NODE_RESOURCE_ADDRESS
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTargets attribute set to NODE_RESOURCE_ADDRESS  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41XX (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/SM/010
	TP Id
	TP/oneM2M/CSE/SM/010

	Test objective
	Check that the IUT rejects UPDATE of <softwareCampaign> resource if it conflicts with any existing <softwareCampaign> resource in the hosting CSE

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT having a <softwareCampaign> resource at SOFTWARE_RESOURCE_ADDRESS
containing
softwareTargets attribute set to SOFTWARE_TARGETS and
campaignEnabled set to TRUE
and the IUT having a <softwareCampaign> resource at TARGET_RESOURCE_ADDRESS
and the AE having the privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
and the IUT having the privileges to perform CREATE operation on SOFTWARE_TARGETS
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE‑ID and   | |
                     | Content containing  | |
                     | softwareCompaign resource representation containing  | |
                     | softwareTargets attribute set to SOFTWARE_TARGETS  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 41XX (SOFTWARE_CAMPAIGN_CONFLICT)  | |
                     |} | |
+———————-+——————————————————————————————————————————————+————-+
TP/oneM2M/CSE/SM/011
	TP Id
	TP/oneM2M/CSE/SM/011

	Test objective
	Check that the IUT rejects UPDATE of <softwareCampaign> resource if the resource referenced in softwareTriggerCriteria attribute does not exist

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT having a <softwareCampaign> resource at TARGET_RESOURCE_ADDRESS
containing
campaignEnabled attribute set to FALSE
and the AE having the privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTriggerCriteria attribute containing  | |
                     | subjectResourceID set to INVALID_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4000 (BAD_REQUEST)  | |
                     |} | |
+———————-+————————————————————————————————————————————-+————-+
TP/oneM2M/CSE/SM/012
	TP Id
	TP/oneM2M/CSE/SM/012

	Test objective
	Check that the IUT rejects UPDATE of <softwareCampaign> resource if the resource referenced in softwareTriggerCriteria attribute is not accessible by the AE

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUT having a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to FALSE
and the IUT having subject resource at SUBJECT_RESOURCE_ADDRESS
and the AE having the privileges to perform UPDATE operation on
TARGET_RESOURCE_ADDRESS
and the AE not having the privileges to perform CREATE operation on SUBJECT_RESOURCE_ADDRESS
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |IUT <= AE |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | softwareCampaign resource representation containing  | |
                     | softwareTriggerCriteria attribute containing  | |
                     | subjectResourceId set to SUBJECT_RESOURCE_ADDRESS  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4103 (ORIGINATOR_HAS_NO_PRIVILEGE)  | |
                     |} | |
+———————-+————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/SM/013
	TP Id
	TP/oneM2M/CSE/SM/013

	Test objective
	Check that the IUT sends the create request for [software] specialization resource on targeted CSE when IUT successfully creates a <softwareCampaign> resource with campaignEnabled attribute set to TRUE

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUT having privileges to perform CREATE operation on NODE_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |  |
                     | the IUT receives a valid CREATE request from AE containing  |AE => IUT |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to AE_ID and  | |
                     | Content containing  | |
                     | <softwareCampaign> resource representation containing  | |
                     | campaignEnabled attribute set to TRUE  | |
                     | softwareTargets attribute set to NODE_RESOURCE_ADDRESS  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |AE <= IUT   |
                     | the IUT sends a valid response to AE containing  |IUT => CSE  |
                     | Response status code set to 2001 (CREATED)  | |
                     |and the IUT sends a valid CREATE request to CSE containing  | |
                     | To set to NODE_RESOURCE_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | [software] specialization resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————–+————-+
TP/oneM2M/CSE/SM/014
	TP Id
	TP/oneM2M/CSE/SM/014

	Test objective
	Check that the IUT sends a CREATE request for <subscription> resource to the [software] specialization resource when the IUT has successfully creates the [software] specialization resource

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE
and the IUT sends a valid CREATE request to CSE containing
To set to NODE_RESOURCE_ADDRESS and
From set to CSE_ID and
Content containing
[software] specialization resource representation
}



·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |  |
                     | the IUT receives a valid Response containing  |IUT <= CSE |
                     | Response Status Code set to 2001(CREATED)  | |
                     |} | |
·                  +----------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |  |
                     |and the IUT sends a valid CREATE request to CSE containing  |IUT => CSE |
                     | To set to SOFTWARE_SPECIALIZATION_ADDRESS and  | |
                     | From set to CSE_ID and  | |
                     | Content containing  | |
                     | <subscription> resource representation  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/SM/015
	TP Id
	TP/oneM2M/CSE/SM/015

	Test objective
	Check that the IUT sets the individualSoftwareStatuses attribute of <softwareCampaign> resource to FAILURE when it is not able to subscribe to the [software] specialization

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE
and the CSEhaving a [software] specialization at
SOFTWARE_SPECIALIZATION_ADDRESS
and the IUT having sent a valid CREATE request to CSE containing
To set to SOFTWARE_SPECIALIZATION_ADDRESS and
From set to CSE_ID and
Content containing
<subscription> resource representation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 4000(BAD_REQUEST)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT |
                     | the IUT updates the <softwareCampaign> resource  | |
                     | individualSoftwareStatuses set to FAILURE for the corresponding [software] specialization  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/SM/016
	TP Id
	TP/oneM2M/CSE/SM/016

	Test objective
	Check that the IUT sets the individualSoftwareStatuses attribute of <softwareCampaign> resource to FAILURE when it is not able to create the [software] specialization

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE
and the IUT having sent a valid CREATE request to CSE containing
To set to NODE_RESOURCE_ADDRESS and
From set to CSE_ID
Content containing
[software] specialization resource representation
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 4000(BAD_REQUEST)  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT |
                     | the IUT updates the <softwareCampaign> resource  | |
                     | individualSoftwareStatuses set to FAILURE for the corresponding [software] specialization  | |
                     |} | |
+———————-+————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/SM/017
	TP Id
	TP/oneM2M/CSE/SM/017

	Test objective
	Check that the IUT sets the individualSoftwareStatuses attribute of <softwareCampaign> resource to FAILURE when it is not able to update the corresponding [software] specialization

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE
and the CSEhaving a [software] specialization at
NODE_RESOURCE_ADDRESS
and the IUT having sent a valid UPDATE request to CSE containing
To set to SOFTWARE_SPECIALIZATION_ADDRESS and
From set to CSE_ID
Content containing
[software] specialization resource representation
}



·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE => IUT |
                     | the IUT receives a valid Response containing  | |
                     | Response Status Code set to 4000(BAD_REQUEST)  | |
                     |} | |
·                  +--------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT |
                     | the IUT updates the <softwareCampaign> resource  | |
                     | individualSoftwareStatuses set to FAILURE for the corresponding [software] specialization  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————–+————-+

TP/oneM2M/CSE/SM/018
	TP Id
	TP/oneM2M/CSE/SM/018

	Test objective
	Check that the IUT rejects the UPDATE <softwareCampaign> request to set the campaignEnabled attribute of <softwareCampaign> resource to FALSE when its local policy is not to cancel the ongoing software management operations

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE and
campaignStatus attribute set to INITIATED and
softwareOperationset to 1(INSTALL)
and the IUT having the local policy to not cancel the ongoing software management operations
and the CSEhaving a [software] specialization at
SOFTWARE_SPECIALIZATION_ADDRESS containing
install set to TRUE
}



·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | <softwareCampaign> resource representationcontaining  | |
                     | campaignEnabled set to FALSE  | |
                     |} | |
·                  +------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4XXX  | |
                     |} | |
+———————-+————————————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/SM/019
	
TP Id
	TP/oneM2M/CSE/SM/019

	Test objective
	Check that the IUT tries to cancel the ongoing software management operation upon receiving an UPDATE <softwareCampaign> request with campaignEnabled attribute set to FALSE when local policy of the IUT is to try to cancel the ongoing software management operations

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE and
campaignStatus attribute set to INITIATED and
softwareOperationset to 1(INSTALL)
and the CSEhaving a [software] specialization at
SOFTWARE_SPECIALIZATION_ADDRESS containing
install set to TRUE
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |AE => IUT |
                     | the IUT receives a valid UPDATE Request from AE containing  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID  | |
                     | Content containing  | |
                     | <softwareCampaign> resource representationcontaining  | |
                     | campaignEnabled set to FALSE  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE  |
                     | the IUT sends a valid UPDATE response to AE containing  |  |
                     | Response Status Code set to 2004 (UPDATED) and  |  |
                     | Content containing  |  |
                     | <softwareCampaign> resource representation containing  |  |
                     | campaignStatus attribute set to CANCELLING  |IUT=> CSE |
                     | and the IUT sends a valid UPDATE Request to CSE containing  | |
                     | Toset to SOFTWARE_SPECIALIZATION_ADDRESSand  | |
                     | From set to CSE_ID  | |
                     | Content containing  | |
                     | [software] specialization resource representationcontaining  | |
                     | install set to FALSE  | |
                     |} | |
+———————-+—————————————————————————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/SM/020
	TP Id
	TP/oneM2M/CSE/SM/020

	Test objective
	Check that the IUT updates campaignStatus attribute of <softwareCampaign> resource based on the response to the update of targeted [software] specialization resource

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE and
campaignStatus attribute set to INITIATED and
SOFTWATE_OPERATIONset to TRUE
and the CSEhaving a [software] specialization at
SOFTWARE_SPECIALIZATION_ADDRESS containing
install set to TRUE
and the IUT having updated the <softwareCampaign> resource
containing
campaignEnabled set to FALSE
and the IUT having sent a valid UPDATE Request to CSE containing
Toset to SOFTWARE_SPECIALIZATION_ADDRESS and
From set to CSE_ID
Content containing
[software] specialization resource representationcontaining
install set to FALSE
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |CSE => IUT |
                     | the IUT receives a valid UPDATE Response from CSE containing  | |
                     | Response Status Code set to RESPONSE_FROM_CSE  | |
                     |} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT updates the <softwareCampaign> resource  | |
                     | campaignStatus attribute set to CAMPAIGN_STATUS  | |
                     |} | |
+———————-+———————————————————————————————————————————————————–+————-+
	TP Id
	RESPONSE_FROM_CSE
	CAMPAIGN_STATUS

	TP/oneM2M/CSE/SM/020/UPD
	2004
	CANCELLED

	TP/oneM2M/CSE/SM/020/NO_UPD
	4XXX
	STATUS_NOT_CANCELLABLE




TP/oneM2M/CSE/SM/021
	
TP Id
	TP/oneM2M/CSE/SM/021

	Test objective
	Check that the IUT sets the individualSoftwareStatuses attribute of <softwareCampaign> resource to FAILURE upon the deletion of [software] specialization and its child <subscription > resource when the expiration time of [software] specialization is exceeded before the completion of software operation

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE having a <node> resource at NODE_RESOURCE_ADDRESS
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attribute set to TRUE
and the CSEhaving a [software] specialization at
NODE_RESOURCE_ADDRESS containing
a child resource <subscription>
and the expiration time has exceeded for the [software] specialization
}



·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {  |CSE => IUT |
                     | the IUT receives a valid NOTIFY response containing  | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to CSE  | |
                     | Content containing  | |
                     | notification indicating deletion of [software] specialization and its child <subscription> resource  | |
                     |} | |
·                  +---------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT |
                     | the IUT updates the <softwareCampaign> resource  | |
                     | individualSoftwareStatuses set to FAILURE for the corresponding [software] specialization  | |
                     | and aggregatedSoftwareStatus set to FAILURE  | |
                     |} | |
+———————-+———————————————————————————————————————————————————————————————————————————————————————————————————+————-+

TP/oneM2M/CSE/SM/022
	TP Id
	TP/oneM2M/CSE/SM/022

	Test objective
	Check that the IUT sets the aggregatedSoftwareStatus attribute of <softwareCampaign> resource to FAILURE when the IUT receives the FAILURE notification from any one of the [software] specialization

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28

	Config Id
	CF02

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the CSE_1 having a <node> resource at NODE_RESOURCE_ADDRESS
and the CSE_2 having a <node> resource at NODE_RESOURCE_ADDRESS_2
and the IUT having a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
campaignEnabled attributeset to TRUE
and the CSE_1having a [software] specialization at
SOFTWARE_SPECIALIZATION_ADDRESS containing
install attributeset to TRUE and
a child resource <subscription>
and the CSE_2having a [software] specialization at
SOFTWARE_SPECIALIZATION_ADDRESS containing
install attributeset to TRUE and
a child resource <subscription>
and the IUT having received a valid NOTIFY Response containing
To set to TARGET_RESOURCE_ADDRESS and
From set to CSE_1 and
Content containing
[software] specialization resource representation containing
installStatus attribute set to SUCCESSFUL
}



·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |CSE_2 => IUT |
                     | the IUT receives a valid NOTIFY Response containing   | |
                     | To set to TARGET_RESOURCE_ADDRESS and  | |
                     | From set to CSE_2 and  | |
                     | Content containing  | |
                     | [software] specialization resource representation containing  | |
                     | installStatus attribute set to FAILURE  | |
                     |} | |
·                  +-------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT |
                     | the IUT updates the <softwareCampaign> resource  | |
                     | individualSoftwareStatus_1 attribute set to SUCCESSFUL  | |
                     | individualSoftwareStatus_2 attribute set to FAILURE  | |
                     | aggregatedSoftwareStatus attribute set to FAILURE  | |
                     | campaignStatus attribute set to FINISHED  | |
                     |} | |
+———————-+——————————————————————————————————————————————————————————————-+————-+

TP/oneM2M/CSE/SM/023
	TP Id
	TP/oneM2M/CSE/SM/023

	Test objective
	Check that the IUT rejects the deletion request when campaignStatus attribute of the <softwareCampaign> resource is set to CAMPAIGN_STATUS

	Reference
	TS-0001 [1], clause 9.6.76, 10.2.28, TS-0004 [2], clause 6.6.3.5, 7.4.XX

	Config Id
	CF01

	Parent Release
	Release 4

	PICS Selection
	PICS_CSE

	Initial conditions
	with {
the IUT being in the "initial state"
and the IUT having registered an AE
and the IUThaving a <softwareCampaign> resource at
TARGET_RESOURCE_ADDRESS containing
camapaignStatus attribute set to CAMPAIGN_STATUS
and the AE having the privileges to perform DELETE operation on
TARGET_RESOURCE_ADDRESS
}



·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |when {   |AE => IUT |
                     | the IUT receives a valid DELETE Request from AE containing  | |
                     | Toset to TARGET _RESOURCE_ADDRESS and  | |
                     | From set to AE_ID} | |
·                  +-----------------------------------------------------------------------------------------------------------------------------------+-------------+

·                      |then {  |IUT => AE |
                     | the IUT sends a valid Response containing  | |
                     | Response Status Code set to 4005 (OPERATION_NOT_ALLOWED)  | |
                     |} | |
+———————-+———————————————————————————————————————————–+————-+
	TP Id
	CAMPAIGN_STATUS

	TP/oneM2M/CSE/SM/0023/CANCEL
	CANCELLING

	TP/oneM2M/CSE/SM/0023/INITIATE
	INITIATED



Annex: A
Conformance Test Requirement
A.1	MQTT Protocol Conformance Test Requirement
	Test Items
	TS Chapter
	Obligation
	Condition for
Optional Item
	Checking point
	Fail condition



·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |TS‑0010, clause 5.1 |Mandatory | |"Retain" flag set as "0" |Fail if DUT sends with "Retain" flag=1 |
+————-+———-+———————+————–+————————————-+———————————————————————————————+————————————————-+ |Connection  |Connect |TS‑0010, clause 6.3 |Mandatory | |Prefix A:: or C:: is added to the ID |Fail if Prefix A:: or C:: are not added to the ID| |Items | | | | | | |
·         +          +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·             | |TS‑0010, clause 6.3 |Mandatory | |if Clean session (ex: Retain) flag is   |Fail when clean session is "True" when  |
            | | | | |set to "False" in CONNECT | DUT want to be connected |
·         +          +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·             | |TS‑0010, clause 6.3 |Mandatory | |if "Will Flag" is not set in CONNECT |Fail when will flag is enabled |
·         +----------+---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·             |Disconnect|TS‑0010 , clause 6.3 |Mandatory | |if Clean session (ex: Retain) flag is   |Fail when clean session is "False" when  |
            | | | | |set to "True" in CONNECT | DUT want to be disconnected |
+————-+———-+———————+————–+————————————-+———————————————————————————————+————————————————-+ |Subscription Items |TS‑0010, clause 5.1 |Mandatory | |if the message is set to Durable |Fail is the message is not Durable |
·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |TS‑0010, clause 6.4.4|Conditional |(for Initial Registration)  |if DUT's Initial ID assigning   |Fail if DUT's ID assigning is other than this |
                       | | |when Originator doesn't knows it's ID|/oneM2M/reg_req/<originator>/<receiver> oneM2M/reg_resp/<originator>/<receiver> | |
+————-+———-+———————+————–+————————————-+———————————————————————————————+————————————————-+ |Publish Item |TS‑0010,   |Conditional |when Originator knows   |if DUT's Initial ID assigning   |Fail if DUT's ID assigning is other than this | | |Figure 6.4.5‑2 | |it's ID | oneM2M/req/<Originator>/<Receiver> | |
·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |TS‑0010,   |Conditional |When Originator uses   |if DUT's Initial ID assigning oneM2M/req/+/<Receiver> |Fail if DUT's ID assigning is other than this |
                       |Figure 6.4.5‑2 | |wild card | | |
·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |MQTT v3.1.1 |Conditional | |if the has proper Primitive contents  |Fail if any of primitive contents feature wrong |
                       | | | | ("op", "fr", "to", "ri", "pc", "ty") | |
+————-+———-+———————+————–+————————————-+———————————————————————————————+————————————————-+ |Reception Item |TS‑0010,   |Conditional |when Originator knows   |if DUT's Initial ID assigning   |Fail if DUT's ID assigning is other than this | | |Figure 6.4.5‑2 | |it's ID |oneM2M/resp/<Originator>/<Receiver> | |
·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |TS‑0010,   |Conditional |When Originator uses   |if DUT's Initial ID assigning   |Fail if DUT's ID assigning is other than this |
                       |Figure 6.4.5‑2 | |wild card |oneM2M/resp/<Originator>/+ | |
·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |TS‑0010,   |Conditional | |server Delete received contents properly   |Fail if Receiver stores message |
                       |Figure 6.4.5‑2 | | |not storing data | |
·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |TS‑0010,   |Conditional | |If the receiver sends PubACK   |Fail if the receiver doesn't send PubACK |
                       |Figure 6.4.5‑2 | | |when receives messages | |
·                    +---------------------+--------------+-------------------------------------+---------------------------------------------------------------------------------------------+-------------------------------------------------+

·                        |MQTT v3.1.1 |Mandatory | |if the has proper Primitive contents  |Fail if any of primitive contents feature wrong |
                       | | | | ("op", "fr", "to", "ri", "pc", "ty") | |
+————-+———-+———————+————–+————————————-+———————————————————————————————+————————————————-+
<PAGE BREAK>
Annex <B>(Informative):
B.1	TP template
	TP Id
	

	Test objective
	

	Reference
	

	Config Id
	

	PICS Selection
	

	Initial conditions
	



·                  +---------------+-------------+

·                      |when {   |IUT <= AE |
                     |} | |
·                  +---------------+-------------+

·                      |then {   |IUT => AE |
                     |} | |
+———————-+—————+————-+
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